(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 70)
    (zones 0)
    (modules 32)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.254)
    (user_via 0.4 0.35)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.508 0.508)
    (pad_drill 0.254)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 93.3 105)
    (grid_origin -3.3 -2.25)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 /A0B0)
  (net 2 /A1B1)
  (net 3 /A2B2)
  (net 4 /A3B3)
  (net 5 /A4B4)
  (net 6 /A5B5)
  (net 7 /A6B6)
  (net 8 /A7B7)
  (net 9 /a0b0)
  (net 10 /a1b1)
  (net 11 /a2b2)
  (net 12 /a3b3)
  (net 13 /a4b4)
  (net 14 /a5b5)
  (net 15 /a6b6)
  (net 16 /a7b7)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0B0)
    (add_net /A1B1)
    (add_net /A2B2)
    (add_net /A3B3)
    (add_net /A4B4)
    (add_net /A5B5)
    (add_net /A6B6)
    (add_net /A7B7)
    (add_net /a0b0)
    (add_net /a1b1)
    (add_net /a2b2)
    (add_net /a3b3)
    (add_net /a4b4)
    (add_net /a5b5)
    (add_net /a6b6)
    (add_net /a7b7)
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 0.325 -9.11)
    (fp_text reference TP24 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 12 /a3b3))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 2.275 -4.11 180)
    (fp_text reference TP9 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 16 /a7b7))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 2.925 -9.11)
    (fp_text reference TP36 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 16 /a7b7))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 2.275 -9.11)
    (fp_text reference TP35 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 15 /a6b6))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 1.625 -9.11)
    (fp_text reference TP34 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 14 /a5b5))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 0.975 -9.11)
    (fp_text reference TP33 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 13 /a4b4))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -0.325 -4.11 180)
    (fp_text reference TP32 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 12 /a3b3))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -0.325 -9.11)
    (fp_text reference TP31 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 11 /a2b2))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -0.975 -9.11)
    (fp_text reference TP30 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 10 /a1b1))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -1.625 -9.11)
    (fp_text reference TP29 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 9 /a0b0))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 1.625 -4.11 180)
    (fp_text reference TP27 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 15 /a6b6))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 0.975 -4.11 180)
    (fp_text reference TP26 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 14 /a5b5))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 0.325 -4.11 180)
    (fp_text reference TP25 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 13 /a4b4))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -0.975 -4.11 180)
    (fp_text reference TP23 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 11 /a2b2))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -1.625 -4.11 180)
    (fp_text reference TP22 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 10 /a1b1))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -2.275 -4.11 180)
    (fp_text reference TP21 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 9 /a0b0))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -0.325 -2.25)
    (fp_text reference TP16 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 3 /A2B2))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 0.325 -2.25)
    (fp_text reference TP15 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 4 /A3B3))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 0.975 -2.25)
    (fp_text reference TP14 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 5 /A4B4))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 1.625 -2.25)
    (fp_text reference TP13 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 6 /A5B5))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 2.275 -2.25)
    (fp_text reference TP12 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 7 /A6B6))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 2.925 -2.25)
    (fp_text reference TP11 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 8 /A7B7))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 2.275 2.75 180)
    (fp_text reference TP9 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 8 /A7B7))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 1.625 2.75 180)
    (fp_text reference TP8 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 7 /A6B6))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 0.975 2.75 180)
    (fp_text reference TP7 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 6 /A5B5))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at 0.325 2.75 180)
    (fp_text reference TP6 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 5 /A4B4))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -0.325 2.75 180)
    (fp_text reference TP5 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 4 /A3B3))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -0.975 2.75 180)
    (fp_text reference TP4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 3 /A2B2))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -0.975 -2.25)
    (fp_text reference TP17 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 2 /A1B1))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -1.625 2.75 180)
    (fp_text reference TP3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 2 /A1B1))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -1.625 -2.25)
    (fp_text reference TP18 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 1 /A0B0))
  )
  (module tom-mechanical:Castellation_5.08_2.54 (layer F.Cu) (tedit 5E310190)
    (at -2.275 2.75 180)
    (fp_text reference TP2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.508 1.016) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 1 /A0B0))
  )
  (gr_text Feb2020 (at -0.3 -6.25) (layer B.SilkS))
  (gr_text Feb2020 (at -0.3 -0.25) (layer B.SilkS))
  (gr_text "ft245\nbypass" (at -0.3 -6.25) (layer F.SilkS))
  (gr_text "ft245\nbypass" (at -0.3 -0.25) (layer F.SilkS))
  (gr_line (start -3.3 -4.11) (end -3.3 -2.25) (layer Edge.Cuts) (width 0.254))
  (gr_line (start -3.29 -4.12) (end -3.31 -4.11) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -4.55 2.75) (end -3.3 2.75) (layer Edge.Cuts) (width 0.254))
  (gr_line (start -4.55 -9.11) (end -4.55 2.75) (layer Edge.Cuts) (width 0.254))
  (gr_line (start -3.3 -9.11) (end -4.55 -9.11) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 3.3 -4.11) (end -3.3 -4.11) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 3.3 -9.11) (end -3.3 -9.11) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 3.3 -4.11) (end 3.3 -9.11) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 3.3 2.75) (end 3.3 -2.25) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 3.3 2.75) (end -3.3 2.75) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 3.3 -2.25) (end -3.3 -2.25) (layer Edge.Cuts) (width 0.254))
)
