(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 7)
    (no_connects 0)
    (area 70.358 51.054 174.244 128.016)
    (thickness 1.6)
    (drawings 30)
    (tracks 85)
    (zones 0)
    (modules 10)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3302)
    (trace_clearance 0.762)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.524)
    (via_drill 0.6858)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad0)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad17A)")
  (net 10 "Net-(J1-Pad3V1)")
  (net 11 "Net-(J1-PadG2)")
  (net 12 "Net-(J1-PadPGM)")
  (net 13 "Net-(J1-PadDAC)")
  (net 14 "Net-(J1-Pad16)")
  (net 15 "Net-(J1-Pad17)")
  (net 16 "Net-(J1-PadG3)")
  (net 17 "Net-(J1-Pad22)")
  (net 18 "Net-(J1-PadVIN)")
  (net 19 "Net-(J1-Pad21)")
  (net 20 "Net-(J1-Pad20)")
  (net 21 "Net-(J1-Pad23)")
  (net 22 "Net-(J1-Pad14)")
  (net 23 "Net-(J1-Pad15)")
  (net 24 /CS)
  (net 25 /RST)
  (net 26 /GND)
  (net 27 /VIN)
  (net 28 "Net-(J1-Pad4)")
  (net 29 /Data)
  (net 30 /CLK)
  (net 31 /DC)
  (net 32 "Net-(J1-Pad18)")
  (net 33 "Net-(J1-Pad19)")
  (net 34 "Net-(J2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.762)
    (trace_width 0.3302)
    (via_dia 1.524)
    (via_drill 0.6858)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CLK)
    (add_net /CS)
    (add_net /DC)
    (add_net /Data)
    (add_net /GND)
    (add_net /RST)
    (add_net /VIN)
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad17A)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad3V1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadG2)")
    (add_net "Net-(J1-PadG3)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVIN)")
    (add_net "Net-(J2-Pad3)")
  )
  (module Wickerlib:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 5773172D)
    (at 102.997 82.423 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab))
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 57731797)
    (at 74.041 81.915 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module Wickerlib:TEENSY-LC (layer F.Cu) (tedit 57379CE3)
    (at 85.598 97.79)
    (fp_text reference J1 (at -10.16 25.4 180) (layer F.SilkS))
    (fp_text value TEENSY-LC (at -2.54 20.32 180) (layer F.Fab))
    (fp_text user "TEENSY LC" (at 2.54 25.4) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GND))
    (pad 0 thru_hole circle (at -10.16 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad0)"))
    (pad 1 thru_hole circle (at -10.16 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /Data))
    (pad 10 thru_hole circle (at -10.16 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CLK))
    (pad 11 thru_hole circle (at -10.16 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /DC))
    (pad 12 thru_hole circle (at -10.16 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /CS))
    (pad 17A thru_hole circle (at -7.62 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad17A)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad3V1)"))
    (pad G2 thru_hole circle (at -2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-PadG2)"))
    (pad PGM thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /RST))
    (pad 16 thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad16)"))
    (pad 3V2 thru_hole circle (at 5.08 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /VIN))
    (pad 18 thru_hole circle (at 5.08 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 5.08 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad17)"))
    (pad G3 thru_hole circle (at 5.08 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-PadG3)"))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J1-Pad19)"))
    (pad 23 thru_hole circle (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J1-Pad23)"))
    (pad 14 thru_hole circle (at 5.08 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad15)"))
  )
  (module Wickerlib:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 103.632 94.234)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0 -5.1) (layer F.SilkS))
    (fp_text value OLED_128x64 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /VIN))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /CS))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /RST))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /DC))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CLK))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /Data))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 572EAEC9)
    (at 103.124 122.809 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 572EAEC9)
    (at 99.187 97.917 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 572EAEC9)
    (at 84.328 100.076 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module Wickerlib:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 577317AE)
    (at 105.791 124.206 90)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 4.38912 90) (layer B.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 -6.56082 90) (layer B.Fab))
  )
  (module teensy-big-oled:oshw-1-front-silk-normal (layer B.Cu) (tedit 0)
    (at 88.265 118.11)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module oshpark:oshw (layer B.Cu) (tedit 0)
    (at 91.44 94.742 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (gr_text "drew@oshpark.com\n" (at 95.631 99.06 270) (layer F.SilkS))
  (gr_text "drew@oshpark.com\n" (at 90.17 129.54) (layer F.SilkS))
  (gr_text "drew@oshpark.com\n" (at 106.934 104.14 90) (layer B.SilkS))
  (gr_text drew@oshpark.com (at 70.2945 96.7105 90) (layer B.Mask))
  (gr_text drew@oshpark.com (at 70.2945 96.7105 90) (layer B.Cu))
  (gr_text drew@oshpark.com (at 90.043 82.931) (layer B.Cu))
  (gr_text "Drew Fustini\n" (at 86.995 80.01) (layer B.Mask))
  (gr_text "Drew Fustini\n" (at 86.995 80.137) (layer F.Mask))
  (gr_text "Drew Fustini\n" (at 82.677 109.982 270) (layer F.Mask))
  (gr_text "Drew Fustini\n" (at 71.882 103.632 270) (layer F.Mask))
  (gr_text "Drew Fustini" (at 71.882 103.632 270) (layer F.Cu))
  (gr_line (start 108.839 125.222) (end 108.839 81.915) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.453 125.857) (end 68.453 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 74.295 82.169) (end 68.453 82.423) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102.997 82.169) (end 102.743 76.327) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.597 76.327) (end 102.997 76.327) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.597 76.327) (end 73.533 76.327) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.822 131.445) (end 103.886 131.445) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.822 131.445) (end 74.422 131.445) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 74.295 125.603) (end 74.549 131.445) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102.997 125.603) (end 108.839 125.349) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 26) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.803 130.048) (xy 103.251 130.048) (xy 107.188 127.254) (xy 107.188 81.661) (xy 104.013 77.978)
        (xy 74.295 77.978) (xy 72.517 78.359) (xy 70.358 81.407) (xy 69.723 82.931) (xy 69.723 127.381)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.295 81.788) (xy 74.295 78.994) (xy 73.533 77.216) (xy 73.533 79.629) (xy 72.39 77.851)
        (xy 72.644 80.01) (xy 70.866 78.74) (xy 71.755 80.518) (xy 69.723 80.518) (xy 71.501 81.407)
        (xy 69.85 82.804) (xy 71.882 82.423) (xy 72.136 84.328) (xy 72.771 82.169) (xy 74.549 83.693)
        (xy 73.025 80.899) (xy 74.676 82.804) (xy 77.089 82.169) (xy 77.089 77.47) (xy 76.708 81.661)
        (xy 75.184 82.169) (xy 76.327 81.28) (xy 76.708 78.232) (xy 75.819 81.153) (xy 74.93 81.915)
        (xy 76.454 77.724) (xy 74.422 81.534) (xy 75.311 77.724)
      )
    )
  )
)
