(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 102)
    (no_connects 1)
    (area 38.323402 27.058619 48.583404 189.745658)
    (thickness 1.6)
    (drawings 31)
    (tracks 455)
    (zones 0)
    (modules 55)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 GND)
  (net 6 -12VA)
  (net 7 +12V)
  (net 8 "Net-(D1-Pad1)")
  (net 9 "Net-(D2-Pad2)")
  (net 10 "Net-(J3-Pad3)")
  (net 11 "Net-(J4-Pad3)")
  (net 12 "Net-(J5-Pad3)")
  (net 13 "Net-(J6-Pad3)")
  (net 14 "Net-(J7-Pad3)")
  (net 15 "Net-(J8-Pad3)")
  (net 16 out2)
  (net 17 out1)
  (net 18 "Net-(J12-Pad2)")
  (net 19 "Net-(J13-Pad2)")
  (net 20 "Net-(J2-Pad3)")
  (net 21 "Net-(J2-Pad2)")
  (net 22 "Net-(J3-Pad2)")
  (net 23 "Net-(J4-Pad2)")
  (net 24 "Net-(J5-Pad2)")
  (net 25 "Net-(J6-Pad2)")
  (net 26 "Net-(J7-Pad2)")
  (net 27 "Net-(J8-Pad2)")
  (net 28 "Net-(J10-Pad1)")
  (net 29 "Net-(J10-Pad2)")
  (net 30 "Net-(J11-Pad1)")
  (net 31 "Net-(J11-Pad2)")
  (net 32 "Net-(J16-Pad2)")
  (net 33 "Net-(J17-Pad2)")
  (net 34 "Net-(J1-Pad2)")
  (net 35 "Net-(J9-Pad2)")
  (net 36 "Net-(J16-Pad1)")
  (net 37 "Net-(J17-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net -12VA)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J11-Pad2)")
    (add_net "Net-(J12-Pad2)")
    (add_net "Net-(J13-Pad2)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J16-Pad2)")
    (add_net "Net-(J17-Pad1)")
    (add_net "Net-(J17-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J9-Pad2)")
    (add_net out1)
    (add_net out2)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5A3DEB85)
    (at 47.5615 152.9715 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.0635 0 180) (layer B.SilkS))
    (fp_text value 47p (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5A3DEAF1)
    (at 40.9575 185.1025 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.0635 -0.127 270) (layer B.SilkS))
    (fp_text value 47p (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A3DEA73)
    (at 41.021 159.385)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 0.0635 90) (layer F.SilkS))
    (fp_text value 22n (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 6 -12VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A3DEA56)
    (at 41.021 155.829)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 0.0635 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 6 -12VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A3DEA68)
    (at 41.021 157.607)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0.0635 0.0635 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 6 -12VA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A3DEA7F)
    (at 41.021 161.036 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -0.0635 270) (layer F.SilkS))
    (fp_text value 22n (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 7 +12V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A3DEA8A)
    (at 41.021 162.7505 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -0.0635 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 7 +12V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A3DEA95)
    (at 41.021 164.465 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0.0635 -0.0635 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 7 +12V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5A3DE967)
    (at 41.0845 153.8605)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 0.0635) (layer F.SilkS))
    (fp_text value 1N5819HW (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Mask)
      (net 6 -12VA))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5A3DE997)
    (at 41.021 166.3065 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0.0635 -0.0635 180) (layer F.SilkS))
    (fp_text value 1N5819HW (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at 0 -2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Mask)
      (net 7 +12V))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599D71)
    (at 46.99 88.9 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0.0635 0.0635 360) (layer B.SilkS))
    (fp_text value 21k5 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 19 "Net-(J13-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 13 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599D9B)
    (at 46.355 104.394 45)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -0.044901 0.044901 135) (layer B.SilkS))
    (fp_text value 43k9 (at 0 -1.75 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 45) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 19 "Net-(J13-Pad2)"))
    (pad 2 smd rect (at 1.35 0 45) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 14 "Net-(J7-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599DBD)
    (at 40.64 124.968 225)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 0 315) (layer B.SilkS))
    (fp_text value 167k (at 0 -1.75 225) (layer B.Fab))
    (fp_text user %R (at 0 0 225) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 225) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 19 "Net-(J13-Pad2)"))
    (pad 2 smd rect (at 1.35 0 225) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 15 "Net-(J8-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599CCB)
    (at 46.863 39.9415 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0.127 0 360) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 19 "Net-(J13-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 20 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599CF3)
    (at 46.609 50.9905 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0.0635 0 360) (layer B.SilkS))
    (fp_text value 10k3 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 19 "Net-(J13-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 10 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599D23)
    (at 46.863 63.8175 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0.0635 0 360) (layer B.SilkS))
    (fp_text value 11k3 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 19 "Net-(J13-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 11 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599D4E)
    (at 46.99 76.708 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0.0635 0 360) (layer B.SilkS))
    (fp_text value 14k1 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 19 "Net-(J13-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 12 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599D85)
    (at 46.0375 98.1075)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0.0635 0 90) (layer B.SilkS))
    (fp_text value 11k3 (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 18 "Net-(J12-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 13 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599DB0)
    (at 46.228 111.0615)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0.0635 0 90) (layer B.SilkS))
    (fp_text value 10k3 (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 18 "Net-(J12-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 14 "Net-(J7-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599CE2)
    (at 41.148 49.4665 45)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 0.089803 135) (layer B.SilkS))
    (fp_text value 167k (at 0 -1.75 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 45) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 18 "Net-(J12-Pad2)"))
    (pad 2 smd rect (at 1.35 0 45) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 20 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599D0A)
    (at 41.2115 62.4205 45)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -0.089803 135) (layer B.SilkS))
    (fp_text value 43k9 (at 0 -1.75 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 45) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 18 "Net-(J12-Pad2)"))
    (pad 2 smd rect (at 1.35 0 45) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 10 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599D3B)
    (at 41.148 74.803 45)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0.044901 -0.044901 135) (layer B.SilkS))
    (fp_text value 21k5 (at 0 -1.75 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 45) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 18 "Net-(J12-Pad2)"))
    (pad 2 smd rect (at 1.35 0 45) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 11 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599D61)
    (at 41.148 87.3125 45)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 0 135) (layer B.SilkS))
    (fp_text value 14k1 (at 0 -1.75 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 45) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 18 "Net-(J12-Pad2)"))
    (pad 2 smd rect (at 1.35 0 45) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 12 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A599DCE)
    (at 45.974 124.587)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0.127 0 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 18 "Net-(J12-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 15 "Net-(J8-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 5A3DEB35)
    (at 45.847 162.3695 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -0.0635 270) (layer B.SilkS))
    (fp_text value TL072 (at 0 -3.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 28 "Net-(J10-Pad1)"))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 33 "Net-(J17-Pad2)"))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 6 -12VA))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 7 +12V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 5A3DE9C0)
    (at 43.815 170.8785)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -0.381 -0.0635) (layer B.SilkS))
    (fp_text value TL072 (at 0 -3.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 30 "Net-(J11-Pad1)"))
    (pad 2 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 32 "Net-(J16-Pad2)"))
    (pad 3 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad 4 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 6 -12VA))
    (pad 5 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 5 GND))
    (pad 6 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 7 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 8 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Mask)
      (net 7 +12V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm (layer B.Cu) (tedit 5A3DE9D2)
    (at 39.8145 151.3205)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J15 (at -3.048 0.254) (layer B.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 1.27 -12.49) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A3DEA20)
    (at 46.1645 148.0185)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 0.0635 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 28 "Net-(J10-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 33 "Net-(J17-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A3DEBA5)
    (at 46.101 146.05)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 0 270) (layer B.SilkS))
    (fp_text value 10k (at 3.683 0.254) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 29 "Net-(J10-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 33 "Net-(J17-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A3DEAAD)
    (at 41.0845 180.9115 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 -0.0635 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 30 "Net-(J11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 32 "Net-(J16-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A3DEAC8)
    (at 41.0845 178.562 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 0 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 31 "Net-(J11-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 32 "Net-(J16-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A3DEB96)
    (at 46.0375 149.86 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at -0.0635 0 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 28 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A3DEADD)
    (at 40.9575 183.007)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0.127 0.0635 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 30 "Net-(J11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A3DEB5A)
    (at 44.958 153.289 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 0.0635 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 37 "Net-(J17-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A3DEB27)
    (at 44.2595 184.531 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at -0.0635 0 360) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 36 "Net-(J16-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A3DEB48)
    (at 45.974 156.6545)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at 0 0 90) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 37 "Net-(J17-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5A3DEB03)
    (at 46.6725 184.4675 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 0 -0.0635 360) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 36 "Net-(J16-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module modular:PJ301CM_OSH (layer F.Cu) (tedit 5A3DF026)
    (at 43.434 31.3055 270)
    (fp_text reference J1 (at 3.1115 4.2545 270) (layer F.SilkS))
    (fp_text value PJ301CM (at 0 -5.715 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.4 -0.8 270) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 0 4.5 270) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 17 out1))
    (pad 2 thru_hole circle (at 0 -3.3 270) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad2)"))
  )
  (module modular:PJ301CM_OSH (layer F.Cu) (tedit 5A3D71DB)
    (at 43.434 44.958 90)
    (fp_text reference J2 (at -1.9431 1.9304 90) (layer F.SilkS))
    (fp_text value PJ301CM (at 0 -5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.4 -0.8 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 0 4.5 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad3)"))
    (pad 2 thru_hole circle (at 0 -3.3 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad2)"))
  )
  (module modular:PJ301CM_OSH (layer F.Cu) (tedit 59D93D68)
    (at 43.434 57.658 90)
    (fp_text reference J3 (at 0 0 90) (layer F.SilkS))
    (fp_text value PJ301CM (at 0 -5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.4 -0.8 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 0 4.5 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 0 -3.3 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad2)"))
  )
  (module modular:PJ301CM_OSH (layer F.Cu) (tedit 59D93D68)
    (at 43.434 70.358 90)
    (fp_text reference J4 (at 0 0 90) (layer F.SilkS))
    (fp_text value PJ301CM (at 0 -5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.4 -0.8 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 0 4.5 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at 0 -3.3 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 23 "Net-(J4-Pad2)"))
  )
  (module modular:PJ301CM_OSH (layer F.Cu) (tedit 5A3D769D)
    (at 43.434 83.058 90)
    (fp_text reference J5 (at 0.127 -0.254 180) (layer F.SilkS))
    (fp_text value PJ301CM (at 0 -5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.4 -0.8 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 0 4.5 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad3)"))
    (pad 2 thru_hole circle (at 0 -3.3 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 24 "Net-(J5-Pad2)"))
  )
  (module modular:PJ301CM_OSH (layer F.Cu) (tedit 59D93D68)
    (at 43.434 95.1865 90)
    (fp_text reference J6 (at 0 0 90) (layer F.SilkS))
    (fp_text value PJ301CM (at 0 -5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.4 -0.8 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 0 4.5 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 13 "Net-(J6-Pad3)"))
    (pad 2 thru_hole circle (at 0 -3.3 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 25 "Net-(J6-Pad2)"))
  )
  (module modular:PJ301CM_OSH (layer F.Cu) (tedit 5A3D7691)
    (at 43.434 107.95 90)
    (fp_text reference J7 (at -1.143 0.254 90) (layer F.SilkS))
    (fp_text value PJ301CM (at 0 -5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.4 -0.8 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 0 4.5 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 14 "Net-(J7-Pad3)"))
    (pad 2 thru_hole circle (at 0 -3.3 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 26 "Net-(J7-Pad2)"))
  )
  (module modular:PJ301CM_OSH (layer F.Cu) (tedit 59D93D68)
    (at 43.434 120.65 90)
    (fp_text reference J8 (at 0 0 90) (layer F.SilkS))
    (fp_text value PJ301CM (at 0 -5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.4 -0.8 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 0 4.5 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 15 "Net-(J8-Pad3)"))
    (pad 2 thru_hole circle (at 0 -3.3 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 27 "Net-(J8-Pad2)"))
  )
  (module modular:PJ301CM_OSH (layer F.Cu) (tedit 59D93D68)
    (at 43.434 133.096 90)
    (fp_text reference J9 (at 0 0 90) (layer F.SilkS))
    (fp_text value PJ301CM (at 0 -5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.4 -0.8 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 0 4.5 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 16 out2))
    (pad 2 thru_hole circle (at 0 -3.3 90) (size 3.6 3.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 35 "Net-(J9-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 5A3DEB9F)
    (at 45.339 141.097 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J10 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value Conn_01x02 (at -5.969 -0.0635 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J10-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J10-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 5A3DEB0A)
    (at 44.7675 180.9115)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J11 (at 5.207 0) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 0 -4.87) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J11-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J11-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 47.3075 100.457 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J12 (at 0 2.33 90) (layer B.SilkS))
    (fp_text value Conn_01x03 (at 0 -7.41 90) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 out1))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J12-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 47.3075 113.157 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J13 (at 0 2.33 90) (layer B.SilkS))
    (fp_text value Conn_01x03 (at 0 -7.41 90) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 out2))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J13-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 47.117 175.5775 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J16 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J16-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J16-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 47.117 188.214 270)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J17 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J17-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J17-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module modular:2hp_align_stereo locked (layer F.Cu) (tedit 0)
    (at 43.4975 82.169)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch1.00mm (layer F.Cu) (tedit 59B55814)
    (at 39.5605 28.2575)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J14 (at 0 -1.56) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 1.56) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 17 out1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch1.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch1.00mm (layer F.Cu) (tedit 59B55814)
    (at 46.863 136.2075)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference J18 (at 0 -1.56) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 1.56) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 16 out2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch1.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "http://\nbenmoren.com" (at 38.989 136.271) (layer F.SilkS))
  (gr_text ":)" (at 44.1325 184.531 270) (layer F.SilkS))
  (gr_text ! (at 47.371 142.3035) (layer F.Mask))
  (gr_text ! (at 39.624 160.3375) (layer B.Mask))
  (gr_text ! (at 40.5765 37.7825) (layer B.Mask))
  (gr_text ! (at 39.878 38.862) (layer B.Mask))
  (gr_text ! (at 39.8145 36.8935) (layer B.Mask))
  (gr_text "ben moren\n& \nlaborcamp\n2018" (at 42.8625 29.464) (layer B.SilkS))
  (gr_text "2hp stereo\nrev2" (at 43.4975 29.7815) (layer F.SilkS))
  (gr_text "ben moren\n& \nlaborcamp\n2018" (at 43.8785 170.942) (layer F.SilkS))
  (gr_text "mxrbkpk | rev2" (at 45.212 155.956 90) (layer F.SilkS))
  (gr_text "red stripe" (at 41.148 140.081) (layer B.SilkS))
  (gr_line (start 48.533403 139.695428) (end 48.533403 189.695657) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 44.243037 139.695428) (end 48.533403 139.695428) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 44.243037 137.108391) (end 44.243037 139.695428) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.533403 137.108391) (end 44.243037 137.108391) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.533403 27.10862) (end 48.533403 137.108391) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 38.373403 27.10862) (end 48.533403 27.10862) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 38.373403 137.108391) (end 38.373403 27.10862) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.479148 137.108391) (end 38.373403 137.108391) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 42.479148 139.695428) (end 42.479148 137.108391) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 38.373403 139.695428) (end 42.479148 139.695428) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 38.373403 189.695657) (end 38.373403 139.695428) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.533403 189.695657) (end 38.373403 189.695657) (layer Edge.Cuts) (width 0.1))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.4505 27.1145) (xy 48.4505 189.738) (xy 38.4175 189.611) (xy 38.4175 27.051)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.514 189.738) (xy 38.4175 189.611) (xy 38.4175 27.305) (xy 48.4505 27.178)
      )
    )
  )
)
