(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 27)
    (tracks 35)
    (zones 0)
    (modules 10)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8128)
    (via_drill 0.4064)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.048 1.524)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 VCC)
  (net 4 GND)
  (net 5 +5V)
  (net 6 "Net-(M1-Pad5)")
  (net 7 "Net-(M1-Pad6)")
  (net 8 "Net-(M1-Pad2)")
  (net 9 "Net-(M1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad5)")
    (add_net "Net-(M1-Pad6)")
  )
  (net_class PWR ""
    (clearance 0.2032)
    (trace_width 0.508)
    (via_dia 1.016)
    (via_drill 0.5588)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net VCC)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 170.815 857.25)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.Fab))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 144.145 839.47)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.Fab))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 172.085 842.01)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "ZX Speccy:MH-M18" (layer F.Cu) (tedit 610785B3)
    (at 152.4 852.17)
    (fp_text reference M1 (at 0 1.27) (layer F.Fab))
    (fp_text value MH-M18 (at 0 0) (layer F.SilkS))
    (fp_text user +5V (at 8.89 -1.27) (layer F.SilkS))
    (fp_text user GND (at 8.89 1.27) (layer F.SilkS))
    (fp_text user L (at 8.89 3.81) (layer F.SilkS))
    (fp_text user R (at 8.89 6.35) (layer F.SilkS))
    (fp_text user MUTE (at 8.89 -3.81) (layer F.SilkS))
    (fp_text user KEY (at 8.89 -6.35) (layer F.SilkS))
    (pad 3 smd oval (at 10.795 -1.27) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 4 smd oval (at 10.795 1.27) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 5 smd oval (at 10.795 3.81) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(M1-Pad5)"))
    (pad 6 smd oval (at 10.795 6.35) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(M1-Pad6)"))
    (pad 2 smd oval (at 10.795 -3.81) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(M1-Pad2)"))
    (pad 1 smd oval (at 10.795 -6.35) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(M1-Pad1)"))
  )
  (module Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 172.085 850.265 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (fp_text reference C1 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.3) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L5.3mm_D2.2mm_P7.62mm_Horizontal_Vishay_IM-1 (layer F.Cu) (tedit 5AE59B05)
    (at 172.085 838.835 180)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.3*2.2mm^2, Vishay, IM-1, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 7.62mm  length 5.3mm diameter 2.2mm Vishay IM-1")
    (fp_text reference L1 (at 3.81 0) (layer F.SilkS))
    (fp_text value 100uH (at 3.81 2.22) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L5.3mm_D2.2mm_P7.62mm_Horizontal_Vishay_IM-1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5A02FF81)
    (at 166.37 850.265 270)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 3.175 -3.56 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(M1-Pad5)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 168.91 842.01 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 100k (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(M1-Pad5)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 166.37 847.09 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 2k2 (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 160.655 840.105 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at -2.54 -3.175) (layer F.SilkS))
    (fp_text value 100uF/6.3V (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "© KWF 2021" (at 145.415 859.155) (layer B.SilkS))
  (gr_text v.0.1 (at 149.86 837.565) (layer B.Cu))
  (dimension 33.02 (width 0.15) (layer Dwgs.User)
    (gr_text "1.3000 in" (at 157.48 832.455) (layer Dwgs.User))
    (feature1 (pts (xy 173.99 836.295) (xy 173.99 833.168579)))
    (feature2 (pts (xy 140.97 836.295) (xy 140.97 833.168579)))
    (crossbar (pts (xy 140.97 833.755) (xy 173.99 833.755)))
    (arrow1a (pts (xy 173.99 833.755) (xy 172.863496 834.341421)))
    (arrow1b (pts (xy 173.99 833.755) (xy 172.863496 833.168579)))
    (arrow2a (pts (xy 140.97 833.755) (xy 142.096504 834.341421)))
    (arrow2b (pts (xy 140.97 833.755) (xy 142.096504 833.168579)))
  )
  (dimension 24.13 (width 0.15) (layer Dwgs.User)
    (gr_text "0.9500 in" (at 178.465 848.36 90) (layer Dwgs.User))
    (feature1 (pts (xy 173.99 836.295) (xy 177.751421 836.295)))
    (feature2 (pts (xy 173.99 860.425) (xy 177.751421 860.425)))
    (crossbar (pts (xy 177.165 860.425) (xy 177.165 836.295)))
    (arrow1a (pts (xy 177.165 836.295) (xy 177.751421 837.421504)))
    (arrow1b (pts (xy 177.165 836.295) (xy 176.578579 837.421504)))
    (arrow2a (pts (xy 177.165 860.425) (xy 177.751421 859.298496)))
    (arrow2b (pts (xy 177.165 860.425) (xy 176.578579 859.298496)))
  )
  (gr_text Audio_OUT (at 165.1 845.82) (layer B.SilkS))
  (gr_text GND (at 165.1 844.55) (layer B.SilkS))
  (gr_text +5V (at 165.1 843.28) (layer B.SilkS))
  (gr_text "ZX-BT\naudio" (at 151.765 840.105) (layer F.SilkS))
  (gr_arc (start 170.815 857.25) (end 170.815 860.425) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 144.145 839.47) (end 144.145 836.295) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 172.72 837.565) (end 173.99 837.565) (angle -90) (layer Edge.Cuts) (width 0.05))
  (dimension 24.13 (width 0.15) (layer Dwgs.User)
    (gr_text "24.130 mm" (at 132.05 848.36 90) (layer Dwgs.User))
    (feature1 (pts (xy 140.97 836.295) (xy 132.763579 836.295)))
    (feature2 (pts (xy 140.97 860.425) (xy 132.763579 860.425)))
    (crossbar (pts (xy 133.35 860.425) (xy 133.35 836.295)))
    (arrow1a (pts (xy 133.35 836.295) (xy 133.936421 837.421504)))
    (arrow1b (pts (xy 133.35 836.295) (xy 132.763579 837.421504)))
    (arrow2a (pts (xy 133.35 860.425) (xy 133.936421 859.298496)))
    (arrow2b (pts (xy 133.35 860.425) (xy 132.763579 859.298496)))
  )
  (dimension 33.02 (width 0.15) (layer Dwgs.User)
    (gr_text "33.020 mm" (at 157.48 865.535) (layer Dwgs.User))
    (feature1 (pts (xy 173.99 860.425) (xy 173.99 864.821421)))
    (feature2 (pts (xy 140.97 860.425) (xy 140.97 864.821421)))
    (crossbar (pts (xy 140.97 864.235) (xy 173.99 864.235)))
    (arrow1a (pts (xy 173.99 864.235) (xy 172.863496 864.821421)))
    (arrow1b (pts (xy 173.99 864.235) (xy 172.863496 863.648579)))
    (arrow2a (pts (xy 140.97 864.235) (xy 142.096504 864.821421)))
    (arrow2b (pts (xy 140.97 864.235) (xy 142.096504 863.648579)))
  )
  (gr_line (start 140.97 860.425) (end 140.97 839.47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.815 860.425) (end 140.97 860.425) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 173.99 837.565) (end 173.99 857.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.145 836.295) (end 172.72 836.295) (layer Edge.Cuts) (width 0.05))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.355 859.79) (xy 148.59 859.79) (xy 148.59 836.93) (xy 173.355 836.93)
      )
    )
  )
)
