<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="46.99" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="21.59" x2="0" y2="0" width="0.1524" layer="20"/>
<wire x1="46.99" y1="0" x2="46.99" y2="21.59" width="0.1524" layer="20"/>
<wire x1="46.99" y1="21.59" x2="0" y2="21.59" width="0.1524" layer="20"/>
<text>D</text>
<text>PWR</text>
<text>IR</text>
<text>12</text>
<text>5</text>
<text>12</text>
<text>5</text>
<text>STAT</text>
<text>USB</text>
<text>Y1</text>
<text>ledkt_v1</text>
<text>(C) Blake Stratton
ledkt.hybridair.me
03.26.2016</text>
<text>B</text>
<text>R</text>
<text>G</text>
<text>+</text>
<text>-</text>
<text>D</text>
<text>-</text>
<text>+</text>
<text>D-</text>
<text>D+</text>
<text>HDD</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="silabs">
<description>Silicon Laboratories&lt;p&gt;
C8051Fxxx family of mixed-signal microcontrollers integrates world-class analog,&lt;br&gt;
a high-speed pipelined 8051 CPU, ISP Flash Memory,&lt;br&gt;
and on-chip JTAG based debug in each device.&lt;br&gt;
The combination of configurable high-performance analog,&lt;br&gt;
100 MIPS 8051 core and in-system field programmability provides the user with complete design flexibility,&lt;br&gt;
improved time-to-market, superior system performance and greater end product differentiation.&lt;p&gt;

Source: http://www.silabs.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MLP28">
<description>&lt;b&gt;MLP 28&lt;/b&gt;&lt;p&gt;
Source: www.silabs.com .. CP2101.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_2.54_SCREWTERM">
</package>
<package name="1X03_NO_SILK">
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="1X04_NO_SILK">
</package>
<package name="2X3">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-PTH">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="ar1logo">
<packages>
<package name="AR1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="silabs" package="MLP28" value="CP2102">
<attribute name="OC_FARNELL" value="9282130"/>
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="CP2102-GM"/>
<attribute name="OC_NEWARK" value="30K5635"/>
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="12V"/>
<element name="JP2" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="5V"/>
<element name="5VLED1" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="5VLED2" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="5VLED3" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="adafruit" package="TO220V" value="IRFZ44N">
<attribute name="NAME"/>
</element>
<element name="JP12" library="SparkFun-Connectors" package="USB-MICROB" value="USB-MICROB">
<attribute name="PROD_ID" value="CONN-09505"/>
</element>
<element name="JP13" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="12V_LED" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP15" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH"/>
<element name="R1" library="SparkFun-Passives" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="330">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="330">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0805" value="330">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="5V_PWR" library="adafruit" package="CHIPLED_0805" value="RED"/>
<element name="STAT" library="adafruit" package="CHIPLED_0805" value="GREEN"/>
<element name="12V_PWR" library="adafruit" package="CHIPLED_0805" value="RED"/>
<element name="Q1" library="adafruit" package="TO220V" value="IRFZ44N">
<attribute name="NAME"/>
</element>
<element name="Q3" library="adafruit" package="TO220V" value="IRFZ44N">
<attribute name="NAME"/>
</element>
<element name="5VLED4" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="5VLED5" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="5VLED6" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="5VLED7" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="5VLED8" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="5VLED9" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="1000uF">
<attribute name="NAME"/>
</element>
<element name="IR" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="RESONATOR-PTH" value=""/>
<element name="U$1" library="ar1logo" package="AR1" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP2" pad="P1"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="JP15" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="EXP"/>
<contactref element="U2" pad="M"/>
<contactref element="C8" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="JP12" pad="GND"/>
<contactref element="JP12" pad="MT1"/>
<contactref element="JP12" pad="MT2"/>
<contactref element="JP13" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="IR" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q1" pad="3"/>
<contactref element="STAT" pad="C"/>
<contactref element="JP1" pad="P2"/>
<contactref element="5VLED8" pad="1"/>
<contactref element="5VLED9" pad="1"/>
<contactref element="5VLED6" pad="1"/>
<contactref element="5VLED7" pad="1"/>
<contactref element="5VLED5" pad="1"/>
<contactref element="5VLED4" pad="1"/>
<contactref element="5VLED2" pad="1"/>
<contactref element="5VLED3" pad="1"/>
<contactref element="5VLED1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="JP2" pad="P2"/>
<contactref element="R1" pad="2"/>
<contactref element="JP15" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="7"/>
<contactref element="C8" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="JP13" pad="1"/>
<contactref element="JP12" pad="VBUS"/>
<contactref element="C3" pad="1"/>
<contactref element="IR" pad="1"/>
<contactref element="5VLED8" pad="3"/>
<contactref element="5VLED9" pad="3"/>
<contactref element="5VLED7" pad="3"/>
<contactref element="5VLED6" pad="3"/>
<contactref element="5VLED4" pad="3"/>
<contactref element="5VLED5" pad="3"/>
<contactref element="5VLED2" pad="3"/>
<contactref element="5VLED3" pad="3"/>
<contactref element="5VLED1" pad="3"/>
<contactref element="5V_PWR" pad="A"/>
</signal>
<signal name="+12V">
<contactref element="12V_LED" pad="4"/>
<contactref element="JP1" pad="P1"/>
<contactref element="12V_PWR" pad="A"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="17"/>
<contactref element="JP15" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="JP15" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="15"/>
<contactref element="JP15" pad="4"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="29"/>
<contactref element="JP15" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="20"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="IR">
<contactref element="IR" pad="3"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="MCU_LEDOUT">
<contactref element="R5" pad="2"/>
<contactref element="5VLED1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="11"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="5VLED2" pad="2"/>
<contactref element="5VLED3" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="5VLED4" pad="2"/>
<contactref element="5VLED5" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="5VLED6" pad="2"/>
<contactref element="5VLED7" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="5VLED8" pad="2"/>
<contactref element="5VLED9" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="U2" pad="6"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="R6" pad="1"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="N$31">
<contactref element="U2" pad="11"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U2" pad="25"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="RX">
<contactref element="U2" pad="26"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="SUSPEND">
<contactref element="U2" pad="12"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="N$34">
<contactref element="JP12" pad="D+"/>
<contactref element="JP13" pad="3"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$36">
<contactref element="U2" pad="5"/>
<contactref element="JP12" pad="D-"/>
<contactref element="JP13" pad="2"/>
</signal>
<signal name="12VLED_R">
<contactref element="Q2" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="12VLED_G">
<contactref element="Q1" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="12VLED_B">
<contactref element="U1" pad="13"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="Q3" pad="2"/>
<contactref element="12V_LED" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="Q2" pad="2"/>
<contactref element="12V_LED" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="Q1" pad="2"/>
<contactref element="12V_LED" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="7"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="8"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="U2" pad="28"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="2"/>
<contactref element="STAT" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="5V_PWR" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="12V_PWR" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
