(kicad_pcb (version 20171130) (host pcbnew 5.1.6+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 132)
    (zones 0)
    (modules 12)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 108.585 147.955)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /SD_MISO)
  (net 2 GND)
  (net 3 /SD_CLK)
  (net 4 +3V3)
  (net 5 /SD_MOSI)
  (net 6 "Net-(J1-Pad8)")
  (net 7 /SD_CS)
  (net 8 /SCSI_IO)
  (net 9 /SCSI_REQ)
  (net 10 /SCSI_CD)
  (net 11 /SCSI_SEL)
  (net 12 /SCSI_RST)
  (net 13 /SCSI_ACK)
  (net 14 /SCSI_BSY)
  (net 15 /SCSI_ATN)
  (net 16 +5V)
  (net 17 /SCSI_MSG)
  (net 18 /SCSI_DBP)
  (net 19 /SCSI_DAT7)
  (net 20 /SCSI_DAT6)
  (net 21 /SCSI_DAT5)
  (net 22 /SCSI_DAT4)
  (net 23 /SCSI_DAT3)
  (net 24 /SCSI_DAT2)
  (net 25 /SCSI_DAT1)
  (net 26 /SCSI_DAT0)
  (net 27 "Net-(U1-Pad42)")
  (net 28 "Net-(U1-Pad41)")
  (net 29 "Net-(U1-Pad29)")
  (net 30 "Net-(U1-Pad28)")
  (net 31 "Net-(U1-Pad17)")
  (net 32 "Net-(U1-Pad14)")
  (net 33 "Net-(U1-Pad8)")
  (net 34 "Net-(U1-Pad7)")
  (net 35 "Net-(U1-Pad4)")
  (net 36 "Net-(U1-Pad3)")
  (net 37 "Net-(U1-Pad2)")
  (net 38 "Net-(U1-Pad1)")
  (net 39 "Net-(J1-Pad1)")
  (net 40 "Net-(U1-Pad6)")
  (net 41 "Net-(U1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /SCSI_ACK)
    (add_net /SCSI_ATN)
    (add_net /SCSI_BSY)
    (add_net /SCSI_CD)
    (add_net /SCSI_DAT0)
    (add_net /SCSI_DAT1)
    (add_net /SCSI_DAT2)
    (add_net /SCSI_DAT3)
    (add_net /SCSI_DAT4)
    (add_net /SCSI_DAT5)
    (add_net /SCSI_DAT6)
    (add_net /SCSI_DAT7)
    (add_net /SCSI_DBP)
    (add_net /SCSI_IO)
    (add_net /SCSI_MSG)
    (add_net /SCSI_REQ)
    (add_net /SCSI_RST)
    (add_net /SCSI_SEL)
    (add_net /SD_CLK)
    (add_net /SD_CS)
    (add_net /SD_MISO)
    (add_net /SD_MOSI)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 95.25 78.74)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.7) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 95.25 144.78)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.7) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module blue:BluePill_STM32F103C (layer F.Cu) (tedit 59B4EF3F)
    (at 75.565 83.185)
    (descr "STM32F103C8 BluePill board")
    (fp_text reference U1 (at 7.1628 49.6062 180) (layer F.SilkS))
    (fp_text value BluePill_STM32F103C (at 10.795 23.7998 90) (layer F.SilkS))
    (pad 42 thru_hole oval (at 6.36 3.7592 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U1-Pad42)"))
    (pad 41 thru_hole oval (at 8.9 3.7592 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U1-Pad41)"))
    (pad 40 thru_hole oval (at 15.24 -0.1016 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 39 thru_hole oval (at 15.24 2.4892 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 38 thru_hole oval (at 15.24 5.0292 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 +5V))
    (pad 37 thru_hole oval (at 15.24 7.5692 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SCSI_DAT1))
    (pad 36 thru_hole oval (at 15.24 10.1092 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /SCSI_DAT0))
    (pad 35 thru_hole oval (at 15.24 12.6492 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SCSI_IO))
    (pad 34 thru_hole oval (at 15.24 15.1892 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SCSI_REQ))
    (pad 33 thru_hole oval (at 15.24 17.7292 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCSI_CD))
    (pad 32 thru_hole oval (at 15.24 20.2692 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCSI_SEL))
    (pad 31 thru_hole oval (at 15.24 22.8092 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /SCSI_MSG))
    (pad 30 thru_hole oval (at 15.24 25.3492 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /SCSI_RST))
    (pad 29 thru_hole oval (at 15.24 27.8892 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U1-Pad29)"))
    (pad 28 thru_hole oval (at 15.24 30.4292 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U1-Pad28)"))
    (pad 27 thru_hole oval (at 15.24 32.9692 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SCSI_ACK))
    (pad 26 thru_hole oval (at 15.24 35.5092 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SCSI_BSY))
    (pad 25 thru_hole oval (at 15.24 38.0492 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /SCSI_ATN))
    (pad 24 thru_hole oval (at 15.24 40.5892 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /SCSI_DAT7))
    (pad 23 thru_hole oval (at 15.24 43.1292 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /SCSI_DAT6))
    (pad 22 thru_hole oval (at 15.24 45.6692 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /SCSI_DAT5))
    (pad 21 thru_hole oval (at 15.24 48.2092 90) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /SCSI_DAT4))
    (pad 20 thru_hole oval (at 0 48.2092 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 19 thru_hole oval (at 0 45.6692 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 18 thru_hole oval (at 0 43.1292 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 17 thru_hole oval (at 0 40.5892 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U1-Pad17)"))
    (pad 16 thru_hole oval (at 0 38.0492 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /SCSI_DAT3))
    (pad 15 thru_hole oval (at 0 35.5092 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /SCSI_DAT2))
    (pad 14 thru_hole oval (at 0 32.9692 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U1-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.4292 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /SCSI_DBP))
    (pad 12 thru_hole oval (at 0 27.8892 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SD_MOSI))
    (pad 11 thru_hole oval (at 0 25.3492 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /SD_MISO))
    (pad 10 thru_hole oval (at 0 22.8092 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SD_CLK))
    (pad 9 thru_hole oval (at 0 20.2692 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SD_CS))
    (pad 8 thru_hole oval (at 0 17.7292 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.1892 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.6492 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.1092 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.5692 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.0292 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.4892 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.0508 270) (size 1.7272 2.25) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U1-Pad1)"))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 92.71 139.7 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(J1-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 79.375 103.505 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -3.175 0) (layer F.SilkS))
    (fp_text value 47K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /SD_CS))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 79.375 111.125 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -3.175 0) (layer F.SilkS))
    (fp_text value 47K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /SD_MOSI))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 79.375 108.585 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -3.175 0) (layer F.SilkS))
    (fp_text value 47K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /SD_MISO))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 73.66 139.7 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 47K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad8)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x25_P2.54mm_Vertical (layer F.Cu) (tedit 5EAC9A07)
    (at 104.775 142.24 180)
    (descr "Through hole IDC box header, 2x25, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x25 2.54mm double row")
    (fp_text reference J2 (at 6.985 -3.81) (layer F.SilkS))
    (fp_text value Conn_02x25_Odd_Even (at 1.27 67.06) (layer F.Fab))
    (fp_text user %R (at 1.27 30.48 90) (layer F.Fab))
    (pad 50 thru_hole circle (at 2.54 60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SCSI_IO))
    (pad 48 thru_hole circle (at 2.54 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SCSI_REQ))
    (pad 46 thru_hole circle (at 2.54 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SCSI_CD))
    (pad 44 thru_hole circle (at 2.54 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SCSI_SEL))
    (pad 42 thru_hole circle (at 2.54 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SCSI_MSG))
    (pad 40 thru_hole circle (at 2.54 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SCSI_RST))
    (pad 38 thru_hole circle (at 2.54 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /SCSI_ACK))
    (pad 36 thru_hole circle (at 2.54 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SCSI_BSY))
    (pad 34 thru_hole circle (at 2.54 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 32 thru_hole circle (at 2.54 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /SCSI_ATN))
    (pad 30 thru_hole circle (at 2.54 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 28 thru_hole circle (at 2.54 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole circle (at 2.54 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +5V))
    (pad 24 thru_hole circle (at 2.54 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 22 thru_hole circle (at 2.54 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole circle (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole circle (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /SCSI_DBP))
    (pad 16 thru_hole circle (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /SCSI_DAT7))
    (pad 14 thru_hole circle (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /SCSI_DAT6))
    (pad 12 thru_hole circle (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SCSI_DAT5))
    (pad 10 thru_hole circle (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /SCSI_DAT4))
    (pad 8 thru_hole circle (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /SCSI_DAT3))
    (pad 6 thru_hole circle (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SCSI_DAT2))
    (pad 4 thru_hole circle (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /SCSI_DAT1))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /SCSI_DAT0))
    (pad 49 thru_hole circle (at 0 60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 47 thru_hole circle (at 0 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 45 thru_hole circle (at 0 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 43 thru_hole circle (at 0 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 41 thru_hole circle (at 0 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 39 thru_hole circle (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 37 thru_hole circle (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole circle (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 33 thru_hole circle (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole circle (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 29 thru_hole circle (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 27 thru_hole circle (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 25 thru_hole circle (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 23 thru_hole circle (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole circle (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 19 thru_hole circle (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 17 thru_hole circle (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole circle (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole circle (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole circle (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole circle (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x25_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Card:microSD_HC_Molex_104031-0811 (layer F.Cu) (tedit 5D235007)
    (at 83.185 140.335 180)
    (descr "1.10mm Pitch microSD Memory Card Connector, Surface Mount, Push-Pull Type, 1.42mm Height, with Detect Switch (https://www.molex.com/pdm_docs/sd/1040310811_sd.pdf)")
    (tags "microSD SD molex")
    (attr smd)
    (fp_text reference J1 (at 8.255 -5.715) (layer F.SilkS))
    (fp_text value Micro_SD_Card (at 0 7.39) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 11 smd rect (at 3.73 5.375 180) (size 1.9 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -2.24 5.375 180) (size 1.9 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -5.74 0.7 180) (size 1.2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -5.74 4.4 180) (size 1.2 1) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -5.565 -5.325 180) (size 1.55 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 5.755 -5.1 180) (size 1.17 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.495 -5.45 180) (size 0.85 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 /SD_MISO))
    (pad 6 smd rect (at 2.395 -5.45 180) (size 0.85 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.295 -5.45 180) (size 0.85 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 /SD_CLK))
    (pad 4 smd rect (at 0.195 -5.45 180) (size 0.85 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 3 smd rect (at -0.905 -5.45 180) (size 0.85 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 /SD_MOSI))
    (pad 2 smd rect (at -2.005 -5.45 180) (size 0.85 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 /SD_CS))
    (pad 8 smd rect (at 4.545 -5.45 180) (size 0.75 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad8)"))
    (pad 1 smd rect (at -3.105 -5.45 180) (size 0.85 1.1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Card.3dshapes/microSD_HC_Molex_104031-0811.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 86.8425 83.185 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 3.0225 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 86.995 90.805 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 108.585 75.565) (end 108.585 147.955) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 71.12 75.565) (end 108.585 75.565) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 71.12 147.955) (end 71.12 75.565) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 108.585 147.955) (end 71.12 147.955) (layer Edge.Cuts) (width 0.05))
  (gr_text "BluePill SCSI 1.0" (at 82.55 78.105) (layer F.Cu))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.22 148.59) (xy 70.485 148.59) (xy 70.485 75.565) (xy 109.22 75.565)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.49 149.86) (xy 69.85 149.86) (xy 69.85 74.93) (xy 110.49 74.93)
      )
    )
  )
)
