(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 1056)
    (zones 0)
    (modules 124)
    (nets 119)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.9)
    (user_trace_width 1.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +24V)
  (net 3 "Net-(C101-Pad1)")
  (net 4 +5V)
  (net 5 +3V3)
  (net 6 /ButtonExpander/RST)
  (net 7 "Net-(C1000-Pad2)")
  (net 8 "Net-(C1400-Pad2)")
  (net 9 "Net-(D300-Pad2)")
  (net 10 "Net-(D300-Pad1)")
  (net 11 "Net-(D310-Pad2)")
  (net 12 "Net-(D310-Pad1)")
  (net 13 "Net-(D320-Pad2)")
  (net 14 "Net-(D320-Pad1)")
  (net 15 "Net-(D350-Pad2)")
  (net 16 "Net-(D350-Pad1)")
  (net 17 "Net-(D360-Pad2)")
  (net 18 "Net-(D360-Pad1)")
  (net 19 "Net-(D370-Pad2)")
  (net 20 "Net-(D370-Pad1)")
  (net 21 "Net-(D380-Pad2)")
  (net 22 "Net-(D380-Pad1)")
  (net 23 "Net-(D1010-Pad2)")
  (net 24 "Net-(D1010-Pad1)")
  (net 25 "Net-(D1020-Pad2)")
  (net 26 "Net-(D1020-Pad1)")
  (net 27 "Net-(D1030-Pad2)")
  (net 28 "Net-(D1030-Pad1)")
  (net 29 "Net-(D1410-Pad2)")
  (net 30 "Net-(D1410-Pad1)")
  (net 31 "Net-(D1420-Pad2)")
  (net 32 "Net-(D1420-Pad1)")
  (net 33 "Net-(D1430-Pad2)")
  (net 34 "Net-(D1430-Pad1)")
  (net 35 "Net-(DS200-Pad18)")
  (net 36 "Net-(DS200-Pad17)")
  (net 37 "Net-(DS200-Pad14)")
  (net 38 "Net-(DS200-Pad13)")
  (net 39 "Net-(DS200-Pad12)")
  (net 40 "Net-(DS200-Pad11)")
  (net 41 "Net-(DS200-Pad6)")
  (net 42 "Net-(DS200-Pad4)")
  (net 43 "Net-(DS200-Pad3)")
  (net 44 "Net-(J100-Pad4)")
  (net 45 "Net-(J400-Pad5)")
  (net 46 "Net-(J400-Pad4)")
  (net 47 "Net-(J400-Pad3)")
  (net 48 "Net-(J400-Pad2)")
  (net 49 "Net-(J401-Pad4)")
  (net 50 "Net-(J401-Pad3)")
  (net 51 "Net-(J401-Pad2)")
  (net 52 "Net-(J401-Pad1)")
  (net 53 /ProbeSheet/Prb.Flow)
  (net 54 /ProbeSheet/Prb.Level1)
  (net 55 "Net-(J1010-Pad4)")
  (net 56 "Net-(J1010-Pad3)")
  (net 57 "Net-(J1010-Pad2)")
  (net 58 "Net-(J1010-Pad1)")
  (net 59 "Net-(J1020-Pad4)")
  (net 60 "Net-(J1020-Pad3)")
  (net 61 "Net-(J1020-Pad2)")
  (net 62 "Net-(J1020-Pad1)")
  (net 63 "Net-(J1030-Pad4)")
  (net 64 "Net-(J1030-Pad3)")
  (net 65 "Net-(J1030-Pad2)")
  (net 66 "Net-(J1030-Pad1)")
  (net 67 "Net-(J1410-Pad4)")
  (net 68 "Net-(J1410-Pad3)")
  (net 69 "Net-(J1410-Pad2)")
  (net 70 "Net-(J1410-Pad1)")
  (net 71 "Net-(J1420-Pad4)")
  (net 72 "Net-(J1420-Pad3)")
  (net 73 "Net-(J1420-Pad2)")
  (net 74 "Net-(J1420-Pad1)")
  (net 75 "Net-(J1430-Pad4)")
  (net 76 "Net-(J1430-Pad3)")
  (net 77 "Net-(J1430-Pad2)")
  (net 78 "Net-(J1430-Pad1)")
  (net 79 "Net-(Q300-Pad1)")
  (net 80 "Net-(Q310-Pad1)")
  (net 81 "Net-(Q320-Pad1)")
  (net 82 "Net-(Q350-Pad1)")
  (net 83 "Net-(Q360-Pad1)")
  (net 84 "Net-(Q370-Pad1)")
  (net 85 "Net-(Q380-Pad1)")
  (net 86 "Net-(Q1010-Pad1)")
  (net 87 "Net-(Q1020-Pad1)")
  (net 88 "Net-(Q1030-Pad1)")
  (net 89 "Net-(Q1410-Pad1)")
  (net 90 "Net-(Q1420-Pad1)")
  (net 91 "Net-(Q1430-Pad1)")
  (net 92 /ButtonExpander/SCL)
  (net 93 /ButtonExpander/SDA)
  (net 94 /ValvesSheet/Vlv.EndDrain)
  (net 95 /ValvesSheet/Vlv.Water)
  (net 96 /ValvesSheet/Vlv.MnfldDrain)
  (net 97 /ValvesSheet/Vlv.Pump1)
  (net 98 /ValvesSheet/Vlv.Pump2)
  (net 99 /ValvesSheet/Vlv.Pump3)
  (net 100 /ValvesSheet/Vlv.Pump4)
  (net 101 /ButtonExpander/INT2)
  (net 102 /GPIOexpander0/ADDR)
  (net 103 "Net-(R1010-Pad1)")
  (net 104 "Net-(R1020-Pad1)")
  (net 105 "Net-(R1030-Pad1)")
  (net 106 /GPIOexpander4/ADDR)
  (net 107 "Net-(R1410-Pad1)")
  (net 108 "Net-(R1420-Pad1)")
  (net 109 "Net-(R1430-Pad1)")
  (net 110 /GPIOexpander0/INT1)
  (net 111 /DisplaySheet/Disp.B)
  (net 112 /DisplaySheet/Disp.G)
  (net 113 /DisplaySheet/Disp.DB7)
  (net 114 /DisplaySheet/Disp.DB6)
  (net 115 /DisplaySheet/Disp.DB5)
  (net 116 /DisplaySheet/Disp.DB4)
  (net 117 /DisplaySheet/Disp.E)
  (net 118 /DisplaySheet/Disp.RS)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ButtonExpander/INT2)
    (add_net /ButtonExpander/RST)
    (add_net /ButtonExpander/SCL)
    (add_net /ButtonExpander/SDA)
    (add_net /DisplaySheet/Disp.B)
    (add_net /DisplaySheet/Disp.DB4)
    (add_net /DisplaySheet/Disp.DB5)
    (add_net /DisplaySheet/Disp.DB6)
    (add_net /DisplaySheet/Disp.DB7)
    (add_net /DisplaySheet/Disp.E)
    (add_net /DisplaySheet/Disp.G)
    (add_net /DisplaySheet/Disp.RS)
    (add_net /GPIOexpander0/ADDR)
    (add_net /GPIOexpander0/INT1)
    (add_net /GPIOexpander4/ADDR)
    (add_net /ProbeSheet/Prb.Flow)
    (add_net /ProbeSheet/Prb.Level1)
    (add_net /ValvesSheet/Vlv.EndDrain)
    (add_net /ValvesSheet/Vlv.MnfldDrain)
    (add_net /ValvesSheet/Vlv.Pump1)
    (add_net /ValvesSheet/Vlv.Pump2)
    (add_net /ValvesSheet/Vlv.Pump3)
    (add_net /ValvesSheet/Vlv.Pump4)
    (add_net /ValvesSheet/Vlv.Water)
    (add_net GND)
    (add_net "Net-(C1000-Pad2)")
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C1400-Pad2)")
    (add_net "Net-(D1010-Pad1)")
    (add_net "Net-(D1010-Pad2)")
    (add_net "Net-(D1020-Pad1)")
    (add_net "Net-(D1020-Pad2)")
    (add_net "Net-(D1030-Pad1)")
    (add_net "Net-(D1030-Pad2)")
    (add_net "Net-(D1410-Pad1)")
    (add_net "Net-(D1410-Pad2)")
    (add_net "Net-(D1420-Pad1)")
    (add_net "Net-(D1420-Pad2)")
    (add_net "Net-(D1430-Pad1)")
    (add_net "Net-(D1430-Pad2)")
    (add_net "Net-(D300-Pad1)")
    (add_net "Net-(D300-Pad2)")
    (add_net "Net-(D310-Pad1)")
    (add_net "Net-(D310-Pad2)")
    (add_net "Net-(D320-Pad1)")
    (add_net "Net-(D320-Pad2)")
    (add_net "Net-(D350-Pad1)")
    (add_net "Net-(D350-Pad2)")
    (add_net "Net-(D360-Pad1)")
    (add_net "Net-(D360-Pad2)")
    (add_net "Net-(D370-Pad1)")
    (add_net "Net-(D370-Pad2)")
    (add_net "Net-(D380-Pad1)")
    (add_net "Net-(D380-Pad2)")
    (add_net "Net-(DS200-Pad11)")
    (add_net "Net-(DS200-Pad12)")
    (add_net "Net-(DS200-Pad13)")
    (add_net "Net-(DS200-Pad14)")
    (add_net "Net-(DS200-Pad17)")
    (add_net "Net-(DS200-Pad18)")
    (add_net "Net-(DS200-Pad3)")
    (add_net "Net-(DS200-Pad4)")
    (add_net "Net-(DS200-Pad6)")
    (add_net "Net-(J100-Pad4)")
    (add_net "Net-(J1010-Pad1)")
    (add_net "Net-(J1010-Pad2)")
    (add_net "Net-(J1010-Pad3)")
    (add_net "Net-(J1010-Pad4)")
    (add_net "Net-(J1020-Pad1)")
    (add_net "Net-(J1020-Pad2)")
    (add_net "Net-(J1020-Pad3)")
    (add_net "Net-(J1020-Pad4)")
    (add_net "Net-(J1030-Pad1)")
    (add_net "Net-(J1030-Pad2)")
    (add_net "Net-(J1030-Pad3)")
    (add_net "Net-(J1030-Pad4)")
    (add_net "Net-(J1410-Pad1)")
    (add_net "Net-(J1410-Pad2)")
    (add_net "Net-(J1410-Pad3)")
    (add_net "Net-(J1410-Pad4)")
    (add_net "Net-(J1420-Pad1)")
    (add_net "Net-(J1420-Pad2)")
    (add_net "Net-(J1420-Pad3)")
    (add_net "Net-(J1420-Pad4)")
    (add_net "Net-(J1430-Pad1)")
    (add_net "Net-(J1430-Pad2)")
    (add_net "Net-(J1430-Pad3)")
    (add_net "Net-(J1430-Pad4)")
    (add_net "Net-(J400-Pad2)")
    (add_net "Net-(J400-Pad3)")
    (add_net "Net-(J400-Pad4)")
    (add_net "Net-(J400-Pad5)")
    (add_net "Net-(J401-Pad1)")
    (add_net "Net-(J401-Pad2)")
    (add_net "Net-(J401-Pad3)")
    (add_net "Net-(J401-Pad4)")
    (add_net "Net-(Q1010-Pad1)")
    (add_net "Net-(Q1020-Pad1)")
    (add_net "Net-(Q1030-Pad1)")
    (add_net "Net-(Q1410-Pad1)")
    (add_net "Net-(Q1420-Pad1)")
    (add_net "Net-(Q1430-Pad1)")
    (add_net "Net-(Q300-Pad1)")
    (add_net "Net-(Q310-Pad1)")
    (add_net "Net-(Q320-Pad1)")
    (add_net "Net-(Q350-Pad1)")
    (add_net "Net-(Q360-Pad1)")
    (add_net "Net-(Q370-Pad1)")
    (add_net "Net-(Q380-Pad1)")
    (add_net "Net-(R1010-Pad1)")
    (add_net "Net-(R1020-Pad1)")
    (add_net "Net-(R1030-Pad1)")
    (add_net "Net-(R1410-Pad1)")
    (add_net "Net-(R1420-Pad1)")
    (add_net "Net-(R1430-Pad1)")
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Horizontal (layer B.Cu) (tedit 5A19A424)
    (at 172.6 80.4 180)
    (descr "Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x04 2.54mm single row")
    (fp_text reference J101 (at -4.38 2.77) (layer B.SilkS))
    (fp_text value Screw_Terminal_01x04 (at -4.38 -10.39) (layer B.Fab))
    (fp_text user %R (at -5.775 -3.81 270) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 /GPIOexpander4/ADDR))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 /GPIOexpander4/ADDR))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Mountinghole (layer F.Cu) (tedit 624541EA)
    (at 180.5 151)
    (fp_text reference H2 (at 0.5 -3.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0.5 -4.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module ProductDoser:Mountinghole (layer F.Cu) (tedit 624541EA)
    (at 87.5 151)
    (fp_text reference H1 (at 0.5 -3.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0.5 -4.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module ProductDoser:WH2004A-CFH-JT (layer F.Cu) (tedit 619055D8)
    (at 95 40)
    (fp_text reference DS200 (at 39 28) (layer F.SilkS))
    (fp_text value WH2004A-CFH-JT (at 39 27) (layer F.Fab))
    (pad 18 thru_hole circle (at 43.18 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(DS200-Pad18)"))
    (pad 17 thru_hole circle (at 40.64 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(DS200-Pad17)"))
    (pad 16 thru_hole circle (at 38.1 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at 35.56 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 14 thru_hole circle (at 33.02 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(DS200-Pad14)"))
    (pad 13 thru_hole circle (at 30.48 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(DS200-Pad13)"))
    (pad 12 thru_hole circle (at 27.94 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(DS200-Pad12)"))
    (pad 11 thru_hole circle (at 25.4 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(DS200-Pad11)"))
    (pad 10 thru_hole circle (at 22.86 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(DS200-Pad6)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(DS200-Pad4)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(DS200-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole circle (at 85.5 55) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at -7.5 55) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 85.5 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at -7.5 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module digikey-footprints:SOIC-28_W7.5mm (layer F.Cu) (tedit 5D28A5C9)
    (at 134.5 76.7 180)
    (attr smd)
    (fp_text reference U1000 (at 0 -10.04) (layer F.SilkS))
    (fp_text value MCP23018T-E_SO (at 0 10.15) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 28 smd rect (at 4.7 -8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 4.7 -6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(J1020-Pad3)"))
    (pad 26 smd rect (at 4.7 -5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(J1020-Pad2)"))
    (pad 25 smd rect (at 4.7 -4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(J1020-Pad1)"))
    (pad 24 smd rect (at 4.7 -3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(R1010-Pad1)"))
    (pad 23 smd rect (at 4.7 -1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J1010-Pad4)"))
    (pad 22 smd rect (at 4.7 -0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J1010-Pad3)"))
    (pad 21 smd rect (at 4.7 0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J1010-Pad2)"))
    (pad 20 smd rect (at 4.7 1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J1010-Pad1)"))
    (pad 19 smd rect (at 4.7 3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /GPIOexpander0/INT1))
    (pad 18 smd rect (at 4.7 4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /GPIOexpander0/INT1))
    (pad 17 smd rect (at 4.7 5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 4.7 6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C1000-Pad2)"))
    (pad 15 smd rect (at 4.7 8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 /GPIOexpander0/ADDR))
    (pad 14 smd rect (at -4.7 8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -4.7 6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 /ButtonExpander/SDA))
    (pad 12 smd rect (at -4.7 5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 /ButtonExpander/SCL))
    (pad 11 smd rect (at -4.7 4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 10 smd rect (at -4.7 3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -4.7 1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R1030-Pad1)"))
    (pad 8 smd rect (at -4.7 0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(J1030-Pad4)"))
    (pad 7 smd rect (at -4.7 -0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(J1030-Pad3)"))
    (pad 6 smd rect (at -4.7 -1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J1030-Pad2)"))
    (pad 5 smd rect (at -4.7 -3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(J1030-Pad1)"))
    (pad 4 smd rect (at -4.7 -4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(R1020-Pad1)"))
    (pad 3 smd rect (at -4.7 -5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(J1020-Pad4)"))
    (pad 2 smd rect (at -4.7 -6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -4.7 -8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 141.5 73.2 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 127.5 68.7625 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1000 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C1000-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 138.3 129.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1021 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D1020-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 145.3 129.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1031 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D1030-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-3_TabPin2 (layer F.Cu) (tedit 5A70F30B)
    (at 103.425 137.175 270)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q370 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value IPD050N03LG (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525 270) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525 270) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525 270) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525 270) (size 3.05 2.75) (layers F.Paste))
    (pad 2 smd rect (at 2.1 0 270) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 20 "Net-(D370-Pad1)"))
    (pad 3 smd rect (at -4.2 2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.2 0 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D370-Pad1)"))
    (pad 1 smd rect (at -4.2 -2.28 270) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(Q370-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 95.2 132.7375 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R352 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(Q350-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 95.2 129.1375 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R350 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(Q350-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /ValvesSheet/Vlv.Pump1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 93.2 129.1375 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R351 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D350-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 92 132.7 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q350 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D350-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(Q350-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 91.2 129.1375 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D350 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D350-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D350-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_6_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BF224)
    (at 130.1 147.5)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J1040 (at 8.75 -5.25) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x06 (at 8.75 4.45) (layer F.Fab))
    (fp_text user %R (at 8.75 2.7) (layer F.Fab))
    (pad 6 thru_hole circle (at 17.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(D1030-Pad1)"))
    (pad 5 thru_hole circle (at 14 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 "Net-(D1020-Pad1)"))
    (pad 3 thru_hole circle (at 7 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(D1010-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 155.8 65.6375 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1401 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 /GPIOexpander4/ADDR))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 157.8 65.6375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1402 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 106 /GPIOexpander4/ADDR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_5_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BC220)
    (at 130.1 122.8)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J1030 (at 7 -5.25) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 7 4.45) (layer F.Fab))
    (fp_text user %R (at 7 2.7) (layer F.Fab))
    (pad 5 thru_hole circle (at 14 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 "Net-(J1030-Pad4)"))
    (pad 3 thru_hole circle (at 7 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 "Net-(J1030-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 "Net-(J1030-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 "Net-(J1030-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Teensy4.1 (layer F.Cu) (tedit 61ABFB37)
    (at 123.25 35.4 90)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference U100 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Teensy4.1 (at 7.62 -2.54 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 270) (layer F.Fab))
    (pad 43 thru_hole oval (at 15.24 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 /ButtonExpander/INT2))
    (pad 42 thru_hole oval (at 15.24 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 /GPIOexpander0/INT1))
    (pad 40 thru_hole oval (at 15.24 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 /ButtonExpander/SDA))
    (pad 46 thru_hole oval (at 15.24 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 44 thru_hole oval (at 15.24 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 48 thru_hole circle (at 15.24 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 37 thru_hole oval (at 15.24 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 47 thru_hole oval (at 15.24 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 45 thru_hole oval (at 15.24 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 41 thru_hole oval (at 15.24 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 /ButtonExpander/SCL))
    (pad 39 thru_hole oval (at 15.24 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 15.24 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 15.24 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at 15.24 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 15.24 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 31 thru_hole oval (at 15.24 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 35 thru_hole oval (at 15.24 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at 15.24 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 15.24 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 15.24 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /ProbeSheet/Prb.Flow))
    (pad 26 thru_hole oval (at 15.24 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 15.24 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J100-Pad4)"))
    (pad 34 thru_hole oval (at 15.24 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 30 thru_hole oval (at 15.24 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /ProbeSheet/Prb.Level1))
    (pad 24 thru_hole oval (at 0 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /ValvesSheet/Vlv.Pump4))
    (pad 23 thru_hole oval (at 0 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 /ValvesSheet/Vlv.Pump3))
    (pad 22 thru_hole oval (at 0 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 /ValvesSheet/Vlv.Pump2))
    (pad 21 thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 /ValvesSheet/Vlv.Pump1))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 /ValvesSheet/Vlv.MnfldDrain))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 /ValvesSheet/Vlv.Water))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 /ValvesSheet/Vlv.EndDrain))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 /DisplaySheet/Disp.B))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 /DisplaySheet/Disp.G))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 /DisplaySheet/Disp.DB7))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 /DisplaySheet/Disp.DB6))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 /DisplaySheet/Disp.DB5))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 /DisplaySheet/Disp.DB4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 /DisplaySheet/Disp.E))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 /DisplaySheet/Disp.RS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 172.3125 27.6)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C402 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 181.5875 27.8)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C401 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:UFQFN-28-1EP_4x4mm (layer F.Cu) (tedit 5D28ACF9)
    (at 177.175 27.825 270)
    (descr http://www.semtech.com/images/datasheet/sx150x_89b.pdf)
    (attr smd)
    (fp_text reference U400 (at 0 -3.87 90) (layer F.SilkS))
    (fp_text value SX1509BIULTRT (at 0 3.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 29 smd rect (at 0 0 270) (size 2.65 2.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at -1.975 1.175 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J400-Pad3)"))
    (pad 27 smd rect (at -1.975 0.775 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J400-Pad2)"))
    (pad 26 smd rect (at -1.975 0.375 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at -1.975 -0.025 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 92 /ButtonExpander/SCL))
    (pad 24 smd rect (at -1.975 -0.425 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 93 /ButtonExpander/SDA))
    (pad 23 smd rect (at -1.975 -0.825 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /ButtonExpander/RST))
    (pad 21 smd rect (at -1.225 -1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -0.825 -1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -0.425 -1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.025 -1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 17 smd rect (at 0.375 -1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 0.775 -1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 1.975 -1.175 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 1.975 -0.775 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 1.975 -0.375 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 11 smd rect (at 1.975 0.025 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 1.975 0.425 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 1.975 0.825 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 101 /ButtonExpander/INT2))
    (pad 7 smd rect (at 1.175 1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J401-Pad3)"))
    (pad 6 smd rect (at 0.775 1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J401-Pad2)"))
    (pad 5 smd rect (at 0.375 1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J401-Pad1)"))
    (pad 4 smd rect (at -0.025 1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 3 smd rect (at -0.425 1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.825 1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J400-Pad5)"))
    (pad 1 smd rect (at -1.225 1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J400-Pad4)"))
    (pad 8 smd rect (at 1.975 1.225 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J401-Pad4)"))
    (pad 15 smd rect (at 1.175 -1.975 270) (size 0.2 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at -1.975 -1.225 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask))
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_6_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BF224)
    (at 189.5 57.1 270)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J500 (at 8.75 -5.25 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x06 (at 8.75 4.45 90) (layer F.Fab))
    (fp_text user %R (at 8.75 2.7 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 17.5 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 5 thru_hole circle (at 14 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 4 thru_hole circle (at 10.5 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 /ProbeSheet/Prb.Flow))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 54 /ProbeSheet/Prb.Level1))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 140.0625 23)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R100 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 /ButtonExpander/SCL))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_2220_5650Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.35 34.3)
    (descr "Capacitor SMD 2220 (5650 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C101 (at 0 -3.65) (layer F.SilkS))
    (fp_text value 22µF (at 0 3.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.55 0) (size 1.8 5.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.138889)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.55 0) (size 1.8 5.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.138889)
      (net 3 "Net-(C101-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_2220_5650Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 133.41 30.0375 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C201 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 125.4625 23 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C200 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TSSOP-20_W4.4mm (layer F.Cu) (tedit 5D28AC99)
    (at 128.71 27.9)
    (descr http://www.ti.com/lit/ds/symlink/txb0108.pdf)
    (attr smd)
    (fp_text reference U200 (at 0 -4.79) (layer F.SilkS))
    (fp_text value TXB0108PWR (at 0 5.22) (layer F.Fab))
    (fp_text user REF** (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at -2.925 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(DS200-Pad4)") (solder_mask_margin 0.07))
    (pad 19 smd rect (at -2.275 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_mask_margin 0.07))
    (pad 18 smd rect (at -1.625 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(DS200-Pad6)") (solder_mask_margin 0.07))
    (pad 17 smd rect (at -0.975 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(DS200-Pad11)") (solder_mask_margin 0.07))
    (pad 16 smd rect (at -0.325 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(DS200-Pad12)") (solder_mask_margin 0.07))
    (pad 15 smd rect (at 0.325 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(DS200-Pad13)") (solder_mask_margin 0.07))
    (pad 14 smd rect (at 0.975 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(DS200-Pad14)") (solder_mask_margin 0.07))
    (pad 13 smd rect (at 1.625 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(DS200-Pad17)") (solder_mask_margin 0.07))
    (pad 12 smd rect (at 2.275 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(DS200-Pad18)") (solder_mask_margin 0.07))
    (pad 11 smd rect (at 2.925 -2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 10 smd rect (at 2.925 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.07))
    (pad 9 smd rect (at 2.275 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 111 /DisplaySheet/Disp.B) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 1.625 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 112 /DisplaySheet/Disp.G) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0.975 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 113 /DisplaySheet/Disp.DB7) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 0.325 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 114 /DisplaySheet/Disp.DB6) (solder_mask_margin 0.07))
    (pad 5 smd rect (at -0.325 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 115 /DisplaySheet/Disp.DB5) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -0.975 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 116 /DisplaySheet/Disp.DB4) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.625 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 117 /DisplaySheet/Disp.E) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -2.275 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -2.925 2.8) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 118 /DisplaySheet/Disp.RS) (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOIC-28_W7.5mm (layer F.Cu) (tedit 5D28A5C9)
    (at 160.8 76.7 180)
    (attr smd)
    (fp_text reference U1400 (at 0 -10.04) (layer F.SilkS))
    (fp_text value MCP23018T-E_SO (at 0 10.15) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 28 smd rect (at 4.7 -8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 4.7 -6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(J1420-Pad3)"))
    (pad 26 smd rect (at 4.7 -5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(J1420-Pad2)"))
    (pad 25 smd rect (at 4.7 -4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(J1420-Pad1)"))
    (pad 24 smd rect (at 4.7 -3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(R1410-Pad1)"))
    (pad 23 smd rect (at 4.7 -1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(J1410-Pad4)"))
    (pad 22 smd rect (at 4.7 -0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J1410-Pad3)"))
    (pad 21 smd rect (at 4.7 0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(J1410-Pad2)"))
    (pad 20 smd rect (at 4.7 1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(J1410-Pad1)"))
    (pad 19 smd rect (at 4.7 3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /GPIOexpander0/INT1))
    (pad 18 smd rect (at 4.7 4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 110 /GPIOexpander0/INT1))
    (pad 17 smd rect (at 4.7 5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 4.7 6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C1400-Pad2)"))
    (pad 15 smd rect (at 4.7 8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 106 /GPIOexpander4/ADDR))
    (pad 14 smd rect (at -4.7 8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -4.7 6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 /ButtonExpander/SDA))
    (pad 12 smd rect (at -4.7 5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 /ButtonExpander/SCL))
    (pad 11 smd rect (at -4.7 4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 10 smd rect (at -4.7 3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -4.7 1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(R1430-Pad1)"))
    (pad 8 smd rect (at -4.7 0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(J1430-Pad4)"))
    (pad 7 smd rect (at -4.7 -0.635 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(J1430-Pad3)"))
    (pad 6 smd rect (at -4.7 -1.905 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(J1430-Pad2)"))
    (pad 5 smd rect (at -4.7 -3.175 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(J1430-Pad1)"))
    (pad 4 smd rect (at -4.7 -4.445 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(R1420-Pad1)"))
    (pad 3 smd rect (at -4.7 -5.715 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(J1420-Pad4)"))
    (pad 2 smd rect (at -4.7 -6.985 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -4.7 -8.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module digikey-footprints:3-SIP_Module_V7805-1000 (layer F.Cu) (tedit 59C4038A)
    (at 104.2 27 90)
    (descr http://www.cui.com/product/resource/v78xx-1000.pdf)
    (fp_text reference U101 (at 2.91 -3.12 90) (layer F.SilkS))
    (fp_text value V7805-1000 (at 2.53 8.04 90) (layer F.Fab))
    (fp_text user %R (at 2.51 3.57 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C101-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 +24V))
  )
  (module ProductDoser:Potentiometer_Bourns_3361_Horizontal (layer F.Cu) (tedit 61AC45AE)
    (at 101.75 35.1 270)
    (descr "Potentiometer, horizontal, Bourns 3314S, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
    (tags "Potentiometer horizontal Bourns 3314S")
    (attr smd)
    (fp_text reference RV200 (at 0 -7.62 90) (layer F.SilkS))
    (fp_text value 10K (at 0 4.15 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at -2.29 -4.255 270) (size 1.2 3.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 4.255 270) (size 1.2 3.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(DS200-Pad3)"))
    (pad 1 smd rect (at 2.29 -4.255 270) (size 1.2 3.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314S_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 175.8375 121.3)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1432 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(Q1430-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 171.6 129.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1431 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(D1430-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 175.8375 119.3)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1430 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(Q1430-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 "Net-(R1430-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 175.8375 111)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1422 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 "Net-(Q1420-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 164.6 129.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1421 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(D1420-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 175.8375 109)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1420 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 "Net-(Q1420-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R1420-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 175.8375 100.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1412 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(Q1410-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 157.6 129.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1411 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(D1410-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 175.8375 98.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1410 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(Q1410-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R1410-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 153.8 68.7625 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1400 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C1400-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 149.5375 121.3)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1032 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(Q1030-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 149.5375 119.3)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1030 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Net-(Q1030-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R1030-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 149.5375 111)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1022 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(Q1020-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 149.5375 109)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1020 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(Q1020-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 104 "Net-(R1020-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 149.5375 100.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1012 (at 4.0625 0) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(Q1010-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 131.3 129.7)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1011 (at 4.0625 0) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D1010-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 149.5375 98.6)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1010 (at 4.0625 0) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(Q1010-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(R1010-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 131.5 65.6375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 /GPIOexpander0/ADDR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 129.5 65.6375 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 /GPIOexpander0/ADDR))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 177.3 31.55 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 /ButtonExpander/INT2))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 181.6 23.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R400 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /ButtonExpander/RST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 115.2 134.2625 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R382 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(Q380-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 115.2 141.1625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R381 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(D380-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 115.2 130.7625 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R380 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(Q380-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 /ValvesSheet/Vlv.Pump4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 112.3375 127.9)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R372 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(Q370-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 108.8375 129.9 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R371 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(D370-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 108.8375 127.9)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R370 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(Q370-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /ValvesSheet/Vlv.Pump3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 95.2 140.2375 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R362 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(Q360-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 93.2 136.6375 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R361 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D360-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 95.2 136.6375 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R360 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(Q360-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /ValvesSheet/Vlv.Pump2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 116.3375 99.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R322 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(Q320-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 112.7375 101.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R321 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D320-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 112.7375 99.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R320 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(Q320-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /ValvesSheet/Vlv.MnfldDrain))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 108.8375 99.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R312 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(Q310-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 105.2375 101.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R311 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D310-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 105.2375 99.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R310 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(Q310-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 /ValvesSheet/Vlv.Water))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 101.3 99.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R302 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(Q300-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 97.7625 101.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R301 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D300-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 97.7625 99.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R300 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(Q300-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /ValvesSheet/Vlv.EndDrain))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 144.5625 23 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R101 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 /ButtonExpander/SDA))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 175.9 125.6 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1430 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D1430-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(Q1430-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 175.9 115.3 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1420 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D1420-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(Q1420-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 175.9 105 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1410 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D1410-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(Q1410-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 149.6 125.6 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1030 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D1030-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(Q1030-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 149.6 115.3 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1020 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1020-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(Q1020-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 149.6 105 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1010 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D1010-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(Q1010-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-3_TabPin2 (layer F.Cu) (tedit 5A70F30B)
    (at 121.875 132.52)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q380 (at 0 -4.5) (layer F.SilkS))
    (fp_text value IPD050N03LG (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad 2 smd rect (at 2.1 0) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 22 "Net-(D380-Pad1)"))
    (pad 3 smd rect (at -4.2 2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.2 0) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D380-Pad1)"))
    (pad 1 smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(Q380-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 92 140.2 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q360 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D360-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(Q360-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 116.3 103 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q320 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D320-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(Q320-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 108.8 103 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q310 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D310-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(Q310-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 101.3 103 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q300 (at 0 -2.5) (layer F.SilkS))
    (fp_text value SI3402-TP (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D300-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(Q300-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Taiyo-Yuden_NR-50xx (layer F.Cu) (tedit 5990349D)
    (at 114.3 28.3 90)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-50xx, 4.9mmx4.9mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L100 (at 0 -3.45 90) (layer F.SilkS))
    (fp_text value "10µH - 24µH" (at 0 3.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.8 0 90) (size 1.5 4.2) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 1 smd rect (at -1.8 0 90) (size 1.5 4.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C101-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Taiyo-Yuden_NR-50xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_6_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BF224)
    (at 156.4 147.5)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J1440 (at 8.75 -5.25) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x06 (at 8.75 4.45) (layer F.Fab))
    (fp_text user %R (at 8.75 2.7) (layer F.Fab))
    (pad 6 thru_hole circle (at 17.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(D1430-Pad1)"))
    (pad 5 thru_hole circle (at 14 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(D1420-Pad1)"))
    (pad 3 thru_hole circle (at 7 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "Net-(D1410-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_5_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BC220)
    (at 156.4 122.8)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J1430 (at 7 -5.25) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 7 4.45) (layer F.Fab))
    (fp_text user %R (at 7 2.7) (layer F.Fab))
    (pad 5 thru_hole circle (at 14 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 "Net-(J1430-Pad4)"))
    (pad 3 thru_hole circle (at 7 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 76 "Net-(J1430-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 77 "Net-(J1430-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 78 "Net-(J1430-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_5_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BC220)
    (at 156.4 112.5)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J1420 (at 7 -5.25) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 7 4.45) (layer F.Fab))
    (fp_text user %R (at 7 2.7) (layer F.Fab))
    (pad 5 thru_hole circle (at 14 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 "Net-(J1420-Pad4)"))
    (pad 3 thru_hole circle (at 7 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 "Net-(J1420-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 "Net-(J1420-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 "Net-(J1420-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_5_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BC220)
    (at 156.4 102.2)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J1410 (at 7 -5.25) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 7 4.45) (layer F.Fab))
    (fp_text user %R (at 7 2.7) (layer F.Fab))
    (pad 5 thru_hole circle (at 14 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 "Net-(J1410-Pad4)"))
    (pad 3 thru_hole circle (at 7 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 "Net-(J1410-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 "Net-(J1410-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 "Net-(J1410-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_5_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BC220)
    (at 130.1 112.5)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J1020 (at 7 -5.25) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 7 4.45) (layer F.Fab))
    (fp_text user %R (at 7 2.7) (layer F.Fab))
    (pad 5 thru_hole circle (at 14 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 "Net-(J1020-Pad4)"))
    (pad 3 thru_hole circle (at 7 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 60 "Net-(J1020-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 "Net-(J1020-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 "Net-(J1020-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_5_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BC220)
    (at 130.1 102.2)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J1010 (at 7 -5.25) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 7 4.45) (layer F.Fab))
    (fp_text user %R (at 7 2.7) (layer F.Fab))
    (pad 5 thru_hole circle (at 14 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 55 "Net-(J1010-Pad4)"))
    (pad 3 thru_hole circle (at 7 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 56 "Net-(J1010-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 57 "Net-(J1010-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 "Net-(J1010-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_5_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BC220)
    (at 189.5 38.75 270)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J401 (at 7 -5.25 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 7 4.45 90) (layer F.Fab))
    (fp_text user %R (at 7 2.7 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 14 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 10.5 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 "Net-(J401-Pad4)"))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "Net-(J401-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(J401-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(J401-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_5_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BC220)
    (at 189.5 20.5 270)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J400 (at 7 -5.25 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 7 4.45 90) (layer F.Fab))
    (fp_text user %R (at 7 2.7 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 14 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "Net-(J400-Pad5)"))
    (pad 4 thru_hole circle (at 10.5 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 "Net-(J400-Pad4)"))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "Net-(J400-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 "Net-(J400-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_6_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BF224)
    (at 98.2 147.5)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J302 (at 8.75 -5.25) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x06 (at 8.75 4.45) (layer F.Fab))
    (fp_text user %R (at 8.75 2.7) (layer F.Fab))
    (pad 6 thru_hole circle (at 17.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (pad 5 thru_hole circle (at 14 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(D380-Pad1)"))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (pad 3 thru_hole circle (at 7 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(D370-Pad1)"))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_6_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BF224)
    (at 98.2 119.4)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J300 (at 8.75 -5.25) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x06 (at 8.75 4.45) (layer F.Fab))
    (fp_text user %R (at 8.75 2.7) (layer F.Fab))
    (pad 6 thru_hole circle (at 17.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (pad 5 thru_hole circle (at 14 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(D320-Pad1)"))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (pad 3 thru_hole circle (at 7 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(D310-Pad1)"))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(D300-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ProductDoser:Wanjie_3.50mm_Angled_5_Pin_Terminal_Blocks (layer F.Cu) (tedit 623BC220)
    (at 89.6 34.6 90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J100 (at 7 -5.25 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 7 4.45 90) (layer F.Fab))
    (fp_text user %R (at 7 2.7 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 14 0 90) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 4 thru_hole circle (at 10.5 0 90) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 "Net-(J100-Pad4)"))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.6 2.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 171.6 137.8 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D1431 (at 0 -4.1 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D1430-Pad1)"))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 171.6 131.8 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1430 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(D1430-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(D1430-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 164.6 137.8 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D1421 (at 0 -4.1 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D1420-Pad1)"))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 164.6 131.8 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1420 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(D1420-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(D1420-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 157.6 137.8 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D1411 (at 0 -4.1 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D1410-Pad1)"))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 157.6 131.8 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1410 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(D1410-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(D1410-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 145.3 137.8 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D1031 (at 0 -4.1 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D1030-Pad1)"))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 145.3 131.8 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1030 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D1030-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D1030-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 138.3 137.8 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D1021 (at 0 0 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1020-Pad1)"))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 138.3 131.8 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1020 (at -3.1375 0) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D1020-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D1020-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 131.3 137.8 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D1011 (at 0 0 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D1010-Pad1)"))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 131.3 131.8 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1010 (at -4.0625 0) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D1010-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D1010-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 122.5 139.5)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D381 (at 0 -4.1) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0 -1.9) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 90) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D380-Pad1)"))
    (pad 1 smd rect (at -3.4 0 90) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 115.2 137.7625 270)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D380 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(D380-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D380-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 110.5 137.9 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D371 (at 0 -4.1 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D370-Pad1)"))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 108.8375 131.9 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D370 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(D370-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(D370-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 91.2 136.6375 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D360 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D360-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(D360-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 114.4 109.8 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D321 (at 0 -4.1 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D320-Pad1)"))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 112.7375 103.8 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D320 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D320-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D320-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 106.9 109.8 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D311 (at 0 -4.1 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D310-Pad1)"))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 105.2375 103.8 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D310 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D310-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D310-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 99.4 109.8 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D301 (at 0 -4.1 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D300-Pad1)"))
    (pad 1 smd rect (at -3.4 0 180) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 97.7625 103.8 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D300 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(D300-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D300-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 167.8 73.1625 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1401 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 153.8 72.2375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1400 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C1400-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 127.5 72.2375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1000 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C1000-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 181.6 25.8 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C400 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /ButtonExpander/RST))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_2220_5650Metric (layer F.Cu) (tedit 5B301BBE)
    (at 115.25 22.3)
    (descr "Capacitor SMD 2220 (5650 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C102 (at 0 -3.65) (layer F.SilkS))
    (fp_text value 22µF (at 0 3.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.55 0) (size 1.8 5.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.138889)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.55 0) (size 1.8 5.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.138889)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_2220_5650Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_2220_5650Metric (layer F.Cu) (tedit 5B301BBE)
    (at 98.6 26.75 90)
    (descr "Capacitor SMD 2220 (5650 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C100 (at 0 -3.65 90) (layer F.SilkS))
    (fp_text value 10µF (at 0 3.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.55 0 90) (size 1.8 5.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.138889)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.55 0 90) (size 1.8 5.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.138889)
      (net 2 +24V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_2220_5650Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Product Doser Test V1" (at 87.1 137.7 90) (layer F.SilkS))
  (gr_line (start 194 18.3) (end 194 76.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 85 18.3) (end 194 18.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 85 153.5) (end 85 18.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 183 153.5) (end 85 153.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 183 76.8) (end 183 153.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 194 76.8) (end 183 76.8) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 194 153.5) (xy 85 153.5) (xy 85 18.3) (xy 194 18.3)
      )
    )
  )
  (zone (net 2) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 102 90) (xy 194 90) (xy 194 153.5) (xy 85 153.5) (xy 85 18.3)
        (xy 102 18.3)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 193.9 87.8) (xy 104.2 87.8) (xy 104.2 40.5) (xy 127.5 40.5) (xy 127.5 18.4)
        (xy 193.9 18.4)
      )
    )
  )
  (zone (net 4) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.6 39.5) (xy 104.2 39.5) (xy 104.2 18.4) (xy 126.6 18.4)
      )
    )
  )
)
