(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6002)
    (drawings 64)
    (tracks 1361)
    (zones 0)
    (modules 91)
    (nets 130)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.8796 1.8796)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 130 110)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x011cc_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 "Net-(ANT1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 +3V3)
  (net 6 "Net-(C6-Pad2)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 /ESP8285/RST)
  (net 9 +5V)
  (net 10 GNDPWR)
  (net 11 "Net-(Cc1-Pad2)")
  (net 12 "Net-(Cc1-Pad1)")
  (net 13 "Net-(Cs1-Pad2)")
  (net 14 "Net-(D3-PadA)")
  (net 15 "Net-(D4-PadA)")
  (net 16 "Net-(D4-PadC)")
  (net 17 "Net-(D5-PadA)")
  (net 18 /Din)
  (net 19 /SDA)
  (net 20 /SCL)
  (net 21 /ESP8285/GPIO15)
  (net 22 /ESP8285/GPIO16)
  (net 23 /USB-UART/D+)
  (net 24 /USB-UART/D-)
  (net 25 "Net-(NE1-Pad1)")
  (net 26 "Net-(NE1-Pad2)")
  (net 27 "Net-(NE2-Pad1)")
  (net 28 "Net-(NE2-Pad2)")
  (net 29 "Net-(Q1-Pad4)")
  (net 30 /ESP8285/GPIO2)
  (net 31 /ESP8285/GPIO4)
  (net 32 /ESP8285/A0)
  (net 33 /ESP8285/CH_PD)
  (net 34 "Net-(R8-Pad1)")
  (net 35 "Net-(R10-Pad1)")
  (net 36 ADC)
  (net 37 /USB-UART/RTS)
  (net 38 "Net-(R27-Pad2)")
  (net 39 /USB-UART/DTR)
  (net 40 /ESP8285/GPIO0)
  (net 41 "Net-(Rf1-Pad2)")
  (net 42 "Net-(U1-Pad15)")
  (net 43 "Net-(U1-Pad16)")
  (net 44 "Net-(U1-Pad17)")
  (net 45 "Net-(U1-Pad18)")
  (net 46 "Net-(U1-Pad19)")
  (net 47 "Net-(U1-Pad20)")
  (net 48 "Net-(U1-Pad21)")
  (net 49 "Net-(U1-Pad22)")
  (net 50 "Net-(U1-Pad23)")
  (net 51 "Net-(U1-Pad24)")
  (net 52 "Net-(U1-Pad25)")
  (net 53 "Net-(U1-Pad26)")
  (net 54 "Net-(U1-Pad28)")
  (net 55 "Net-(U1-Pad31)")
  (net 56 "Net-(U1-Pad32)")
  (net 57 "Net-(U1-Pad34)")
  (net 58 "Net-(U1-Pad35)")
  (net 59 "Net-(U1-Pad36)")
  (net 60 "Net-(U1-Pad37)")
  (net 61 "Net-(U1-Pad38)")
  (net 62 "Net-(U1-Pad39)")
  (net 63 "Net-(U1-Pad40)")
  (net 64 "Net-(U1-Pad41)")
  (net 65 /ESP8285/GPIO13)
  (net 66 /ESP8285/GPIO12)
  (net 67 /ESP8285/GPIO14)
  (net 68 "Net-(U2-Pad6)")
  (net 69 "Net-(U2-Pad9)")
  (net 70 "Net-(U3-Pad5)")
  (net 71 "Net-(U3-Pad20)")
  (net 72 "Net-(U3-Pad21)")
  (net 73 "Net-(U3-Pad22)")
  (net 74 "Net-(U3-Pad23)")
  (net 75 /USB-UART/CTS)
  (net 76 /HVPS_SMD/Vadj)
  (net 77 "Net-(C14-Pad1)")
  (net 78 "Net-(D2-PadA)")
  (net 79 "Net-(D3-PadC)")
  (net 80 "Net-(Q1-Pad5)")
  (net 81 "Net-(R21-Pad2)")
  (net 82 "Net-(R23-Pad2)")
  (net 83 "Net-(R24-Pad1)")
  (net 84 "Net-(R26-Pad2)")
  (net 85 "Net-(T1-Pad3)")
  (net 86 "Net-(T1-Pad12)")
  (net 87 "Net-(T1-Pad11)")
  (net 88 "Net-(T1-Pad10)")
  (net 89 "Net-(U4-Pad4)")
  (net 90 "Net-(U6-Pad1)")
  (net 91 "Net-(U6-Pad10)")
  (net 92 "Net-(U6-Pad12)")
  (net 93 "Net-(U6-Pad16)")
  (net 94 "Net-(U6-Pad17)")
  (net 95 "Net-(U6-Pad22)")
  (net 96 /HV6)
  (net 97 /HV12)
  (net 98 /HV5)
  (net 99 /HV11)
  (net 100 /HV4)
  (net 101 /HV10)
  (net 102 /HV3)
  (net 103 /HV9)
  (net 104 /HV2)
  (net 105 /HV8)
  (net 106 /HV1)
  (net 107 /HV7)
  (net 108 "Net-(J1-Pad15)")
  (net 109 "Net-(J4-Pad1)")
  (net 110 "Net-(J4-Pad2)")
  (net 111 "Net-(J4-Pad3)")
  (net 112 /VBus)
  (net 113 /HV13)
  (net 114 /HV14)
  (net 115 /HV15)
  (net 116 Vcc)
  (net 117 HV)
  (net 118 "Net-(IC1-Pad4)")
  (net 119 /USB-UART/VBusDet)
  (net 120 "Net-(R18-Pad1)")
  (net 121 /USB-UART/CHG_DET)
  (net 122 /USB-UART/CHG_AL)
  (net 123 "Net-(M1-PadDP_H)")
  (net 124 "Net-(M1-PadDM_H)")
  (net 125 "Net-(U6-Pad11)")
  (net 126 "Net-(U6-Pad24)")
  (net 127 "Net-(D6-Pad1)")
  (net 128 "Net-(U3-Pad24)")
  (net 129 "Net-(J3-Pad4)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net +5V)
    (add_net /Din)
    (add_net /ESP8285/A0)
    (add_net /ESP8285/CH_PD)
    (add_net /ESP8285/GPIO0)
    (add_net /ESP8285/GPIO12)
    (add_net /ESP8285/GPIO13)
    (add_net /ESP8285/GPIO14)
    (add_net /ESP8285/GPIO15)
    (add_net /ESP8285/GPIO16)
    (add_net /ESP8285/GPIO2)
    (add_net /ESP8285/GPIO4)
    (add_net /ESP8285/RST)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV11)
    (add_net /HV12)
    (add_net /HV13)
    (add_net /HV14)
    (add_net /HV15)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net /HVPS_SMD/Vadj)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /USB-UART/CHG_AL)
    (add_net /USB-UART/CHG_DET)
    (add_net /USB-UART/CTS)
    (add_net /USB-UART/D+)
    (add_net /USB-UART/D-)
    (add_net /USB-UART/DTR)
    (add_net /USB-UART/RTS)
    (add_net /USB-UART/VBusDet)
    (add_net /VBus)
    (add_net ADC)
    (add_net GND)
    (add_net GNDPWR)
    (add_net HV)
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(Cc1-Pad1)")
    (add_net "Net-(Cc1-Pad2)")
    (add_net "Net-(Cs1-Pad2)")
    (add_net "Net-(D2-PadA)")
    (add_net "Net-(D3-PadA)")
    (add_net "Net-(D3-PadC)")
    (add_net "Net-(D4-PadA)")
    (add_net "Net-(D4-PadC)")
    (add_net "Net-(D5-PadA)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(M1-PadDM_H)")
    (add_net "Net-(M1-PadDP_H)")
    (add_net "Net-(NE1-Pad1)")
    (add_net "Net-(NE1-Pad2)")
    (add_net "Net-(NE2-Pad1)")
    (add_net "Net-(NE2-Pad2)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(Q1-Pad5)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R24-Pad1)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(Rf1-Pad2)")
    (add_net "Net-(T1-Pad10)")
    (add_net "Net-(T1-Pad11)")
    (add_net "Net-(T1-Pad12)")
    (add_net "Net-(T1-Pad3)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(U3-Pad21)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad23)")
    (add_net "Net-(U3-Pad24)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U6-Pad1)")
    (add_net "Net-(U6-Pad10)")
    (add_net "Net-(U6-Pad11)")
    (add_net "Net-(U6-Pad12)")
    (add_net "Net-(U6-Pad16)")
    (add_net "Net-(U6-Pad17)")
    (add_net "Net-(U6-Pad22)")
    (add_net "Net-(U6-Pad24)")
    (add_net Vcc)
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class 50Ohm ""
    (clearance 0.1524)
    (trace_width 0.8001)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm locked (layer F.Cu) (tedit 59650532)
    (at 119.84 92.54 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Nixie (at -4.26 10.16 180) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 HV))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 HV))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 /HV6))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 /HV12))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 /HV5))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 /HV11))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /HV4))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 /HV10))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 /HV3))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 /HV9))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 /HV2))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 /HV8))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 /HV1))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 /HV7))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(J1-Pad15)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 130 80)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference Mount3 (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 154 128)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference Mount2 (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 106 128)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference Mount1 (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 128.349 84.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.549 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 76 /HVPS_SMD/Vadj))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 157.5 95 225)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.456489 0.038184 225) (layer F.SilkS))
    (fp_text value 12pF (at 0 1.5 225) (layer F.Fab))
    (fp_text user %R (at 0 0 225) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 225) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 225) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 154 91.5 45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.276884 0.062225 45) (layer F.SilkS))
    (fp_text value 12pF (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 153.48239 103.52618)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.17161 0.12382) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 153.48239 102.02618)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.17161 -0.15418) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 143.127 86.873 315)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0.070711 -2.012426 315) (layer F.SilkS))
    (fp_text value 5.6pF (at 0 1.5 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 315) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -0.75 0 315) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 121 140.861 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 1.861 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /ESP8285/RST))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 115 79.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -1.8 1.25) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GNDPWR))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 138.75 115.24428 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 2.75 0.04428 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 138.75 113.74428 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 2.75 0.14428 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 108.430803 110.528243 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 -1.5 135) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.5 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C14-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 106.002389 104.917849 45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference Cc1 (at 0 -1.5 45) (layer F.SilkS))
    (fp_text value 22nF (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Cc1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Cc1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 118.824 111.778 45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference Cs1 (at 0 -1.5 45) (layer F.SilkS))
    (fp_text value 360pF (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Cs1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 45) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 116 Vcc))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-LED:SparkFun-LED-LED-0603 (layer B.Cu) (tedit 200000)
    (at 159.7 121.6)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference D3 (at 2.558 0) (layer B.SilkS))
    (fp_text value TX (at -2.750837 3.647123) (layer B.SilkS) hide)
    (pad C smd rect (at 0.8763 0 90) (size 0.99822 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(D3-PadC)"))
    (pad A smd rect (at -0.8763 0 90) (size 0.99822 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D3-PadA)"))
  )
  (module SparkFun-LED:SparkFun-LED-LED-0603 (layer B.Cu) (tedit 200000)
    (at 159.7237 120)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference D4 (at -0.1237 -1.2) (layer B.SilkS))
    (fp_text value RX (at 1.529273 7.137202) (layer B.SilkS) hide)
    (pad C smd rect (at 0.8763 0 90) (size 0.99822 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D4-PadC)"))
    (pad A smd rect (at -0.8763 0 90) (size 0.99822 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D4-PadA)"))
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm locked (layer F.Cu) (tedit 59650532)
    (at 162.5 115.08 180)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J2 (at 4.56 -2.286 180) (layer F.SilkS) hide)
    (fp_text value Expansion (at 1.27 12.49 180) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 /VBus))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 Vcc))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /SDA))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /SCL))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /ESP8285/GPIO15))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /ESP8285/GPIO16))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /ESP8285/RST))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "nixiemisc:nixiemisc-B3U-1100P(M)" (layer F.Cu) (tedit 200000)
    (at 124.50248 140 270)
    (attr smd)
    (fp_text reference K1 (at 4.572 -1.0414 270) (layer F.SilkS) hide)
    (fp_text value RST (at -2.822 0.09048) (layer F.SilkS))
    (pad GND smd rect (at 0 1.64846 270) (size 0.79756 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.74752 0 270) (size 0.59944 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 8 /ESP8285/RST))
    (pad 1 smd rect (at -1.74752 0 270) (size 0.59944 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module nixiemisc:nixiemisc-THT-100-35 (layer F.Cu) (tedit 200000)
    (at 107.14 133 317.5)
    (attr virtual)
    (fp_text reference NE1 (at 1.349102 -2.287389 317.5) (layer F.SilkS))
    (fp_text value Left (at 0 0 317.5) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 2.54 0 317.5) (size 1.778 1.778) (drill 0.89916) (layers *.Cu *.Mask)
      (net 26 "Net-(NE1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 317.5) (size 1.778 1.778) (drill 0.89916) (layers *.Cu *.Mask)
      (net 25 "Net-(NE1-Pad1)"))
  )
  (module nixiemisc:nixiemisc-THT-100-35 (layer F.Cu) (tedit 200000)
    (at 150.955 134.892 42.5)
    (attr virtual)
    (fp_text reference NE2 (at 1.34 -2.3 42.5) (layer F.SilkS))
    (fp_text value Right (at 0 0 42.5) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 2.54 0 42.5) (size 1.778 1.778) (drill 0.89916) (layers *.Cu *.Mask)
      (net 28 "Net-(NE2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 42.5) (size 1.778 1.778) (drill 0.89916) (layers *.Cu *.Mask)
      (net 27 "Net-(NE2-Pad1)"))
  )
  (module nixiemisc:nixiemisc-SO08 (layer F.Cu) (tedit 200000)
    (at 116.653068 106.62353 315)
    (descr "SOIC, 0.15 INCH WIDTH")
    (tags "SOIC, 0.15 INCH WIDTH")
    (attr smd)
    (fp_text reference Q1 (at 0.087258 0.020887 135) (layer F.SilkS))
    (fp_text value AO4294 (at 0.19703 0 315) (layer F.SilkS) hide)
    (pad 8 smd rect (at -1.905 -2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(Q1-Pad5)"))
    (pad 7 smd rect (at -0.635 -2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(Q1-Pad5)"))
    (pad 6 smd rect (at 0.635 -2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(Q1-Pad5)"))
    (pad 5 smd rect (at 1.905 -2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(Q1-Pad5)"))
    (pad 4 smd rect (at 1.905 2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q1-Pad4)"))
    (pad 3 smd rect (at 0.635 2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at -0.635 2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C14-Pad1)"))
    (pad 1 smd rect (at -1.905 2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C14-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 113 133 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 120k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 117 HV))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(NE1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 147.387 133)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.638) (layer F.SilkS))
    (fp_text value 120k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 117 HV))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(NE2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 130.762 84.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.638 180) (layer F.SilkS))
    (fp_text value 2k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 /ESP8285/GPIO4))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 /HVPS_SMD/Vadj))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixiemisc:nixiemisc-THT-150-35 (layer F.Cu) (tedit 200000)
    (at 127.94 138.6)
    (attr virtual)
    (fp_text reference R5 (at 0 0) (layer F.SilkS))
    (fp_text value R_PHOTO (at 1.96 -2) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.778 1.778) (drill 0.89916) (layers *.Cu *.Mask)
      (net 32 /ESP8285/A0))
    (pad 1 thru_hole circle (at 0 0) (size 1.778 1.778) (drill 0.89916) (layers *.Cu *.Mask)
      (net 5 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 134.9 138.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /ESP8285/A0))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 144.716 95.374 315)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0.115966 1.530179 315) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 315) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.75 0 315) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /ESP8285/CH_PD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 151.73 90.52 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0.078 1.384 90) (layer F.SilkS))
    (fp_text value 12K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 149.76 90.44 45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 2.190617 0.038184 45) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 45) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.75 0 45) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /ESP8285/RST))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 5BF1A515)
    (at 140.135 83.881 315)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R10 (at -2.617002 -0.137886 315) (layer F.SilkS))
    (fp_text value 0 (at -2.556898 -0.244659 315) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.84836 0 315) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 1 smd rect (at -0.84836 0 315) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R10-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 147.4 101.3 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0.444 1.396 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /ESP8285/GPIO15))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-Resistors:SparkFun-Resistors-0603 (layer F.Cu) (tedit 5BF1A4FB)
    (at 142.635 82.881 225)
    (descr "GENERIC 1608 (0603) PACKAGE")
    (tags "GENERIC 1608 (0603) PACKAGE")
    (attr smd)
    (fp_text reference R12 (at -2.578111 -0.059397 225) (layer F.SilkS))
    (fp_text value 0 (at 0 1.066801 225) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.84836 0 225) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 1 smd rect (at -0.84836 0 225) (size 1.09982 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(ANT1-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 145.478 93.088 45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.45 45) (layer F.SilkS))
    (fp_text value 220K (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 45) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /ESP8285/A0))
    (pad 2 smd rect (at 0.75 0 45) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 ADC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 146.748 94.358 225)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -2.421134 -0.115966 225) (layer F.SilkS))
    (fp_text value 100K (at 0 1.5 225) (layer F.Fab))
    (fp_text user %R (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 ADC))
    (pad 2 smd rect (at 0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 151.55 102.78 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /ESP8285/GPIO2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 157.686 125.113)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 1.872 -0.133 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R18-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 143 118.001)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at -2.459 -0.127) (layer F.SilkS))
    (fp_text value 1K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 146.094 103.619)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 1.94 0.031 90) (layer F.SilkS))
    (fp_text value 12K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 /USB-UART/RTS))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R23-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 146.095 108.086)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at -0.093 1.406) (layer F.SilkS))
    (fp_text value 12K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R24-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 /USB-UART/DTR))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 149.5 106.03 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 /ESP8285/GPIO0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 108.477263 100.675208 315)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at -2.653398 0.142874 315) (layer F.SilkS))
    (fp_text value 10.2k (at 0 1.5 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 315) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R27-Pad2)"))
    (pad 2 smd rect (at 0.75 0 315) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 109.891477 99.260994 315)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at -2.653398 0.021555 315) (layer F.SilkS))
    (fp_text value 30k (at 0 1.5 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 315) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 /HVPS_SMD/Vadj))
    (pad 2 smd rect (at 0.75 0 315) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R27-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 121.166317 109.106438 45)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference Rs1 (at 0 -1.850001 45) (layer F.SilkS))
    (fp_text value 249 (at 0 1.95 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 45) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Cs1-Pad2)"))
    (pad 2 smd rect (at 1.45 0 45) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(Q1-Pad5)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2010 (layer F.Cu) (tedit 58E0A804)
    (at 109.537923 107.039169 135)
    (descr "Resistor SMD 2010, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2010")
    (attr smd)
    (fp_text reference Rsen1 (at 0 -2.25 135) (layer F.SilkS))
    (fp_text value 0.04 (at 0 2.4 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -2.450001 0 135) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 2.450001 0 135) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2010.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixiemisc:nixiemisc-QFN-44-7X7 (layer F.Cu) (tedit 200000)
    (at 129.05004 101.92026 270)
    (descr "QFN-44 (7X7X1.8MM)")
    (tags "QFN-44 (7X7X1.8MM)")
    (attr smd)
    (fp_text reference U1 (at -4.62026 -0.18796) (layer F.SilkS) hide)
    (fp_text value HV5523 (at 4.97974 -0.24996) (layer F.SilkS))
    (pad EXP smd rect (at 0 0 270) (size 5.14858 5.14858) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 44 smd rect (at -2.49936 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 115 /HV15))
    (pad 43 smd rect (at -1.99898 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 114 /HV14))
    (pad 42 smd rect (at -1.4986 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 113 /HV13))
    (pad 41 smd rect (at -0.99822 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U1-Pad41)"))
    (pad 40 smd rect (at -0.49784 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad40)"))
    (pad 39 smd rect (at 0 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U1-Pad39)"))
    (pad 38 smd rect (at 0.49784 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U1-Pad38)"))
    (pad 37 smd rect (at 0.99822 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U1-Pad37)"))
    (pad 36 smd rect (at 1.4986 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U1-Pad36)"))
    (pad 35 smd rect (at 1.99898 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U1-Pad35)"))
    (pad 34 smd rect (at 2.49936 -3.32486 180) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U1-Pad34)"))
    (pad 33 smd rect (at 3.32486 -2.49936 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 32 smd rect (at 3.32486 -1.99898 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-Pad32)"))
    (pad 31 smd rect (at 3.32486 -1.4986 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U1-Pad31)"))
    (pad 30 smd rect (at 3.32486 -0.99822 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 29 smd rect (at 3.32486 -0.49784 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 28 smd rect (at 3.32486 0 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U1-Pad28)"))
    (pad 27 smd rect (at 3.32486 0.49784 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at 3.32486 0.99822 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U1-Pad26)"))
    (pad 25 smd rect (at 3.32486 1.4986 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U1-Pad25)"))
    (pad 24 smd rect (at 3.32486 1.99898 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-Pad24)"))
    (pad 23 smd rect (at 3.32486 2.49936 90) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad23)"))
    (pad 22 smd rect (at 2.49936 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-Pad22)"))
    (pad 21 smd rect (at 1.99898 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U1-Pad21)"))
    (pad 20 smd rect (at 1.4986 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad20)"))
    (pad 19 smd rect (at 0.99822 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad19)"))
    (pad 18 smd rect (at 0.49784 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad18)"))
    (pad 17 smd rect (at 0 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad17)"))
    (pad 16 smd rect (at -0.49784 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad16)"))
    (pad 15 smd rect (at -0.99822 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad15)"))
    (pad 14 smd rect (at -1.4986 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(NE2-Pad1)"))
    (pad 13 smd rect (at -1.99898 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(NE1-Pad1)"))
    (pad 12 smd rect (at -2.49936 3.32486) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 97 /HV12))
    (pad 11 smd rect (at -3.32486 2.49936 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 99 /HV11))
    (pad 10 smd rect (at -3.32486 1.99898 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 101 /HV10))
    (pad 9 smd rect (at -3.32486 1.4986 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 103 /HV9))
    (pad 8 smd rect (at -3.32486 0.99822 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 105 /HV8))
    (pad 7 smd rect (at -3.32486 0.49784 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 107 /HV7))
    (pad 6 smd rect (at -3.32486 0 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 96 /HV6))
    (pad 5 smd rect (at -3.32486 -0.49784 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 98 /HV5))
    (pad 4 smd rect (at -3.32486 -0.99822 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 100 /HV4))
    (pad 3 smd rect (at -3.32486 -1.4986 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 102 /HV3))
    (pad 2 smd rect (at -3.32486 -1.99898 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 104 /HV2))
    (pad 1 smd rect (at -3.32486 -2.49936 270) (size 0.79756 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 106 /HV1))
  )
  (module nixiemisc:nixiemisc-VQFN-14 (layer F.Cu) (tedit 200000)
    (at 136.84022 108.10262 90)
    (attr smd)
    (fp_text reference U2 (at 2.80262 0.05978 180) (layer F.SilkS))
    (fp_text value TXS0104 (at -0.5715 2.9972 90) (layer F.SilkS) hide)
    (pad 15 smd rect (at 0 0 90) (size 2.04978 2.04978) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -1.68402 -0.7493 90) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 13 smd rect (at -0.99822 -1.68402) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 18 /Din))
    (pad 12 smd rect (at -0.49784 -1.68402) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-Pad32)"))
    (pad 11 smd rect (at 0 -1.68402) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U1-Pad31)"))
    (pad 10 smd rect (at 0.49784 -1.68402) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U1-Pad28)"))
    (pad 9 smd rect (at 0.99822 -1.68402) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U2-Pad9)"))
    (pad 8 smd rect (at 1.68402 -0.7493 270) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 7 smd rect (at 1.68402 0.7493 270) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.99822 1.68402 180) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at 0.49784 1.68402 180) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(J4-Pad1)"))
    (pad 4 smd rect (at 0 1.68402 180) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(J4-Pad2)"))
    (pad 3 smd rect (at -0.49784 1.68402 180) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(J4-Pad3)"))
    (pad 2 smd rect (at -0.99822 1.68402 180) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 40 /ESP8285/GPIO0))
    (pad 1 smd rect (at -1.68402 0.7493 90) (size 0.89916 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
  )
  (module nixiemisc:nixiemisc-QFN-32 (layer F.Cu) (tedit 5BF1A4D4)
    (at 151.031631 96.502998 225)
    (descr "QFN 32-PIN PACKAGE W/ THERMAL PAD")
    (tags "QFN 32-PIN PACKAGE W/ THERMAL PAD")
    (attr smd)
    (fp_text reference U3 (at -1.447707 -4.011679 225) (layer F.SilkS) hide)
    (fp_text value 8285 (at -0.010866 -3.652469 225) (layer F.SilkS))
    (pad EP smd rect (at 0 0 225) (size 3.1496 3.1496) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 32 smd rect (at -2.49936 1.74752 225) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 8 /ESP8285/RST))
    (pad 31 smd rect (at -2.49936 1.24968 225) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R8-Pad1)"))
    (pad 30 smd rect (at -2.49936 0.749301 225) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 29 smd rect (at -2.499359 0.24892 225) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 28 smd rect (at -2.499359 -0.24892 225) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 27 smd rect (at -2.49936 -0.749301 225) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 26 smd rect (at -2.49936 -1.24968 225) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 20 /SCL))
    (pad 25 smd rect (at -2.49936 -1.74752 225) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 19 /SDA))
    (pad 24 smd rect (at -1.74752 -2.49936 135) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(U3-Pad24)"))
    (pad 23 smd rect (at -1.24968 -2.49936 135) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U3-Pad23)"))
    (pad 22 smd rect (at -0.749301 -2.49936 135) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U3-Pad22)"))
    (pad 21 smd rect (at -0.24892 -2.499359 135) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U3-Pad21)"))
    (pad 20 smd rect (at 0.24892 -2.499359 135) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U3-Pad20)"))
    (pad 19 smd rect (at 0.749301 -2.49936 135) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 122 /USB-UART/CHG_AL))
    (pad 18 smd rect (at 1.24968 -2.49936 135) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 121 /USB-UART/CHG_DET))
    (pad 17 smd rect (at 1.74752 -2.49936 135) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 16 smd rect (at 2.49936 -1.74752 45) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 31 /ESP8285/GPIO4))
    (pad 15 smd rect (at 2.49936 -1.24968 45) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 40 /ESP8285/GPIO0))
    (pad 14 smd rect (at 2.49936 -0.749301 45) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 30 /ESP8285/GPIO2))
    (pad 13 smd rect (at 2.499359 -0.24892 45) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 21 /ESP8285/GPIO15))
    (pad 12 smd rect (at 2.499359 0.24892 45) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 65 /ESP8285/GPIO13))
    (pad 11 smd rect (at 2.49936 0.749301 45) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 10 smd rect (at 2.49936 1.24968 45) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 66 /ESP8285/GPIO12))
    (pad 9 smd rect (at 2.49936 1.74752 45) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 67 /ESP8285/GPIO14))
    (pad 8 smd rect (at 1.74752 2.49936 315) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 22 /ESP8285/GPIO16))
    (pad 7 smd rect (at 1.24968 2.49936 315) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 33 /ESP8285/CH_PD))
    (pad 6 smd rect (at 0.749301 2.49936 315) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 36 ADC))
    (pad 5 smd rect (at 0.24892 2.499359 315) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U3-Pad5)"))
    (pad 4 smd rect (at -0.24892 2.499359 315) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 3 smd rect (at -0.749301 2.49936 315) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at -1.24968 2.49936 315) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -1.74752 2.49936 315) (size 0.79756 0.28448) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
  )
  (module adafruit:adafruit-U.FL locked (layer F.Cu) (tedit 200000)
    (at 138.57414 78.5 270)
    (attr smd)
    (fp_text reference X1 (at 0 3.97414) (layer F.SilkS))
    (fp_text value ANTENNA_U.FL (at -4 -0.42586) (layer F.SilkS) hide)
    (pad 3 smd rect (at 1.524 0 270) (size 0.79756 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 0 1.37414 270) (size 2.19964 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -1.37414 270) (size 2.19964 1.04902) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module nixiemisc:nixiemisc-CRYSTAL2.0X1.6 (layer F.Cu) (tedit 200000)
    (at 155.609559 93.378269 135)
    (attr smd)
    (fp_text reference Y1 (at -0.254 -1.4732 135) (layer F.SilkS))
    (fp_text value 26MHz (at 0.05702 1.58102 135) (layer F.SilkS))
    (pad 4 smd rect (at -0.6985 -0.54356 135) (size 0.889 0.7874) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.6985 -0.54356 135) (size 0.889 0.7874) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.6985 0.54356 135) (size 0.889 0.7874) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.6985 0.54356 135) (size 0.889 0.7874) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 140.2 121.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.340187 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 116 Vcc))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 143.081 116.35)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -2.6 -0.2) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58AA84E2)
    (at 111.077 118.89 135)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C13 (at 0 -2.25 135) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.5 135) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 135) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 135) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 116 Vcc))
    (pad 2 smd rect (at 1.5 0 135) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58AA84E2)
    (at 115.474107 100.656512 225)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C15 (at -2.886696 0.021651 315) (layer F.SilkS))
    (fp_text value 0.22uF (at 0 2.5 225) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 225) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 225) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 117 HV))
    (pad 2 smd rect (at 1.5 0 225) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-LED:SparkFun-LED-LED-0603 (layer B.Cu) (tedit 200000)
    (at 159.7 123.3)
    (descr "LED 0603 SMT")
    (tags "LED 0603 SMT")
    (attr smd)
    (fp_text reference D2 (at 0.1 1.4) (layer B.SilkS))
    (fp_text value SPND (at -1.418006 3.276608) (layer B.SilkS) hide)
    (pad C smd rect (at 0.8763 0 90) (size 0.99822 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad A smd rect (at -0.8763 0 90) (size 0.99822 0.99822) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(D2-PadA)"))
  )
  (module nixiemisc:nixiemisc-DO-219AB (layer F.Cu) (tedit 200000)
    (at 120.742477 103.803562 315)
    (attr smd)
    (fp_text reference D5 (at 0.038156 -1.598829 315) (layer F.SilkS))
    (fp_text value "ES1FL R3G" (at 0 1.524 315) (layer F.SilkS) hide)
    (pad C smd rect (at -1.5494 0 315) (size 1.1938 1.397) (layers F.Cu F.Paste F.Mask)
      (net 117 HV))
    (pad A smd rect (at 1.5494 0 135) (size 1.1938 1.397) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D5-PadA)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 140.2 119.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at -2.66817 0.167784) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 116 Vcc))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 115 82)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 1.4) (layer F.SilkS))
    (fp_text value 1M (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 GNDPWR))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 113.073457 96.432567 135)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at 2.903397 -0.170335 135) (layer F.SilkS))
    (fp_text value 604k (at 0 1.75 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.949999 0 135) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 117 HV))
    (pad 2 smd rect (at 0.949999 0 135) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R26-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 111.482467 98.023558 315)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at -2.974109 -0.029056 315) (layer F.SilkS))
    (fp_text value 604k (at 0 1.75 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.949999 0 315) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at 0.949999 0 315) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R27-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixiemisc:nixiemisc-WE-FLEX_ER11_5 (layer F.Cu) (tedit 200000)
    (at 126.143346 116.396142 45)
    (attr smd)
    (fp_text reference T1 (at -0.033378 -0.169344 45) (layer F.SilkS))
    (fp_text value WE-FLEX_ER11_5 (at -3.175 8.89 45) (layer F.SilkS) hide)
    (pad 12 smd rect (at 4.99872 5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(T1-Pad12)"))
    (pad 11 smd rect (at 2.99974 5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(T1-Pad11)"))
    (pad 10 smd rect (at 0.998221 5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(T1-Pad10)"))
    (pad 9 smd rect (at -0.998221 5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(T1-Pad10)"))
    (pad 8 smd rect (at -2.99974 5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -4.99872 5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(T1-Pad11)"))
    (pad 6 smd rect (at -4.99872 -5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(T1-Pad12)"))
    (pad 5 smd rect (at -2.99974 -5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 116 Vcc))
    (pad 4 smd rect (at -0.998221 -5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(T1-Pad3)"))
    (pad 3 smd rect (at 0.998221 -5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(T1-Pad3)"))
    (pad 2 smd rect (at 2.99974 -5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(Q1-Pad5)"))
    (pad 1 smd rect (at 4.99872 -5.97408 225) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D5-PadA)"))
  )
  (module nixiemisc:nixiemisc-SOT25 (layer F.Cu) (tedit 200000)
    (at 143.34996 121.09794)
    (descr "SMALL OUTLINE TRANSISTOR")
    (tags "SMALL OUTLINE TRANSISTOR")
    (attr smd)
    (fp_text reference U4 (at 2.65004 0.10206 180) (layer F.SilkS))
    (fp_text value AP2112 (at 1.905 2.794) (layer F.SilkS) hide)
    (pad 5 smd rect (at -0.94996 -1.29794) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 4 smd rect (at 0.94996 -1.29794) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U4-Pad4)"))
    (pad 3 smd rect (at 0.94996 1.29794) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 116 Vcc))
    (pad 2 smd rect (at 0 1.29794) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.94996 1.29794) (size 0.54864 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 116 Vcc))
  )
  (module nixiemisc:nixiemisc-SOT143 (layer F.Cu) (tedit 200000)
    (at 114.08182 85.80904 270)
    (descr SOT-143)
    (tags SOT-143)
    (attr smd)
    (fp_text reference U5 (at 0.19096 3.08182) (layer F.SilkS))
    (fp_text value ESD (at 2.39096 0.08182) (layer F.SilkS))
    (pad 4 smd rect (at -0.94996 -1.09982 270) (size 0.99822 1.43764) (layers F.Cu F.Paste F.Mask)
      (net 23 /USB-UART/D+))
    (pad 3 smd rect (at 0.94996 -1.09982 270) (size 0.99822 1.43764) (layers F.Cu F.Paste F.Mask)
      (net 24 /USB-UART/D-))
    (pad 2 smd rect (at 0.94996 1.09982 270) (size 0.99822 1.43764) (layers F.Cu F.Paste F.Mask)
      (net 112 /VBus))
    (pad 1 smd rect (at -0.7493 1.09982 270) (size 1.19888 1.43764) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module nixiemisc:nixiemisc-UMT6 (layer F.Cu) (tedit 200000)
    (at 146.094 105.619)
    (descr "UMT6 PACKAGE EIAJ: SC-88")
    (tags "UMT6 PACKAGE EIAJ: SC-88")
    (attr smd)
    (fp_text reference U7 (at -2.378 1.079) (layer F.SilkS))
    (fp_text value UMH3NUMT6 (at 2.54 1.905) (layer F.SilkS) hide)
    (pad 6 smd rect (at 0.92456 -0.6477 180) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 8 /ESP8285/RST))
    (pad 5 smd rect (at 0.92456 0 180) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R23-Pad2)"))
    (pad 4 smd rect (at 0.92456 0.6477 180) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 39 /USB-UART/DTR))
    (pad 3 smd rect (at -0.92456 0.6477) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 40 /ESP8285/GPIO0))
    (pad 2 smd rect (at -0.92456 0) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R24-Pad1)"))
    (pad 1 smd rect (at -0.92456 -0.6477) (size 0.49784 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 37 /USB-UART/RTS))
  )
  (module nixiemisc:nixiemisc-SO08 (layer F.Cu) (tedit 200000)
    (at 112.398821 112.797903 315)
    (descr "SOIC, 0.15 INCH WIDTH")
    (tags "SOIC, 0.15 INCH WIDTH")
    (attr smd)
    (fp_text reference U8 (at 0.073027 0.07136 135) (layer F.SilkS))
    (fp_text value LM3478SOIC8 (at 0.160704 0 315) (layer F.SilkS) hide)
    (pad 8 smd rect (at -1.905 -2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 116 Vcc))
    (pad 7 smd rect (at -0.635 -2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(Rf1-Pad2)"))
    (pad 6 smd rect (at 0.635 -2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q1-Pad4)"))
    (pad 5 smd rect (at 1.905 -2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R27-Pad2)"))
    (pad 2 smd rect (at -0.635 2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Cc1-Pad1)"))
    (pad 1 smd rect (at -1.905 2.79908 315) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C14-Pad1)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 156 123.3)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at -3.4 0.1) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 120 "Net-(R18-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(D2-PadA)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 156 121.6)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at -3.4 0) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D3-PadA)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 156 120)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at -3.4 0.1) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D4-PadA)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 136.604 95.522 45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.555635 45) (layer F.SilkS))
    (fp_text value 330 (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 45) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /Din))
    (pad 2 smd rect (at 0.75 0 45) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(J1-Pad15)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 142.3 100.5 225)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at 0.070711 1.343503 225) (layer F.SilkS))
    (fp_text value 330 (at 0 1.5 225) (layer F.Fab))
    (fp_text user %R (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 /ESP8285/GPIO14))
    (pad 2 smd rect (at 0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 143.4 101.6 225)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at -2.404163 0 225) (layer F.SilkS))
    (fp_text value 330 (at 0 1.5 225) (layer F.Fab))
    (fp_text user %R (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 /ESP8285/GPIO12))
    (pad 2 smd rect (at 0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 144.4 102.7 225)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at -2.474874 -0.070711 225) (layer F.SilkS))
    (fp_text value 330 (at 0 1.5 225) (layer F.Fab))
    (fp_text user %R (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 /ESP8285/GPIO13))
    (pad 2 smd rect (at 0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X03_NO_SILK (layer F.Cu) (tedit 200000)
    (at 139.103949 100.703949 315)
    (descr "PLATED THROUGH HOLE - 3 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 3 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J4 (at 0.254 -1.7018 315) (layer F.SilkS) hide)
    (fp_text value Test (at 0.5588 1.7272 315) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 5.079999 0 315) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 111 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 315) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 110 "Net-(J4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 315) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 109 "Net-(J4-Pad1)"))
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 132.9 130.2 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x09_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 119.84 87.46 90)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value NixieExt (at 0 22.65 90) (layer F.Fab))
    (fp_text user %R (at 0 10.16 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 /HV15))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 /HV6))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 /HV5))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /HV4))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 /HV3))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 /HV2))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 /HV1))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 /HV14))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 /HV13))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixiemisc:nixiemisc-SOT23-5 (layer F.Cu) (tedit 200000)
    (at 117.86388 127.07896 45)
    (attr smd)
    (fp_text reference IC1 (at -2.54 0 315) (layer F.SilkS))
    (fp_text value MAX40200 (at 2.54 0 315) (layer F.SilkS))
    (pad 5 smd rect (at 1.19888 -0.94996 45) (size 1.19888 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 116 Vcc))
    (pad 4 smd rect (at 1.19888 0.94996 45) (size 1.19888 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(IC1-Pad4)"))
    (pad 3 smd rect (at -1.19888 0.94996 45) (size 1.19888 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 112 /VBus))
    (pad 2 smd rect (at -1.19888 0 45) (size 1.19888 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.19888 -0.94996 45) (size 1.19888 0.59944) (layers F.Cu F.Paste F.Mask)
      (net 112 /VBus))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 150.701 117.874)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 1.5) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 119 /USB-UART/VBusDet))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 149.939 115.969 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value 22.1K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 112 /VBus))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 119 /USB-UART/VBusDet))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 151.463 115.969 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at 0 -1.651 270) (layer F.SilkS))
    (fp_text value 47.5K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 119 /USB-UART/VBusDet))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixiemisc:nixiemisc-UQFN-10 (layer F.Cu) (tedit 200000)
    (at 146.3195 113.5687 90)
    (attr smd)
    (fp_text reference M1 (at 0 -2.99974 90) (layer F.SilkS) hide)
    (fp_text value BQ24392 (at 2.4257 -1.8415 180) (layer F.SilkS))
    (pad VBUS smd rect (at -0.7493 -0.6985 180) (size 0.6985 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 112 /VBus))
    (pad SW_OPEN smd rect (at -0.7493 0.6985 180) (size 0.6985 0.29972) (layers F.Cu F.Paste F.Mask))
    (pad GOOD_BAT smd rect (at 0.94488 0 90) (size 0.79756 0.34798) (layers F.Cu F.Paste F.Mask))
    (pad GND smd rect (at 0.7493 -0.6985 180) (size 0.6985 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad DP_HOST smd rect (at 0.24892 0.6985 180) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask))
    (pad DP_CON smd rect (at 0.24892 -0.6985 180) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask))
    (pad DM_HOST smd rect (at -0.24892 0.6985 180) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask))
    (pad DM_CON smd rect (at -0.24892 -0.6985 180) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask))
    (pad C_DET smd rect (at -0.94488 0 90) (size 0.79756 0.34798) (layers F.Cu F.Paste F.Mask))
    (pad C_AL_N smd rect (at 0.7493 0.6985 180) (size 0.6985 0.29972) (layers F.Cu F.Paste F.Mask))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 148.542 110.254 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 122 /USB-UART/CHG_AL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 148.542 117.747 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R37 (at -2.54 0.127 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 121 /USB-UART/CHG_DET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 146.256 116.858 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D6 (at 2.159 0) (layer F.SilkS))
    (fp_text value 1SS367.H3F (at 0.1 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 270) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 121 /USB-UART/CHG_DET))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nixiemisc:nixiemisc-QFN24-4X4 (layer F.Cu) (tedit 200000)
    (at 153.64232 111.91008)
    (descr "UF PACKAGE 24-LEAD (4MM × 4MM) PLASTIC QFN")
    (tags "UF PACKAGE 24-LEAD (4MM × 4MM) PLASTIC QFN")
    (attr smd)
    (fp_text reference U6 (at 0.10668 -3.13436) (layer F.SilkS))
    (fp_text value CP2102N-24 (at 1.80848 3.11404) (layer F.SilkS) hide)
    (pad EXP smd rect (at 0 0) (size 2.44856 2.44856) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at -1.24968 -1.89992 270) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(U6-Pad24)"))
    (pad 23 smd rect (at -0.7493 -1.89992 270) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 39 /USB-UART/DTR))
    (pad 22 smd rect (at -0.24892 -1.89992 270) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U6-Pad22)"))
    (pad 21 smd rect (at 0.24892 -1.89992 270) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 19 /SDA))
    (pad 20 smd rect (at 0.7493 -1.89992 270) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 20 /SCL))
    (pad 19 smd rect (at 1.24968 -1.89992 270) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 37 /USB-UART/RTS))
    (pad 18 smd rect (at 1.89992 -1.24968 180) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 75 /USB-UART/CTS))
    (pad 17 smd rect (at 1.89992 -0.7493 180) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U6-Pad17)"))
    (pad 16 smd rect (at 1.89992 -0.24892 180) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U6-Pad16)"))
    (pad 15 smd rect (at 1.89992 0.24892 180) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R18-Pad1)"))
    (pad 14 smd rect (at 1.89992 0.7493 180) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(D3-PadC)"))
    (pad 13 smd rect (at 1.89992 1.24968 180) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D4-PadC)"))
    (pad 12 smd rect (at 1.24968 1.89992 90) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U6-Pad12)"))
    (pad 11 smd rect (at 0.7493 1.89992 90) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(U6-Pad11)"))
    (pad 10 smd rect (at 0.24892 1.89992 90) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U6-Pad10)"))
    (pad 9 smd rect (at -0.24892 1.89992 90) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(R21-Pad2)"))
    (pad 8 smd rect (at -0.7493 1.89992 90) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 119 /USB-UART/VBusDet))
    (pad 7 smd rect (at -1.24968 1.89992 90) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 6 smd rect (at -1.89992 1.24968) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 5 smd rect (at -1.89992 0.7493) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 4 smd rect (at -1.89992 0.24892) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(M1-PadDM_H)"))
    (pad 3 smd rect (at -1.89992 -0.24892) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(M1-PadDP_H)"))
    (pad 2 smd rect (at -1.89992 -0.7493) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.89992 -1.24968) (size 0.6985 0.24892) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U6-Pad1)"))
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 137.112 127.526 225)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2.000001 225) (layer F.SilkS))
    (fp_text value B130LAW-7-F (at 0 2.1 225) (layer F.Fab))
    (fp_text user %R (at 0 -2 225) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 225) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 1.65 0 225) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 112 /VBus))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_USB:USB_Micro-B_Molex-105017-0001 (layer F.Cu) (tedit 598B308E)
    (at 121.531 79.329 180)
    (descr http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
    (tags "Micro-USB SMD Typ-B")
    (attr smd)
    (fp_text reference J3 (at 0 -4 180) (layer F.SilkS))
    (fp_text value USB_OTG (at 0.3 3.45 180) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 1.8 180) (layer Dwgs.User))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 6 smd rect (at 1 0.35 180) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 10 GNDPWR))
    (pad 6 thru_hole circle (at -2.5 -2.35 180) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 10 GNDPWR))
    (pad 2 smd rect (at -0.65 -2.35 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 24 /USB-UART/D-))
    (pad 1 smd rect (at -1.3 -2.35 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 112 /VBus))
    (pad 5 smd rect (at 1.3 -2.35 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 -2.35 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(J3-Pad4)"))
    (pad 3 smd rect (at 0 -2.35 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 23 /USB-UART/D+))
    (pad 6 thru_hole circle (at 2.5 -2.35 180) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 10 GNDPWR))
    (pad 6 smd rect (at -1 0.35 180) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 10 GNDPWR))
    (pad 6 thru_hole oval (at -3.5 0.35) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 10 GNDPWR))
    (pad 6 thru_hole oval (at 3.5 0.35 180) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 10 GNDPWR))
    (pad 6 smd rect (at 2.9 0.35 180) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 10 GNDPWR))
    (pad 6 smd rect (at -2.9 0.35 180) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 10 GNDPWR))
    (model ${KISYS3DMOD}/Connectors_USB.3dshapes/USB_Micro-B_Molex-105017-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 107.239826 102.266198 315)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference Rc1 (at 0 -1.45 315) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.5 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 315) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Cc1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 315) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 111.30569 103.503635 225)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference Rf1 (at 0 -1.45 225) (layer F.SilkS))
    (fp_text value 47k (at 0 1.5 225) (layer F.Fab))
    (fp_text user %R (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /ESP8285/GPIO2))
    (pad 2 smd rect (at 0.75 0 225) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(Rf1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 2450AT18B100E:ANT_2450AT18B100E (layer F.Cu) (tedit 5BF1A58A)
    (at 149.304 82.695 325)
    (attr smd)
    (fp_text reference ANT1 (at 0.18756 2.039206 325) (layer F.SilkS))
    (fp_text value 2450AT18B100E (at -0.265 2.055 325) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.3 0 325) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.3 0 325) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(ANT1-Pad1)"))
  )
  (dimension 30 (width 0.127) (layer Dwgs.User)
    (gr_text "30.000 mm" (at 145 151.554) (layer Dwgs.User))
    (feature1 (pts (xy 160 110) (xy 160 152.108)))
    (feature2 (pts (xy 130 110) (xy 130 152.108)))
    (crossbar (pts (xy 130 151) (xy 160 151)))
    (arrow1a (pts (xy 160 151) (xy 158.873496 151.586421)))
    (arrow1b (pts (xy 160 151) (xy 158.873496 150.413579)))
    (arrow2a (pts (xy 130 151) (xy 131.126504 151.586421)))
    (arrow2b (pts (xy 130 151) (xy 131.126504 150.413579)))
  )
  (dimension 48 (width 0.127) (layer Dwgs.User)
    (gr_text "48.000 mm" (at 130 149.554) (layer Dwgs.User))
    (feature1 (pts (xy 154 128) (xy 154 150.108)))
    (feature2 (pts (xy 106 128) (xy 106 150.108)))
    (crossbar (pts (xy 106 149) (xy 154 149)))
    (arrow1a (pts (xy 154 149) (xy 152.873496 149.586421)))
    (arrow1b (pts (xy 154 149) (xy 152.873496 148.413579)))
    (arrow2a (pts (xy 106 149) (xy 107.126504 149.586421)))
    (arrow2b (pts (xy 106 149) (xy 107.126504 148.413579)))
  )
  (dimension 24 (width 0.127) (layer Dwgs.User)
    (gr_text "24.000 mm" (at 142 147.554) (layer Dwgs.User))
    (feature1 (pts (xy 130 128) (xy 130 148.108)))
    (feature2 (pts (xy 154 128) (xy 154 148.108)))
    (crossbar (pts (xy 154 147) (xy 130 147)))
    (arrow1a (pts (xy 130 147) (xy 131.126504 146.413579)))
    (arrow1b (pts (xy 130 147) (xy 131.126504 147.586421)))
    (arrow2a (pts (xy 154 147) (xy 152.873496 146.413579)))
    (arrow2b (pts (xy 154 147) (xy 152.873496 147.586421)))
  )
  (dimension 18 (width 0.127) (layer Dwgs.User)
    (gr_text "18.000 mm" (at 173.554 119 90) (layer Dwgs.User))
    (feature1 (pts (xy 154 110) (xy 174.108 110)))
    (feature2 (pts (xy 154 128) (xy 174.108 128)))
    (crossbar (pts (xy 173 128) (xy 173 110)))
    (arrow1a (pts (xy 173 110) (xy 173.586421 111.126504)))
    (arrow1b (pts (xy 173 110) (xy 172.413579 111.126504)))
    (arrow2a (pts (xy 173 128) (xy 173.586421 126.873496)))
    (arrow2b (pts (xy 173 128) (xy 172.413579 126.873496)))
  )
  (dimension 4.6 (width 0.127) (layer Dwgs.User)
    (gr_text "4.600 mm" (at 138.7 70.246) (layer Dwgs.User))
    (feature1 (pts (xy 141 78.5) (xy 141 69.692)))
    (feature2 (pts (xy 136.4 78.5) (xy 136.4 69.692)))
    (crossbar (pts (xy 136.4 70.8) (xy 141 70.8)))
    (arrow1a (pts (xy 141 70.8) (xy 139.873496 71.386421)))
    (arrow1b (pts (xy 141 70.8) (xy 139.873496 70.213579)))
    (arrow2a (pts (xy 136.4 70.8) (xy 137.526504 71.386421)))
    (arrow2b (pts (xy 136.4 70.8) (xy 137.526504 70.213579)))
  )
  (dimension 8.7 (width 0.127) (layer Dwgs.User)
    (gr_text "8.700 mm" (at 134.25 72.546) (layer Dwgs.User))
    (feature1 (pts (xy 138.6 80) (xy 138.6 71.992)))
    (feature2 (pts (xy 129.9 80) (xy 129.9 71.992)))
    (crossbar (pts (xy 129.9 73.1) (xy 138.6 73.1)))
    (arrow1a (pts (xy 138.6 73.1) (xy 137.473496 73.686421)))
    (arrow1b (pts (xy 138.6 73.1) (xy 137.473496 72.513579)))
    (arrow2a (pts (xy 129.9 73.1) (xy 131.026504 73.686421)))
    (arrow2b (pts (xy 129.9 73.1) (xy 131.026504 72.513579)))
  )
  (dimension 9 (width 0.127) (layer Dwgs.User)
    (gr_text "9.000 mm" (at 121.5 72.446) (layer Dwgs.User))
    (feature1 (pts (xy 117 80) (xy 117 71.892)))
    (feature2 (pts (xy 126 80) (xy 126 71.892)))
    (crossbar (pts (xy 126 73) (xy 117 73)))
    (arrow1a (pts (xy 117 73) (xy 118.126504 72.413579)))
    (arrow1b (pts (xy 117 73) (xy 118.126504 73.586421)))
    (arrow2a (pts (xy 126 73) (xy 124.873496 72.413579)))
    (arrow2b (pts (xy 126 73) (xy 124.873496 73.586421)))
  )
  (dimension 4 (width 0.127) (layer Dwgs.User)
    (gr_text "4.000 mm" (at 128 72.446) (layer Dwgs.User))
    (feature1 (pts (xy 126 80) (xy 126 71.892)))
    (feature2 (pts (xy 130 80) (xy 130 71.892)))
    (crossbar (pts (xy 130 73) (xy 126 73)))
    (arrow1a (pts (xy 126 73) (xy 127.126504 72.413579)))
    (arrow1b (pts (xy 126 73) (xy 127.126504 73.586421)))
    (arrow2a (pts (xy 130 73) (xy 128.873496 72.413579)))
    (arrow2b (pts (xy 130 73) (xy 128.873496 73.586421)))
  )
  (dimension 17.5 (width 0.127) (layer Dwgs.User)
    (gr_text "17.500 mm" (at 89.446 101.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 130 110) (xy 88.892 110)))
    (feature2 (pts (xy 130 92.5) (xy 88.892 92.5)))
    (crossbar (pts (xy 90 92.5) (xy 90 110)))
    (arrow1a (pts (xy 90 110) (xy 89.413579 108.873496)))
    (arrow1b (pts (xy 90 110) (xy 90.586421 108.873496)))
    (arrow2a (pts (xy 90 92.5) (xy 89.413579 93.626504)))
    (arrow2b (pts (xy 90 92.5) (xy 90.586421 93.626504)))
  )
  (dimension 30 (width 0.127) (layer Dwgs.User)
    (gr_text "30.000 mm" (at 173.054 95 270) (layer Dwgs.User))
    (feature1 (pts (xy 130 110) (xy 173.608 110)))
    (feature2 (pts (xy 130 80) (xy 173.608 80)))
    (crossbar (pts (xy 172.5 80) (xy 172.5 110)))
    (arrow1a (pts (xy 172.5 110) (xy 171.913579 108.873496)))
    (arrow1b (pts (xy 172.5 110) (xy 173.086421 108.873496)))
    (arrow2a (pts (xy 172.5 80) (xy 171.913579 81.126504)))
    (arrow2b (pts (xy 172.5 80) (xy 173.086421 81.126504)))
  )
  (dimension 70 (width 0.127) (layer Dwgs.User)
    (gr_text "70.000 mm" (at 130 65.137043) (layer Dwgs.User))
    (feature1 (pts (xy 165 113.191043) (xy 165 64.583043)))
    (feature2 (pts (xy 95 113.191043) (xy 95 64.583043)))
    (crossbar (pts (xy 95 65.691043) (xy 165 65.691043)))
    (arrow1a (pts (xy 165 65.691043) (xy 163.873496 66.277464)))
    (arrow1b (pts (xy 165 65.691043) (xy 163.873496 65.104622)))
    (arrow2a (pts (xy 95 65.691043) (xy 96.126504 66.277464)))
    (arrow2b (pts (xy 95 65.691043) (xy 96.126504 65.104622)))
  )
  (gr_text VBus (at 163.782 117.366) (layer B.SilkS))
  (gr_text VBus (at 163.782 117.366) (layer F.SilkS))
  (gr_text Vcc (at 158.194 115.08) (layer F.SilkS))
  (gr_text Vcc (at 158.067 115.08) (layer B.SilkS))
  (gr_text Din (at 138.509 91.077) (layer B.SilkS))
  (gr_text 12 (at 123.269 91.204) (layer B.SilkS))
  (gr_text 11 (at 125.809 91.204) (layer B.SilkS))
  (gr_text 10 (at 128.349 91.204) (layer B.SilkS))
  (gr_text 9 (at 130.889 91.204) (layer B.SilkS))
  (gr_text 8 (at 133.429 91.204) (layer B.SilkS))
  (gr_text 5 (at 124.92 85.362) (layer B.SilkS))
  (gr_text 4 (at 127.46 85.362) (layer B.SilkS))
  (gr_text 3 (at 130 85.362) (layer B.SilkS))
  (gr_text 2 (at 132.54 85.362) (layer B.SilkS))
  (gr_text 5 (at 124.92 94.887) (layer B.SilkS))
  (gr_text 4 (at 127.46 94.887) (layer B.SilkS))
  (gr_text 3 (at 130 94.887) (layer B.SilkS))
  (gr_text 2 (at 132.54 94.887) (layer B.SilkS))
  (gr_text 13 (at 140.2 85.362) (layer B.SilkS))
  (gr_text 14 (at 137.6 85.362) (layer B.SilkS))
  (gr_text 1 (at 135 85.362) (layer B.SilkS))
  (gr_text 15 (at 119.8 85.362) (layer B.SilkS))
  (gr_text 6 (at 122.4 85.362) (layer B.SilkS))
  (gr_arc (start 130 110) (end 126.2 75.2) (angle 344.0653944) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 116.8 77.6) (end 126.19 77.615) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 126.19 77.615) (end 126.2 75.2) (layer Edge.Cuts) (width 0.127))
  (gr_text 1 (at 135.08 94.887) (layer B.SilkS))
  (gr_text 7 (at 135.969 91.204) (layer B.SilkS))
  (gr_text 6 (at 122.38 94.887) (layer B.SilkS))
  (gr_text A (at 117.808 91.204) (layer B.SilkS))
  (gr_text Din (at 137.62 94.887) (layer B.SilkS))
  (gr_text 5V (at 140.16 94.887) (layer B.SilkS))
  (gr_text GND (at 143.2 90) (layer B.SilkS))
  (gr_text SCL (at 164.29 107.46 90) (layer B.SilkS))
  (gr_text SDA (at 164.29 110 90) (layer B.SilkS))
  (gr_text 5V (at 164.417 111.524 90) (layer B.SilkS))
  (gr_text 3V3 (at 158.194 112.54) (layer B.SilkS))
  (gr_text GND (at 158.194 110) (layer B.SilkS))
  (gr_text IO15 (at 158.194 107.46) (layer B.SilkS))
  (gr_text RST (at 158.194 104.92) (layer B.SilkS))
  (gr_text IO16 (at 162.004 102.634) (layer B.SilkS))
  (gr_text SCL (at 164.29 107.46 90) (layer F.SilkS))
  (gr_text IO15 (at 158.448 107.46) (layer F.SilkS))
  (gr_text SDA (at 164.29 110 90) (layer F.SilkS))
  (gr_text IO16 (at 162.004 102.634) (layer F.SilkS))
  (gr_text 5V (at 164.417 111.778 90) (layer F.SilkS))
  (gr_text 3V3 (at 158.575 112.54) (layer F.SilkS))
  (gr_text GND (at 158.702 110) (layer F.SilkS))
  (gr_text RST (at 158.194 104.92) (layer F.SilkS))
  (gr_text MOSI (at 140.668 106.698 45) (layer F.SilkS))
  (gr_text LE (at 139.398 104.158 45) (layer F.SilkS))
  (gr_text CLK (at 137.366 102.634 45) (layer F.SilkS))
  (gr_text "nixies.us\nOne Tube Clock v1.0" (at 131.3 130.1) (layer B.Mask))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.399 79.774) (xy 152.600615 83.41621) (xy 148.958405 88.617825) (xy 143.75679 84.975615)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.508))
    (polygon
      (pts
        (xy 93.9 74.3) (xy 167 74.587292) (xy 167 144.587292) (xy 93.9 144.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.423256 108.766744) (xy 133.81 115.08) (xy 124.829744 124.060256) (xy 118.443 117.747)
      )
    )
  )
  (zone (net 112) (net_name /VBus) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.142 82.568) (xy 124.158 82.568) (xy 124.031 85.362) (xy 119.078 86.124) (xy 117.204 88.121)
        (xy 115.776 88.156) (xy 115.903 85.87) (xy 116.538 84.727) (xy 117.3 83.076) (xy 122.634 83.076)
        (xy 122.634 82.568) (xy 123.396 82.568)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.45818 79.764306) (xy 152.659795 83.406516) (xy 149.017585 88.608131) (xy 143.81597 84.965921)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 2.54))
    (polygon
      (pts
        (xy 165.06 94.48) (xy 153.83 105.65) (xy 141.97 94.51) (xy 144.26 91.85) (xy 143.1 90.760579)
        (xy 143 91.2) (xy 139 91.3) (xy 139 89) (xy 138.740727 86.666541) (xy 134.07 82.28)
        (xy 134.129351 75.009481) (xy 164.94 74.74)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.508))
    (polygon
      (pts
        (xy 134.129351 75.009481) (xy 134.07 75.01) (xy 134.13 74.93)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.062 84.727) (xy 118.062 83.076) (xy 119.205 82.949) (xy 119.332 82.568) (xy 118.443 82.06)
        (xy 116.538 82.06) (xy 116.284 82.695) (xy 115.014 82.695) (xy 115 79.3) (xy 113.5 79.3)
        (xy 110.4 81.4) (xy 110.4 85.7) (xy 117.808 85.616) (xy 117.808 84.727)
      )
    )
  )
  (zone (net 112) (net_name /VBus) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.189 90.442) (xy 116.284 90.95) (xy 103.076 102.126) (xy 103.076 112.032) (xy 106.886 115.969)
        (xy 109.426 119.906) (xy 113.998 124.351) (xy 121.618 131.082) (xy 130.889 131.082) (xy 136.477 126.637)
        (xy 138.255 128.415) (xy 142.319 128.923) (xy 147.526 126.002) (xy 156.924 121.049) (xy 160.988 116.858)
        (xy 161.369 114.191) (xy 168.989 114.318) (xy 146.002 134.511) (xy 117.173 134.638) (xy 116.912466 133.685753)
        (xy 117.1 134) (xy 107.3 124.5) (xy 97.6 116.1) (xy 95.992934 111.546647) (xy 95.71 111.27)
        (xy 98.25 97.3) (xy 105.616 86.124) (xy 116.411 86.124) (xy 117.427 83.838) (xy 119.84 83.838)
      )
    )
  )
  (zone (net 116) (net_name Vcc) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.839 121.684) (xy 118.316 127.018) (xy 121.872 130.32) (xy 130.254 130.32) (xy 137.747 124.478)
        (xy 141.43 128.034) (xy 147.526 124.859) (xy 156.416 120.541) (xy 160.48 116.604) (xy 160.861 114.064)
        (xy 159.591 114.064) (xy 140.2 118.4) (xy 138.4 118.4) (xy 127.968 126.891) (xy 118.062 117.874)
        (xy 121.237 114.318) (xy 114.506 107.079) (xy 106.251 114.064) (xy 110.315 120.16)
      )
    )
  )
  (zone (net 80) (net_name "Net-(Q1-Pad5)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.682 110.254) (xy 117.046 101.618) (xy 113.236 105.428) (xy 118.062 110.254) (xy 119.84 108.476)
        (xy 121.618 110.254) (xy 122.126 109.746) (xy 122.38 109.746) (xy 124.158 111.524)
      )
    )
  )
  (zone (net 29) (net_name "Net-(Q1-Pad4)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.998 111.27) (xy 116.03 109.238) (xy 116.538 109.746) (xy 116.792 110) (xy 114.76 112.032)
      )
    )
  )
)
