(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 106)
    (zones 0)
    (modules 4)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J3-Pad9)")
  (net 2 "Net-(J3-Pad8)")
  (net 3 "Net-(J3-Pad7)")
  (net 4 "Net-(J3-Pad6)")
  (net 5 "Net-(J3-Pad5)")
  (net 6 "Net-(J3-Pad4)")
  (net 7 "Net-(J3-Pad3)")
  (net 8 "Net-(J3-Pad2)")
  (net 9 "Net-(J3-Pad1)")
  (net 10 "Net-(J2-Pad2b)")
  (net 11 "Net-(J1-Pad5a)")
  (net 12 "Net-(J1-Pad4a)")
  (net 13 "Net-(J1-Pad3a)")
  (net 14 "Net-(J1-Pad2a)")
  (net 15 "Net-(J1-Pad1a)")
  (net 16 "Net-(J2-Pad1b)")
  (net 17 "Net-(J2-Pad1a)")
  (net 18 "Net-(J1-Pad1b)")
  (net 19 "Net-(J1-Pad2b)")
  (net 20 "Net-(J1-Pad3b)")
  (net 21 "Net-(J1-Pad4b)")
  (net 22 "Net-(J1-Pad5b)")
  (net 23 "Net-(J2-Pad2a)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1a)")
    (add_net "Net-(J1-Pad1b)")
    (add_net "Net-(J1-Pad2a)")
    (add_net "Net-(J1-Pad2b)")
    (add_net "Net-(J1-Pad3a)")
    (add_net "Net-(J1-Pad3b)")
    (add_net "Net-(J1-Pad4a)")
    (add_net "Net-(J1-Pad4b)")
    (add_net "Net-(J1-Pad5a)")
    (add_net "Net-(J1-Pad5b)")
    (add_net "Net-(J2-Pad1a)")
    (add_net "Net-(J2-Pad1b)")
    (add_net "Net-(J2-Pad2a)")
    (add_net "Net-(J2-Pad2b)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
  )
  (module vfd:PinHeader_2x02_P2.54mm_Verticalab (layer F.Cu) (tedit 5CAD8518)
    (at 93.98 116.84 180)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value Cathodes (at 1.27 4.87 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 1.27 270) (layer F.Fab))
    (pad 2b thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2b)"))
    (pad 2a thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad2a)"))
    (pad 1b thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad1b)"))
    (pad 1a thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad1a)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vfd:PinHeader_2x05_P2.54mm_Verticalab (layer F.Cu) (tedit 5CAD8470)
    (at 95.25 91.44)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Grids (at 1.27 12.49) (layer F.SilkS))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 5b thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad5b)"))
    (pad 5a thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad5a)"))
    (pad 4b thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad4b)"))
    (pad 4a thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad4a)"))
    (pad 3b thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad3b)"))
    (pad 3a thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad3a)"))
    (pad 2b thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad2b)"))
    (pad 2a thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad2a)"))
    (pad 1b thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad1b)"))
    (pad 1a thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad1a)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vfd:ILV2-7_5 (layer F.Cu) (tedit 5CAD7A49)
    (at 118.11 106.68)
    (fp_text reference U1 (at -10.16 -2.54 90) (layer F.SilkS))
    (fp_text value IVL2-7_5 (at -10.16 7.62 90) (layer F.SilkS))
    (pad 17 thru_hole circle (at -12.7 -27.94) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad2b)"))
    (pad 18 thru_hole circle (at -12.7 -22.86) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad5a)"))
    (pad 19 thru_hole circle (at -12.7 -15.24) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad4a)"))
    (pad 20 thru_hole circle (at -12.7 -10.16) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad3a)"))
    (pad 21 thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad2a)"))
    (pad 22 thru_hole circle (at -12.7 5.08) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad1a)"))
    (pad 23 thru_hole circle (at -12.7 10.16) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad1b)"))
    (pad 1 thru_hole circle (at 15.24 10.16) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad1a)"))
    (pad 2 thru_hole circle (at 15.24 7.62) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad1b)"))
    (pad 3 thru_hole circle (at 15.24 5.08) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 2 "Net-(J3-Pad8)"))
    (pad 4 thru_hole circle (at 15.24 2.54) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad7)"))
    (pad 5 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad5)"))
    (pad 6 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad2b)"))
    (pad 7 thru_hole circle (at 15.24 -5.08) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 8 thru_hole circle (at 15.24 -7.62) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad3b)"))
    (pad 9 thru_hole circle (at 15.24 -10.16) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 1 "Net-(J3-Pad9)"))
    (pad 10 thru_hole circle (at 15.24 -12.7) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad4)"))
    (pad 11 thru_hole circle (at 15.24 -15.24) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad4b)"))
    (pad 12 thru_hole circle (at 15.24 -17.78) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (pad 13 thru_hole circle (at 15.24 -20.32) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 4 "Net-(J3-Pad6)"))
    (pad 14 thru_hole circle (at 15.24 -22.86) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad1)"))
    (pad 15 thru_hole circle (at 15.24 -25.4) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad5b)"))
    (pad 16 thru_hole circle (at 15.24 -27.94) (size 1.524 1.524) (drill 0.914) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad2a)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 144.78 87.63)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Anodes (at 0 22.65) (layer F.SilkS))
    (fp_text user %R (at 0 10.16 90) (layer F.Fab))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J3-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J3-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J3-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J3-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 152.4 76.2) (end 82.55 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 121.92) (end 152.4 76.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82.55 121.92) (end 152.4 121.92) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82.55 76.2) (end 82.55 121.92) (layer Edge.Cuts) (width 0.05))
  (gr_text "1\n2\nC\n4\n5" (at 100.33 96.52) (layer F.SilkS))
  (gr_text "1\n2\nC\n4\n5" (at 92.71 96.52) (layer F.SilkS))
  (gr_text "B\nA" (at 96.52 115.57) (layer F.SilkS))
  (gr_text "B\nA" (at 88.9 115.57) (layer F.SilkS))
  (gr_text "a\nb\nc\nd\ne\nf\ng\nct\ncb" (at 147.32 97.79) (layer F.SilkS))
)
