(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "CS")
	(net 2 "GND")
	(net 3 "MISO")
	(net 4 "MOSI")
	(net 5 "SCKL")
	(net 6 "5V")
	(footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD_SWD"
		(layer "F.Cu")
		(at 116.656 76.962 -90)
		(descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
		(tags "Surface mounted pin header SMD 2x05 1.27mm double row")
		(property "Reference" "J2"
			(at -3.048 -4.248 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x05_Odd_Even"
			(at 4.699 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD_SWD"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "Transimpedence-adaptor.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 -1.905 270)
			(size 1.02 1.02)
			(drill 1.02)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 1.905 270)
			(size 1.02 1.02)
			(drill 1.02)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -1.95 -2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SCKL")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.95 -2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.95 -1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "CS")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.95 -1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.95 0 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "MISO")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.95 0 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -1.95 1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "MOSI")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.95 1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -1.95 2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 1.95 2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "5V")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 110.306 69.088 90)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "J1"
			(at -2.286 -1.467 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x06"
			(at -3.81 15.043 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Transimpedence-adaptor.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 360)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "MOSI")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "MISO")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "SCKL")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "CS")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 107.656 66.548)
		(end 125.656 82.548)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "BG Transimpedance Adpt V1.1"
		(at 113.411 82.042 0)
		(layer "B.SilkS")
	)
	(gr_text "SCKL"
		(at 119.408876 71.628 0)
		(layer "F.SilkS")
	)
	(gr_text "MOSI"
		(at 114.365162 71.628 0)
		(layer "F.SilkS")
	)
	(gr_text "CS"
		(at 122.408495 71.628 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 109.744781 71.628 0)
		(layer "F.SilkS")
	)
	(gr_text "MISO"
		(at 116.905162 71.628 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 111.970305 71.628 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(locked yes)
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.476 82.423) (xy 125.476 66.675) (xy 107.823 66.675) (xy 107.823 82.423)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.476 82.423) (xy 125.476 66.675) (xy 107.823 66.675) (xy 107.823 82.423)
			)
		)
	)
)
