(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 68)
    (zones 0)
    (modules 7)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /VCC)
  (net 3 "Net-(U1-Pad9)")
  (net 4 "Net-(U1-Pad8)")
  (net 5 /RESET)
  (net 6 /DIO0)
  (net 7 /NSS)
  (net 8 /MOSI)
  (net 9 /MISO)
  (net 10 /SCK)
  (net 11 /ANT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ANT)
    (add_net /DIO0)
    (add_net /GND)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /NSS)
    (add_net /RESET)
    (add_net /SCK)
    (add_net /VCC)
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (module 0xFD:nicerf-lora-sx127x (layer F.Cu) (tedit 611BC697)
    (at 133.223 71.3232)
    (fp_text reference U1 (at 0.1016 8.9916) (layer F.SilkS) hide)
    (fp_text value "NiceRF SX127X" (at -0.0762 -11.6205) (layer F.Fab) hide)
    (pad 13 smd rect (at 7.874 -8.7) (size 3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 /ANT))
    (pad 14 smd rect (at 7.874 -7.2) (size 3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 12 smd rect (at -8.5 5.47) (size 3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 5 /RESET))
    (pad 11 smd rect (at -8.5 4.2) (size 3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 2 /VCC))
    (pad 10 smd rect (at -8.5 2.93) (size 3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 6 /DIO0))
    (pad 9 smd rect (at -8.5 1.66) (size 3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -8.5 0.39) (size 3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad8)"))
    (pad 7 smd rect (at -8.5 -0.88) (size 3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 7 /NSS))
    (pad 6 smd rect (at -8.5 -2.15) (size 3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 8 /MOSI))
    (pad 5 smd rect (at -8.5 -3.42) (size 3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 9 /MISO))
    (pad 4 smd rect (at -8.5 -4.69) (size 3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCK))
    (pad 1 smd rect (at -8.5 -8.5) (size 3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 136.7028 72.289 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -3.2512 -0.0762 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.192308)
      (net 2 /VCC))
    (pad 1 smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.192308)
      (net 5 /RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 132.9944 64.2366 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 120.7008 61.2648)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x08_Female (at 0 20.11) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.89 90) (layer F.Fab) hide)
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RESET))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /DIO0))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /NSS))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /MOSI))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /MISO))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SCK))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0xFD:IPEX_Antenna_Connector (layer B.Cu) (tedit 60EF5E61)
    (at 141.097 62.6618 270)
    (fp_text reference J2 (at 0.4445 -2.8829 90) (layer B.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0.1016 -2.4384 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at -0.0254 1.397) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 11 /ANT))
    (pad 1 smd rect (at 1.2954 0 270) (size 1 2) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at -1.3208 0) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 131.1402 72.3392 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 3.2004 -0.0254) (layer B.SilkS))
    (fp_text value 102pF (at 0 -1.85 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.188679)
      (net 1 /GND))
    (pad 1 smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.188679)
      (net 2 /VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 134.0104 72.3392 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 3.2258 0.1524) (layer B.SilkS))
    (fp_text value 100pF (at 0 -1.85 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.188679)
      (net 1 /GND))
    (pad 1 smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.188679)
      (net 2 /VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "NiceRF LoRa\nSX127X" (at 133.6294 69.7992) (layer F.SilkS))
  (gr_text ANT (at 137.9982 60.6298) (layer B.SilkS))
  (dimension 25.4 (width 0.15) (layer Dwgs.User)
    (gr_text "25.400 mm" (at 131.318 84.3834) (layer Dwgs.User))
    (feature1 (pts (xy 144.018 81.4832) (xy 144.018 83.669821)))
    (feature2 (pts (xy 118.618 81.4832) (xy 118.618 83.669821)))
    (crossbar (pts (xy 118.618 83.0834) (xy 144.018 83.0834)))
    (arrow1a (pts (xy 144.018 83.0834) (xy 142.891496 83.669821)))
    (arrow1b (pts (xy 144.018 83.0834) (xy 142.891496 82.496979)))
    (arrow2a (pts (xy 118.618 83.0834) (xy 119.744504 83.669821)))
    (arrow2b (pts (xy 118.618 83.0834) (xy 119.744504 82.496979)))
  )
  (gr_text "NiceRF SX127x breakout\n(c) 2021 dushin.net\nv0.1.0" (at 141.2748 80.4926 -90) (layer B.SilkS))
  (dimension 21.9456 (width 0.15) (layer Dwgs.User)
    (gr_text "21.946 mm" (at 150.779 70.1294 270) (layer Dwgs.User))
    (feature1 (pts (xy 144.2466 81.1022) (xy 150.065421 81.1022)))
    (feature2 (pts (xy 144.2466 59.1566) (xy 150.065421 59.1566)))
    (crossbar (pts (xy 149.479 59.1566) (xy 149.479 81.1022)))
    (arrow1a (pts (xy 149.479 81.1022) (xy 148.892579 79.975696)))
    (arrow1b (pts (xy 149.479 81.1022) (xy 150.065421 79.975696)))
    (arrow2a (pts (xy 149.479 59.1566) (xy 148.892579 60.283104)))
    (arrow2b (pts (xy 149.479 59.1566) (xy 150.065421 60.283104)))
  )
  (gr_text +3.3v (at 124.8664 79.0702) (layer B.SilkS))
  (gr_text RESET (at 124.6632 76.708) (layer B.SilkS))
  (gr_text DIO_0 (at 124.714 73.9902) (layer B.SilkS))
  (gr_text NSS (at 124.333 71.5264) (layer B.SilkS))
  (gr_text MOSI (at 124.7394 68.8594) (layer B.SilkS))
  (gr_text MISO (at 124.7394 66.421) (layer B.SilkS))
  (gr_text SCK (at 124.333 63.7032) (layer B.SilkS))
  (gr_text GND (at 124.2822 61.4426) (layer B.SilkS))
  (gr_line (start 118.618 81.1022) (end 118.618 59.1566) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.018 81.1022) (end 118.618 81.1022) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.018 59.1566) (end 144.018 81.1022) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.618 59.1566) (end 144.018 59.1566) (layer Edge.Cuts) (width 0.05))
)
