(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 139.624999 85.014999 171.525001 97.865001)
    (thickness 1.6)
    (drawings 7)
    (tracks 8)
    (zones 0)
    (modules 3)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad_Via (layer F.Cu) (tedit 58B79E8D)
    (at 146.05 91.44)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (fp_text reference P1 (at 0 -4.5) (layer F.Fab))
    (fp_text value CONN_01X01 (at 0 4.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad "" thru_hole circle (at 2.625 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.856155 1.856155) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.625) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.856155 1.856155) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.625 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.856155 -1.856155) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.625) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.856155 -1.856155) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad_Via (layer F.Cu) (tedit 58B79E92)
    (at 165.1 91.44)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (fp_text reference P2 (at 0 -4.5) (layer F.Fab))
    (fp_text value CONN_01X01 (at 0 4.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad "" thru_hole circle (at 2.625 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.856155 1.856155) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.625) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.856155 1.856155) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.625 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.856155 -1.856155) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.625) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.856155 -1.856155) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Jacks:Thonkiconn_3.5mm_Switching_Jack_Compact_With_Hole (layer F.Cu) (tedit 58B79F31)
    (at 155.575 91.44 180)
    (fp_text reference J1 (at 0 -2.5 180) (layer F.Fab))
    (fp_text value JACK_2P (at 0 -7.62 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -4.92 180) (size 2.1 2.1) (drill 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 3.302 180) (size 2.1 2.1) (drill 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 5.715 180) (size 2.1 2.1) (drill 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad1)"))
    (pad 4 thru_hole circle (at 0 0 180) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text M (at 169.672 93.345 260) (layer F.SilkS))
  (gr_text C (at 169.672 89.535 280) (layer F.SilkS))
  (gr_text O (at 170.053 91.44 90) (layer F.SilkS))
  (gr_line (start 165.1 97.79) (end 146.05 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 85.09) (end 165.1 85.09) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.1 91.44) (end 165.1 85.09) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.05 91.44) (end 146.05 97.79) (angle 180) (layer Edge.Cuts) (width 0.15))
)
