(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 35)
    (tracks 506)
    (zones 0)
    (modules 26)
    (nets 33)
  )
  (page USLetter)
  (title_block
    (title "Light Sensor")
    (date 2019-02-01)
    (rev R006)
    (company "Indiana University")
    (comment 1 "Bryce Himebaugh")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.16)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.52 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.53 0.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "mfg/"))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 /SWDCLK)
  (net 5 /SWDIO)
  (net 6 /RX)
  (net 7 /TX)
  (net 8 "Net-(R1-Pad1)")
  (net 9 /SWO)
  (net 10 /rtc_data)
  (net 11 /sensor_data)
  (net 12 /sensor_clock)
  (net 13 /rtc_clock)
  (net 14 /NRST)
  (net 15 /oscillator)
  (net 16 /sensor_int)
  (net 17 /rtc_nINT)
  (net 18 /rtc_EVI)
  (net 19 /sensor_power)
  (net 20 "Net-(J1-Pad1)")
  (net 21 "Net-(J1-Pad2)")
  (net 22 /tsl237_freq)
  (net 23 /tsl237_pwr)
  (net 24 /sm_237t_freq)
  (net 25 /sm_237t_pwr)
  (net 26 "Net-(BT1-Pad1)")
  (net 27 /sensor_vdd)
  (net 28 /tsl237_vdd)
  (net 29 "Net-(J2-Pad2)")
  (net 30 /sm_237t_vdd)
  (net 31 /rtc_vdd)
  (net 32 /l432_pwr)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /NRST)
    (add_net /RX)
    (add_net /SWDCLK)
    (add_net /SWDIO)
    (add_net /SWO)
    (add_net /TX)
    (add_net /l432_pwr)
    (add_net /oscillator)
    (add_net /rtc_EVI)
    (add_net /rtc_clock)
    (add_net /rtc_data)
    (add_net /rtc_nINT)
    (add_net /rtc_vdd)
    (add_net /sensor_clock)
    (add_net /sensor_data)
    (add_net /sensor_int)
    (add_net /sensor_power)
    (add_net /sensor_vdd)
    (add_net /sm_237t_freq)
    (add_net /sm_237t_pwr)
    (add_net /sm_237t_vdd)
    (add_net /tsl237_freq)
    (add_net /tsl237_pwr)
    (add_net /tsl237_vdd)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net VDD)
  )
  (module logo:iu_trident (layer F.Cu) (tedit 0)
    (at 96.774 113.538)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module logo:hnf_logo (layer F.Cu) (tedit 0)
    (at 105.918 113.538)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module bhimebau_battery:Keystone_1091TR (layer B.Cu) (tedit 5D2CDD3F)
    (at 113.21 107.11 180)
    (fp_text reference BT1 (at 0 -0.5) (layer B.SilkS))
    (fp_text value Battery_Cell (at 0 0.5) (layer B.Fab))
    (pad 1 smd rect (at 0 10.9 180) (size 3.17 3.96) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 0 -10.9 180) (size 3.17 3.96) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Connector_JST:JST_XH_B3B-XH-AM_1x03_P2.50mm_Vertical (layer B.Cu) (tedit 5C28146E)
    (at 130.106969 113.334889 230)
    (descr "JST XH series connector, B3B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical boss")
    (fp_text reference J1 (at 2.5 3.55 230) (layer B.SilkS))
    (fp_text value Conn_01x03 (at 2.5 -4.6 230) (layer B.Fab))
    (fp_text user %R (at 2.5 -2.7 230) (layer B.Fab))
    (pad 1 thru_hole roundrect (at 0 0 230) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 20 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 230) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 230) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -1.6 -2 230) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-AM_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bhimebau_inductor:ftsh_14p_connector (layer B.Cu) (tedit 5C7B1BAD)
    (at 98.5 116.75 132)
    (fp_text reference U2 (at -5.464 -2.8916 222) (layer B.SilkS))
    (fp_text value STDC14 (at 0 7 312) (layer B.Fab))
    (pad 14 smd rect (at 3.81 2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 7 /TX))
    (pad 13 smd rect (at 3.81 -2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 6 /RX))
    (pad 12 smd rect (at 2.54 2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 14 /NRST))
    (pad 11 smd rect (at 2.54 -2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 1.27 2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 1.27 -2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 0 2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 9 /SWO))
    (pad 7 smd rect (at 0 -2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1.27 2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 4 /SWDCLK))
    (pad 5 smd rect (at -1.27 -2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.54 2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 5 /SWDIO))
    (pad 3 smd rect (at -2.54 -2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -3.81 2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -3.81 -2.032 132) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask))
  )
  (module SamacSys_Parts:TSL25911FN (layer F.Cu) (tedit 5C6305C2)
    (at 107.95254 105.25252)
    (descr TSL25911FN)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC1 (at 0.1098 -2.25252) (layer F.SilkS) hide)
    (fp_text value TSL25911FN (at 0.11684 -2.15392) (layer F.SilkS) hide)
    (pad 6 smd rect (at 0.75 -0.65 90) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /sensor_data))
    (pad 5 smd rect (at 0.75 0 90) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 /sensor_vdd))
    (pad 4 smd rect (at 0.75 0.65 90) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.75 0.65 90) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.75 0 90) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 /sensor_int))
    (pad 1 smd rect (at -0.75 -0.65 90) (size 0.35 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 /sensor_clock))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 92.013 103.607 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 2.907 -0.013 90) (layer F.SilkS))
    (fp_text value 300 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 105.88548 98.52844)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 2.80162 0.01016) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /l432_pwr))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 105.9312 96.913)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at 2.7178 0.0762 -180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /l432_pwr))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 96.75 105 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 3.3 0.1 90) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /l432_pwr))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 98.5 105.125 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 3.375 -0.05 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /l432_pwr))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 93.62336 103.3354 90)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D1 (at 3.0354 0.07664 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_DFN_QFN:QFN-32-1EP_5x5mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 102.5144 102.3874 270)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at -3.5179 3.1115) (layer F.SilkS))
    (fp_text value STM32L432KCUx (at 0 3.75 270) (layer F.Fab))
    (pad 33 smd rect (at -0.8625 -0.8625 270) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625 270) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625 270) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 0.8625 270) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 32 smd rect (at -1.75 -2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 31 smd rect (at -1.25 -2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 30 smd rect (at -0.75 -2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at -0.25 -2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 0.25 -2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 0.75 -2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /rtc_data))
    (pad 26 smd rect (at 1.25 -2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /SWO))
    (pad 25 smd rect (at 1.75 -2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 2.4 -1.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /SWDCLK))
    (pad 23 smd rect (at 2.4 -1.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /SWDIO))
    (pad 22 smd rect (at 2.4 -0.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 2.4 -0.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /sensor_power))
    (pad 20 smd rect (at 2.4 0.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /sensor_data))
    (pad 19 smd rect (at 2.4 0.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /sensor_clock))
    (pad 18 smd rect (at 2.4 1.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /sensor_int))
    (pad 17 smd rect (at 2.4 1.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 /l432_pwr))
    (pad 16 smd rect (at 1.75 2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 1.25 2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 0.75 2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad1)"))
    (pad 13 smd rect (at 0.25 2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /rtc_clock))
    (pad 12 smd rect (at -0.25 2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /rtc_nINT))
    (pad 11 smd rect (at -0.75 2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /tsl237_freq))
    (pad 10 smd rect (at -1.25 2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /tsl237_pwr))
    (pad 9 smd rect (at -1.75 2.4) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /RX))
    (pad 8 smd rect (at -2.4 1.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /TX))
    (pad 7 smd rect (at -2.4 1.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 /sm_237t_freq))
    (pad 6 smd rect (at -2.4 0.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /sm_237t_pwr))
    (pad 5 smd rect (at -2.4 0.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 /l432_pwr))
    (pad 4 smd rect (at -2.4 -0.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /NRST))
    (pad 3 smd rect (at -2.4 -0.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /rtc_EVI))
    (pad 2 smd rect (at -2.4 -1.25 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /oscillator))
    (pad 1 smd rect (at -2.4 -1.75 270) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 /l432_pwr))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tag_fp:RV-8803-C7 (layer F.Cu) (tedit 5B2036C6)
    (at 99.25 94.5 180)
    (fp_text reference U5 (at 1.8542 -0.75692 270) (layer F.SilkS) hide)
    (fp_text value RV-8803-C7 (at 0 -3.3 180) (layer F.Fab) hide)
    (pad 8 smd rect (at 0.6 -1.35 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /rtc_clock))
    (pad 7 smd rect (at 0.6 -0.45 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /rtc_EVI))
    (pad 6 smd rect (at 0.6 0.45 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /rtc_nINT))
    (pad 5 smd rect (at 0.6 1.35 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.6 1.35 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 /rtc_vdd))
    (pad 3 smd rect (at -0.6 0.45 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 /rtc_vdd))
    (pad 2 smd rect (at -0.6 -0.45 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /oscillator))
    (pad 1 smd rect (at -0.6 -1.35 180) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /rtc_data))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 120.875 113.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.725 0) (layer F.SilkS))
    (fp_text value 200 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /RX))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts_3:TSL237S-LF (layer F.Cu) (tedit 0)
    (at 113.30178 101.22916 180)
    (descr TSL237S-LF)
    (tags "Integrated Circuit")
    (fp_text reference IC2 (at 0.05178 -2.12084) (layer F.SilkS))
    (fp_text value TSL237S-LF (at -0.151 -1.731) (layer F.SilkS) hide)
    (fp_text user %R (at -0.151 -1.731) (layer F.Fab))
    (pad 1 thru_hole circle (at -2 0 180) (size 1.33 1.33) (drill 0.83) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.33 1.33) (drill 0.83) (layers *.Cu *.Mask)
      (net 28 /tsl237_vdd))
    (pad 3 thru_hole circle (at 2 0 180) (size 1.33 1.33) (drill 0.83) (layers *.Cu *.Mask)
      (net 22 /tsl237_freq))
  )
  (module bhimebau_lightsensor:tsl237t (layer F.Cu) (tedit 5D49BAE6)
    (at 119.78132 102.47884)
    (fp_text reference U3 (at -0.4 0.1) (layer F.SilkS))
    (fp_text value sm_tsl237 (at -0.2 -1.4) (layer F.Fab))
    (pad 1 smd rect (at -2.1 2.1) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.1 3.6) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.8 3.6) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /sm_237t_vdd))
    (pad 4 smd rect (at 0.8 2.1) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 24 /sm_237t_freq))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 120.75 111.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 2.8 0) (layer F.SilkS))
    (fp_text value 200 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /TX))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B4B-XH-AM_1x04_P2.50mm_Vertical (layer B.Cu) (tedit 5C28146E)
    (at 116.26 123.95 180)
    (descr "JST XH series connector, B4B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical boss")
    (fp_text reference J2 (at 11.26 2.01) (layer B.SilkS))
    (fp_text value Conn_01x04_Male (at 3.75 -4.6) (layer B.Fab))
    (fp_text user %R (at 3.75 -2.7) (layer B.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 7.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -1.6 -2 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B4B-XH-AM_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 121.28 126.09)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0.19 -7.72) (layer B.SilkS))
    (fp_text value Conn_01x03_Male (at 0 -7.41) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad2)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 119.82 109.22 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at -2.19 -2.59 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /TX))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /RX))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 124.67 90.21)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 3.092 -2.072) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /tsl237_pwr))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /tsl237_vdd))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /tsl237_freq))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 124.79 100.45)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 3.226 -1.644) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /sm_237t_freq))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /sm_237t_vdd))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /sm_237t_pwr))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 103.378 91.694)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J7 (at -2.794 -0.762) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /l432_pwr))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 117.856 84.328)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J8 (at -5.842 -0.508) (layer F.SilkS) hide)
    (fp_text value Conn_01x07_Male (at 0 17.57) (layer F.Fab))
    (fp_text user %R (at 0 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /rtc_clock))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /rtc_data))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /rtc_EVI))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /rtc_nINT))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /oscillator))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /rtc_vdd))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 132.266 96.81)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J9 (at 2.862 12.156) (layer F.SilkS) hide)
    (fp_text value Conn_01x05_Male (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /sensor_clock))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /sensor_data))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /sensor_int))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /sensor_vdd))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /sensor_power))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text pwr (at 120.65 96.774) (layer F.SilkS))
  (gr_text in (at 120.142 99.568) (layer F.SilkS))
  (gr_text osc (at 120.65 94.234) (layer F.SilkS))
  (gr_text nint (at 120.65 91.694) (layer F.SilkS))
  (gr_text evi (at 120.396 89.154) (layer F.SilkS))
  (gr_text data (at 120.904 86.614) (layer F.SilkS))
  (gr_text clk (at 120.142 84.074) (layer F.SilkS))
  (gr_text rtc (at 117.602 82.296) (layer F.SilkS))
  (gr_text L432 (at 103.378 89.154) (layer F.SilkS))
  (gr_text in (at 105.41 93.98) (layer F.SilkS))
  (gr_text 237 (at 124.714 88.138) (layer F.SilkS))
  (gr_text in (at 126.746 95.504) (layer F.SilkS))
  (gr_text pwr (at 127.254 92.71) (layer F.SilkS))
  (gr_text "hz\n" (at 126.746 90.17) (layer F.SilkS))
  (gr_text in (at 134.366 106.934) (layer F.SilkS))
  (gr_text pwr (at 134.874 104.2) (layer F.SilkS))
  (gr_text int (at 134.62 101.6) (layer F.SilkS))
  (gr_text data (at 135.382 99.314) (layer F.SilkS))
  (gr_text clk (at 134.62 96.68) (layer F.SilkS))
  (gr_text 25911 (at 132.588 94.742) (layer F.SilkS))
  (gr_text 237t (at 124.83 98.298) (layer F.SilkS))
  (gr_text pwr (at 127.508 102.85) (layer F.SilkS))
  (gr_text "in\n" (at 127 105.42) (layer F.SilkS))
  (gr_text hz (at 127 100.33) (layer F.SilkS))
  (gr_text tx (at 117.602 109.22) (layer F.SilkS))
  (gr_text rx (at 124.93 109.22) (layer F.SilkS))
  (gr_text batt (at 124.62 120.79) (layer B.SilkS))
  (gr_text board (at 125.222 123.444) (layer B.SilkS))
  (gr_text mon (at 124.6 126.11) (layer B.SilkS))
  (gr_text pwr (at 105.918 91.44) (layer F.SilkS))
  (gr_circle (center 113.36 105.22) (end 138.437402 105.22) (layer Edge.Cuts) (width 0.15))
  (gr_text R006 (at 99.568 122.428) (layer F.SilkS))
  (gr_text "Dark Sky" (at 99.568 119.888) (layer F.SilkS))
  (zone (net 1) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.25 78.5) (xy 83.5 132) (xy 141 131.75) (xy 140 78.75)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.25 78.5) (xy 83.5 132) (xy 141 131.75) (xy 140 78.75)
      )
    )
  )
)
