(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 46)
    (no_connects 0)
    (area 158.699999 68.529999 247.700001 96.570001)
    (thickness 1.6)
    (drawings 25)
    (tracks 152)
    (zones 0)
    (modules 29)
    (nets 23)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 2.032)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.254)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 1 0.5)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.4 3.4)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 210.82 95.25)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +BATT)
  (net 3 "Net-(BT1-Pad1)")
  (net 4 "Net-(CON1-Pad1)")
  (net 5 "Net-(CON1-Pad3)")
  (net 6 "Net-(CON1-Pad4)")
  (net 7 "Net-(CON1-Pad5)")
  (net 8 "Net-(D1-Pad1)")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D0-Pad2)")
  (net 11 "Net-(D0-Pad1)")
  (net 12 "Net-(D2-Pad2)")
  (net 13 "Net-(D2-Pad1)")
  (net 14 "Net-(D3-Pad2)")
  (net 15 "Net-(D3-Pad1)")
  (net 16 "Net-(D4-Pad1)")
  (net 17 "Net-(D5-Pad1)")
  (net 18 "Net-(D6-Pad1)")
  (net 19 "Net-(D7-Pad2)")
  (net 20 "Net-(D7-Pad1)")
  (net 21 "Net-(IC1-Pad2)")
  (net 22 "Net-(IC1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(CON1-Pad4)")
    (add_net "Net-(CON1-Pad5)")
    (add_net "Net-(D0-Pad1)")
    (add_net "Net-(D0-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad5)")
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5976A0AA)
    (at 195.834 93.726 135)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U1 (at 2.529479 -2.122485 315) (layer F.SilkS))
    (fp_text value MLX92231 (at 0 3 135) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 225) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at 5.08 0 225) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(IC1-Pad5)"))
    (pad 1 thru_hole circle (at 0 0 225) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +BATT))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module myFootPrints:AVR-ISP-6 (layer B.Cu) (tedit 59769CE5)
    (at 183.515 75.565 90)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference CON1 (at 0 2.54 90) (layer B.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 0 3.72 90) (layer B.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.762) (layers *.Cu B.SilkS B.Mask)
      (net 4 "Net-(CON1-Pad1)"))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 1.6 1.6) (drill 0.762) (layers *.Cu B.SilkS B.Mask)
      (net 2 +BATT))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.6 1.6) (drill 0.762) (layers *.Cu B.SilkS B.Mask)
      (net 5 "Net-(CON1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.6 1.6) (drill 0.762) (layers *.Cu B.SilkS B.Mask)
      (net 6 "Net-(CON1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.6 1.6) (drill 0.762) (layers *.Cu B.SilkS B.Mask)
      (net 7 "Net-(CON1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.6 1.6) (drill 0.762) (layers *.Cu B.SilkS B.Mask)
      (net 1 GND))
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 593A1D84)
    (at 189.23 70.485 270)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference IC1 (at 0 -5.22 270) (layer F.SilkS) hide)
    (fp_text value ATTINY84-S (at 3.937 7.493 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +BATT))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(CON1-Pad5)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D7-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(CON1-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(CON1-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(CON1-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D3-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D2-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D1-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D0-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Lego_Drill (layer F.Cu) (tedit 5938B9BC)
    (at 241.3 90.17)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:SW_PUSH_SMALL (layer F.Cu) (tedit 57A15124)
    (at 168.91 75.565 270)
    (fp_text reference SW1 (at 0 0 270) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 2 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 3.25 -2.25 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(IC1-Pad2)"))
    (pad 2 thru_hole circle (at 3.25 2.25 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(IC1-Pad2)"))
    (pad 2 thru_hole circle (at -3.25 2.25 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module myFootPrints:Lego_Drill (layer F.Cu) (tedit 59879AE0)
    (at 163.195 76.835)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.4 3.4) (drill 3) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:BATT_CR2032 (layer F.Cu) (tedit 0)
    (at 227.33 83.058)
    (tags battery)
    (fp_text reference BT1 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text value Battery (at 0 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -10.414 1.524) (size 2.286 2.286) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole circle (at 10.414 1.524) (size 2.286 2.286) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole circle (at -10.414 -1.524) (size 2.286 2.286) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole circle (at 10.414 -1.524) (size 2.286 2.286) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 2 smd circle (at 0 0) (size 17.78 17.78) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module myFootPrints:Lego_Drill (layer F.Cu) (tedit 5938B9BC)
    (at 241.3 74.93)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:Lego_Drill (layer F.Cu) (tedit 59879AD4)
    (at 163.322 88.138)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.4 3.4) (drill 3) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:MadeInOregonRev25 (layer F.Cu) (tedit 0)
    (at 228.854 84.836)
    (fp_text reference VAL (at 0 0) (layer F.SilkS) hide)
    (fp_text value MadeInOregonRev25 (at 0 0) (layer F.SilkS) hide)
  )
  (module project_footprints:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5937975F)
    (at 203.2 82.55)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.6 -0.5) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 24 24) (drill 22.025) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module myFootPrints:C1 (layer F.Cu) (tedit 59769C43)
    (at 192.405 72.39 270)
    (descr "Condensateur e = 1 pas")
    (tags C)
    (fp_text reference C1 (at -1.905 -1.905 270) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at -1.016 -2.159 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +BATT))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/capa_1_pas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 187.96 83.82 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D0 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D0-Pad1)"))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D0-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 184.15 83.82 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D1-Pad1)"))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 180.34 83.82 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D2-Pad1)"))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 176.53 83.82 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D3-Pad1)"))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 172.72 83.82 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D4 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D4-Pad1)"))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(CON1-Pad3)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 168.91 83.82 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D5 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D5-Pad1)"))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(CON1-Pad1)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 165.1 83.82 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D6 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D6-Pad1)"))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(CON1-Pad4)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 57578FCB)
    (at 161.29 83.82 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D7 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D7-Pad1)"))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D7-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 593A1335)
    (at 189.23 90.17 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R0 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(D0-Pad1)"))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 186.055 90.17 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 182.88 90.17 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R2 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 179.705 90.17 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R3 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 176.53 90.17 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R4 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 16 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 173.355 90.17 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R5 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 170.18 90.17 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R6 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5664956A)
    (at 167.005 90.17 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R7 (at 0 -1.905 270) (layer F.Fab))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 20 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 3.175 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:mySwitchDPDT (layer F.Cu) (tedit 59769EE5)
    (at 241.935 83.185 270)
    (descr "Switch Nikkai ref G1xJP")
    (tags "SWITCH DEV TOGGLE ILLUM SPDT")
    (fp_text reference SW2 (at -0.127 0 270) (layer F.SilkS))
    (fp_text value SPST (at 0.254 -3.302 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 1.27 270) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 2 +BATT))
    (pad 2 thru_hole circle (at 0 1.27 270) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 1.27 270) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 2.54 -1.27 270) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 0 -1.27 270) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -2.54 -1.27 270) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask F.SilkS))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_NKK_G1xJP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.33 0.33 0.33))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text - (at 176.53 71.755) (layer B.SilkS))
  (gr_text + (at 185.42 71.755) (layer B.SilkS))
  (gr_text D7 (at 162.814 85.09) (layer F.SilkS))
  (gr_text D6 (at 166.624 85.09) (layer F.SilkS))
  (gr_text D5 (at 170.434 85.09) (layer F.SilkS))
  (gr_text D4 (at 174.244 85.09) (layer F.SilkS))
  (gr_text D3 (at 178.054 85.09) (layer F.SilkS))
  (gr_text D2 (at 181.864 85.09) (layer F.SilkS))
  (gr_text D0 (at 189.738 85.09) (layer F.SilkS))
  (gr_text D1 (at 185.928 85.09) (layer F.SilkS))
  (gr_text CR2032 (at 227.457 93.599) (layer F.SilkS))
  (gr_text "GEEK\nSPINNER" (at 233.68 75.565) (layer B.SilkS))
  (gr_text ON (at 243.84 78.105) (layer F.SilkS))
  (gr_line (start 233.68 68.58) (end 172.72 68.58) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 172.72 96.52) (end 233.68 96.52) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "Rev 1.1\nSep 2017" (at 229.235 92.075) (layer B.SilkS))
  (gr_text www.MakersBox.us (at 177.8 90.17) (layer B.SilkS))
  (gr_arc (start 233.68 82.55) (end 247.65 82.55) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 233.68 82.55) (end 233.68 68.58) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 172.72 82.55) (end 158.75 82.55) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 172.72 82.55) (end 172.72 96.52) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.2 96.52) (xy 158.75 96.52) (xy 158.75 67.31) (xy 203.2 67.31)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 204.47 98.425) (xy 157.48 97.79) (xy 157.48 66.04) (xy 204.47 66.675)
      )
    )
  )
)
