(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 1064)
    (zones 0)
    (modules 8)
    (nets 61)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1778)
    (user_trace_width 0.5)
    (trace_clearance 0.1778)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(CON1-PadB1)")
  (net 2 "Net-(CON1-PadB2)")
  (net 3 "Net-(CON1-PadB3)")
  (net 4 /A8)
  (net 5 /A9)
  (net 6 /A17)
  (net 7 /A18)
  (net 8 "Net-(CON1-PadB10)")
  (net 9 "Net-(CON1-PadB11)")
  (net 10 "Net-(CON1-PadB12)")
  (net 11 "Net-(CON1-PadB13)")
  (net 12 "Net-(CON1-PadB14)")
  (net 13 "Net-(CON1-PadB15)")
  (net 14 /OE)
  (net 15 /CE)
  (net 16 "Net-(CON1-PadB18)")
  (net 17 "Net-(CON1-PadB19)")
  (net 18 "Net-(CON1-PadB20)")
  (net 19 "Net-(CON1-PadB21)")
  (net 20 /D15)
  (net 21 /D14)
  (net 22 /D13)
  (net 23 /D12)
  (net 24 "Net-(CON1-PadB26)")
  (net 25 /RESET)
  (net 26 /WE)
  (net 27 "Net-(CON1-PadB29)")
  (net 28 "Net-(CON1-PadB30)")
  (net 29 /TIME)
  (net 30 GND)
  (net 31 /A10)
  (net 32 +5V)
  (net 33 /A7)
  (net 34 /A6)
  (net 35 /A12)
  (net 36 /A4)
  (net 37 /A11)
  (net 38 /A5)
  (net 39 /A13)
  (net 40 /A2)
  (net 41 /A15)
  (net 42 /A3)
  (net 43 /A14)
  (net 44 /A1)
  (net 45 /A16)
  (net 46 /D0)
  (net 47 /D7)
  (net 48 /A0)
  (net 49 /D8)
  (net 50 /D6)
  (net 51 /D4)
  (net 52 /D3)
  (net 53 /D11)
  (net 54 /D1)
  (net 55 /D9)
  (net 56 /D5)
  (net 57 /D2)
  (net 58 /D10)
  (net 59 "Net-(CON1-PadB8)")
  (net 60 "Net-(CON1-PadB9)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CE)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D14)
    (add_net /D15)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /OE)
    (add_net /RESET)
    (add_net /TIME)
    (add_net /WE)
    (add_net "Net-(CON1-PadB1)")
    (add_net "Net-(CON1-PadB10)")
    (add_net "Net-(CON1-PadB11)")
    (add_net "Net-(CON1-PadB12)")
    (add_net "Net-(CON1-PadB13)")
    (add_net "Net-(CON1-PadB14)")
    (add_net "Net-(CON1-PadB15)")
    (add_net "Net-(CON1-PadB18)")
    (add_net "Net-(CON1-PadB19)")
    (add_net "Net-(CON1-PadB2)")
    (add_net "Net-(CON1-PadB20)")
    (add_net "Net-(CON1-PadB21)")
    (add_net "Net-(CON1-PadB26)")
    (add_net "Net-(CON1-PadB29)")
    (add_net "Net-(CON1-PadB3)")
    (add_net "Net-(CON1-PadB30)")
    (add_net "Net-(CON1-PadB8)")
    (add_net "Net-(CON1-PadB9)")
  )
  (net_class POWER ""
    (clearance 0.1778)
    (trace_width 0.508)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net +5V)
    (add_net GND)
  )
  (module Package_LCC:PLCC-32_11.4x14.0mm_P1.27mm (layer F.Cu) (tedit 5B298677)
    (at 118.12524 80.19542 90)
    (descr "PLCC, 32 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/doc0015.pdf), generated with kicad-footprint-generator ipc_plcc_jLead_generator.py")
    (tags "PLCC LCC")
    (attr smd)
    (fp_text reference U1 (at -11.24458 0.61976 180) (layer F.SilkS))
    (fp_text value SST39SF040 (at 0 8.52 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 32 smd roundrect (at 1.27 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (pad 31 smd roundrect (at 2.54 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (pad 30 smd roundrect (at 3.81 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /A17))
    (pad 29 smd roundrect (at 5.5625 -5.08 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /A14))
    (pad 28 smd roundrect (at 5.5625 -3.81 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /A13))
    (pad 27 smd roundrect (at 5.5625 -2.54 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /A8))
    (pad 26 smd roundrect (at 5.5625 -1.27 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /A9))
    (pad 25 smd roundrect (at 5.5625 0 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /A11))
    (pad 24 smd roundrect (at 5.5625 1.27 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /OE))
    (pad 23 smd roundrect (at 5.5625 2.54 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /A10))
    (pad 22 smd roundrect (at 5.5625 3.81 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /CE))
    (pad 21 smd roundrect (at 5.5625 5.08 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /D7))
    (pad 20 smd roundrect (at 3.81 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /D6))
    (pad 19 smd roundrect (at 2.54 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /D5))
    (pad 18 smd roundrect (at 1.27 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /D4))
    (pad 17 smd roundrect (at 0 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /D3))
    (pad 16 smd roundrect (at -1.27 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 GND))
    (pad 15 smd roundrect (at -2.54 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /D2))
    (pad 14 smd roundrect (at -3.81 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /D1))
    (pad 13 smd roundrect (at -5.5625 5.08 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /D0))
    (pad 12 smd roundrect (at -5.5625 3.81 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /A0))
    (pad 11 smd roundrect (at -5.5625 2.54 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /A1))
    (pad 10 smd roundrect (at -5.5625 1.27 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /A2))
    (pad 9 smd roundrect (at -5.5625 0 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /A3))
    (pad 8 smd roundrect (at -5.5625 -1.27 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /A4))
    (pad 7 smd roundrect (at -5.5625 -2.54 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /A5))
    (pad 6 smd roundrect (at -5.5625 -3.81 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /A6))
    (pad 5 smd roundrect (at -5.5625 -5.08 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /A7))
    (pad 4 smd roundrect (at -3.81 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /A12))
    (pad 3 smd roundrect (at -2.54 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /A15))
    (pad 2 smd roundrect (at -1.27 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /A16))
    (pad 1 smd roundrect (at 0 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /A18))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-32_11.4x14.0mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:GENESIS-EDGE (layer F.Cu) (tedit 5F01832B)
    (at 92.075 109.728)
    (fp_text reference CON1 (at 0.8 -5.2) (layer F.SilkS) hide)
    (fp_text value GENESIS-EDGE (at 3.9 -7.4) (layer F.Fab) hide)
    (fp_line (start 81.28 3.175) (end 81.28 -3.81) (layer Edge.Cuts) (width 0.254))
    (fp_line (start 80.01 4.445) (end 81.28 3.175) (layer Edge.Cuts) (width 0.254))
    (fp_line (start -1.27 4.445) (end 80.01 4.445) (layer Edge.Cuts) (width 0.254))
    (fp_line (start -2.54 3.175) (end -1.27 4.445) (layer Edge.Cuts) (width 0.254))
    (fp_line (start -2.54 -3.81) (end -2.54 3.175) (layer Edge.Cuts) (width 0.254))
    (pad B1 smd rect (at 0 0) (size 1.905 6.858) (layers F.Cu)
      (net 1 "Net-(CON1-PadB1)"))
    (pad B2 smd rect (at 2.54 0) (size 1.905 6.858) (layers F.Cu)
      (net 2 "Net-(CON1-PadB2)"))
    (pad B3 smd rect (at 5.08 0) (size 1.905 6.858) (layers F.Cu)
      (net 3 "Net-(CON1-PadB3)"))
    (pad B4 smd rect (at 7.62 0) (size 1.905 6.858) (layers F.Cu)
      (net 4 /A8))
    (pad B5 smd rect (at 10.16 0) (size 1.905 6.858) (layers F.Cu)
      (net 5 /A9))
    (pad B6 smd rect (at 12.7 0) (size 1.905 6.858) (layers F.Cu)
      (net 6 /A17))
    (pad B7 smd rect (at 15.24 0) (size 1.905 6.858) (layers F.Cu)
      (net 7 /A18))
    (pad B8 smd rect (at 17.78 0) (size 1.905 6.858) (layers F.Cu)
      (net 59 "Net-(CON1-PadB8)"))
    (pad B9 smd rect (at 20.32 0) (size 1.905 6.858) (layers F.Cu)
      (net 60 "Net-(CON1-PadB9)"))
    (pad B10 smd rect (at 22.86 0) (size 1.905 6.858) (layers F.Cu)
      (net 8 "Net-(CON1-PadB10)"))
    (pad B11 smd rect (at 25.4 0) (size 1.905 6.858) (layers F.Cu)
      (net 9 "Net-(CON1-PadB11)"))
    (pad B12 smd rect (at 27.94 0) (size 1.905 6.858) (layers F.Cu)
      (net 10 "Net-(CON1-PadB12)"))
    (pad B13 smd rect (at 30.48 0) (size 1.905 6.858) (layers F.Cu)
      (net 11 "Net-(CON1-PadB13)"))
    (pad B14 smd rect (at 33.02 0) (size 1.905 6.858) (layers F.Cu)
      (net 12 "Net-(CON1-PadB14)"))
    (pad B15 smd rect (at 35.56 0) (size 1.905 6.858) (layers F.Cu)
      (net 13 "Net-(CON1-PadB15)"))
    (pad B16 smd rect (at 38.1 0) (size 1.905 6.858) (layers F.Cu)
      (net 14 /OE))
    (pad B17 smd rect (at 40.64 0) (size 1.905 6.858) (layers F.Cu)
      (net 15 /CE))
    (pad B18 smd rect (at 43.18 0) (size 1.905 6.858) (layers F.Cu)
      (net 16 "Net-(CON1-PadB18)"))
    (pad B19 smd rect (at 45.72 0) (size 1.905 6.858) (layers F.Cu)
      (net 17 "Net-(CON1-PadB19)"))
    (pad B20 smd rect (at 48.26 0) (size 1.905 6.858) (layers F.Cu)
      (net 18 "Net-(CON1-PadB20)"))
    (pad B21 smd rect (at 50.8 0) (size 1.905 6.858) (layers F.Cu)
      (net 19 "Net-(CON1-PadB21)"))
    (pad B22 smd rect (at 53.34 0) (size 1.905 6.858) (layers F.Cu)
      (net 20 /D15))
    (pad B23 smd rect (at 55.88 0) (size 1.905 6.858) (layers F.Cu)
      (net 21 /D14))
    (pad B24 smd rect (at 58.42 0) (size 1.905 6.858) (layers F.Cu)
      (net 22 /D13))
    (pad B25 smd rect (at 60.96 0) (size 1.905 6.858) (layers F.Cu)
      (net 23 /D12))
    (pad B26 smd rect (at 63.5 0) (size 1.905 6.858) (layers F.Cu)
      (net 24 "Net-(CON1-PadB26)"))
    (pad B27 smd rect (at 66.04 0) (size 1.905 6.858) (layers F.Cu)
      (net 25 /RESET))
    (pad B28 smd rect (at 68.58 0) (size 1.905 6.858) (layers F.Cu)
      (net 26 /WE))
    (pad B29 smd rect (at 71.12 0) (size 1.905 6.858) (layers F.Cu)
      (net 27 "Net-(CON1-PadB29)"))
    (pad B30 smd rect (at 73.66 0) (size 1.905 6.858) (layers F.Cu)
      (net 28 "Net-(CON1-PadB30)"))
    (pad B31 smd rect (at 76.2 0) (size 1.905 6.858) (layers F.Cu)
      (net 29 /TIME))
    (pad B32 smd rect (at 78.74 0) (size 1.905 6.858) (layers F.Cu)
      (net 30 GND))
    (pad A4 smd rect (at 7.62 0) (size 1.905 6.858) (layers B.Cu)
      (net 31 /A10))
    (pad A2 smd rect (at 2.54 0) (size 1.905 6.858) (layers B.Cu)
      (net 32 +5V))
    (pad A1 smd rect (at 0 0) (size 1.905 6.858) (layers B.Cu)
      (net 30 GND))
    (pad A3 smd rect (at 5.08 0) (size 1.905 6.858) (layers B.Cu)
      (net 33 /A7))
    (pad A5 smd rect (at 10.16 0) (size 1.905 6.858) (layers B.Cu)
      (net 34 /A6))
    (pad A8 smd rect (at 17.78 0) (size 1.905 6.858) (layers B.Cu)
      (net 35 /A12))
    (pad A9 smd rect (at 20.32 0) (size 1.905 6.858) (layers B.Cu)
      (net 36 /A4))
    (pad A6 smd rect (at 12.7 0) (size 1.905 6.858) (layers B.Cu)
      (net 37 /A11))
    (pad A7 smd rect (at 15.24 0) (size 1.905 6.858) (layers B.Cu)
      (net 38 /A5))
    (pad A10 smd rect (at 22.86 0) (size 1.905 6.858) (layers B.Cu)
      (net 39 /A13))
    (pad A13 smd rect (at 30.48 0) (size 1.905 6.858) (layers B.Cu)
      (net 40 /A2))
    (pad A14 smd rect (at 33.02 0) (size 1.905 6.858) (layers B.Cu)
      (net 41 /A15))
    (pad A11 smd rect (at 25.4 0) (size 1.905 6.858) (layers B.Cu)
      (net 42 /A3))
    (pad A12 smd rect (at 27.94 0) (size 1.905 6.858) (layers B.Cu)
      (net 43 /A14))
    (pad A15 smd rect (at 35.56 0) (size 1.905 6.858) (layers B.Cu)
      (net 44 /A1))
    (pad A16 smd rect (at 38.1 0) (size 1.905 6.858) (layers B.Cu)
      (net 45 /A16))
    (pad A18 smd rect (at 43.18 0) (size 1.905 6.858) (layers B.Cu)
      (net 30 GND))
    (pad A20 smd rect (at 48.26 0) (size 1.905 6.858) (layers B.Cu)
      (net 46 /D0))
    (pad A19 smd rect (at 45.72 0) (size 1.905 6.858) (layers B.Cu)
      (net 47 /D7))
    (pad A17 smd rect (at 40.64 0) (size 1.905 6.858) (layers B.Cu)
      (net 48 /A0))
    (pad A21 smd rect (at 50.8 0) (size 1.905 6.858) (layers B.Cu)
      (net 49 /D8))
    (pad A22 smd rect (at 53.34 0) (size 1.905 6.858) (layers B.Cu)
      (net 50 /D6))
    (pad A31 smd rect (at 76.2 0) (size 1.905 6.858) (layers B.Cu)
      (net 32 +5V))
    (pad A28 smd rect (at 68.58 0) (size 1.905 6.858) (layers B.Cu)
      (net 51 /D4))
    (pad A29 smd rect (at 71.12 0) (size 1.905 6.858) (layers B.Cu)
      (net 52 /D3))
    (pad A30 smd rect (at 73.66 0) (size 1.905 6.858) (layers B.Cu)
      (net 53 /D11))
    (pad A32 smd rect (at 78.74 0) (size 1.905 6.858) (layers B.Cu)
      (net 30 GND))
    (pad A23 smd rect (at 55.88 0) (size 1.905 6.858) (layers B.Cu)
      (net 54 /D1))
    (pad A24 smd rect (at 58.42 0) (size 1.905 6.858) (layers B.Cu)
      (net 55 /D9))
    (pad A25 smd rect (at 60.96 0) (size 1.905 6.858) (layers B.Cu)
      (net 56 /D5))
    (pad A26 smd rect (at 63.5 0) (size 1.905 6.858) (layers B.Cu)
      (net 57 /D2))
    (pad A27 smd rect (at 66.04 0) (size 1.905 6.858) (layers B.Cu)
      (net 58 /D10))
    (pad "" np_thru_hole circle (at 5.715 -29.718) (size 6.096 6.096) (drill 6.096) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 75.057 -29.718) (size 6.096 6.096) (drill 6.096) (layers *.Cu *.Mask))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x32_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A422)
    (at 169.672 99.822 270)
    (descr "Through hole straight socket strip, 1x32, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x32 2.54mm single row")
    (fp_text reference J2 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x32_Male (at 0 81.51 90) (layer F.Fab))
    (fp_text user %R (at 0 39.37) (layer F.Fab))
    (pad 32 thru_hole oval (at 0 78.74 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(CON1-PadB1)"))
    (pad 31 thru_hole oval (at 0 76.2 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(CON1-PadB2)"))
    (pad 30 thru_hole oval (at 0 73.66 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(CON1-PadB3)"))
    (pad 29 thru_hole oval (at 0 71.12 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A8))
    (pad 28 thru_hole oval (at 0 68.58 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A9))
    (pad 27 thru_hole oval (at 0 66.04 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A17))
    (pad 26 thru_hole oval (at 0 63.5 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A18))
    (pad 25 thru_hole oval (at 0 60.96 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(CON1-PadB8)"))
    (pad 24 thru_hole oval (at 0 58.42 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(CON1-PadB9)"))
    (pad 23 thru_hole oval (at 0 55.88 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(CON1-PadB10)"))
    (pad 22 thru_hole oval (at 0 53.34 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(CON1-PadB11)"))
    (pad 21 thru_hole oval (at 0 50.8 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(CON1-PadB12)"))
    (pad 20 thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(CON1-PadB13)"))
    (pad 19 thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(CON1-PadB14)"))
    (pad 18 thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(CON1-PadB15)"))
    (pad 17 thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /OE))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /CE))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(CON1-PadB18)"))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(CON1-PadB19)"))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(CON1-PadB20)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(CON1-PadB21)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /D15))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /D14))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /D13))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /D12))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(CON1-PadB26)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /RESET))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /WE))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(CON1-PadB29)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(CON1-PadB30)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /TIME))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x32_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LCC:PLCC-32_11.4x14.0mm_P1.27mm (layer F.Cu) (tedit 5B298677)
    (at 146.96948 80.22082 90)
    (descr "PLCC, 32 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/doc0015.pdf), generated with kicad-footprint-generator ipc_plcc_jLead_generator.py")
    (tags "PLCC LCC")
    (attr smd)
    (fp_text reference U2 (at -11.21918 -0.91948) (layer F.SilkS))
    (fp_text value SST39SF040 (at 0 8.52 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 32 smd roundrect (at 1.27 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (pad 31 smd roundrect (at 2.54 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 +5V))
    (pad 30 smd roundrect (at 3.81 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /A17))
    (pad 29 smd roundrect (at 5.5625 -5.08 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /A14))
    (pad 28 smd roundrect (at 5.5625 -3.81 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /A13))
    (pad 27 smd roundrect (at 5.5625 -2.54 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /A8))
    (pad 26 smd roundrect (at 5.5625 -1.27 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /A9))
    (pad 25 smd roundrect (at 5.5625 0 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /A11))
    (pad 24 smd roundrect (at 5.5625 1.27 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /OE))
    (pad 23 smd roundrect (at 5.5625 2.54 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /A10))
    (pad 22 smd roundrect (at 5.5625 3.81 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /CE))
    (pad 21 smd roundrect (at 5.5625 5.08 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /D15))
    (pad 20 smd roundrect (at 3.81 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /D14))
    (pad 19 smd roundrect (at 2.54 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /D13))
    (pad 18 smd roundrect (at 1.27 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /D12))
    (pad 17 smd roundrect (at 0 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /D11))
    (pad 16 smd roundrect (at -1.27 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 GND))
    (pad 15 smd roundrect (at -2.54 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /D10))
    (pad 14 smd roundrect (at -3.81 6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /D9))
    (pad 13 smd roundrect (at -5.5625 5.08 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /D8))
    (pad 12 smd roundrect (at -5.5625 3.81 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /A0))
    (pad 11 smd roundrect (at -5.5625 2.54 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /A1))
    (pad 10 smd roundrect (at -5.5625 1.27 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /A2))
    (pad 9 smd roundrect (at -5.5625 0 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /A3))
    (pad 8 smd roundrect (at -5.5625 -1.27 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /A4))
    (pad 7 smd roundrect (at -5.5625 -2.54 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /A5))
    (pad 6 smd roundrect (at -5.5625 -3.81 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /A6))
    (pad 5 smd roundrect (at -5.5625 -5.08 90) (size 1.475 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /A7))
    (pad 4 smd roundrect (at -3.81 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /A12))
    (pad 3 smd roundrect (at -2.54 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /A15))
    (pad 2 smd roundrect (at -1.27 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /A16))
    (pad 1 smd roundrect (at 0 -6.8375 90) (size 0.6 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /A18))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-32_11.4x14.0mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 149.34184 80.95234)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.65 180) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 30 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 32 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 114.74196 80.74406)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 1.65 180) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 30 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 32 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 163.69792 87.41156 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C3 (at 2.5 -5.25 180) (layer F.SilkS))
    (fp_text value 47u (at 2.5 5.25 90) (layer F.Fab))
    (fp_text user %R (at 2.447959 0.077459 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x32_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A422)
    (at 92.202 102.616 90)
    (descr "Through hole straight socket strip, 1x32, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x32 2.54mm single row")
    (fp_text reference J1 (at 0 -1.702 90) (layer F.SilkS))
    (fp_text value Conn_01x32_Male (at 0 81.51 90) (layer F.Fab))
    (fp_text user %R (at 0 39.37) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /A7))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /A10))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A6))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /A11))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /A5))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /A12))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /A4))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /A13))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /A3))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /A14))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /A2))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /A15))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /A1))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /A16))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /A0))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /D7))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /D0))
    (pad 21 thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /D8))
    (pad 22 thru_hole oval (at 0 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /D6))
    (pad 23 thru_hole oval (at 0 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /D1))
    (pad 24 thru_hole oval (at 0 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /D9))
    (pad 25 thru_hole oval (at 0 60.96 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /D5))
    (pad 26 thru_hole oval (at 0 63.5 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /D2))
    (pad 27 thru_hole oval (at 0 66.04 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /D10))
    (pad 28 thru_hole oval (at 0 68.58 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /D4))
    (pad 29 thru_hole oval (at 0 71.12 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /D3))
    (pad 30 thru_hole oval (at 0 73.66 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /D11))
    (pad 31 thru_hole oval (at 0 76.2 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 +5V))
    (pad 32 thru_hole oval (at 0 78.74 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x32_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text SST39SF040 (at 132.715 92.075) (layer F.SilkS))
  (gr_text "PLCC ROM cart P1\nDesigned by rfmerrill@berkeley.edu 2021-06-20\nBased on Genesis FRAM cart by github.com/soniccd123" (at 132.5 92) (layer B.SilkS))
  (gr_text "LO BYTE 7:0" (at 118.745 92.71) (layer F.SilkS))
  (gr_text "HI BYTE 15:8" (at 146.685 92.71) (layer F.SilkS))
  (gr_text B1 (at 92.075 105.029) (layer F.SilkS))
  (gr_text A1 (at 92.075 105.029) (layer B.SilkS))
  (gr_text B32 (at 170.815 105.029) (layer F.SilkS))
  (gr_text A32 (at 170.815 105.029) (layer B.SilkS))
  (gr_line (start 173.355 71.1708) (end 173.355001 105.918) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.535 71.1708) (end 173.355 71.1708) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.535001 105.918) (end 89.535 71.1708) (layer Edge.Cuts) (width 0.05))
  (zone (net 30) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 89.535 53.34) (xy 89.535 105.918) (xy 173.355 105.918) (xy 173.355 53.34)
      )
    )
  )
  (zone (net 32) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 174.1678 69.71538) (xy 173.355 105.918) (xy 89.535 105.918) (xy 88.62314 69.38518)
      )
    )
    (polygon
      (pts
        (xy 154.305 88.9) (xy 95.885 88.9) (xy 94.996 89.535) (xy 94.996 95.885) (xy 95.885 96.52)
        (xy 153.67 96.52) (xy 154.94 95.25) (xy 154.94 89.535)
      )
    )
  )
  (zone (net 30) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 96.52 89.408) (xy 153.67 89.408) (xy 154.432 90.17) (xy 154.432 94.615) (xy 153.035 95.885)
        (xy 96.52 96.011158) (xy 95.504 95.25) (xy 95.504 90.17)
      )
    )
  )
)
