(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 837)
    (no_connects 0)
    (area 7.070879 14.075 132.221001 86.31072)
    (thickness 1.6002)
    (drawings 17)
    (tracks 4131)
    (zones 0)
    (modules 230)
    (nets 237)
  )
  (page A3)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (user_trace_width 0.7)
    (trace_clearance 0.1524)
    (zone_clearance 0.16)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 2.1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFCE1F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 /fpga1/ASDO)
  (net 2 /fpga1/DATA0)
  (net 3 /fpga1/DCLK)
  (net 4 /fpga1/HDMITX_HSYNC)
  (net 5 /fpga1/HDMITX_INT_N)
  (net 6 /fpga1/HDMITX_PCLK)
  (net 7 /fpga1/HDMITX_R0)
  (net 8 /fpga1/HDMITX_R1)
  (net 9 /fpga1/HDMITX_R2)
  (net 10 /fpga1/HDMITX_R3)
  (net 11 /fpga1/HDMITX_R4)
  (net 12 /fpga1/HDMITX_R5)
  (net 13 /fpga1/HDMITX_R6)
  (net 14 /fpga1/HDMITX_R7)
  (net 15 /fpga1/HDMITX_VSYNC)
  (net 16 /fpga1/IR_RX)
  (net 17 /fpga1/LED0)
  (net 18 /fpga1/LED1)
  (net 19 /fpga1/SCL)
  (net 20 /fpga1/SDA)
  (net 21 /fpga1/SD_CLK)
  (net 22 /fpga1/SD_CMD)
  (net 23 /fpga1/SD_DAT0)
  (net 24 /fpga1/SD_DAT1)
  (net 25 /fpga1/SD_DAT2)
  (net 26 /fpga1/SD_DAT3)
  (net 27 /fpga1/TCK)
  (net 28 /fpga1/TDI)
  (net 29 /fpga1/TDO)
  (net 30 /fpga1/TMS)
  (net 31 /fpga1/VCCA)
  (net 32 /fpga1/VCCD_PLL)
  (net 33 /fpga1/VCCINT)
  (net 34 /fpga1/nCSO)
  (net 35 /hdmitx1/AVCC1V8)
  (net 36 /hdmitx1/AVDD3V3)
  (net 37 /hdmitx1/B0)
  (net 38 /hdmitx1/B1)
  (net 39 /hdmitx1/B2)
  (net 40 /hdmitx1/B3)
  (net 41 /hdmitx1/B4)
  (net 42 /hdmitx1/B5)
  (net 43 /hdmitx1/B6)
  (net 44 /hdmitx1/B7)
  (net 45 /hdmitx1/DDC_SCL)
  (net 46 /hdmitx1/DDC_SDA)
  (net 47 /hdmitx1/DE)
  (net 48 /hdmitx1/DVDD1V8)
  (net 49 /hdmitx1/DVDD3V3)
  (net 50 /hdmitx1/G0)
  (net 51 /hdmitx1/G1)
  (net 52 /hdmitx1/G2)
  (net 53 /hdmitx1/G3)
  (net 54 /hdmitx1/G4)
  (net 55 /hdmitx1/G5)
  (net 56 /hdmitx1/G6)
  (net 57 /hdmitx1/G7)
  (net 58 /hdmitx1/HPD)
  (net 59 /hdmitx1/TMDS_CLK+)
  (net 60 /hdmitx1/TMDS_CLK-)
  (net 61 /hdmitx1/TMDS_D0+)
  (net 62 /hdmitx1/TMDS_D0-)
  (net 63 /hdmitx1/TMDS_D1+)
  (net 64 /hdmitx1/TMDS_D1-)
  (net 65 /hdmitx1/TMDS_D2+)
  (net 66 /hdmitx1/TMDS_D2-)
  (net 67 /tvp_board1/AVDD)
  (net 68 /tvp_board1/B0)
  (net 69 /tvp_board1/B1)
  (net 70 /tvp_board1/B2)
  (net 71 /tvp_board1/B3)
  (net 72 /tvp_board1/B4)
  (net 73 /tvp_board1/B5)
  (net 74 /tvp_board1/B6)
  (net 75 /tvp_board1/B7)
  (net 76 /tvp_board1/DVDD)
  (net 77 /tvp_board1/FID)
  (net 78 /tvp_board1/G0)
  (net 79 /tvp_board1/G1)
  (net 80 /tvp_board1/G2)
  (net 81 /tvp_board1/G3)
  (net 82 /tvp_board1/G4)
  (net 83 /tvp_board1/G5)
  (net 84 /tvp_board1/G6)
  (net 85 /tvp_board1/G7)
  (net 86 /tvp_board1/HSYNC)
  (net 87 /tvp_board1/PCLK)
  (net 88 /tvp_board1/R0)
  (net 89 /tvp_board1/R1)
  (net 90 /tvp_board1/R2)
  (net 91 /tvp_board1/R3)
  (net 92 /tvp_board1/R4)
  (net 93 /tvp_board1/R5)
  (net 94 /tvp_board1/R6)
  (net 95 /tvp_board1/R7)
  (net 96 /tvp_board1/RGB1_B)
  (net 97 /tvp_board1/RGB1_G)
  (net 98 /tvp_board1/RGB1_R)
  (net 99 /tvp_board1/RGB1_S)
  (net 100 /tvp_board1/RGB2_B)
  (net 101 /tvp_board1/RGB2_G)
  (net 102 /tvp_board1/RGB2_R)
  (net 103 /tvp_board1/RGB3_B)
  (net 104 /tvp_board1/RGB3_G)
  (net 105 /tvp_board1/RGB3_R)
  (net 106 /tvp_board1/VSYNC)
  (net 107 GND)
  (net 108 "Net-(C1-Pad2)")
  (net 109 "Net-(C2-Pad2)")
  (net 110 "Net-(C3-Pad2)")
  (net 111 "Net-(C4-Pad2)")
  (net 112 "Net-(C5-Pad2)")
  (net 113 "Net-(C6-Pad2)")
  (net 114 "Net-(C7-Pad2)")
  (net 115 "Net-(C11-Pad2)")
  (net 116 "Net-(C12-Pad2)")
  (net 117 "Net-(C13-Pad2)")
  (net 118 "Net-(C15-Pad2)")
  (net 119 "Net-(C16-Pad2)")
  (net 120 "Net-(C17-Pad2)")
  (net 121 "Net-(C19-Pad1)")
  (net 122 "Net-(C19-Pad2)")
  (net 123 "Net-(C20-Pad2)")
  (net 124 "Net-(C24-Pad1)")
  (net 125 "Net-(C25-Pad1)")
  (net 126 "Net-(C29-Pad2)")
  (net 127 "Net-(C30-Pad1)")
  (net 128 "Net-(C30-Pad2)")
  (net 129 "Net-(C74-Pad1)")
  (net 130 "Net-(C77-Pad1)")
  (net 131 "Net-(C80-Pad1)")
  (net 132 "Net-(J1-Pad9)")
  (net 133 "Net-(J1-Pad4)")
  (net 134 "Net-(J1-Pad11)")
  (net 135 "Net-(J1-Pad12)")
  (net 136 "Net-(J1-Pad15)")
  (net 137 "Net-(P1-Pad6)")
  (net 138 "Net-(P1-Pad8)")
  (net 139 "Net-(R11-Pad2)")
  (net 140 "Net-(R16-Pad2)")
  (net 141 "Net-(R24-Pad1)")
  (net 142 "Net-(R25-Pad1)")
  (net 143 "Net-(R26-Pad1)")
  (net 144 "Net-(U1-Pad25)")
  (net 145 "Net-(U1-Pad37)")
  (net 146 "Net-(U1-Pad38)")
  (net 147 "Net-(U1-Pad51)")
  (net 148 "Net-(U1-Pad52)")
  (net 149 "Net-(U1-Pad64)")
  (net 150 "Net-(U1-Pad65)")
  (net 151 "Net-(D1-Pad1)")
  (net 152 "Net-(D2-Pad1)")
  (net 153 "Net-(J3-Pad3)")
  (net 154 "Net-(J3-Pad8)")
  (net 155 "Net-(J3-Pad10)")
  (net 156 "Net-(J3-Pad12)")
  (net 157 "Net-(J3-Pad16)")
  (net 158 "Net-(J3-Pad19)")
  (net 159 "Net-(J3-Pad1)")
  (net 160 "Net-(J4-Pad13)")
  (net 161 "Net-(P1-Pad7)")
  (net 162 "Net-(U3-Pad45)")
  (net 163 "Net-(Y1-Pad1)")
  (net 164 /fpga1/CLK27)
  (net 165 "Net-(R17-Pad1)")
  (net 166 "Net-(R18-Pad2)")
  (net 167 "Net-(R19-Pad1)")
  (net 168 "Net-(R23-Pad2)")
  (net 169 "Net-(DS1-Pad11)")
  (net 170 "Net-(U17-Pad1)")
  (net 171 "Net-(U17-Pad20)")
  (net 172 "Net-(F1-Pad1)")
  (net 173 /tvp_board1/RGB_12_G)
  (net 174 /tvp_board1/RGB_12_R)
  (net 175 "Net-(C76-Pad2)")
  (net 176 /tvp_board1/RGB_12_B)
  (net 177 "Net-(C100-Pad2)")
  (net 178 "Net-(C103-Pad2)")
  (net 179 "Net-(C104-Pad2)")
  (net 180 "Net-(C105-Pad2)")
  (net 181 /tvp_board1/RGB3_HS)
  (net 182 /tvp_board1/RGB3_VS)
  (net 183 /tvp_board1/RGB3_VS_B)
  (net 184 /tvp_board1/RGB3_HS_B)
  (net 185 "Net-(C106-Pad1)")
  (net 186 "Net-(C107-Pad1)")
  (net 187 /fpga1/LCD_CS_N)
  (net 188 /fpga1/LCD_RS)
  (net 189 /fpga1/BTN0)
  (net 190 /fpga1/BTN1)
  (net 191 "Net-(C23-Pad1)")
  (net 192 /tvp_board1/AVDD_F)
  (net 193 "Net-(C102-Pad1)")
  (net 194 "Net-(C33-Pad2)")
  (net 195 "Net-(C36-Pad1)")
  (net 196 /fpga1/RESET_N)
  (net 197 "Net-(Q1-Pad1)")
  (net 198 "Net-(Q1-Pad3)")
  (net 199 "Net-(Q2-Pad1)")
  (net 200 "Net-(Q2-Pad3)")
  (net 201 /fpga1/LCD_BLEN)
  (net 202 /hdmitx1/5V)
  (net 203 "Net-(MH1-Pad1)")
  (net 204 "Net-(MH2-Pad1)")
  (net 205 "Net-(MH3-Pad1)")
  (net 206 "Net-(MH4-Pad1)")
  (net 207 /hdmitx1/5V_FUSED)
  (net 208 "Net-(C111-Pad1)")
  (net 209 "Net-(C112-Pad1)")
  (net 210 /hdmitx1/AV2_AUD_R)
  (net 211 "Net-(C116-Pad2)")
  (net 212 /hdmitx1/AV1_AUD_R)
  (net 213 "Net-(C119-Pad1)")
  (net 214 "Net-(C120-Pad1)")
  (net 215 /hdmitx1/AV2_AUD_L)
  (net 216 "Net-(C121-Pad2)")
  (net 217 /hdmitx1/AV1_AUD_L)
  (net 218 "Net-(C123-Pad1)")
  (net 219 /hdmitx1/AV3_AUD_R)
  (net 220 "Net-(C124-Pad1)")
  (net 221 "Net-(C125-Pad1)")
  (net 222 /hdmitx1/AV3_AUD_L)
  (net 223 "Net-(C126-Pad1)")
  (net 224 "Net-(J4-Pad14)")
  (net 225 "Net-(J6-Pad3)")
  (net 226 "Net-(J6-Pad2)")
  (net 227 /hdmitx1/I2S_DATA)
  (net 228 /hdmitx1/I2S_WS)
  (net 229 /hdmitx1/I2S_BCK)
  (net 230 "Net-(U8-Pad5)")
  (net 231 "Net-(U8-Pad19)")
  (net 232 "Net-(U8-Pad20)")
  (net 233 "Net-(U8-Pad21)")
  (net 234 "Net-(U8-Pad22)")
  (net 235 "Net-(U8-Pad3)")
  (net 236 "Net-(U8-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /fpga1/BTN0)
    (add_net /fpga1/BTN1)
    (add_net /fpga1/CLK27)
    (add_net /fpga1/LCD_BLEN)
    (add_net /fpga1/LCD_CS_N)
    (add_net /fpga1/LCD_RS)
    (add_net /fpga1/LED0)
    (add_net /fpga1/LED1)
    (add_net /fpga1/RESET_N)
    (add_net /fpga1/SD_CLK)
    (add_net /fpga1/SD_CMD)
    (add_net /fpga1/SD_DAT0)
    (add_net /fpga1/SD_DAT1)
    (add_net /fpga1/SD_DAT2)
    (add_net /fpga1/SD_DAT3)
    (add_net /fpga1/TCK)
    (add_net /fpga1/TDI)
    (add_net /fpga1/TDO)
    (add_net /fpga1/TMS)
    (add_net /hdmitx1/5V)
    (add_net /hdmitx1/5V_FUSED)
    (add_net /hdmitx1/AV1_AUD_L)
    (add_net /hdmitx1/AV1_AUD_R)
    (add_net /hdmitx1/AV2_AUD_L)
    (add_net /hdmitx1/AV2_AUD_R)
    (add_net /hdmitx1/AV3_AUD_L)
    (add_net /hdmitx1/AV3_AUD_R)
    (add_net /hdmitx1/DDC_SCL)
    (add_net /hdmitx1/DDC_SDA)
    (add_net /hdmitx1/HPD)
    (add_net /hdmitx1/I2S_BCK)
    (add_net /hdmitx1/I2S_DATA)
    (add_net /hdmitx1/I2S_WS)
    (add_net /tvp_board1/AVDD_F)
    (add_net /tvp_board1/RGB3_HS)
    (add_net /tvp_board1/RGB3_HS_B)
    (add_net /tvp_board1/RGB3_VS)
    (add_net /tvp_board1/RGB3_VS_B)
    (add_net /tvp_board1/RGB_12_B)
    (add_net /tvp_board1/RGB_12_G)
    (add_net /tvp_board1/RGB_12_R)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C100-Pad2)")
    (add_net "Net-(C102-Pad1)")
    (add_net "Net-(C103-Pad2)")
    (add_net "Net-(C104-Pad2)")
    (add_net "Net-(C105-Pad2)")
    (add_net "Net-(C106-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C111-Pad1)")
    (add_net "Net-(C112-Pad1)")
    (add_net "Net-(C116-Pad2)")
    (add_net "Net-(C119-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C120-Pad1)")
    (add_net "Net-(C121-Pad2)")
    (add_net "Net-(C123-Pad1)")
    (add_net "Net-(C124-Pad1)")
    (add_net "Net-(C125-Pad1)")
    (add_net "Net-(C126-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C29-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C30-Pad2)")
    (add_net "Net-(C33-Pad2)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C74-Pad1)")
    (add_net "Net-(C76-Pad2)")
    (add_net "Net-(C77-Pad1)")
    (add_net "Net-(C80-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(DS1-Pad11)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad16)")
    (add_net "Net-(J3-Pad19)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J4-Pad13)")
    (add_net "Net-(J4-Pad14)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(MH1-Pad1)")
    (add_net "Net-(MH2-Pad1)")
    (add_net "Net-(MH3-Pad1)")
    (add_net "Net-(MH4-Pad1)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R24-Pad1)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R26-Pad1)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad51)")
    (add_net "Net-(U1-Pad52)")
    (add_net "Net-(U1-Pad64)")
    (add_net "Net-(U1-Pad65)")
    (add_net "Net-(U17-Pad1)")
    (add_net "Net-(U17-Pad20)")
    (add_net "Net-(U3-Pad45)")
    (add_net "Net-(U8-Pad19)")
    (add_net "Net-(U8-Pad20)")
    (add_net "Net-(U8-Pad21)")
    (add_net "Net-(U8-Pad22)")
    (add_net "Net-(U8-Pad3)")
    (add_net "Net-(U8-Pad4)")
    (add_net "Net-(U8-Pad5)")
    (add_net "Net-(Y1-Pad1)")
  )
  (net_class 75ohm_vid ""
    (clearance 0.24)
    (trace_width 0.64)
    (via_dia 0.686)
    (via_drill 0.35)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /tvp_board1/RGB1_B)
    (add_net /tvp_board1/RGB1_G)
    (add_net /tvp_board1/RGB1_R)
    (add_net /tvp_board1/RGB1_S)
    (add_net /tvp_board1/RGB2_B)
    (add_net /tvp_board1/RGB2_G)
    (add_net /tvp_board1/RGB2_R)
    (add_net /tvp_board1/RGB3_B)
    (add_net /tvp_board1/RGB3_G)
    (add_net /tvp_board1/RGB3_R)
  )
  (net_class FAT_power ""
    (clearance 0.16)
    (trace_width 1)
    (via_dia 1.5)
    (via_drill 1.1)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /hdmitx1/DVDD3V3)
    (add_net "Net-(C107-Pad1)")
    (add_net "Net-(F1-Pad1)")
  )
  (net_class Power ""
    (clearance 0.16)
    (trace_width 0.25)
    (via_dia 0.686)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /fpga1/VCCA)
    (add_net /fpga1/VCCD_PLL)
    (add_net /fpga1/VCCINT)
    (add_net /hdmitx1/AVCC1V8)
    (add_net /hdmitx1/AVDD3V3)
    (add_net /hdmitx1/DVDD1V8)
    (add_net /tvp_board1/AVDD)
    (add_net /tvp_board1/DVDD)
    (add_net GND)
  )
  (net_class digi_hs ""
    (clearance 0.16)
    (trace_width 0.18)
    (via_dia 0.686)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /fpga1/ASDO)
    (add_net /fpga1/DATA0)
    (add_net /fpga1/DCLK)
    (add_net /fpga1/HDMITX_HSYNC)
    (add_net /fpga1/HDMITX_INT_N)
    (add_net /fpga1/HDMITX_PCLK)
    (add_net /fpga1/HDMITX_R0)
    (add_net /fpga1/HDMITX_R1)
    (add_net /fpga1/HDMITX_R2)
    (add_net /fpga1/HDMITX_R3)
    (add_net /fpga1/HDMITX_R4)
    (add_net /fpga1/HDMITX_R5)
    (add_net /fpga1/HDMITX_R6)
    (add_net /fpga1/HDMITX_R7)
    (add_net /fpga1/HDMITX_VSYNC)
    (add_net /fpga1/IR_RX)
    (add_net /fpga1/SCL)
    (add_net /fpga1/SDA)
    (add_net /fpga1/nCSO)
    (add_net /hdmitx1/B0)
    (add_net /hdmitx1/B1)
    (add_net /hdmitx1/B2)
    (add_net /hdmitx1/B3)
    (add_net /hdmitx1/B4)
    (add_net /hdmitx1/B5)
    (add_net /hdmitx1/B6)
    (add_net /hdmitx1/B7)
    (add_net /hdmitx1/DE)
    (add_net /hdmitx1/G0)
    (add_net /hdmitx1/G1)
    (add_net /hdmitx1/G2)
    (add_net /hdmitx1/G3)
    (add_net /hdmitx1/G4)
    (add_net /hdmitx1/G5)
    (add_net /hdmitx1/G6)
    (add_net /hdmitx1/G7)
    (add_net /hdmitx1/TMDS_CLK+)
    (add_net /hdmitx1/TMDS_CLK-)
    (add_net /hdmitx1/TMDS_D0+)
    (add_net /hdmitx1/TMDS_D0-)
    (add_net /hdmitx1/TMDS_D1+)
    (add_net /hdmitx1/TMDS_D1-)
    (add_net /hdmitx1/TMDS_D2+)
    (add_net /hdmitx1/TMDS_D2-)
    (add_net /tvp_board1/B0)
    (add_net /tvp_board1/B1)
    (add_net /tvp_board1/B2)
    (add_net /tvp_board1/B3)
    (add_net /tvp_board1/B4)
    (add_net /tvp_board1/B5)
    (add_net /tvp_board1/B6)
    (add_net /tvp_board1/B7)
    (add_net /tvp_board1/FID)
    (add_net /tvp_board1/G0)
    (add_net /tvp_board1/G1)
    (add_net /tvp_board1/G2)
    (add_net /tvp_board1/G3)
    (add_net /tvp_board1/G4)
    (add_net /tvp_board1/G5)
    (add_net /tvp_board1/G6)
    (add_net /tvp_board1/G7)
    (add_net /tvp_board1/HSYNC)
    (add_net /tvp_board1/PCLK)
    (add_net /tvp_board1/R0)
    (add_net /tvp_board1/R1)
    (add_net /tvp_board1/R2)
    (add_net /tvp_board1/R3)
    (add_net /tvp_board1/R4)
    (add_net /tvp_board1/R5)
    (add_net /tvp_board1/R6)
    (add_net /tvp_board1/R7)
    (add_net /tvp_board1/VSYNC)
  )
  (module custom_components:TSSOP-30_4.4x7.8mm_Pitch0.5mm_Handsoldering (layer F.Cu) (tedit 58D2D345)
    (at 110.622 69.23 270)
    (descr "TSSOP30: plastic thin shrink small outline package; 24 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot355-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U8 (at 0 -4.95 270) (layer F.SilkS))
    (fp_text value PCM1862 (at 0 4.95 270) (layer F.Fab))
    (pad 16 smd rect (at 3 3.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 228 /hdmitx1/I2S_WS))
    (pad 17 smd rect (at 3 3 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 229 /hdmitx1/I2S_BCK))
    (pad 18 smd rect (at 3 2.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 227 /hdmitx1/I2S_DATA))
    (pad 19 smd rect (at 3 2 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(U8-Pad19)"))
    (pad 20 smd rect (at 3 1.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(U8-Pad20)"))
    (pad 21 smd rect (at 3 1 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(U8-Pad21)"))
    (pad 22 smd rect (at 3 0.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(U8-Pad22)"))
    (pad 23 smd rect (at 3 0 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /fpga1/SDA))
    (pad 24 smd rect (at 3 -0.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /fpga1/SCL))
    (pad 25 smd rect (at 3 -1 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 26 smd rect (at 3 -1.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 27 smd rect (at 3 -2 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(C126-Pad1)"))
    (pad 28 smd rect (at 3 -2.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(C124-Pad1)"))
    (pad 29 smd rect (at 3 -3 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(C125-Pad1)"))
    (pad 30 smd rect (at 3 -3.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(C123-Pad1)"))
    (pad 1 smd rect (at -3 -3.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(C121-Pad2)"))
    (pad 2 smd rect (at -3 -3 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(C116-Pad2)"))
    (pad 3 smd rect (at -3 -2.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(U8-Pad3)"))
    (pad 4 smd rect (at -3 -2 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(U8-Pad4)"))
    (pad 5 smd rect (at -3 -1.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(U8-Pad5)"))
    (pad 6 smd rect (at -3 -1 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(C119-Pad1)"))
    (pad 7 smd rect (at -3 -0.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 8 smd rect (at -3 0 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 9 smd rect (at -3 0.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(C111-Pad1)"))
    (pad 10 smd rect (at -3 1 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(C112-Pad1)"))
    (pad 11 smd rect (at -3 1.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(C120-Pad1)"))
    (pad 12 smd rect (at -3 2 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 13 smd rect (at -3 2.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 14 smd rect (at -3 3 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 15 smd rect (at -3 3.5 270) (size 1.2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model Housings_SSOP.3dshapes/TSSOP-24_4.4x7.8mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:IRM-V5XX_TR1 (layer F.Cu) (tedit 569513E8)
    (at 73.2641 21.3605)
    (fp_text reference U11 (at 3.7465 -1.19634 90) (layer F.SilkS))
    (fp_text value IRM-V538/TR1 (at 0.25146 3.09626) (layer F.Fab))
    (pad 1 smd rect (at 1.7 0.5) (size 0.7 1.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /fpga1/IR_RX))
    (pad 2 smd rect (at 0 0.5) (size 0.7 1.9) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(C102-Pad1)"))
    (pad 3 smd rect (at -1.7 0.5) (size 0.7 1.9) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 3 smd rect (at 1.68 -2.85) (size 1.4 1.9) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
  )
  (module Connect:VASCH5x2 (layer F.Cu) (tedit 569EC875)
    (at 88.4 21.59 180)
    (descr CONNECTOR)
    (tags CONNECTOR)
    (attr virtual)
    (fp_text reference P1 (at 10.996 -4.661 270) (layer F.SilkS))
    (fp_text value JTAG_CONN (at 1.27 6.35 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 1.27 180) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 27 /fpga1/TCK))
    (pad 2 thru_hole circle (at -5.08 -1.27 180) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 107 GND))
    (pad 3 thru_hole circle (at -2.54 1.27 180) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 29 /fpga1/TDO))
    (pad 4 thru_hole circle (at -2.54 -1.27 180) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 31 /fpga1/VCCA))
    (pad 5 thru_hole circle (at 0 1.27 180) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 30 /fpga1/TMS))
    (pad 6 thru_hole circle (at 0 -1.27 180) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 137 "Net-(P1-Pad6)"))
    (pad 7 thru_hole circle (at 2.54 1.27 180) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 161 "Net-(P1-Pad7)"))
    (pad 8 thru_hole circle (at 2.54 -1.27 180) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 138 "Net-(P1-Pad8)"))
    (pad 9 thru_hole circle (at 5.08 1.27 180) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 28 /fpga1/TDI))
    (pad 10 thru_hole circle (at 5.08 -1.27 180) (size 1.50622 1.50622) (drill 0.99822) (layers *.Cu *.Mask)
      (net 107 GND))
  )
  (module Connect:1pin (layer F.Cu) (tedit 55A2224D)
    (at 11.13 20.6)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference MH1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 203 "Net-(MH1-Pad1)"))
  )
  (module Connect:1pin (layer F.Cu) (tedit 55A22249)
    (at 11.13 82.2)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference MH3 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 205 "Net-(MH3-Pad1)"))
  )
  (module Connect:1pin (layer F.Cu) (tedit 55A22245)
    (at 128.3 82.2)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference MH4 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 206 "Net-(MH4-Pad1)"))
  )
  (module Connect:1pin (layer F.Cu) (tedit 55A22240)
    (at 128.3 20.6)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference MH2 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 204 "Net-(MH2-Pad1)"))
  )
  (module custom_components:ACHL-OSC (layer F.Cu) (tedit 55F30EBC)
    (at 29.9945 39.6993 270)
    (tags "SMA Connector")
    (fp_text reference Y1 (at -4.191 -7.2898 270) (layer F.SilkS))
    (fp_text value ACHL-27MHZ-EK (at 0.254 0 270) (layer F.Fab))
    (pad 5 thru_hole circle (at 3.81 -3.81 270) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 164 /fpga1/CLK27))
    (pad 8 thru_hole circle (at -3.81 -3.81 270) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(C25-Pad1)"))
    (pad 1 thru_hole circle (at -3.81 3.81 270) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 163 "Net-(Y1-Pad1)"))
    (pad 4 thru_hole circle (at 3.81 3.81 270) (size 1.5 1.5) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (model connectors/sma.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 -90))
    )
  )
  (module custom_components:SOT-23-5_Handsoldering (layer B.Cu) (tedit 564B97ED)
    (at 28.702 47.3701 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (zone_connect 2)
    (attr smd)
    (fp_text reference U7 (at 2.4631 -0.112 180) (layer B.SilkS))
    (fp_text value NCP703SN19T1G (at 2.35 -0.05 360) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 107 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.95 -1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 4 smd rect (at 0.95 1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (zone_connect 2))
    (pad 5 smd rect (at -0.95 1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 67 /tvp_board1/AVDD) (zone_connect 2))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom_components:SOT-23-5_Handsoldering (layer B.Cu) (tedit 564B9E4D)
    (at 39.986 38.862 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (zone_connect 2)
    (attr smd)
    (fp_text reference U9 (at 2.263 -0.05 180) (layer B.SilkS))
    (fp_text value TLV70019 (at 2.35 -0.05 360) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 107 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.95 -1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 4 smd rect (at 0.95 1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (zone_connect 2))
    (pad 5 smd rect (at -0.95 1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 76 /tvp_board1/DVDD) (zone_connect 2))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom_components:SOT-23-5_Handsoldering (layer B.Cu) (tedit 55A22268)
    (at 102.7938 58.9534 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (zone_connect 2)
    (attr smd)
    (fp_text reference U15 (at -2.55 -0.05 270) (layer B.SilkS))
    (fp_text value TLV70018 (at 2.35 -0.05 450) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 107 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.95 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 4 smd rect (at 0.95 1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (zone_connect 2))
    (pad 5 smd rect (at -0.95 1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 48 /hdmitx1/DVDD1V8) (zone_connect 2))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom_components:SOT-23-5_Handsoldering (layer B.Cu) (tedit 56868374)
    (at 112.39 58.9534 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (zone_connect 2)
    (attr smd)
    (fp_text reference U16 (at -2.55 -0.05 270) (layer B.SilkS))
    (fp_text value TLV70018 (at -1.834 -2.0366 450) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 107 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.95 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 4 smd rect (at 0.95 1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (zone_connect 2))
    (pad 5 smd rect (at -0.95 1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 35 /hdmitx1/AVCC1V8) (zone_connect 2))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom_components:SOT-23-5_Handsoldering (layer B.Cu) (tedit 55A220DF)
    (at 28.702 52.324 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (zone_connect 2)
    (attr smd)
    (fp_text reference U6 (at -2.55 -0.05 180) (layer B.SilkS))
    (fp_text value TLV70033 (at 2.35 -0.05 360) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 202 /hdmitx1/5V) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 107 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.95 -1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 202 /hdmitx1/5V) (zone_connect 2))
    (pad 4 smd rect (at 0.95 1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (zone_connect 2))
    (pad 5 smd rect (at -0.95 1.65) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 36 /hdmitx1/AVDD3V3) (zone_connect 2))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom_components:SOT-23-5_Handsoldering (layer B.Cu) (tedit 55FC64D0)
    (at 73.7 59.0246 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (zone_connect 2)
    (attr smd)
    (fp_text reference U12 (at 2.514 0.035 270) (layer B.SilkS))
    (fp_text value TLV70012 (at 2.35 -0.05 450) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 107 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.95 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 4 smd rect (at 0.95 1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (zone_connect 2))
    (pad 5 smd rect (at -0.95 1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT) (zone_connect 2))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom_components:SOT-23-5_Handsoldering (layer B.Cu) (tedit 5694EAD7)
    (at 78.306 59.0026 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (zone_connect 2)
    (attr smd)
    (fp_text reference U13 (at -2.55 -0.7004 270) (layer B.SilkS))
    (fp_text value TLV70025 (at 2.35 -0.05 450) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 107 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.95 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 4 smd rect (at 0.95 1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (zone_connect 2))
    (pad 5 smd rect (at -0.95 1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 31 /fpga1/VCCA) (zone_connect 2))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom_components:SOT-23-5_Handsoldering (layer B.Cu) (tedit 55A221E9)
    (at 92.034 58.278 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (zone_connect 2)
    (attr smd)
    (fp_text reference U14 (at -2.55 -0.05 270) (layer B.SilkS))
    (fp_text value TLV70012 (at 2.35 -0.05 450) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 2 smd rect (at 0 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 107 GND) (zone_connect 2))
    (pad 3 smd rect (at 0.95 -1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 4 smd rect (at 0.95 1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (zone_connect 2))
    (pad 5 smd rect (at -0.95 1.65 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 32 /fpga1/VCCD_PLL) (zone_connect 2))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom_components:DM3D-SF (layer B.Cu) (tedit 55DF705E)
    (at 67.988 19.305)
    (fp_text reference P3 (at 11.9253 3.81 270) (layer B.SilkS))
    (fp_text value mSD_CONN (at 3.53314 4.37896 270) (layer B.Fab))
    (pad 6 smd rect (at 10.1 10.1) (size 1.5 1.9) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 6 smd rect (at -1.4 8.35) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 1 smd rect (at 7.7 -0.875) (size 0.4 1.75) (layers B.Cu B.Paste B.Mask)
      (net 25 /fpga1/SD_DAT2))
    (pad 2 smd rect (at 6.6 -0.875) (size 0.4 1.75) (layers B.Cu B.Paste B.Mask)
      (net 26 /fpga1/SD_DAT3))
    (pad 3 smd rect (at 5.5 -0.875) (size 0.4 1.75) (layers B.Cu B.Paste B.Mask)
      (net 22 /fpga1/SD_CMD))
    (pad 4 smd rect (at 4.4 -0.875) (size 0.4 1.75) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 5 smd rect (at 3.3 -0.875) (size 0.4 1.75) (layers B.Cu B.Paste B.Mask)
      (net 21 /fpga1/SD_CLK))
    (pad 6 smd rect (at 2.2 -0.875) (size 0.4 1.75) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 7 smd rect (at 1.1 -0.875) (size 0.4 1.75) (layers B.Cu B.Paste B.Mask)
      (net 23 /fpga1/SD_DAT0))
    (pad 8 smd rect (at 0 -0.875) (size 0.4 1.75) (layers B.Cu B.Paste B.Mask)
      (net 24 /fpga1/SD_DAT1))
  )
  (module custom_components:SOT-23-6_Handsoldering (layer F.Cu) (tedit 55FC6069)
    (at 27.4933 49.2878 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at -0.1848 3.3683 450) (layer F.SilkS))
    (fp_text value SN74LVC2G17 (at -1.9978 -0.2437 360) (layer F.Fab))
    (pad 5 smd rect (at 0 -1.65) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 1 smd rect (at -0.95 1.65) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 181 /tvp_board1/RGB3_HS))
    (pad 2 smd rect (at 0 1.65) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 3 smd rect (at 0.95 1.65) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(C24-Pad1)"))
    (pad 4 smd rect (at 0.95 -1.65) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 183 /tvp_board1/RGB3_VS_B))
    (pad 6 smd rect (at -0.95 -1.65) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 184 /tvp_board1/RGB3_HS_B))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom_components:SOD-323_Handsoldering (layer B.Cu) (tedit 55F1B709)
    (at 18.654 21.915 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D5 (at -2.8702 -0.0254 360) (layer B.SilkS))
    (fp_text value SD05-7 (at 0.1 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -1.4 0 90) (size 1.4 0.45) (layers B.Cu B.Paste B.Mask)
      (net 186 "Net-(C107-Pad1)"))
    (pad 2 smd rect (at 1.4 0 90) (size 1.4 0.45) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
  )
  (module custom_components:VGA_CONN (layer F.Cu) (tedit 55FD22CE)
    (at 17.1555 59.2954 270)
    (fp_text reference J1 (at 15.70228 -0.00508 360) (layer F.SilkS))
    (fp_text value VGA (at 0.0381 5.57784 270) (layer F.Fab))
    (pad 8 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 9 thru_hole circle (at -2.29 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -4.58 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 1 thru_hole circle (at 3.44 -2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 105 /tvp_board1/RGB3_R))
    (pad 2 thru_hole circle (at 1.15 -2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 104 /tvp_board1/RGB3_G))
    (pad 3 thru_hole circle (at -1.14 -2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 103 /tvp_board1/RGB3_B))
    (pad 4 thru_hole circle (at -3.43 -2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 133 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -5.72 -2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 6 thru_hole circle (at 4.58 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 7 thru_hole circle (at 2.29 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 11 thru_hole circle (at 3.44 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at 1.15 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 135 "Net-(J1-Pad12)"))
    (pad 13 thru_hole circle (at -1.14 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 181 /tvp_board1/RGB3_HS))
    (pad 14 thru_hole circle (at -3.43 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 182 /tvp_board1/RGB3_VS))
    (pad 15 thru_hole circle (at -5.72 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 136 "Net-(J1-Pad15)"))
    (pad 10 thru_hole circle (at 11.62 0 270) (size 4.5 4.5) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 10 thru_hole circle (at -13.38 0 270) (size 4.5 4.5) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
  )
  (module custom_components:SOT-223_Handsoldering (layer F.Cu) (tedit 5648C28B)
    (at 31.577 27.656)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (zone_connect 2)
    (attr smd)
    (fp_text reference U5 (at 2.987 -2.876) (layer F.SilkS))
    (fp_text value AP7361C (at -0.00254 0.28956) (layer F.Fab))
    (pad 2 smd rect (at 0 3.6) (size 1.2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 107 GND) (zone_connect 2))
    (pad 1 smd rect (at -2.3 3.6) (size 1.2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 202 /hdmitx1/5V) (zone_connect 2))
    (pad 3 smd rect (at 2.3 3.6) (size 1.2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3) (zone_connect 2))
    (pad 2 smd rect (at 0 -3.6) (size 3.3 2.4) (layers F.Cu F.Paste F.Mask)
      (net 107 GND) (zone_connect 2))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer B.Cu) (tedit 564B9753)
    (at 58.316 25.317 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 2.862 0.404 270) (layer B.SilkS))
    (fp_text value BC847 (at 0 -3.81 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.50114 270) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 197 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 -1.50114 270) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 3 smd rect (at 0 1.50114 270) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 198 "Net-(Q1-Pad3)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer F.Cu) (tedit 564B7521)
    (at 54.193 25.329 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 1.676 -2.012 360) (layer F.SilkS))
    (fp_text value BC857 (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 3 smd rect (at 0 -1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(Q2-Pad3)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:TSSOP-20_4.4x6.5mm_Pitch0.65mm_Handsoldering (layer F.Cu) (tedit 5687A730)
    (at 46.888 67.324 90)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U17 (at -3.451 -4.384 90) (layer F.SilkS))
    (fp_text value THS7353 (at 0 4.3 90) (layer F.Fab))
    (pad 1 smd rect (at -3.22 -2.925 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(U17-Pad1)"))
    (pad 2 smd rect (at -3.22 -2.275 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(C12-Pad2)"))
    (pad 3 smd rect (at -3.22 -1.625 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C3-Pad2)"))
    (pad 4 smd rect (at -3.22 -0.975 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(C4-Pad2)"))
    (pad 5 smd rect (at -3.22 -0.325 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(C5-Pad2)"))
    (pad 6 smd rect (at -3.22 0.325 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(C6-Pad2)"))
    (pad 7 smd rect (at -3.22 0.975 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(C7-Pad2)"))
    (pad 8 smd rect (at -3.22 1.625 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 9 smd rect (at -3.22 2.275 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 10 smd rect (at -3.22 2.925 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 11 smd rect (at 3.22 2.925 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 12 smd rect (at 3.22 2.275 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(C36-Pad1)"))
    (pad 13 smd rect (at 3.22 1.625 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(C33-Pad2)"))
    (pad 14 smd rect (at 3.22 0.975 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 176 /tvp_board1/RGB_12_B))
    (pad 15 smd rect (at 3.22 0.325 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 176 /tvp_board1/RGB_12_B))
    (pad 16 smd rect (at 3.22 -0.325 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 174 /tvp_board1/RGB_12_R))
    (pad 17 smd rect (at 3.22 -0.975 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 174 /tvp_board1/RGB_12_R))
    (pad 18 smd rect (at 3.22 -1.625 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 173 /tvp_board1/RGB_12_G))
    (pad 19 smd rect (at 3.22 -2.275 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 173 /tvp_board1/RGB_12_G))
    (pad 20 smd rect (at 3.22 -2.925 90) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(U17-Pad20)"))
    (model Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:TQFP-100_custom (layer F.Cu) (tedit 56867A2E)
    (at 107.3 47.9 90)
    (descr "100-Lead Plastic Thin Quad Flatpack (PF) - 14x14x1 mm Body 2.00 mm Footprint [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U3 (at 0 -9.45 90) (layer F.SilkS))
    (fp_text value IT6613 (at 0 9.45 90) (layer F.Fab))
    (pad 1 smd rect (at -7.8 -6 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 /hdmitx1/DE))
    (pad 2 smd rect (at -7.8 -5.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /fpga1/HDMITX_HSYNC))
    (pad 3 smd rect (at -7.8 -5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /fpga1/HDMITX_VSYNC))
    (pad 4 smd rect (at -7.8 -4.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 5 smd rect (at -7.8 -4 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 6 smd rect (at -7.8 -3.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 7 smd rect (at -7.8 -3 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 8 smd rect (at -7.8 -2.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 9 smd rect (at -7.8 -2 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 227 /hdmitx1/I2S_DATA))
    (pad 10 smd rect (at -7.8 -1.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 228 /hdmitx1/I2S_WS))
    (pad 11 smd rect (at -7.8 -1 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 229 /hdmitx1/I2S_BCK))
    (pad 12 smd rect (at -7.8 -0.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 13 smd rect (at -7.8 0 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 14 smd rect (at -7.8 0.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 15 smd rect (at -7.8 1 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 16 smd rect (at -7.8 1.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 17 smd rect (at -7.8 2 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 18 smd rect (at -7.8 2.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 19 smd rect (at -7.8 3 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 20 smd rect (at -7.8 3.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 21 smd rect (at -7.8 4 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 22 smd rect (at -7.8 4.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 23 smd rect (at -7.8 5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 24 smd rect (at -7.8 5.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /fpga1/HDMITX_INT_N))
    (pad 25 smd rect (at -7.8 6 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 196 /fpga1/RESET_N))
    (pad 26 smd rect (at -6 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 27 smd rect (at -5.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R25-Pad1)"))
    (pad 28 smd rect (at -5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(C74-Pad1)"))
    (pad 29 smd rect (at -4.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 30 smd rect (at -4 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 60 /hdmitx1/TMDS_CLK-))
    (pad 31 smd rect (at -3.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 /hdmitx1/TMDS_CLK+))
    (pad 32 smd rect (at -3 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(C77-Pad1)"))
    (pad 33 smd rect (at -2.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 62 /hdmitx1/TMDS_D0-))
    (pad 34 smd rect (at -2 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 /hdmitx1/TMDS_D0+))
    (pad 35 smd rect (at -1.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 36 smd rect (at -1 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 /hdmitx1/TMDS_D1-))
    (pad 37 smd rect (at -0.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 63 /hdmitx1/TMDS_D1+))
    (pad 38 smd rect (at 0 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(C77-Pad1)"))
    (pad 39 smd rect (at 0.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 /hdmitx1/TMDS_D2-))
    (pad 40 smd rect (at 1 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 65 /hdmitx1/TMDS_D2+))
    (pad 41 smd rect (at 1.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 42 smd rect (at 2 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(C80-Pad1)"))
    (pad 43 smd rect (at 2.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 44 smd rect (at 3 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 45 smd rect (at 3.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(U3-Pad45)"))
    (pad 46 smd rect (at 4 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /hdmitx1/DDC_SCL))
    (pad 47 smd rect (at 4.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 /hdmitx1/DDC_SDA))
    (pad 48 smd rect (at 5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /fpga1/SCL))
    (pad 49 smd rect (at 5.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /fpga1/SDA))
    (pad 50 smd rect (at 6 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 51 smd rect (at 7.8 6 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 /hdmitx1/HPD))
    (pad 52 smd rect (at 7.8 5.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(R26-Pad1)"))
    (pad 53 smd rect (at 7.8 5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 54 smd rect (at 7.8 4.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 55 smd rect (at 7.8 4 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 56 smd rect (at 7.8 3.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /fpga1/HDMITX_R7))
    (pad 57 smd rect (at 7.8 3 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /fpga1/HDMITX_R6))
    (pad 58 smd rect (at 7.8 2.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /fpga1/HDMITX_R5))
    (pad 59 smd rect (at 7.8 2 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /fpga1/HDMITX_R4))
    (pad 60 smd rect (at 7.8 1.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /fpga1/HDMITX_R3))
    (pad 61 smd rect (at 7.8 1 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /fpga1/HDMITX_R2))
    (pad 62 smd rect (at 7.8 0.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /fpga1/HDMITX_R1))
    (pad 63 smd rect (at 7.8 0 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /fpga1/HDMITX_R0))
    (pad 64 smd rect (at 7.8 -0.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 65 smd rect (at 7.8 -1 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 66 smd rect (at 7.8 -1.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 67 smd rect (at 7.8 -2 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 68 smd rect (at 7.8 -2.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 69 smd rect (at 7.8 -3 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 70 smd rect (at 7.8 -3.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 71 smd rect (at 7.8 -4 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 /hdmitx1/G7))
    (pad 72 smd rect (at 7.8 -4.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 /hdmitx1/G6))
    (pad 73 smd rect (at 7.8 -5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 /hdmitx1/G5))
    (pad 74 smd rect (at 7.8 -5.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 /hdmitx1/G4))
    (pad 75 smd rect (at 7.8 -6 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 /hdmitx1/G3))
    (pad 76 smd rect (at 6 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 77 smd rect (at 5.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 /hdmitx1/G2))
    (pad 78 smd rect (at 5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 /hdmitx1/G1))
    (pad 79 smd rect (at 4.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 /hdmitx1/G0))
    (pad 80 smd rect (at 4 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 81 smd rect (at 3.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 82 smd rect (at 3 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 83 smd rect (at 2.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 84 smd rect (at 2 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 /hdmitx1/B7))
    (pad 85 smd rect (at 1.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /hdmitx1/B6))
    (pad 86 smd rect (at 1 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 /hdmitx1/B5))
    (pad 87 smd rect (at 0.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 88 smd rect (at 0 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /fpga1/HDMITX_PCLK))
    (pad 89 smd rect (at -0.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 90 smd rect (at -1 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 /hdmitx1/B4))
    (pad 91 smd rect (at -1.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /hdmitx1/B3))
    (pad 92 smd rect (at -2 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /hdmitx1/B2))
    (pad 93 smd rect (at -2.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 /hdmitx1/B1))
    (pad 94 smd rect (at -3 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /hdmitx1/B0))
    (pad 95 smd rect (at -3.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 96 smd rect (at -4 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 97 smd rect (at -4.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 98 smd rect (at -5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 99 smd rect (at -5.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 100 smd rect (at -6 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model Housings_QFP.3dshapes/TQFP-100_14x14mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SCART_CONN (layer F.Cu) (tedit 5697EF23)
    (at 112.7546 81.8212)
    (fp_text reference J3 (at -39.8886 -7.0922 90) (layer F.SilkS))
    (fp_text value SCART-F (at 5.78358 -4.64312 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 212 /hdmitx1/AV1_AUD_R))
    (pad 3 thru_hole circle (at -1.905 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(J3-Pad3)"))
    (pad 4 thru_hole circle (at -3.81 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 5 thru_hole circle (at -5.715 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 6 thru_hole circle (at -7.62 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 217 /hdmitx1/AV1_AUD_L))
    (pad 7 thru_hole circle (at -9.525 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 96 /tvp_board1/RGB1_B))
    (pad 8 thru_hole circle (at -11.43 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 154 "Net-(J3-Pad8)"))
    (pad 9 thru_hole circle (at -13.335 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 10 thru_hole circle (at -15.24 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 155 "Net-(J3-Pad10)"))
    (pad 11 thru_hole circle (at -17.145 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 97 /tvp_board1/RGB1_G))
    (pad 12 thru_hole circle (at -19.05 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 156 "Net-(J3-Pad12)"))
    (pad 13 thru_hole circle (at -20.955 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 20 thru_hole circle (at -34.29 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 99 /tvp_board1/RGB1_S))
    (pad 15 thru_hole circle (at -24.765 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 98 /tvp_board1/RGB1_R))
    (pad 14 thru_hole circle (at -22.86 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 17 thru_hole circle (at -28.575 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 16 thru_hole circle (at -26.67 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 157 "Net-(J3-Pad16)"))
    (pad 19 thru_hole circle (at -32.385 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 158 "Net-(J3-Pad19)"))
    (pad 18 thru_hole circle (at -30.48 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 21 thru_hole circle (at -36.195 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 1 thru_hole circle (at 1.905 -5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 159 "Net-(J3-Pad1)"))
  )
  (module custom_components:SW_PUSH-SKHCBFA010 (layer F.Cu) (tedit 5697EFC9)
    (at 106.131 24.7 90)
    (fp_text reference SW3 (at -7.106 -5.395 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.25 -2.5 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 190 /fpga1/BTN1))
    (pad 2 thru_hole circle (at 6.25 2.5 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 1 thru_hole circle (at -6.25 -2.5 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 190 /fpga1/BTN1))
    (pad 2 thru_hole circle (at -6.25 2.5 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad "" thru_hole circle (at 0 4.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 0 -4.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SW_PUSH-SKHCBFA010 (layer F.Cu) (tedit 58CEB771)
    (at 118.918 24.7 90)
    (fp_text reference SW2 (at -2.597 8.041 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.25 -2.5 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 189 /fpga1/BTN0))
    (pad 2 thru_hole circle (at 6.25 2.5 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 1 thru_hole circle (at -6.25 -2.5 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 189 /fpga1/BTN0))
    (pad 2 thru_hole circle (at -6.25 2.5 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad "" thru_hole circle (at 0 4.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 0 -4.5 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SOIC-8_3.9x4.9mm_Pitch1.27mm_Handsoldering (layer B.Cu) (tedit 56951480)
    (at 92.3903 30.0092 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U10 (at -0.1127 -3.4348 180) (layer B.SilkS))
    (fp_text value S25FL216K (at 0 -3.5 180) (layer B.Fab))
    (pad 1 smd rect (at -3.1 1.905 180) (size 2.35 0.6) (layers B.Cu B.Paste B.Mask)
      (net 34 /fpga1/nCSO))
    (pad 2 smd rect (at -3.1 0.635 180) (size 2.35 0.6) (layers B.Cu B.Paste B.Mask)
      (net 168 "Net-(R23-Pad2)"))
    (pad 3 smd rect (at -3.1 -0.635 180) (size 2.35 0.6) (layers B.Cu B.Paste B.Mask)
      (net 141 "Net-(R24-Pad1)"))
    (pad 4 smd rect (at -3.1 -1.905 180) (size 2.35 0.6) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 5 smd rect (at 3.1 -1.905 180) (size 2.35 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 /fpga1/ASDO))
    (pad 6 smd rect (at 3.1 -0.635 180) (size 2.35 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /fpga1/DCLK))
    (pad 7 smd rect (at 3.1 0.635 180) (size 2.35 0.6) (layers B.Cu B.Paste B.Mask)
      (net 167 "Net-(R19-Pad1)"))
    (pad 8 smd rect (at 3.1 1.905 180) (size 2.35 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:3xRCA_CONN (layer F.Cu) (tedit 5918F097)
    (at 44.196 81.7762)
    (fp_text reference J2 (at 22.113 -2.9242 90) (layer F.SilkS))
    (fp_text value 3XRCA_CONN (at 6.51002 0.6096) (layer F.Fab))
    (pad "" thru_hole circle (at 7.5 -4.2) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -7.5 -4.2) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -10.53338 3.14452) (size 2.3 2.3) (drill 2.3) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 10.53338 3.14452) (size 2.3 2.3) (drill 2.3) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 11.25 -4.5) (size 4.2 4.2) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 100 /tvp_board1/RGB2_B))
    (pad 2 thru_hole circle (at 18.75 -4.5) (size 4.2 4.2) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 100 /tvp_board1/RGB2_B))
    (pad 3 thru_hole circle (at -18.75 -4.5) (size 4.2 4.2) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 102 /tvp_board1/RGB2_R))
    (pad 3 thru_hole circle (at -11.25 -4.5) (size 4.2 4.2) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 102 /tvp_board1/RGB2_R))
    (pad 4 thru_hole circle (at -15 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 4 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 4 thru_hole circle (at 15 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad "" thru_hole oval (at 19.8 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole oval (at -19.8 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at 3.75 -4.5) (size 4.2 4.2) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 101 /tvp_board1/RGB2_G))
    (pad 1 thru_hole circle (at -3.75 -4.5) (size 4.2 4.2) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 101 /tvp_board1/RGB2_G))
  )
  (module custom_components:BARREL_JACK_roundconn (layer F.Cu) (tedit 5918F4A5)
    (at 15.002 28.649)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J5 (at 8.029 -3.332 90) (layer F.SilkS))
    (fp_text value 5VDC_IN (at 0 -5.99948) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 6.20014 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 172 "Net-(F1-Pad1)"))
    (pad 2 thru_hole rect (at 0.20066 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 3 thru_hole rect (at 3.2004 4.699) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
  )
  (module custom_components:LED-0603 (layer F.Cu) (tedit 569D72F1)
    (at 17.179 19.545 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -3.14 -0.076 90) (layer F.SilkS))
    (fp_text value LEDR (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
  )
  (module custom_components:LED-0603 (layer F.Cu) (tedit 569D72F8)
    (at 15.549 19.545 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -3.178 0.03 90) (layer F.SilkS))
    (fp_text value LEDG (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
  )
  (module custom_components:SM0805_libcms (layer F.Cu) (tedit 569D731F)
    (at 69.494 21.361 270)
    (attr smd)
    (fp_text reference C102 (at -2.169 0.802 360) (layer F.SilkS))
    (fp_text value 47u (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0805_libcms (layer F.Cu) (tedit 569D733C)
    (at 53.538 63.155 90)
    (attr smd)
    (fp_text reference C71 (at -2.141 -0.118 180) (layer F.SilkS))
    (fp_text value 47u (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0805_libcms (layer B.Cu) (tedit 569D6D67)
    (at 16.071 22.106 90)
    (attr smd)
    (fp_text reference C107 (at -2.159 0 360) (layer B.SilkS))
    (fp_text value 47u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 186 "Net-(C107-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 40.6886 59.9812 90)
    (attr smd)
    (fp_text reference R1 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 75 (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 105 /tvp_board1/RGB3_R))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569ECA52)
    (at 46.06 58.938 90)
    (attr smd)
    (fp_text reference R2 (at 1.788 0.011 360) (layer B.SilkS))
    (fp_text value 75 (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 103 /tvp_board1/RGB3_B))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 38.2629 67.7155 90)
    (attr smd)
    (fp_text reference R4 (at -1.8288 0 180) (layer F.SilkS))
    (fp_text value 75 (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 102 /tvp_board1/RGB2_R))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569ECE34)
    (at 53.1727 74.0782)
    (attr smd)
    (fp_text reference R5 (at 1.8133 0.5638 90) (layer F.SilkS))
    (fp_text value 75 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 100 /tvp_board1/RGB2_B))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC93A)
    (at 55.2809 72.7701 270)
    (attr smd)
    (fp_text reference R6 (at -0.8781 -1.5391 360) (layer F.SilkS))
    (fp_text value 75 (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 97 /tvp_board1/RGB1_G))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC93D)
    (at 55.0015 69.3665 90)
    (attr smd)
    (fp_text reference R7 (at -0.9205 1.4775 180) (layer F.SilkS))
    (fp_text value 75 (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 98 /tvp_board1/RGB1_R))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC946)
    (at 54.997 66.785 90)
    (attr smd)
    (fp_text reference R8 (at -0.845 1.447 180) (layer F.SilkS))
    (fp_text value 75 (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 96 /tvp_board1/RGB1_B))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC91D)
    (at 40.104 73.015 90)
    (attr smd)
    (fp_text reference R9 (at 1.814 -0.008 180) (layer F.SilkS))
    (fp_text value 75 (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 101 /tvp_board1/RGB2_G))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569ECA6D)
    (at 31.242 55.626)
    (attr smd)
    (fp_text reference R10 (at -1.798 0.808 270) (layer B.SilkS))
    (fp_text value 75 (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 104 /tvp_board1/RGB3_G))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC8CA)
    (at 36.063 49.779)
    (attr smd)
    (fp_text reference R11 (at 1.417 1.468 90) (layer F.SilkS))
    (fp_text value 1.5k (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(C20-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R11-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC83A)
    (at 24.6358 51.7643 180)
    (attr smd)
    (fp_text reference R12 (at 1.8668 0.0323 270) (layer F.SilkS))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 182 /tvp_board1/RGB3_VS))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 39.37 41.656 270)
    (attr smd)
    (fp_text reference R13 (at -1.8288 0 360) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 /fpga1/SDA))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC903)
    (at 44.931 36.606 90)
    (attr smd)
    (fp_text reference R14 (at 1.783 -0.359 180) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 /fpga1/SCL))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC8FE)
    (at 45.6162 39.7755 270)
    (attr smd)
    (fp_text reference R15 (at -1.7165 -1.2468 360) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 196 /fpga1/RESET_N))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 81.788 37.4904 90)
    (attr smd)
    (fp_text reference R16 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 10k (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 140 "Net-(R16-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569ECA06)
    (at 79.8068 37.4904 270)
    (attr smd)
    (fp_text reference R17 (at 1.8596 0.0098 540) (layer B.SilkS))
    (fp_text value 10k (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 165 "Net-(R17-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569ECD23)
    (at 77.089 52.5526 270)
    (attr smd)
    (fp_text reference R18 (at -0.9116 1.666 540) (layer B.SilkS))
    (fp_text value 10k (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 166 "Net-(R18-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 87.0436 28.8662 90)
    (attr smd)
    (fp_text reference R19 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 4.7k (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 167 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 96 21.7 90)
    (attr smd)
    (fp_text reference R20 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 1k (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 27 /fpga1/TCK))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 77.567 32.349 90)
    (attr smd)
    (fp_text reference R21 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 10k (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 31 /fpga1/VCCA))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 30 /fpga1/TMS))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 79.116 32.349 90)
    (attr smd)
    (fp_text reference R22 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 10k (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 31 /fpga1/VCCA))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 28 /fpga1/TDI))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 92.2252 29.6663)
    (attr smd)
    (fp_text reference R23 (at -1.8288 0 90) (layer F.SilkS))
    (fp_text value 25 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 /fpga1/DATA0))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(R23-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 97.6862 29.8568 90)
    (attr smd)
    (fp_text reference R24 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 4.7k (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 141 "Net-(R24-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC993)
    (at 116.693 55.961 270)
    (attr smd)
    (fp_text reference R25 (at 1.886 -0.019 360) (layer F.SilkS))
    (fp_text value 698 (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R25-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 35 /hdmitx1/AVCC1V8))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569EC9C7)
    (at 114.2 40.2)
    (attr smd)
    (fp_text reference R26 (at 1.878 -0.002 270) (layer B.SilkS))
    (fp_text value 1k (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 143 "Net-(R26-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC89D)
    (at 66.6093 24.6371 90)
    (attr smd)
    (fp_text reference R28 (at -1.9109 0.0087 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 24 /fpga1/SD_DAT1))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC898)
    (at 68.2222 24.6498 90)
    (attr smd)
    (fp_text reference R29 (at -1.8872 0.0038 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 23 /fpga1/SD_DAT0))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC893)
    (at 69.8351 24.6498 90)
    (attr smd)
    (fp_text reference R30 (at -1.9252 0.0139 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 /fpga1/SD_CMD))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 71.448 25.5261 90)
    (attr smd)
    (fp_text reference R31 (at -1.8288 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 26 /fpga1/SD_DAT3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 73.0863 26.758 90)
    (attr smd)
    (fp_text reference R32 (at -1.8288 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 25 /fpga1/SD_DAT2))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC871)
    (at 74.2293 24.5482)
    (attr smd)
    (fp_text reference R33 (at 1.9017 -0.0122 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 /fpga1/IR_RX))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC85B)
    (at 67.1046 21.551 180)
    (attr smd)
    (fp_text reference R34 (at 1.8236 0.085 270) (layer F.SilkS))
    (fp_text value 47 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC826)
    (at 19.159 19.691 270)
    (attr smd)
    (fp_text reference R35 (at 1.914 0.044 360) (layer F.SilkS))
    (fp_text value 330 (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 /fpga1/LED0))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569EC82C)
    (at 20.709 19.687 270)
    (attr smd)
    (fp_text reference R36 (at 1.918 -0.097 360) (layer F.SilkS))
    (fp_text value 330 (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 /fpga1/LED1))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 57.912 24.516 270)
    (attr smd)
    (fp_text reference R27 (at -1.8288 0 360) (layer F.SilkS))
    (fp_text value 47 (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(DS1-Pad11)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(Q2-Pad3)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569D6DC4)
    (at 35.9007 59.5367)
    (attr smd)
    (fp_text reference R3 (at -1.8288 0 90) (layer F.SilkS))
    (fp_text value 75 (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 99 /tvp_board1/RGB1_S))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569ECA23)
    (at 21.184 24.079 90)
    (attr smd)
    (fp_text reference F1 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value F0603E1R50FSTR (at 0 0 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 172 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 186 "Net-(C107-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569ECA43)
    (at 41.5649 54.3551 270)
    (attr smd)
    (fp_text reference FB6 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value MPZ1608S221A (at 0 0 360) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 67 /tvp_board1/AVDD))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 192 /tvp_board1/AVDD_F))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569EC9E4)
    (at 112.992 53.221)
    (attr smd)
    (fp_text reference FB1 (at -1.8288 0 270) (layer B.SilkS))
    (fp_text value MPZ1608S221A (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 35 /hdmitx1/AVCC1V8))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 129 "Net-(C74-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569EC9DD)
    (at 112.989 51.407)
    (attr smd)
    (fp_text reference FB2 (at -1.8288 0 270) (layer B.SilkS))
    (fp_text value MPZ1608S221A (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 35 /hdmitx1/AVCC1V8))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 130 "Net-(C77-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569EC9D5)
    (at 112.997 45.811)
    (attr smd)
    (fp_text reference FB4 (at -1.8288 0 270) (layer B.SilkS))
    (fp_text value MPZ1608S221A (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 35 /hdmitx1/AVCC1V8))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 131 "Net-(C80-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569ECA32)
    (at 35.334 34.046)
    (attr smd)
    (fp_text reference FB5 (at 1.833 0.343 270) (layer B.SilkS))
    (fp_text value MPZ1608S221A (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 125 "Net-(C25-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 113.629 19.766 270)
    (attr smd)
    (fp_text reference R42 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 10k (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 189 /fpga1/BTN0))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 100.988 19.919 270)
    (attr smd)
    (fp_text reference R43 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 10k (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 190 /fpga1/BTN1))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569ECA7B)
    (at 35.0625 48.0178)
    (attr smd)
    (fp_text reference FB7 (at 1.8695 -0.2298 270) (layer B.SilkS))
    (fp_text value MPZ1608S221A (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 67 /tvp_board1/AVDD))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 191 "Net-(C23-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 63.749 25.077 270)
    (attr smd)
    (fp_text reference R37 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 1k (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 197 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 201 /fpga1/LCD_BLEN))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569ECA61)
    (at 53.142 61.509 90)
    (attr smd)
    (fp_text reference R38 (at 1.783 0.046 360) (layer B.SilkS))
    (fp_text value 100 (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 194 "Net-(C33-Pad2)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 19 /fpga1/SCL))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 53.721 63.764 180)
    (attr smd)
    (fp_text reference R44 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 100 (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 20 /fpga1/SDA))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 195 "Net-(C36-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 62.133 25.085 270)
    (attr smd)
    (fp_text reference R39 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 10k (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 197 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569ECA18)
    (at 55.47 23.694 180)
    (attr smd)
    (fp_text reference R40 (at 1.833 -0.5 450) (layer B.SilkS))
    (fp_text value 1k (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 198 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 199 "Net-(Q2-Pad1)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569EC9BA)
    (at 115.41 37.72 90)
    (attr smd)
    (fp_text reference R41 (at 1.829 -0.023 360) (layer B.SilkS))
    (fp_text value 4.7k (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 58 /hdmitx1/HPD))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 569ECA88)
    (at 116.69 60.14 90)
    (attr smd)
    (fp_text reference F2 (at -1.8288 0 180) (layer F.SilkS))
    (fp_text value MF-FSMF020X-2 (at 0 0 360) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 202 /hdmitx1/5V))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 207 /hdmitx1/5V_FUSED))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 58E0CE1F)
    (at 120.69 57.5 90)
    (attr smd)
    (fp_text reference R45 (at -1.9 -0.02 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 207 /hdmitx1/5V_FUSED))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 46 /hdmitx1/DDC_SDA))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer F.Cu) (tedit 58E0CDFE)
    (at 118.93 57.5 90)
    (attr smd)
    (fp_text reference R46 (at -1.91 0.01 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 207 /hdmitx1/5V_FUSED))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 45 /hdmitx1/DDC_SCL))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB0F)
    (at 42.873 60.9972)
    (attr smd)
    (fp_text reference C1 (at 0.881 1.4668 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 105 /tvp_board1/RGB3_R))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 108 "Net-(C1-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB12)
    (at 46.8354 60.9972)
    (attr smd)
    (fp_text reference C2 (at -0.7594 1.4408 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 103 /tvp_board1/RGB3_B))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 109 "Net-(C2-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECD97)
    (at 40.3965 68.1727)
    (attr smd)
    (fp_text reference C3 (at 1.8945 0.0163 90) (layer F.SilkS))
    (fp_text value 1u (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 102 /tvp_board1/RGB2_R))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(C3-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDA5)
    (at 50.5184 74.066 180)
    (attr smd)
    (fp_text reference C4 (at 1.8574 -0.008 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 100 /tvp_board1/RGB2_B))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(C4-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDAA)
    (at 52.8425 72.224 180)
    (attr smd)
    (fp_text reference C5 (at 1.8445 -0.039 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 97 /tvp_board1/RGB1_G))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(C5-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDAF)
    (at 52.8171 70.3571 180)
    (attr smd)
    (fp_text reference C6 (at 1.8321 -0.0369 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 98 /tvp_board1/RGB1_R))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(C6-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDB5)
    (at 52.8171 68.0584 180)
    (attr smd)
    (fp_text reference C7 (at 1.8701 0.0884 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 96 /tvp_board1/RGB1_B))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(C7-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB24)
    (at 43.688 55.372)
    (attr smd)
    (fp_text reference C8 (at -0.665 -1.392 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 192 /tvp_board1/AVDD_F))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB50)
    (at 50.292 55.372)
    (attr smd)
    (fp_text reference C9 (at -0.8 -1.407 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 192 /tvp_board1/AVDD_F))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB39)
    (at 46.99 55.372)
    (attr smd)
    (fp_text reference C10 (at 1.265 1.646 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECD90)
    (at 40.3584 61.5052 90)
    (attr smd)
    (fp_text reference C11 (at -1.8268 -0.5214 180) (layer F.SilkS))
    (fp_text value 1n (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 173 /tvp_board1/RGB_12_G))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(C11-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECD9E)
    (at 42.301 74.066)
    (attr smd)
    (fp_text reference C12 (at 1.87 -0.005 90) (layer F.SilkS))
    (fp_text value 1u (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 101 /tvp_board1/RGB2_G))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(C12-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECD8A)
    (at 34.872 57.4158 90)
    (attr smd)
    (fp_text reference C13 (at 1.8048 -0.026 180) (layer F.SilkS))
    (fp_text value 1n (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 99 /tvp_board1/RGB1_S))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(C13-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB79)
    (at 54.102 55.372 90)
    (attr smd)
    (fp_text reference C14 (at -1.819 -0.615 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECAE3)
    (at 34.036 55.626)
    (attr smd)
    (fp_text reference C15 (at 1.854 0.469 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 104 /tvp_board1/RGB3_G))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 118 "Net-(C15-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECAEC)
    (at 34.036 54.102)
    (attr smd)
    (fp_text reference C16 (at 1.849 -0.244 270) (layer B.SilkS))
    (fp_text value 1n (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 104 /tvp_board1/RGB3_G))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 119 "Net-(C16-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569D6DAF)
    (at 32.84 54.317)
    (attr smd)
    (fp_text reference C17 (at -1.8288 0 90) (layer F.SilkS))
    (fp_text value 10n (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(C17-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 39.116 52.324 270)
    (attr smd)
    (fp_text reference C18 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECD7A)
    (at 35.277 51.283 180)
    (attr smd)
    (fp_text reference C19 (at -0.628 -1.668 270) (layer F.SilkS))
    (fp_text value 4.7n (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(C19-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569D6DAF)
    (at 33.528 49.779)
    (attr smd)
    (fp_text reference C20 (at -1.8288 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(C19-Pad2)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(C20-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 54.61 50.292 90)
    (attr smd)
    (fp_text reference C21 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 76 /tvp_board1/DVDD))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB81)
    (at 54.61 47.498 90)
    (attr smd)
    (fp_text reference C22 (at 1.803 0.025 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECD6E)
    (at 36.062 48.265 180)
    (attr smd)
    (fp_text reference C23 (at 1.841 0.274 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECD63)
    (at 26.7059 52.7803 270)
    (attr smd)
    (fp_text reference C24 (at 1.8777 0.0279 360) (layer F.SilkS))
    (fp_text value 1n (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECABE)
    (at 32.728 34.046 180)
    (attr smd)
    (fp_text reference C25 (at 0.887 -1.631 450) (layer B.SilkS))
    (fp_text value 10n (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 125 "Net-(C25-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 51.308 42.926 180)
    (attr smd)
    (fp_text reference C26 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB94)
    (at 44.196 41.402)
    (attr smd)
    (fp_text reference C27 (at 1.052 -1.615 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 76 /tvp_board1/DVDD))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 45.72 42.926 180)
    (attr smd)
    (fp_text reference C28 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 46.421 29.444)
    (attr smd)
    (fp_text reference C29 (at -1.8288 0 270) (layer B.SilkS))
    (fp_text value 1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 126 "Net-(C29-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 49.3754 27.7613 180)
    (attr smd)
    (fp_text reference C30 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 127 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 128 "Net-(C30-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECD50)
    (at 26.645 31.313 90)
    (attr smd)
    (fp_text reference C31 (at -0.866 -1.72 180) (layer F.SilkS))
    (fp_text value 10u (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 202 /hdmitx1/5V))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 25.2962 47.586 270)
    (attr smd)
    (fp_text reference C32 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 1u (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 36.593 39.639 90)
    (attr smd)
    (fp_text reference C34 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 32.0653 47.5479 90)
    (attr smd)
    (fp_text reference C35 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 67 /tvp_board1/AVDD))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB9A)
    (at 43.365 39.045 90)
    (attr smd)
    (fp_text reference C37 (at 1.824 0.039 360) (layer B.SilkS))
    (fp_text value 1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 76 /tvp_board1/DVDD))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 25.187 53.015 90)
    (attr smd)
    (fp_text reference C38 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 202 /hdmitx1/5V))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECC83)
    (at 84.115 34.011 90)
    (attr smd)
    (fp_text reference C39 (at -1.976 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 76.5 36.1 180)
    (attr smd)
    (fp_text reference C40 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECBC0)
    (at 72.6 34.061)
    (attr smd)
    (fp_text reference C41 (at 0.867 -1.661 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECBBB)
    (at 69.101 34.064 180)
    (attr smd)
    (fp_text reference C42 (at 0.958 1.664 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDE8)
    (at 66 34 90)
    (attr smd)
    (fp_text reference C43 (at 1.788 -0.453 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 32 /fpga1/VCCD_PLL))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECC88)
    (at 85.786 34.006 90)
    (attr smd)
    (fp_text reference C44 (at -2.032 0.005 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 31 /fpga1/VCCA))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECBAA)
    (at 73.3 36.1 180)
    (attr smd)
    (fp_text reference C45 (at -0.893 -1.655 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569D6DAF)
    (at 68 31.8 180)
    (attr smd)
    (fp_text reference C46 (at -1.8288 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 31 /fpga1/VCCA))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDD6)
    (at 66.6 55.9 180)
    (attr smd)
    (fp_text reference C47 (at 1.906 0.061 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 32 /fpga1/VCCD_PLL))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 66.3 36.6 270)
    (attr smd)
    (fp_text reference C48 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 88.3 38.4 90)
    (attr smd)
    (fp_text reference C50 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 66.3 39.2 90)
    (attr smd)
    (fp_text reference C51 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDEF)
    (at 66.5204 18.63 270)
    (attr smd)
    (fp_text reference C52 (at -0.83 -1.6986 360) (layer F.SilkS))
    (fp_text value 1u (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 68.524 46.558 270)
    (attr smd)
    (fp_text reference C53 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 88.3 45 90)
    (attr smd)
    (fp_text reference C54 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569D6DAF)
    (at 92.2125 27.8883 180)
    (attr smd)
    (fp_text reference C55 (at -1.8288 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 44.8796 27.7105)
    (attr smd)
    (fp_text reference C56 (at -1.8288 0 270) (layer B.SilkS))
    (fp_text value 1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECC75)
    (at 85.8 48.9 90)
    (attr smd)
    (fp_text reference C57 (at -1.859 -0.349 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 88.3 49 90)
    (attr smd)
    (fp_text reference C58 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 66.3 51.1 90)
    (attr smd)
    (fp_text reference C59 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDE2)
    (at 88.021 33.498)
    (attr smd)
    (fp_text reference C60 (at 1.948 0.038 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 32 /fpga1/VCCD_PLL))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECC59)
    (at 86.1 55.7)
    (attr smd)
    (fp_text reference C61 (at 1.921 -0.033 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 31 /fpga1/VCCA))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECD18)
    (at 79.3 53.1)
    (attr smd)
    (fp_text reference C62 (at 0.847 -1.619 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 72.8 53.1)
    (attr smd)
    (fp_text reference C63 (at -1.8288 0 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECBE5)
    (at 68.4 55.7 180)
    (attr smd)
    (fp_text reference C64 (at 1.797 0.063 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 31 /fpga1/VCCA))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDDC)
    (at 88.5 55.3 270)
    (attr smd)
    (fp_text reference C65 (at 1.85 0.039 360) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 32 /fpga1/VCCD_PLL))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 82.088 55.621 180)
    (attr smd)
    (fp_text reference C66 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECC20)
    (at 76.219 55.625)
    (attr smd)
    (fp_text reference C67 (at -0.39 1.632 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECBF1)
    (at 71 55.63)
    (attr smd)
    (fp_text reference C68 (at -0.815 1.606 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 106.5 55.6 180)
    (attr smd)
    (fp_text reference C69 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 107.6 57.3 180)
    (attr smd)
    (fp_text reference C73 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECCBA)
    (at 115 53.7 270)
    (attr smd)
    (fp_text reference C74 (at -0.822 -1.672 540) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 129 "Net-(C74-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECCD7)
    (at 99.6 53.6 270)
    (attr smd)
    (fp_text reference C75 (at -1.803 0.315 540) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECCB3)
    (at 115 50.2 90)
    (attr smd)
    (fp_text reference C77 (at 0.807 1.708 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 130 "Net-(C77-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECCA1)
    (at 115 47.3 90)
    (attr smd)
    (fp_text reference C78 (at -0.858 1.738 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 130 "Net-(C77-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 99.5 47.7 90)
    (attr smd)
    (fp_text reference C79 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECC9A)
    (at 115 44.6 90)
    (attr smd)
    (fp_text reference C80 (at 1.776 0.011 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 131 "Net-(C80-Pad1)"))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569D6DAF)
    (at 118.04 45.01 270)
    (attr smd)
    (fp_text reference C81 (at -1.8288 0 360) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 99.6 42.6 270)
    (attr smd)
    (fp_text reference C82 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECCE3)
    (at 106.5 38.5)
    (attr smd)
    (fp_text reference C83 (at 1.897 -0.065 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 106.5 40.2 180)
    (attr smd)
    (fp_text reference C84 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 111.5 40.2)
    (attr smd)
    (fp_text reference C85 (at -1.8288 0 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E42609)
    (at 112.1 38.5 180)
    (attr smd)
    (fp_text reference C86 (at -1.22 1.65 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 103.561 62.316 180)
    (attr smd)
    (fp_text reference C87 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 113.167 62.311 180)
    (attr smd)
    (fp_text reference C88 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECCD0)
    (at 103 55.6 180)
    (attr smd)
    (fp_text reference C89 (at 1.827 -0.011 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECCC0)
    (at 112.5586 55.6006 180)
    (attr smd)
    (fp_text reference C90 (at 1.8296 0.0556 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 35 /hdmitx1/AVCC1V8))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 79.097 62.3956 180)
    (attr smd)
    (fp_text reference C91 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 92.202 61.6966 180)
    (attr smd)
    (fp_text reference C92 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECD55)
    (at 36.405 31.318 90)
    (attr smd)
    (fp_text reference C93 (at 1.821 0.049 180) (layer F.SilkS))
    (fp_text value 10u (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 74.468 62.3906 180)
    (attr smd)
    (fp_text reference C94 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECAFB)
    (at 32.1056 52.1462 90)
    (attr smd)
    (fp_text reference C95 (at 0.8582 1.7014 360) (layer B.SilkS))
    (fp_text value 1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECC16)
    (at 73.6854 55.63 180)
    (attr smd)
    (fp_text reference C96 (at -0.0406 -1.474 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECC52)
    (at 78.76 55.625 180)
    (attr smd)
    (fp_text reference C97 (at -1.448 -1.594 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 31 /fpga1/VCCA))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 92.1004 54.9148 180)
    (attr smd)
    (fp_text reference C98 (at -1.8288 0 450) (layer B.SilkS))
    (fp_text value 1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 32 /fpga1/VCCD_PLL))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 68.9356 37.6936 270)
    (attr smd)
    (fp_text reference C99 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECC7D)
    (at 85.8 42.7 90)
    (attr smd)
    (fp_text reference C101 (at 1.834 0.268 360) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDBD)
    (at 51.763 63.49 90)
    (attr smd)
    (fp_text reference C70 (at -1.844 -0.153 180) (layer F.SilkS))
    (fp_text value 10n (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECD68)
    (at 29.1443 52.4755 270)
    (attr smd)
    (fp_text reference C72 (at 1.9465 0.0893 360) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDCB)
    (at 46.2258 61.2512 90)
    (attr smd)
    (fp_text reference C76 (at -0.8818 -1.7708 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 174 /tvp_board1/RGB_12_R))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(C76-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569ECDC5)
    (at 49.985 61.2258 90)
    (attr smd)
    (fp_text reference C100 (at 0.8978 1.976 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 176 /tvp_board1/RGB_12_B))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(C100-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569D6DAF)
    (at 41.9586 61.5052 90)
    (attr smd)
    (fp_text reference C103 (at -1.8288 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 173 /tvp_board1/RGB_12_G))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(C103-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 43.312 58.929 270)
    (attr smd)
    (fp_text reference C104 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 10n (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 179 "Net-(C104-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 50.703 58.9398 270)
    (attr smd)
    (fp_text reference C105 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 10n (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 180 "Net-(C105-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 569D6DAF)
    (at 36.8278 57.3904 270)
    (attr smd)
    (fp_text reference C106 (at -1.8288 0 360) (layer F.SilkS))
    (fp_text value 10n (at 0 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(C106-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB6B)
    (at 51.656 61.509 270)
    (attr smd)
    (fp_text reference C33 (at 0.861 1.707 540) (layer B.SilkS))
    (fp_text value 22p (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 194 "Net-(C33-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB61)
    (at 51.664 64.244 270)
    (attr smd)
    (fp_text reference C36 (at 1.867 0 540) (layer B.SilkS))
    (fp_text value 22p (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 195 "Net-(C36-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECBD7)
    (at 67.807 50.932 90)
    (attr smd)
    (fp_text reference C49 (at -1.971 0.204 360) (layer B.SilkS))
    (fp_text value 10u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECBD0)
    (at 65.791 47.859 180)
    (attr smd)
    (fp_text reference C108 (at 1.829 0.051 450) (layer B.SilkS))
    (fp_text value 10u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569ECB8A)
    (at 42.667 42.896 180)
    (attr smd)
    (fp_text reference C109 (at 1.812 0.087 450) (layer B.SilkS))
    (fp_text value 10u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 76 /tvp_board1/DVDD))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 569D6DAF)
    (at 101.15 53.404 270)
    (attr smd)
    (fp_text reference C110 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 10u (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 48 /hdmitx1/DVDD1V8))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SW_SPDT (layer F.Cu) (tedit 5733AFD4)
    (at 14.966 38.298 180)
    (tags "Switch Micro SPST")
    (fp_text reference SW1 (at -7.277 0.056 270) (layer F.SilkS))
    (fp_text value SPST (at -0.14478 4.66344 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -4.7 0 180) (size 3.3 3.3) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 202 /hdmitx1/5V))
    (pad 2 thru_hole circle (at 0 0 180) (size 3.3 3.3) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 186 "Net-(C107-Pad1)"))
    (pad 3 thru_hole circle (at 4.7 0 180) (size 3.3 3.3) (drill 2.1) (layers *.Cu *.Mask F.SilkS))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_Micro_SPST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.33 0.33 0.33))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:NHD-C0216CZ_vertmount (layer F.Cu) (tedit 5733B00F)
    (at 43.3762 21.9066 180)
    (fp_text reference DS1 (at -0.2098 -1.1994 180) (layer F.SilkS))
    (fp_text value CONN_01X12 (at -11.23188 -1.15062 180) (layer F.Fab))
    (fp_text user K (at 19.3042 -0.9424 180) (layer F.SilkS))
    (fp_text user A (at -19.2948 -0.9194 180) (layer F.SilkS))
    (pad 10 smd rect (at -6.75 -2.5 180) (size 0.9 3.6) (layers B.Cu B.Paste B.Mask)
      (net 127 "Net-(C30-Pad1)"))
    (pad 9 smd rect (at -5.25 -2.5 180) (size 0.9 3.6) (layers B.Cu B.Paste B.Mask)
      (net 128 "Net-(C30-Pad2)"))
    (pad 4 smd rect (at 2.25 -2.5 180) (size 0.9 3.6) (layers B.Cu B.Paste B.Mask)
      (net 19 /fpga1/SCL))
    (pad 5 smd rect (at 0.75 -2.5 180) (size 0.9 3.6) (layers B.Cu B.Paste B.Mask)
      (net 20 /fpga1/SDA))
    (pad 6 smd rect (at -0.75 -2.5 180) (size 0.9 3.6) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 7 smd rect (at -2.25 -2.5 180) (size 0.9 3.6) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 3 smd rect (at 3.75 -2.5 180) (size 0.9 3.6) (layers B.Cu B.Paste B.Mask)
      (net 187 /fpga1/LCD_CS_N))
    (pad 2 smd rect (at 5.25 -2.5 180) (size 0.9 3.6) (layers B.Cu B.Paste B.Mask)
      (net 188 /fpga1/LCD_RS))
    (pad 1 smd rect (at 6.75 -2.5 180) (size 0.9 3.6) (layers B.Cu B.Paste B.Mask)
      (net 196 /fpga1/RESET_N))
    (pad 8 smd rect (at -3.75 -2.5 180) (size 0.9 3.6) (layers B.Cu B.Paste B.Mask)
      (net 126 "Net-(C29-Pad2)"))
    (pad 11 smd rect (at -17.3 -2.5 180) (size 2.5 4) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(DS1-Pad11)"))
    (pad 12 smd rect (at 17.3 -2.5 180) (size 2.5 4) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425D2)
    (at 101.42 70.58 180)
    (attr smd)
    (fp_text reference C111 (at -1.85 -0.22 450) (layer B.SilkS))
    (fp_text value 30p (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 208 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425D1)
    (at 101.41 68.84 180)
    (attr smd)
    (fp_text reference C112 (at -1.81 0.31 450) (layer B.SilkS))
    (fp_text value 30p (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 209 "Net-(C112-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425EA)
    (at 110.07 65.99 90)
    (attr smd)
    (fp_text reference C113 (at -2.47 0.21 90) (layer B.SilkS))
    (fp_text value 10u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425EF)
    (at 111.82 65.99 90)
    (attr smd)
    (fp_text reference C114 (at -2.45 0.27 90) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425E1)
    (at 106.22 65.51 180)
    (attr smd)
    (fp_text reference C115 (at 1.83 0.03 450) (layer B.SilkS))
    (fp_text value 10u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425B2)
    (at 115.17 67.63 180)
    (attr smd)
    (fp_text reference C116 (at -1.83 -0.15 450) (layer B.SilkS))
    (fp_text value 10u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 219 /hdmitx1/AV3_AUD_R))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 211 "Net-(C116-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425DE)
    (at 106.22 67.24 180)
    (attr smd)
    (fp_text reference C118 (at -0.98 -1.84 450) (layer B.SilkS))
    (fp_text value 0.1u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 58E41F8E)
    (at 112.41 64.35)
    (attr smd)
    (fp_text reference C119 (at 1.82 -1.45 90) (layer F.SilkS))
    (fp_text value 2.2u (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(C119-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer F.Cu) (tedit 58E41F88)
    (at 109.035 64.359 180)
    (attr smd)
    (fp_text reference C120 (at 0.945 1.869 270) (layer F.SilkS))
    (fp_text value 2.2u (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(C120-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425AF)
    (at 115.17 65.91 180)
    (attr smd)
    (fp_text reference C121 (at -1.8 0.31 450) (layer B.SilkS))
    (fp_text value 10u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 222 /hdmitx1/AV3_AUD_L))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 216 "Net-(C121-Pad2)"))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425BA)
    (at 115.18 73.86)
    (attr smd)
    (fp_text reference C123 (at 1.89 0.23 270) (layer B.SilkS))
    (fp_text value 10u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 218 "Net-(C123-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 210 /hdmitx1/AV2_AUD_R))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425C3)
    (at 110.83 73.88 180)
    (attr smd)
    (fp_text reference C124 (at 1.83 -0.3 450) (layer B.SilkS))
    (fp_text value 10u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 220 "Net-(C124-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 212 /hdmitx1/AV1_AUD_R))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425B8)
    (at 115.17 72.12)
    (attr smd)
    (fp_text reference C125 (at 1.92 -0.11 270) (layer B.SilkS))
    (fp_text value 10u (at 0 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 221 "Net-(C125-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 215 /hdmitx1/AV2_AUD_L))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Capa_libcms (layer B.Cu) (tedit 58E425C8)
    (at 110.82 72.12 180)
    (attr smd)
    (fp_text reference C126 (at 1.88 0.16 450) (layer B.SilkS))
    (fp_text value 10u (at 0 0 450) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 223 "Net-(C126-Pad1)"))
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 217 /hdmitx1/AV1_AUD_L))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SOD-323_Handsoldering (layer B.Cu) (tedit 55F1B69A)
    (at 119.04 20.422)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 0 1.85) (layer B.SilkS))
    (fp_text value SD05-7 (at 0.1 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -1.4 0) (size 1.4 0.45) (layers B.Cu B.Paste B.Mask)
      (net 189 /fpga1/BTN0))
    (pad 2 smd rect (at 1.4 0) (size 1.4 0.45) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
  )
  (module custom_components:SOD-323_Handsoldering (layer B.Cu) (tedit 55F1B69A)
    (at 106.208 20.368)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at 0 1.85) (layer B.SilkS))
    (fp_text value SD05-7 (at 0.1 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -1.4 0) (size 1.4 0.45) (layers B.Cu B.Paste B.Mask)
      (net 190 /fpga1/BTN1))
    (pad 2 smd rect (at 1.4 0) (size 1.4 0.45) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
  )
  (module custom_components:TQFP-144_thermal (layer F.Cu) (tedit 56867A9C)
    (at 77.3 44.7 270)
    (descr "P/PG-TQFP-144-2, -3, -7 (see MAXIM 21-0087.PDF and 90-0144.PDF)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U2 (at 0 -12.475 270) (layer F.SilkS))
    (fp_text value EP4CE15E22 (at 0 12.475 270) (layer F.Fab))
    (pad 1 smd rect (at -10.8 -8.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /fpga1/VCCD_PLL))
    (pad 2 smd rect (at -10.8 -8.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 3 smd rect (at -10.8 -7.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /fpga1/VCCA))
    (pad 4 smd rect (at -10.8 -7.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 5 smd rect (at -10.8 -6.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 6 smd rect (at -10.8 -6.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /fpga1/ASDO))
    (pad 7 smd rect (at -10.8 -5.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /fpga1/HDMITX_R5))
    (pad 8 smd rect (at -10.8 -5.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 /fpga1/nCSO))
    (pad 9 smd rect (at -10.8 -4.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R16-Pad2)"))
    (pad 10 smd rect (at -10.8 -4.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /fpga1/HDMITX_R6))
    (pad 11 smd rect (at -10.8 -3.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /fpga1/HDMITX_R7))
    (pad 12 smd rect (at -10.8 -3.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /fpga1/DCLK))
    (pad 13 smd rect (at -10.8 -2.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /fpga1/DATA0))
    (pad 14 smd rect (at -10.8 -2.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(R17-Pad1)"))
    (pad 15 smd rect (at -10.8 -1.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /fpga1/TDI))
    (pad 16 smd rect (at -10.8 -1.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /fpga1/TCK))
    (pad 17 smd rect (at -10.8 -0.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 18 smd rect (at -10.8 -0.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /fpga1/TMS))
    (pad 19 smd rect (at -10.8 0.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 20 smd rect (at -10.8 0.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /fpga1/TDO))
    (pad 21 smd rect (at -10.8 1.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 22 smd rect (at -10.8 1.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 23 smd rect (at -10.8 2.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /fpga1/IR_RX))
    (pad 24 smd rect (at -10.8 2.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 25 smd rect (at -10.8 3.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 164 /fpga1/CLK27))
    (pad 26 smd rect (at -10.8 3.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 27 smd rect (at -10.8 4.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 28 smd rect (at -10.8 4.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /fpga1/SD_DAT2))
    (pad 29 smd rect (at -10.8 5.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 30 smd rect (at -10.8 5.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /fpga1/SD_DAT3))
    (pad 31 smd rect (at -10.8 6.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /fpga1/SD_CMD))
    (pad 32 smd rect (at -10.8 6.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /fpga1/SD_CLK))
    (pad 33 smd rect (at -10.8 7.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /fpga1/SD_DAT0))
    (pad 34 smd rect (at -10.8 7.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 35 smd rect (at -10.8 8.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /fpga1/VCCA))
    (pad 36 smd rect (at -10.8 8.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 37 smd rect (at -8.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /fpga1/VCCD_PLL))
    (pad 38 smd rect (at -8.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 39 smd rect (at -7.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /fpga1/SD_DAT1))
    (pad 40 smd rect (at -7.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 41 smd rect (at -6.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 42 smd rect (at -6.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 188 /fpga1/LCD_RS))
    (pad 43 smd rect (at -5.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 187 /fpga1/LCD_CS_N))
    (pad 44 smd rect (at -5.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /fpga1/LED1))
    (pad 45 smd rect (at -4.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 46 smd rect (at -4.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /fpga1/LED0))
    (pad 47 smd rect (at -3.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 48 smd rect (at -3.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 49 smd rect (at -2.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /fpga1/SDA))
    (pad 50 smd rect (at -2.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /fpga1/SCL))
    (pad 51 smd rect (at -1.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 201 /fpga1/LCD_BLEN))
    (pad 52 smd rect (at -1.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 88 /tvp_board1/R0))
    (pad 53 smd rect (at -0.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 89 /tvp_board1/R1))
    (pad 54 smd rect (at -0.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 90 /tvp_board1/R2))
    (pad 55 smd rect (at 0.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 91 /tvp_board1/R3))
    (pad 56 smd rect (at 0.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 57 smd rect (at 1.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 58 smd rect (at 1.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 92 /tvp_board1/R4))
    (pad 59 smd rect (at 2.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 /tvp_board1/R5))
    (pad 60 smd rect (at 2.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 94 /tvp_board1/R6))
    (pad 61 smd rect (at 3.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 95 /tvp_board1/R7))
    (pad 62 smd rect (at 3.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 63 smd rect (at 4.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 64 smd rect (at 4.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 78 /tvp_board1/G0))
    (pad 65 smd rect (at 5.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 79 /tvp_board1/G1))
    (pad 66 smd rect (at 5.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 80 /tvp_board1/G2))
    (pad 67 smd rect (at 6.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 81 /tvp_board1/G3))
    (pad 68 smd rect (at 6.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 82 /tvp_board1/G4))
    (pad 69 smd rect (at 7.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 83 /tvp_board1/G5))
    (pad 70 smd rect (at 7.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 71 smd rect (at 8.25 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 84 /tvp_board1/G6))
    (pad 72 smd rect (at 8.75 10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 85 /tvp_board1/G7))
    (pad 73 smd rect (at 10.8 8.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /fpga1/VCCD_PLL))
    (pad 74 smd rect (at 10.8 8.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 75 smd rect (at 10.8 7.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /fpga1/VCCA))
    (pad 76 smd rect (at 10.8 7.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 68 /tvp_board1/B0))
    (pad 77 smd rect (at 10.8 6.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 69 /tvp_board1/B1))
    (pad 78 smd rect (at 10.8 6.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 79 smd rect (at 10.8 5.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 80 smd rect (at 10.8 5.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 /tvp_board1/B2))
    (pad 81 smd rect (at 10.8 4.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 82 smd rect (at 10.8 4.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 83 smd rect (at 10.8 3.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 71 /tvp_board1/B3))
    (pad 84 smd rect (at 10.8 3.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 85 smd rect (at 10.8 2.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 /tvp_board1/B4))
    (pad 86 smd rect (at 10.8 2.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 /tvp_board1/B5))
    (pad 87 smd rect (at 10.8 1.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 /tvp_board1/B6))
    (pad 88 smd rect (at 10.8 1.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 /tvp_board1/B7))
    (pad 89 smd rect (at 10.8 0.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 87 /tvp_board1/PCLK))
    (pad 90 smd rect (at 10.8 0.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 /tvp_board1/HSYNC))
    (pad 91 smd rect (at 10.8 -0.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 106 /tvp_board1/VSYNC))
    (pad 92 smd rect (at 10.8 -0.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(R18-Pad2)"))
    (pad 93 smd rect (at 10.8 -1.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 94 smd rect (at 10.8 -1.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 95 smd rect (at 10.8 -2.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 96 smd rect (at 10.8 -2.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /fpga1/VCCA))
    (pad 97 smd rect (at 10.8 -3.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 98 smd rect (at 10.8 -3.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 77 /tvp_board1/FID))
    (pad 99 smd rect (at 10.8 -4.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 196 /fpga1/RESET_N))
    (pad 100 smd rect (at 10.8 -4.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /fpga1/HDMITX_INT_N))
    (pad 101 smd rect (at 10.8 -5.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /fpga1/HDMITX_VSYNC))
    (pad 102 smd rect (at 10.8 -5.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 103 smd rect (at 10.8 -6.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /fpga1/HDMITX_HSYNC))
    (pad 104 smd rect (at 10.8 -6.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 /hdmitx1/DE))
    (pad 105 smd rect (at 10.8 -7.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /hdmitx1/B0))
    (pad 106 smd rect (at 10.8 -7.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 /hdmitx1/B1))
    (pad 107 smd rect (at 10.8 -8.25 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /fpga1/VCCA))
    (pad 108 smd rect (at 10.8 -8.75 270) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 109 smd rect (at 8.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /fpga1/VCCD_PLL))
    (pad 110 smd rect (at 8.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /hdmitx1/B2))
    (pad 111 smd rect (at 7.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /hdmitx1/B3))
    (pad 112 smd rect (at 7.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 /hdmitx1/B4))
    (pad 113 smd rect (at 6.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /fpga1/HDMITX_PCLK))
    (pad 114 smd rect (at 6.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 /hdmitx1/B5))
    (pad 115 smd rect (at 5.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /hdmitx1/B6))
    (pad 116 smd rect (at 5.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 117 smd rect (at 4.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 118 smd rect (at 4.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 119 smd rect (at 3.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 /hdmitx1/B7))
    (pad 120 smd rect (at 3.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 /hdmitx1/G0))
    (pad 121 smd rect (at 2.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 /hdmitx1/G1))
    (pad 122 smd rect (at 2.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 123 smd rect (at 1.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 124 smd rect (at 1.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 125 smd rect (at 0.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 /hdmitx1/G2))
    (pad 126 smd rect (at 0.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 127 smd rect (at -0.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 128 smd rect (at -0.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 189 /fpga1/BTN0))
    (pad 129 smd rect (at -1.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 190 /fpga1/BTN1))
    (pad 130 smd rect (at -1.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 131 smd rect (at -2.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 132 smd rect (at -2.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 /hdmitx1/G3))
    (pad 133 smd rect (at -3.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 /hdmitx1/G4))
    (pad 134 smd rect (at -3.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 /hdmitx1/G5))
    (pad 135 smd rect (at -4.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 /hdmitx1/G6))
    (pad 136 smd rect (at -4.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 /hdmitx1/G7))
    (pad 137 smd rect (at -5.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /fpga1/HDMITX_R0))
    (pad 138 smd rect (at -5.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /fpga1/VCCINT))
    (pad 139 smd rect (at -6.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 140 smd rect (at -6.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 141 smd rect (at -7.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /fpga1/HDMITX_R1))
    (pad 142 smd rect (at -7.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /fpga1/HDMITX_R2))
    (pad 143 smd rect (at -8.25 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /fpga1/HDMITX_R3))
    (pad 144 smd rect (at -8.75 -10.8) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /fpga1/HDMITX_R4))
    (pad 41 smd rect (at 0 0 270) (size 6.7 6.7) (layers *.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 41 thru_hole circle (at -2.55 -2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -1.7 -2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -0.85 -2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 0 -2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 0.85 -2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 1.7 -2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 2.55 -2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -2.55 -1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -1.7 -1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -0.85 -1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 0 -1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 0.85 -1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 1.7 -1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 2.55 -1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -2.55 -0.85 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -1.7 -0.85 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 1.7 -0.85 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 2.55 -0.85 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -2.55 0 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -1.7 0 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 1.7 0 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 2.55 0 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -2.55 0.85 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -1.7 0.85 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 1.7 0.85 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 2.55 0.85 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -2.55 1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -1.7 1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -0.85 1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 0 1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 0.85 1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 1.7 1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 2.55 1.7 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -2.55 2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -1.7 2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at -0.85 2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 0 2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 0.85 2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 1.7 2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 2.55 2.55 270) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 41 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (model Housings_QFP.3dshapes/TQFP-144_20x20mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:TQFP-100_thermal (layer F.Cu) (tedit 58CC2AEE)
    (at 46.736 50.292 90)
    (descr "100-Lead Plastic Thin Quad Flatpack (PF) - 14x14x1 mm Body 2.00 mm Footprint [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at -2.743 -9.566 90) (layer F.SilkS))
    (fp_text value TVP7002PZP (at 0 9.45 90) (layer F.Fab))
    (pad 1 smd rect (at -7.8 -6 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at -7.8 -5.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(C103-Pad2)"))
    (pad 3 smd rect (at -7.8 -5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 4 smd rect (at -7.8 -4.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 192 /tvp_board1/AVDD_F))
    (pad 5 smd rect (at -7.8 -4 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 6 smd rect (at -7.8 -3.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 192 /tvp_board1/AVDD_F))
    (pad 7 smd rect (at -7.8 -3 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 192 /tvp_board1/AVDD_F))
    (pad 8 smd rect (at -7.8 -2.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 9 smd rect (at -7.8 -2 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(C1-Pad2)"))
    (pad 10 smd rect (at -7.8 -1.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(C104-Pad2)"))
    (pad 11 smd rect (at -7.8 -1 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(C76-Pad2)"))
    (pad 12 smd rect (at -7.8 -0.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 13 smd rect (at -7.8 0 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 14 smd rect (at -7.8 0.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 15 smd rect (at -7.8 1 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 16 smd rect (at -7.8 1.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(C2-Pad2)"))
    (pad 17 smd rect (at -7.8 2 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(C105-Pad2)"))
    (pad 18 smd rect (at -7.8 2.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(C100-Pad2)"))
    (pad 19 smd rect (at -7.8 3 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 192 /tvp_board1/AVDD_F))
    (pad 20 smd rect (at -7.8 3.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 21 smd rect (at -7.8 4 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 22 smd rect (at -7.8 4.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 77 /tvp_board1/FID))
    (pad 23 smd rect (at -7.8 5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 106 /tvp_board1/VSYNC))
    (pad 24 smd rect (at -7.8 5.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 /tvp_board1/HSYNC))
    (pad 25 smd rect (at -7.8 6 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at -6 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 27 smd rect (at -5.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 28 smd rect (at -5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 87 /tvp_board1/PCLK))
    (pad 29 smd rect (at -4.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 /tvp_board1/B7))
    (pad 30 smd rect (at -4 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 /tvp_board1/B6))
    (pad 31 smd rect (at -3.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 /tvp_board1/B5))
    (pad 32 smd rect (at -3 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 /tvp_board1/B4))
    (pad 33 smd rect (at -2.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 71 /tvp_board1/B3))
    (pad 34 smd rect (at -2 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 /tvp_board1/B2))
    (pad 35 smd rect (at -1.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 69 /tvp_board1/B1))
    (pad 36 smd rect (at -1 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 68 /tvp_board1/B0))
    (pad 37 smd rect (at -0.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 0 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(U1-Pad38)"))
    (pad 39 smd rect (at 0.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 76 /tvp_board1/DVDD))
    (pad 40 smd rect (at 1 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 41 smd rect (at 1.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 42 smd rect (at 2 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 43 smd rect (at 2.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 85 /tvp_board1/G7))
    (pad 44 smd rect (at 3 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 84 /tvp_board1/G6))
    (pad 45 smd rect (at 3.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 83 /tvp_board1/G5))
    (pad 46 smd rect (at 4 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 82 /tvp_board1/G4))
    (pad 47 smd rect (at 4.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 81 /tvp_board1/G3))
    (pad 48 smd rect (at 5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 80 /tvp_board1/G2))
    (pad 49 smd rect (at 5.5 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 79 /tvp_board1/G1))
    (pad 50 smd rect (at 6 7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 78 /tvp_board1/G0))
    (pad 51 smd rect (at 7.8 6 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(U1-Pad51)"))
    (pad 52 smd rect (at 7.8 5.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(U1-Pad52)"))
    (pad 53 smd rect (at 7.8 5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 54 smd rect (at 7.8 4.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 55 smd rect (at 7.8 4 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 95 /tvp_board1/R7))
    (pad 56 smd rect (at 7.8 3.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 94 /tvp_board1/R6))
    (pad 57 smd rect (at 7.8 3 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 /tvp_board1/R5))
    (pad 58 smd rect (at 7.8 2.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 92 /tvp_board1/R4))
    (pad 59 smd rect (at 7.8 2 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 91 /tvp_board1/R3))
    (pad 60 smd rect (at 7.8 1.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 61 smd rect (at 7.8 1 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 90 /tvp_board1/R2))
    (pad 62 smd rect (at 7.8 0.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 89 /tvp_board1/R1))
    (pad 63 smd rect (at 7.8 0 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 88 /tvp_board1/R0))
    (pad 64 smd rect (at 7.8 -0.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(U1-Pad64)"))
    (pad 65 smd rect (at 7.8 -1 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(U1-Pad65)"))
    (pad 66 smd rect (at 7.8 -1.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 /hdmitx1/DVDD3V3))
    (pad 67 smd rect (at 7.8 -2 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 68 smd rect (at 7.8 -2.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 69 smd rect (at 7.8 -3 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 76 /tvp_board1/DVDD))
    (pad 70 smd rect (at 7.8 -3.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 71 smd rect (at 7.8 -4 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 196 /fpga1/RESET_N))
    (pad 72 smd rect (at 7.8 -4.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 73 smd rect (at 7.8 -5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 74 smd rect (at 7.8 -5.5 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /fpga1/SCL))
    (pad 75 smd rect (at 7.8 -6 90) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /fpga1/SDA))
    (pad 76 smd rect (at 6 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 77 smd rect (at 5.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 78 smd rect (at 5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 183 /tvp_board1/RGB3_VS_B))
    (pad 79 smd rect (at 4.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 80 smd rect (at 4 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 164 /fpga1/CLK27))
    (pad 81 smd rect (at 3.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 184 /tvp_board1/RGB3_HS_B))
    (pad 82 smd rect (at 3 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 83 smd rect (at 2.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 84 smd rect (at 2 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(C23-Pad1)"))
    (pad 85 smd rect (at 1.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(C23-Pad1)"))
    (pad 86 smd rect (at 1 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 87 smd rect (at 0.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R11-Pad2)"))
    (pad 88 smd rect (at 0 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(C19-Pad1)"))
    (pad 89 smd rect (at -0.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(C19-Pad2)"))
    (pad 90 smd rect (at -1 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 91 smd rect (at -1.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 92 smd rect (at -2 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 93 smd rect (at -2.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 94 smd rect (at -3 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /hdmitx1/AVDD3V3))
    (pad 95 smd rect (at -3.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 96 smd rect (at -4 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(C17-Pad2)"))
    (pad 97 smd rect (at -4.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(C16-Pad2)"))
    (pad 98 smd rect (at -5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(C15-Pad2)"))
    (pad 99 smd rect (at -5.5 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(C13-Pad2)"))
    (pad 100 smd rect (at -6 -7.8 180) (size 1.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(C106-Pad1)"))
    (pad 40 smd rect (at 0 0 90) (size 6.2 6.2) (layers *.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 40 thru_hole circle (at -2.4 -2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -1.6 -2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -0.8 -2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 0 -2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 0.8 -2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 1.6 -2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 2.4 -2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -2.4 -1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -1.6 -1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -0.8 -1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 0 -1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 0.8 -1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 1.6 -1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 2.4 -1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -2.4 -0.8 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -1.6 -0.8 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 1.6 -0.8 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 2.4 -0.8 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -2.4 0 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -1.6 0 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 1.6 0 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 2.4 0 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -2.4 0.8 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -1.6 0.8 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 1.6 0.8 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 2.4 0.8 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -2.4 1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -1.6 1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -0.8 1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 0 1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 0.8 1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 1.6 1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 2.4 1.6 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -2.4 2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -1.6 2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at -0.8 2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 0 2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 0.8 2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 1.6 2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 2.4 2.4 90) (size 0.69 0.69) (drill 0.33) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 40 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (model Housings_QFP.3dshapes/TQFP-100_14x14mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:HDMI_CONN-10029449-111RLF (layer F.Cu) (tedit 58CEB976)
    (at 124.4 53.8 90)
    (fp_text reference J4 (at -10.38098 3.06324 180) (layer F.SilkS))
    (fp_text value HDMI_CONN (at 0.10414 5.22732 90) (layer F.Fab))
    (pad 17 thru_hole circle (at 7.25 0 90) (size 2.7 2.7) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 17 thru_hole circle (at -7.25 0 90) (size 2.7 2.7) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 17 thru_hole circle (at -7.85 4.95 90) (size 2.7 2.7) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 17 thru_hole circle (at 7.85 4.95 90) (size 2.7 2.7) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
    (pad 1 smd rect (at 4.75 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 65 /hdmitx1/TMDS_D2+))
    (pad 2 smd rect (at 4.25 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 3 smd rect (at 3.75 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 66 /hdmitx1/TMDS_D2-))
    (pad 4 smd rect (at 3.25 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 63 /hdmitx1/TMDS_D1+))
    (pad 5 smd rect (at 2.75 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 6 smd rect (at 2.25 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 64 /hdmitx1/TMDS_D1-))
    (pad 7 smd rect (at 1.75 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 61 /hdmitx1/TMDS_D0+))
    (pad 8 smd rect (at 1.25 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 9 smd rect (at 0.75 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 62 /hdmitx1/TMDS_D0-))
    (pad 10 smd rect (at 0.25 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 59 /hdmitx1/TMDS_CLK+))
    (pad 11 smd rect (at -0.25 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 12 smd rect (at -0.75 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 60 /hdmitx1/TMDS_CLK-))
    (pad 13 smd rect (at -1.25 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(J4-Pad13)"))
    (pad 14 smd rect (at -1.75 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(J4-Pad14)"))
    (pad 15 smd rect (at -2.25 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /hdmitx1/DDC_SCL))
    (pad 16 smd rect (at -2.75 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 46 /hdmitx1/DDC_SDA))
    (pad 17 smd rect (at -3.25 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 18 smd rect (at -3.75 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 207 /hdmitx1/5V_FUSED))
    (pad 19 smd rect (at -4.25 -1.1 90) (size 0.3 2.2) (layers F.Cu F.Paste F.Mask)
      (net 58 /hdmitx1/HPD))
  )
  (module custom_components:MS22 (layer F.Cu) (tedit 58E0D001)
    (at 125.04 66.52 270)
    (fp_text reference SW4 (at 0.44704 -5.51688 270) (layer F.SilkS))
    (fp_text value DPDT (at 0.0889 6.3246 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.65 -2.5 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 215 /hdmitx1/AV2_AUD_L))
    (pad 2 thru_hole circle (at -1.65 0 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 226 "Net-(J6-Pad2)"))
    (pad 3 thru_hole circle (at -1.65 2.5 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 217 /hdmitx1/AV1_AUD_L))
    (pad 4 thru_hole circle (at 1.65 -2.5 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 210 /hdmitx1/AV2_AUD_R))
    (pad 5 thru_hole circle (at 1.65 0 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 225 "Net-(J6-Pad3)"))
    (pad 6 thru_hole circle (at 1.65 2.5 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 212 /hdmitx1/AV1_AUD_R))
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 126.25 33.8 270)
    (attr smd)
    (fp_text reference R47 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 100k (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 222 /hdmitx1/AV3_AUD_L))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 123.97 33.79 270)
    (attr smd)
    (fp_text reference R48 (at -1.8288 0 540) (layer B.SilkS))
    (fp_text value 100k (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 219 /hdmitx1/AV3_AUD_R))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 58EA7E0B)
    (at 122.58 70.87 270)
    (attr smd)
    (fp_text reference R49 (at 1.82 -0.06 540) (layer B.SilkS))
    (fp_text value 100k (at 0 0 540) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 215 /hdmitx1/AV2_AUD_L))
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 120.21 70.87 90)
    (attr smd)
    (fp_text reference R50 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 100k (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 212 /hdmitx1/AV1_AUD_R))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 120.24 74.41 90)
    (attr smd)
    (fp_text reference R51 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 100k (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 210 /hdmitx1/AV2_AUD_R))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:SM0603_Resistor_libcms (layer B.Cu) (tedit 569D6DC4)
    (at 120.2 66.6 90)
    (attr smd)
    (fp_text reference R52 (at -1.8288 0 360) (layer B.SilkS))
    (fp_text value 100k (at 0 0 360) (layer B.SilkS))
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 217 /hdmitx1/AV1_AUD_L))
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 107 GND))
    (model smd\capacitors\C0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_components:ECS-3X9X (layer F.Cu) (tedit 58EE76AA)
    (at 103.861 69.647 90)
    (descr "Crystal, Quarz, Rundgehaeuse, round, vertical, stehend, Uhrenquarz, Diam. 3mm,")
    (tags "Crystal Quarz Rundgehaeuse round vertical stehend Uhrenquarz Diam. 3mm")
    (fp_text reference Y2 (at 0.36576 -2.59842 90) (layer F.SilkS))
    (fp_text value 24.576MHz (at 0.2413 2.5146 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.55 0 90) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 208 "Net-(C111-Pad1)"))
    (pad 2 thru_hole circle (at 0.55 0 90) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 209 "Net-(C112-Pad1)"))
  )
  (module custom_components:SLP2510P8 (layer F.Cu) (tedit 58EE78C0)
    (at 120.12 53.31 270)
    (fp_text reference D7 (at 2.04 0.01 360) (layer F.SilkS))
    (fp_text value RClamp0524P (at -2.95148 -1.6764 270) (layer F.Fab))
    (pad 3 smd rect (at 0 0 270) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 6 smd rect (at 1 -0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 60 /hdmitx1/TMDS_CLK-))
    (pad 7 smd rect (at 0.5 -0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 59 /hdmitx1/TMDS_CLK+))
    (pad 9 smd rect (at -0.5 -0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 62 /hdmitx1/TMDS_D0-))
    (pad 10 smd rect (at -1 -0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 61 /hdmitx1/TMDS_D0+))
    (pad 5 smd rect (at 1 0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 60 /hdmitx1/TMDS_CLK-))
    (pad 4 smd rect (at 0.5 0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 59 /hdmitx1/TMDS_CLK+))
    (pad 1 smd rect (at -1 0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 61 /hdmitx1/TMDS_D0+))
    (pad 2 smd rect (at -0.5 0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 62 /hdmitx1/TMDS_D0-))
    (pad 8 smd rect (at 0 0 270) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
  )
  (module custom_components:SLP2510P8 (layer F.Cu) (tedit 58EE78D5)
    (at 120.12 50.31 270)
    (fp_text reference D6 (at -1.95 -0.01 360) (layer F.SilkS))
    (fp_text value RClamp0524P (at -2.95148 -1.6764 270) (layer F.Fab))
    (pad 3 smd rect (at 0 0 270) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
    (pad 6 smd rect (at 1 -0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 64 /hdmitx1/TMDS_D1-))
    (pad 7 smd rect (at 0.5 -0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 63 /hdmitx1/TMDS_D1+))
    (pad 9 smd rect (at -0.5 -0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 66 /hdmitx1/TMDS_D2-))
    (pad 10 smd rect (at -1 -0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 65 /hdmitx1/TMDS_D2+))
    (pad 5 smd rect (at 1 0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 64 /hdmitx1/TMDS_D1-))
    (pad 4 smd rect (at 0.5 0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 63 /hdmitx1/TMDS_D1+))
    (pad 1 smd rect (at -1 0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 65 /hdmitx1/TMDS_D2+))
    (pad 2 smd rect (at -0.5 0.4497 270) (size 0.2 0.7) (layers F.Cu F.Paste F.Mask)
      (net 66 /hdmitx1/TMDS_D2-))
    (pad 8 smd rect (at 0 0 270) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 107 GND))
  )
  (module custom_components:SJ1-3533NG (layer F.Cu) (tedit 592EFBAD)
    (at 130.706 75.73 180)
    (fp_text reference J6 (at 1.60274 6.08584 180) (layer F.SilkS))
    (fp_text value SJ1-3533NG (at 5.60578 -4.09448 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.9 -1.1 180) (size 2.5 2.5) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 225 "Net-(J6-Pad3)"))
    (pad 2 thru_hole circle (at 2.4 -1.1 180) (size 2.5 2.5) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 226 "Net-(J6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0.9 180) (size 2.5 2.5) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
  )
  (module custom_components:SJ1-3533NG (layer F.Cu) (tedit 592EFBAD)
    (at 130.698 36.576 180)
    (fp_text reference J7 (at 1.60274 6.08584 180) (layer F.SilkS))
    (fp_text value SJ1-3533NG (at 5.60578 -4.09448 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.9 -1.1 180) (size 2.5 2.5) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 219 /hdmitx1/AV3_AUD_R))
    (pad 2 thru_hole circle (at 2.4 -1.1 180) (size 2.5 2.5) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 222 /hdmitx1/AV3_AUD_L))
    (pad 1 thru_hole circle (at 0 0.9 180) (size 2.5 2.5) (drill 2.1) (layers *.Cu *.Mask F.SilkS)
      (net 107 GND))
  )
  (gr_line (start 68.165 85.764) (end 7.368 85.764) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "OSSC v1.6" (at 81.473 71.526) (layer F.SilkS))
  (gr_line (start 68.165 82.25) (end 68.165 85.764) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.244 82.25) (end 68.165 82.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.244 85.764) (end 71.244 82.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.491 85.764) (end 71.244 85.764) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.491 82.248) (end 120.491 85.764) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.55 82.248) (end 120.491 82.248) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.55 85.764) (end 123.55 82.248) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 22.0228 17.018) (end 7.3638 17.018) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 22.0228 21.0557) (end 22.0228 17.018) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6789 21.0557) (end 22.0228 21.0557) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.6789 17.0171) (end 64.6789 21.0557) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 7.368 85.764) (end 7.368 17.018) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.55 85.764) (end 131.934 85.764) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.934 17.018) (end 131.934 85.764) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.691 17.018) (end 131.934 17.018) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 107) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.9332 85.739) (xy 7.3912 85.7644) (xy 7.3912 17.0184) (xy 131.9332 16.993)
      )
    )
  )
  (zone (net 107) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.9332 85.764) (xy 7.3912 85.764) (xy 7.3912 17.018) (xy 131.9332 17.018)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.161 69.574) (xy 50.163 71.538) (xy 43.617 71.534) (xy 43.615 69.558002)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.614 69.558) (xy 43.615 69.558) (xy 43.615 69.558002) (xy 43.614 69.558)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.429 57.3) (xy 53.041 57.296) (xy 53.043 58.891) (xy 40.432 58.886) (xy 40.431 57.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.144 43.987) (xy 39.726 43.992) (xy 39.732 56.599) (xy 38.143 56.598) (xy 38.146 43.989)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53.043 43.288) (xy 40.429 43.289) (xy 40.436 41.703) (xy 53.038 41.698)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.33 56.599) (xy 53.741 56.604) (xy 53.745 43.99) (xy 55.327 43.989)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.999 54.907) (xy 113.602 54.906) (xy 113.604 56.495) (xy 100.996 56.495) (xy 100.998 54.907)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.297 54.193) (xy 98.713 54.201) (xy 98.708 41.601) (xy 100.292 41.601)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.604 39.311) (xy 113.602 40.9) (xy 100.999 40.893) (xy 100.998001 39.306002)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.993 39.306) (xy 100.998 39.305) (xy 100.998001 39.306002)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.308 41.598) (xy 114.311 54.188) (xy 115.896 54.199) (xy 115.891 41.601) (xy 114.311 41.598)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.347 54.712) (xy 86.346 56.298) (xy 68.252 56.289) (xy 68.246 54.709)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65.712 35.649) (xy 67.295 35.646) (xy 67.295 53.753) (xy 65.706 53.756)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.352 33.108) (xy 86.354 34.696) (xy 68.246 34.695) (xy 68.244 33.103)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.891 35.648) (xy 88.894 53.755) (xy 87.309 53.755) (xy 87.308 35.646)
      )
    )
  )
)
