<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="29.19" y2="0" width="0" layer="20"/>
<wire x1="29.19" y1="0" x2="29.19" y2="19.99" width="0" layer="20"/>
<wire x1="29.19" y1="19.99" x2="0" y2="19.99" width="0" layer="20"/>
<wire x1="0" y1="19.99" x2="0" y2="0" width="0" layer="20"/>
<text>Laser Power Adapter</text>
<text>2023 laserlance.com</text>
</plain>
<libraries>
<library name="Connector">
<description>&lt;b&gt;Pin Headers,Terminal blocks, D-Sub, Backplane, FFC/FPC, Socket</description>
<packages>
<package name="B2B-XH-A">
</package>
</packages>
</library>
<library name="Connector">
<description>&lt;b&gt;Pin Headers,Terminal blocks, D-Sub, Backplane, FFC/FPC, Socket</description>
<packages>
<package name="B2B-XH-A">
</package>
</packages>
</library>
<library name="Resistor">
<description>&lt;B&gt;Resistors, Potentiometers, TrimPot</description>
<packages>
<package name="RESAD1176W63L850D250B">
<description>AXIAL Resistor, 11.76 mm pitch, 8.5 mm body length, 2.5 mm body diameter
&lt;p&gt;AXIAL Resistor package with 11.76 mm pitch, 0.63 mm lead diameter, 8.5 mm body length and 2.5 mm body diameter&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Resistor">
<description>&lt;B&gt;Resistors, Potentiometers, TrimPot</description>
<packages>
<package name="RESAD1176W63L850D250B">
<description>AXIAL Resistor, 11.76 mm pitch, 8.5 mm body length, 2.5 mm body diameter
&lt;p&gt;AXIAL Resistor package with 11.76 mm pitch, 0.63 mm lead diameter, 8.5 mm body length and 2.5 mm body diameter&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="12VIN" library="Connector" package="B2B-XH-A" value="3A/250V">
<attribute name="CATEGORY" value="CONNECTOR"/>
<attribute name="DESCRIPTION" value="2.5mm pitch/disconnectable crimp style connector"/>
<attribute name="MANUFACTURER" value="JST (XH CONNECTOR)"/>
<attribute name="MPN" value="B2B-XH-A"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value="-25°C ~ 85°C"/>
<attribute name="PART_STATUS" value="ACTIVE"/>
<attribute name="ROHS_COMPLIANT" value="COMPLIANT"/>
<attribute name="SERIES" value="B_B-XH-A"/>
<attribute name="SUB_CATEGORY" value="Through hole connector"/>
<attribute name="TYPE" value="top entry"/>
<attribute name="VALUE" value="3A/250V"/>
</element>
<element name="FAN_IN" library="Connector" package="B2B-XH-A" value="3A/250V">
<attribute name="CATEGORY" value="CONNECTOR"/>
<attribute name="DESCRIPTION" value="2.5mm pitch/disconnectable crimp style connector"/>
<attribute name="MANUFACTURER" value="JST (XH CONNECTOR)"/>
<attribute name="MPN" value="B2B-XH-A"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value="-25°C ~ 85°C"/>
<attribute name="PART_STATUS" value="ACTIVE"/>
<attribute name="ROHS_COMPLIANT" value="COMPLIANT"/>
<attribute name="SERIES" value="B_B-XH-A"/>
<attribute name="SUB_CATEGORY" value="Through hole connector"/>
<attribute name="TYPE" value="top entry"/>
<attribute name="VALUE" value="3A/250V"/>
</element>
<element name="LASER_POWER" library="Connector" package="B2B-XH-A" value="3A/250V">
<attribute name="CATEGORY" value="CONNECTOR"/>
<attribute name="DESCRIPTION" value="2.5mm pitch/disconnectable crimp style connector"/>
<attribute name="MANUFACTURER" value="JST (XH CONNECTOR)"/>
<attribute name="MPN" value="B2B-XH-A"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value="-25°C ~ 85°C"/>
<attribute name="PART_STATUS" value="ACTIVE"/>
<attribute name="ROHS_COMPLIANT" value="COMPLIANT"/>
<attribute name="SERIES" value="B_B-XH-A"/>
<attribute name="SUB_CATEGORY" value="Through hole connector"/>
<attribute name="TYPE" value="top entry"/>
<attribute name="VALUE" value="3A/250V"/>
</element>
<element name="R1" library="Resistor" package="RESAD1176W63L850D250B" value="18K 1/4W">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</element>
<element name="R2" library="Resistor" package="RESAD1176W63L850D250B" value="4.7K 1/4W">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
</element>
<element name="TTL" library="Connector" package="B2B-XH-A" value="3A/250V">
<attribute name="CATEGORY" value="CONNECTOR"/>
<attribute name="DESCRIPTION" value="2.5mm pitch/disconnectable crimp style connector"/>
<attribute name="MANUFACTURER" value="JST (XH CONNECTOR)"/>
<attribute name="MPN" value="B2B-XH-A"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value="-25°C ~ 85°C"/>
<attribute name="PART_STATUS" value="ACTIVE"/>
<attribute name="ROHS_COMPLIANT" value="COMPLIANT"/>
<attribute name="SERIES" value="B_B-XH-A"/>
<attribute name="SUB_CATEGORY" value="Through hole connector"/>
<attribute name="TYPE" value="top entry"/>
<attribute name="VALUE" value="3A/250V"/>
</element>
</elements>
<signals>
<signal name="+12V">
<contactref element="12VIN" pad="1"/>
<contactref element="LASER_POWER" pad="2"/>
</signal>
<signal name="GND">
<contactref element="12VIN" pad="2"/>
<contactref element="FAN_IN" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="TTL" pad="1"/>
<contactref element="LASER_POWER" pad="1"/>
</signal>
<signal name="FAN_INPUT">
<contactref element="FAN_IN" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="TTL_OUT">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="TTL" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
