(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "D")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 389 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 535.5 250 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0 180) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0 180) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 379 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 470.5 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 423 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 433 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 480.5 250 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0 180) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0 180) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 355 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 525.51 250 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0 180) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0 180) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 490.5 250 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0 180) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0 180) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 335 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 515.5 250 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0 180) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0 180) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 443 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 399 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:HVC2512" (layer "F.Cu")
    (at 345 250)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "REF**" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "HVC2512" (at 0 2.62) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (pad "2" smd roundrect (at 2.95 0) (size 2.1 3.5) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.2040819048))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:Resistor-link-loop-small" (layer "B.Cu")
    (at 323 250 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 270 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 6 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -6) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 455 282 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 411 218 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 455 218 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 411 238.2 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 455 261.8 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 411 261.8 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 411 282 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 323 282 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 323 218 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 367 261.8 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 323 238.2 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:Resistor-link-loop-small" (layer "B.Cu")
    (at 367 250 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 270 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 6 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -6) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:Resistor-link-loop-small" (layer "B.Cu")
    (at 455 250 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 270 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 6 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -6) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 367 218 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 506 228)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75 -360) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75 -360) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:Resistor-link-loop-small" (layer "B.Cu")
    (at 411 250 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 270 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 6 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -6) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 90) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 90) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 455 238.2 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:Resistor-link-loop" (layer "B.Cu")
    (at 506 250)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 -180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 90 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 15.3) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -15.3 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 270) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 270) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 323 261.8 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 545 228)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75 -360) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75 -360) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 367 282 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 506 272)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75 -360) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75 -360) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 367 238.2 180)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0 180) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0 180) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:Resistor-link-loop" (layer "B.Cu")
    (at 545 250)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 -180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Resistor-link-loop" (at -2.54 5.08 90 unlocked) (layer "B.Fab") hide)
    (pad "1" connect roundrect (at 0 15.3) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "2" connect roundrect (at 0 -15.3 180) (size 1.25 2.5) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25))
    (pad "3" thru_hole circle (at -2.65 -1 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at -2.65 0 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "3" connect roundrect (at -2.65 0 270) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "3" thru_hole circle (at -2.65 1 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 -1 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" thru_hole circle (at 2.65 0 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "4" connect roundrect (at 2.65 0 270) (size 3.5 1.25) (layers "F.Cu") (roundrect_rratio 0.25)
      (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.65 1 270) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Library:MountingHole_4.3mm_M4_DIN965_Pad_TopOnly" (layer "B.Cu")
    (at 545 272)
    (descr "Mounting Hole 4.3mm, M4, DIN965")
    (tags "mounting hole 4.3mm m4 din965")
    (property "Sheetfile" "mockup_resistor_link_barrel_A.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "HD1" (at 0 4.75 -360) (layer "B.Fab") hide)
    (fp_text value "MountingHole_Pad" (at 0 -4.75 -360) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.1) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 7.9 7.9) (layers "B.Cu" "B.Mask"))
    (pad "2" thru_hole circle (at -3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 3 0) (size 0.5 0.5) (drill 0.3) (layers "*.Cu" "*.Mask"))
  )
  (gr_arc (start 326.790019 253.708492) (mid 327.152508 253.203302) (end 327.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.675 247.51) (mid 323 246.185) (end 324.325 247.51)
    (layer "Edge.Cuts"))
  (gr_line (start 546.325 238.01) (end 546.325 262.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 326.790019 253.708492) (mid 326.052003 255.056744) (end 324.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_line (start 509.975 244.01) (end 509.975 238.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 365.142337 256.024216) (mid 363.947997 255.056744) (end 363.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_line (start 371 238.21) (end 371 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 415 282.01) (mid 411 286.01) (end 407 282.01)
    (layer "Edge.Cuts"))
  (gr_line (start 543.675 233.611705) (end 543.675 232.436553)
    (layer "Edge.Cuts"))
  (gr_arc (start 509.975 262.01) (mid 509.404765 264.061393) (end 507.857663 265.524216)
    (layer "Edge.Cuts"))
  (gr_arc (start 368.857663 243.995784) (mid 368.468455 243.627779) (end 368.325 243.111705)
    (layer "Edge.Cuts"))
  (gr_arc (start 507.857663 234.495784) (mid 509.40478 235.958605) (end 509.975 238.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 319 218.01) (mid 323 214.01) (end 327 218.01)
    (layer "Edge.Cuts"))
  (gr_circle (center 545 250.01) (end 544.99 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_arc (start 507.86 268.468757) (mid 507.469137 268.100656) (end 507.325 267.583447)
    (layer "Edge.Cuts"))
  (gr_line (start 327 261.81) (end 327 282.01)
    (layer "Edge.Cuts"))
  (gr_line (start 365.675 243.111705) (end 365.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 453.675 252.51) (end 453.675 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.14 241.751243) (mid 321.530878 242.119339) (end 321.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 543.14 231.551243) (mid 545 224.01) (end 546.86 231.551243)
    (layer "Edge.Cuts"))
  (gr_line (start 501.025 245.01) (end 482.825 245.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 412.857663 243.995784) (mid 414.052003 244.963256) (end 414.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 453.14 241.751243) (mid 451.576551 240.278816) (end 451 238.21)
    (layer "Edge.Cuts"))
  (gr_arc (start 543.142337 265.524216) (mid 543.531547 265.892221) (end 543.675 266.408295)
    (layer "Edge.Cuts"))
  (gr_line (start 456.325 243.111705) (end 456.325 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 453.675 256.908295) (end 453.675 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 507.325 262.01) (mid 506 263.335) (end 504.675 262.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 548.975 262.01) (mid 548.404764 264.061392) (end 546.857663 265.524216)
    (layer "Edge.Cuts"))
  (gr_arc (start 507.325 232.436553) (mid 507.469163 231.919369) (end 507.86 231.551243)
    (layer "Edge.Cuts"))
  (gr_arc (start 456.325 242.636553) (mid 456.469146 242.119354) (end 456.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_line (start 409.675 252.51) (end 409.675 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 319 261.81) (mid 319.576551 259.741184) (end 321.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 370.790019 253.708492) (mid 370.052003 255.056744) (end 368.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 507.325 266.408295) (mid 507.468474 265.89224) (end 507.857663 265.524216)
    (layer "Edge.Cuts"))
  (gr_arc (start 504.675 233.611705) (mid 504.531559 234.127792) (end 504.142337 234.495784)
    (layer "Edge.Cuts"))
  (gr_arc (start 407 261.81) (mid 407.576551 259.741184) (end 409.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 456.86 258.268757) (mid 458.423449 259.741184) (end 459 261.81)
    (layer "Edge.Cuts"))
  (gr_line (start 541.025 256.01) (end 541.025 262.01)
    (layer "Edge.Cuts"))
  (gr_line (start 548.975 256.01) (end 548.975 262.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 543.142337 265.524216) (mid 541.595237 264.061391) (end 541.025 262.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 365.675 247.51) (mid 367 246.185) (end 368.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 368.86 258.268757) (mid 370.423449 259.741184) (end 371 261.81)
    (layer "Edge.Cuts"))
  (gr_arc (start 456.325 252.51) (mid 455 253.835) (end 453.675 252.51)
    (layer "Edge.Cuts"))
  (gr_line (start 507.325 266.408295) (end 507.325 267.583447)
    (layer "Edge.Cuts"))
  (gr_arc (start 414.790019 253.708492) (mid 414.052003 255.056744) (end 412.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 453.14 241.751243) (mid 453.530878 242.119339) (end 453.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 324.325 243.111705) (end 324.325 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 362.256518 247.01) (end 327.743482 247.01)
    (layer "Edge.Cuts"))
  (gr_line (start 451 238.21) (end 451 218.01)
    (layer "Edge.Cuts"))
  (gr_circle (center 323 250.01) (end 323.01 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_arc (start 546.857663 234.495784) (mid 546.468455 234.127779) (end 546.325 233.611705)
    (layer "Edge.Cuts"))
  (gr_arc (start 546.325 232.436553) (mid 546.469159 231.919362) (end 546.86 231.551243)
    (layer "Edge.Cuts"))
  (gr_arc (start 502.025 238.01) (mid 502.595237 235.95861) (end 504.142337 234.495784)
    (layer "Edge.Cuts"))
  (gr_line (start 406.256518 253.01) (end 371.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_line (start 546.325 233.611705) (end 546.325 232.436553)
    (layer "Edge.Cuts"))
  (gr_line (start 362.256518 253.01) (end 327.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 363 218.01) (mid 367 214.01) (end 371 218.01)
    (layer "Edge.Cuts"))
  (gr_line (start 543.675 266.408295) (end 543.675 267.583447)
    (layer "Edge.Cuts"))
  (gr_line (start 406.256518 247.01) (end 371.743482 247.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.14 241.751243) (mid 319.576551 240.278816) (end 319 238.21)
    (layer "Edge.Cuts"))
  (gr_line (start 368.325 256.908295) (end 368.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 543.14 231.551243) (mid 543.53088 231.919339) (end 543.675 232.436553)
    (layer "Edge.Cuts"))
  (gr_line (start 365.675 252.51) (end 365.675 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.675 257.383447) (mid 321.530854 257.900646) (end 321.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 543.675 267.583447) (mid 543.530843 268.10064) (end 543.14 268.468757)
    (layer "Edge.Cuts"))
  (gr_arc (start 456.857663 243.995784) (mid 457.368647 244.317801) (end 457.824944 244.713518)
    (layer "Edge.Cuts"))
  (gr_line (start 407 261.81) (end 407 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 412.325 252.51) (mid 411 253.835) (end 409.675 252.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 319.209981 246.311508) (mid 319.947997 244.963256) (end 321.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_line (start 507.325 233.611705) (end 507.325 232.436553)
    (layer "Edge.Cuts"))
  (gr_line (start 509.975 256.01) (end 509.975 262.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.325 256.908295) (mid 324.468457 256.392223) (end 324.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_line (start 415 261.81) (end 415 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 409.675 243.111705) (mid 409.531543 243.627777) (end 409.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 456.325 256.908295) (mid 456.468457 256.392223) (end 456.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 543.675 238.01) (mid 545 236.685) (end 546.325 238.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 365.14 241.751243) (mid 365.530878 242.119339) (end 365.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 456.325 252.51) (end 456.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.325 242.636553) (mid 324.469146 242.119354) (end 324.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_line (start 456.325 256.908295) (end 456.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 456.857663 243.995784) (mid 456.468455 243.627779) (end 456.325 243.111705)
    (layer "Edge.Cuts"))
  (gr_arc (start 453.142337 256.024216) (mid 451.947997 255.056744) (end 451.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_line (start 324.325 256.908295) (end 324.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 412.86 258.268757) (mid 412.469122 257.900661) (end 412.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_line (start 368.325 243.111705) (end 368.325 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 543.675 238.01) (end 543.675 262.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 457.824944 255.306482) (mid 457.368647 255.702199) (end 456.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 507.857663 234.495784) (mid 507.46847 234.127775) (end 507.325 233.611705)
    (layer "Edge.Cuts"))
  (gr_arc (start 501.025 255.01) (mid 501.732122 255.302891) (end 502.025 256.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 409.142337 256.024216) (mid 409.531545 256.392221) (end 409.675 256.908295)
    (layer "Edge.Cuts"))
  (gr_line (start 502.025 244.01) (end 502.025 238.01)
    (layer "Edge.Cuts"))
  (gr_line (start 502.025 256.01) (end 502.025 262.01)
    (layer "Edge.Cuts"))
  (gr_line (start 450.256518 247.01) (end 415.743482 247.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 453.675 243.111705) (mid 453.531543 243.627777) (end 453.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_line (start 412.325 256.908295) (end 412.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 371.743482 247.01) (mid 371.152518 246.816685) (end 370.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 368.86 258.268757) (mid 368.469122 257.900661) (end 368.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 409.142337 256.024216) (mid 407.947997 255.056744) (end 407.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 543.675 233.611705) (mid 543.531541 234.127775) (end 543.142337 234.495784)
    (layer "Edge.Cuts"))
  (gr_line (start 546.325 266.408295) (end 546.325 267.583447)
    (layer "Edge.Cuts"))
  (gr_line (start 321.675 243.111705) (end 321.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 504.675 238.01) (end 504.675 262.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 459 282.01) (mid 455 286.01) (end 451 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 368.325 242.636553) (mid 368.469146 242.119354) (end 368.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_line (start 368.325 252.51) (end 368.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 451 218.01) (mid 455 214.01) (end 459 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 546.857663 234.495784) (mid 548.404765 235.958608) (end 548.975 238.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 504.675 238.01) (mid 506 236.685) (end 507.325 238.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 365.675 243.111705) (mid 365.531543 243.627777) (end 365.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 327 282.01) (mid 323 286.01) (end 319 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 450.256518 253.01) (mid 450.847482 253.203315) (end 451.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 327.743482 247.01) (mid 327.152518 246.816685) (end 326.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 412.857663 243.995784) (mid 412.468455 243.627779) (end 412.325 243.111705)
    (layer "Edge.Cuts"))
  (gr_line (start 409.675 256.908295) (end 409.675 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 546.86 268.468757) (mid 545 276.01) (end 543.14 268.468757)
    (layer "Edge.Cuts"))
  (gr_arc (start 504.14 231.551243) (mid 504.530857 231.919345) (end 504.675 232.436553)
    (layer "Edge.Cuts"))
  (gr_line (start 450.256518 253.01) (end 415.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_line (start 407 238.21) (end 407 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 409.675 257.383447) (mid 409.530854 257.900646) (end 409.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.142337 256.024216) (mid 319.947997 255.056744) (end 319.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.857663 243.995784) (mid 326.052003 244.963256) (end 326.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.675 243.111705) (mid 321.531543 243.627777) (end 321.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 457.824944 255.306482) (mid 458.1506 255.087089) (end 458.535622 255.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 365.14 241.751243) (mid 363.576551 240.278816) (end 363 238.21)
    (layer "Edge.Cuts"))
  (gr_arc (start 507.86 268.468757) (mid 506 276.01) (end 504.14 268.468757)
    (layer "Edge.Cuts"))
  (gr_arc (start 368.325 256.908295) (mid 368.468457 256.392223) (end 368.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_arc (start 502.025 244.01) (mid 501.732122 244.717135) (end 501.025 245.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 412.86 258.268757) (mid 414.423449 259.741184) (end 415 261.81)
    (layer "Edge.Cuts"))
  (gr_line (start 321.675 252.51) (end 321.675 247.51)
    (layer "Edge.Cuts"))
  (gr_line (start 458.535622 255.01) (end 471.35 255.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 546.325 266.408295) (mid 546.468457 265.892223) (end 546.857663 265.524216)
    (layer "Edge.Cuts"))
  (gr_line (start 319.209981 246.311508) (end 319.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_line (start 540.025 245.01) (end 510.975 245.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 368.857663 243.995784) (mid 370.052003 244.963256) (end 370.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_arc (start 459 238.21) (mid 458.423449 240.278816) (end 456.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 546.86 268.468757) (mid 546.469123 268.10066) (end 546.325 267.583447)
    (layer "Edge.Cuts"))
  (gr_arc (start 368.325 252.51) (mid 367 253.835) (end 365.675 252.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 415.743482 247.01) (mid 415.152518 246.816685) (end 414.790019 246.311508)
    (layer "Edge.Cuts"))
  (gr_line (start 321.675 256.908295) (end 321.675 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 458.535622 245.01) (mid 458.150601 244.932908) (end 457.824944 244.713518)
    (layer "Edge.Cuts"))
  (gr_line (start 458.535622 245.01) (end 471.35 245.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 363 261.81) (mid 363.576551 259.741184) (end 365.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_circle (center 506 250.01) (end 505.99 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_line (start 324.325 252.51) (end 324.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 504.14 231.551243) (mid 506 224.01) (end 507.86 231.551243)
    (layer "Edge.Cuts"))
  (gr_line (start 319 261.81) (end 319 282.01)
    (layer "Edge.Cuts"))
  (gr_circle (center 411 250.01) (end 411.01 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_arc (start 371 282.01) (mid 367 286.01) (end 363 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 546.325 262.01) (mid 545 263.335) (end 543.675 262.01)
    (layer "Edge.Cuts"))
  (gr_line (start 409.675 243.111705) (end 409.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 453.142337 256.024216) (mid 453.531545 256.392221) (end 453.675 256.908295)
    (layer "Edge.Cuts"))
  (gr_arc (start 541.025 238.01) (mid 541.595236 235.958608) (end 543.142337 234.495784)
    (layer "Edge.Cuts"))
  (gr_arc (start 407.209981 246.311508) (mid 406.847492 246.816698) (end 406.256518 247.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 453.675 247.51) (mid 455 246.185) (end 456.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 540.025 255.01) (mid 540.732122 255.302891) (end 541.025 256.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 327 238.21) (mid 326.423449 240.278816) (end 324.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 365.675 257.383447) (mid 365.530854 257.900646) (end 365.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 407 218.01) (mid 411 214.01) (end 415 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 451 261.81) (mid 451.576551 259.741184) (end 453.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_arc (start 412.325 256.908295) (mid 412.468457 256.392223) (end 412.857663 256.024216)
    (layer "Edge.Cuts"))
  (gr_line (start 453.675 243.111705) (end 453.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 370.790019 253.708492) (mid 371.152508 253.203302) (end 371.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.325 252.51) (mid 323 253.835) (end 321.675 252.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 541.025 244.01) (mid 540.732108 244.717109) (end 540.025 245.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 415 238.21) (mid 414.423449 240.278816) (end 412.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 453.675 257.383447) (mid 453.530854 257.900646) (end 453.14 258.268757)
    (layer "Edge.Cuts"))
  (gr_line (start 319 238.21) (end 319 218.01)
    (layer "Edge.Cuts"))
  (gr_line (start 540.025 255.01) (end 510.975 255.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 409.14 241.751243) (mid 409.530878 242.119339) (end 409.675 242.636553)
    (layer "Edge.Cuts"))
  (gr_arc (start 362.256518 253.01) (mid 362.847482 253.203315) (end 363.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_line (start 415 238.21) (end 415 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 321.142337 256.024216) (mid 321.531545 256.392221) (end 321.675 256.908295)
    (layer "Edge.Cuts"))
  (gr_arc (start 371 238.21) (mid 370.423449 240.278816) (end 368.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_line (start 459 261.81) (end 459 282.01)
    (layer "Edge.Cuts"))
  (gr_circle (center 455 250.01) (end 455.01 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_arc (start 504.142337 265.524216) (mid 502.595252 264.061388) (end 502.025 262.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 504.675 267.583447) (mid 504.530882 268.100659) (end 504.14 268.468757)
    (layer "Edge.Cuts"))
  (gr_circle (center 367 250.01) (end 367.01 250.01)
    (fill solid) (layer "Edge.Cuts"))
  (gr_arc (start 451.209981 246.311508) (mid 450.847492 246.816698) (end 450.256518 247.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 504.142337 265.524216) (mid 504.531525 265.892226) (end 504.675 266.408295)
    (layer "Edge.Cuts"))
  (gr_line (start 482.825 245.01) (end 471.35 245.01)
    (layer "Edge.Cuts"))
  (gr_line (start 504.675 266.408295) (end 504.675 267.583447)
    (layer "Edge.Cuts"))
  (gr_line (start 548.975 256.01) (end 548.975 244.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 412.325 242.636553) (mid 412.469146 242.119354) (end 412.86 241.751243)
    (layer "Edge.Cuts"))
  (gr_arc (start 409.675 247.51) (mid 411 246.185) (end 412.325 247.51)
    (layer "Edge.Cuts"))
  (gr_arc (start 363.209981 246.311508) (mid 362.847492 246.816698) (end 362.256518 247.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 407.209981 246.311508) (mid 407.947997 244.963256) (end 409.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 365.142337 256.024216) (mid 365.531545 256.392221) (end 365.675 256.908295)
    (layer "Edge.Cuts"))
  (gr_line (start 365.675 256.908295) (end 365.675 257.383447)
    (layer "Edge.Cuts"))
  (gr_line (start 482.825 255.01) (end 471.35 255.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.857663 243.995784) (mid 324.468455 243.627779) (end 324.325 243.111705)
    (layer "Edge.Cuts"))
  (gr_arc (start 409.14 241.751243) (mid 407.576551 240.278816) (end 407 238.21)
    (layer "Edge.Cuts"))
  (gr_line (start 412.325 252.51) (end 412.325 247.51)
    (layer "Edge.Cuts"))
  (gr_line (start 507.325 238.01) (end 507.325 262.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 406.256518 253.01) (mid 406.847482 253.203315) (end 407.209981 253.708492)
    (layer "Edge.Cuts"))
  (gr_line (start 412.325 243.111705) (end 412.325 242.636553)
    (layer "Edge.Cuts"))
  (gr_line (start 501.025 255.01) (end 482.825 255.01)
    (layer "Edge.Cuts"))
  (gr_line (start 363 238.21) (end 363 218.01)
    (layer "Edge.Cuts"))
  (gr_line (start 327 238.21) (end 327 218.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 363.209981 246.311508) (mid 363.947997 244.963256) (end 365.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 509.975 256.01) (mid 510.267908 255.302921) (end 510.975 255.01)
    (layer "Edge.Cuts"))
  (gr_line (start 363 261.81) (end 363 282.01)
    (layer "Edge.Cuts"))
  (gr_line (start 548.975 244.01) (end 548.975 238.01)
    (layer "Edge.Cuts"))
  (gr_line (start 459 238.21) (end 459 218.01)
    (layer "Edge.Cuts"))
  (gr_line (start 371 261.81) (end 371 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.86 258.268757) (mid 324.469122 257.900661) (end 324.325 257.383447)
    (layer "Edge.Cuts"))
  (gr_arc (start 324.86 258.268757) (mid 326.423449 259.741184) (end 327 261.81)
    (layer "Edge.Cuts"))
  (gr_line (start 504.675 233.611705) (end 504.675 232.436553)
    (layer "Edge.Cuts"))
  (gr_line (start 541.025 244.01) (end 541.025 238.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 414.790019 253.708492) (mid 415.152508 253.203302) (end 415.743482 253.01)
    (layer "Edge.Cuts"))
  (gr_line (start 451 261.81) (end 451 282.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 451.209981 246.311508) (mid 451.947997 244.963256) (end 453.142337 243.995784)
    (layer "Edge.Cuts"))
  (gr_arc (start 510.975 245.01) (mid 510.267908 244.717104) (end 509.975 244.01)
    (layer "Edge.Cuts"))
  (gr_arc (start 456.86 258.268757) (mid 456.469122 257.900661) (end 456.325 257.383447)
    (layer "Edge.Cuts"))
  (zone (net 0) (net_name "") (layers "*.Mask") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 565 200)
        (xy 310 200)
        (xy 310 300)
        (xy 565 300)
      )
    )
  )
)
