(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 72)
    (no_connects 0)
    (area 114.138143 76.366 167.324 123.22519)
    (thickness 1.6)
    (drawings 67)
    (tracks 190)
    (zones 0)
    (modules 37)
    (nets 24)
  )
  (page USLetter)
  (title_block
    (title "Buck Converter (Step-Down Voltage Regulator)")
    (rev E3-0-0)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.381)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.127)
    (edge_width 0.0254)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.025400)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(D3-Pad1)")
  (net 4 +9V)
  (net 5 +6V)
  (net 6 +BATT)
  (net 7 "Net-(D4-Pad1)")
  (net 8 "Net-(D5-Pad1)")
  (net 9 +12V)
  (net 10 /~RST)
  (net 11 /ADC3)
  (net 12 /ADC2)
  (net 13 /MOSI)
  (net 14 /MISO)
  (net 15 /SCK)
  (net 16 "Net-(D6-Pad1)")
  (net 17 /GREEN)
  (net 18 /BLUE)
  (net 19 "Net-(IC1-Pad5)")
  (net 20 /RED)
  (net 21 /ADC1)
  (net 22 /OPT)
  (net 23 "Net-(POT1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /ADC1)
    (add_net /ADC2)
    (add_net /ADC3)
    (add_net /BLUE)
    (add_net /GREEN)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /OPT)
    (add_net /RED)
    (add_net /SCK)
    (add_net /~RST)
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(POT1-Pad1)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 1.27)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +6V)
    (add_net +9V)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(D3-Pad1)")
  )
  (module lib:pcc_pot (layer F.Cu) (tedit 59764E79)
    (at 151.765 82.55)
    (fp_text reference POT1 (at 2.54 -2.54 180) (layer F.SilkS))
    (fp_text value 20k (at 0.635 2.54) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 5.08 0) (size 1.51 1.51) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 +6V))
    (pad 1 thru_hole circle (at 0 0) (size 1.51 1.51) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(POT1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 1.51 1.51) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(POT1-Pad1)"))
  )
  (module lib:Inductor_075in (layer F.Cu) (tedit 59813469)
    (at 139.7 93.98)
    (fp_text reference L1 (at 0 0.635) (layer F.SilkS))
    (fp_text value 100u (at 0 10.795) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.35 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 5 +6V))
    (pad 2 thru_hole circle (at -6.35 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D3-Pad1)"))
  )
  (module lib:pcc-Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5988BF13)
    (at 146.685 80.645)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at 2.54 3.81 180) (layer F.SilkS))
    (fp_text value uC_Bypass (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /OPT))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes_ThroughHole:D_DO-201AD_P5.08mm_Vertical_AnodeUp (layer F.Cu) (tedit 59DD0E15)
    (at 127.635 104.14 270)
    (descr "D, DO-201AD series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Vertical pin pitch 5.08mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at -3.175 -1.905 540) (layer F.SilkS))
    (fp_text value SR340 (at 2.54 5.438 270) (layer F.Fab))
    (fp_text user K (at -3.36 0 270) (layer F.Fab))
    (fp_text user %R (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 +9V))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 +BATT))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P5.08mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:pcc-barrel_jack placed (layer F.Cu) (tedit 59765A95)
    (at 114.935 98.425)
    (fp_text reference P1 (at 4.826 -1.778) (layer F.SilkS))
    (fp_text value +Vin1 (at 7.112 -10.033) (layer F.Fab))
    (pad 3 thru_hole rect (at 10.7 0.2) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole rect (at 7.7 -4.5) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 13.7 -4.6) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
  )
  (module Diodes_ThroughHole:D_DO-201AD_P15.24mm_Horizontal (layer B.Cu) (tedit 59768731)
    (at 132.08 87.376)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D3 (at 7.62 -3.556) (layer B.SilkS))
    (fp_text value 1N5822 (at 7.62 -3.66) (layer B.Fab))
    (fp_text user %R (at 7.62 -3.556) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 59C172EB)
    (at 147.32 107.95 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.905 540) (layer B.SilkS))
    (fp_text value 2.2uF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 -1.905 540) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D13.0mm_P5.00mm (layer F.Cu) (tedit 59DF8573)
    (at 154.94 97.155)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=13mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 13mm Electrolytic Capacitor")
    (fp_text reference C3 (at -2.54 5.715) (layer F.SilkS))
    (fp_text value 1000u (at 2.5 7.81) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 +6V))
    (pad 2 thru_hole circle (at 5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D13.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 59DCF1FA)
    (at 132.715 114.3 180)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D4 (at 0 1.905 360) (layer F.SilkS))
    (fp_text value Red (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 59DCF205)
    (at 139.7 114.3 180)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D5 (at 0 1.905 360) (layer F.SilkS))
    (fp_text value Green (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module lib:pcc-TerminalBlock (layer F.Cu) (tedit 56E9A973)
    (at 119.38 103.505 270)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P2 (at -0.635 -3.81 270) (layer F.SilkS) hide)
    (fp_text value +Vin2 (at 5.08 -3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 6 +BATT))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5B3E48FE)
    (at 152.4 88.9)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.778 1.524 180) (layer F.SilkS))
    (fp_text value 1K (at 1.27 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(POT1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59DD0D28)
    (at 132.715 114.3)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.905 180) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 20 /RED))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59DD0D24)
    (at 139.7 114.3)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.905 180) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 17 /GREEN))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59DD0D1B)
    (at 146.685 114.3)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -1.905 180) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 18 /BLUE))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59DD0D48)
    (at 132.08 99.06 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 3.81 0 360) (layer B.SilkS))
    (fp_text value 39K (at 0 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 -1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 9 +12V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 21 /ADC1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59DD0D54)
    (at 134.62 99.06 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -3.81 0 180) (layer B.SilkS))
    (fp_text value 2.2K (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.905 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 21 /ADC1))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59DD0D41)
    (at 138.43 99.06 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 3.81 0 360) (layer B.SilkS))
    (fp_text value 39K (at 0 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 1.905 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 6 +BATT))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 /ADC2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 59DD0E28)
    (at 132.715 109.22 90)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U1 (at -0.635 -1.905 360) (layer F.SilkS))
    (fp_text value LM2950-50 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at -0.508 -2.413 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +9V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module lib:LM2576_Vert_min2 (layer F.Cu) (tedit 56DDA985)
    (at 139.7 81.28)
    (descr Pentawatt_Neutral_Straight_Vertical_TO220-5-T05A)
    (tags Pentawatt_Neutral_Straight_Vertical_TO220-5-T05A)
    (fp_text reference U2 (at -4.445 2.54) (layer F.SilkS))
    (fp_text value LM2576 (at 0 1.27 180) (layer F.Fab))
    (fp_text user 1 (at -4.445 0.635) (layer F.SilkS))
    (pad 3 thru_hole oval (at 0 -0.59944 90) (size 2.49936 1.50114) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole oval (at -3.404 -0.635 90) (size 2.49936 1.50114) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 4 +9V))
    (pad 5 thru_hole oval (at 3.404 -0.635 90) (size 2.49936 1.50114) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 22 /OPT))
    (pad 4 thru_hole oval (at 1.702 -0.635 90) (size 2.49936 1.50114) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(POT1-Pad1)"))
    (pad 2 thru_hole oval (at -1.702 -0.635 90) (size 2.49936 1.50114) (drill 1.09982) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D3-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/Pentawatt_Neutral_Straight_Vertical_TO220-5-T05A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-201AD_P5.08mm_Vertical_KathodeUp (layer F.Cu) (tedit 5977B265)
    (at 123.825 81.28 270)
    (descr "D, DO-201AD series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Vertical pin pitch 5.08mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D1 (at 4.445 4.445 360) (layer F.SilkS))
    (fp_text value SR340 (at 2.54 5.438 270) (layer F.Fab))
    (fp_text user K (at -2.3 0 270) (layer F.Fab))
    (fp_text user %R (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 +9V))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 9 +12V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P5.08mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:pcc-Pin_Header_Straight_1x02 (layer B.Cu) (tedit 59FB2BF3)
    (at 118.745 116.84 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -0.508 2.159 90) (layer B.SilkS) hide)
    (fp_text value +Vout (at 0 3.1 90) (layer B.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 +6V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lib:pcc-Pin_Header_Straight_1x02 (layer B.Cu) (tedit 59765DE1)
    (at 163.195 116.84 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at -2.54 -3.175 90) (layer B.SilkS) hide)
    (fp_text value +Vout (at 0 3.1 90) (layer B.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 +6V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lib:pcc_SW_PUSH_SMALL (layer F.Cu) (tedit 59767437)
    (at 139.7 107.95 180)
    (fp_text reference SW1 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.54 180) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(IC1-Pad5)"))
    (pad 1 thru_hole circle (at 3.25 -2.25 180) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(IC1-Pad5)"))
    (pad 2 thru_hole circle (at 3.25 2.25 180) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25 180) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(IC1-Pad5)"))
    (pad 2 thru_hole circle (at -3.25 2.25 180) (size 1.778 1.778) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5977B267)
    (at 130.175 81.915 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.715 2.54 360) (layer F.SilkS))
    (fp_text value 100u (at 1.25 5.31 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +9V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:pcc-Pin_Header_Straight_1x02 (layer B.Cu) (tedit 59C17138)
    (at 118.745 119.38 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at -2.54 -3.175 90) (layer B.SilkS) hide)
    (fp_text value +Vout (at 0 3.1 90) (layer B.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 +6V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 59DCF201)
    (at 146.685 114.3 180)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D6 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value Blue (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59DD0D5C)
    (at 140.97 99.06 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at -3.81 0 180) (layer B.SilkS))
    (fp_text value 2.2K (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 /ADC2))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59DD0D62)
    (at 147.32 99.06 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 3.81 2.54 360) (layer B.SilkS))
    (fp_text value 39K (at 0 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 +6V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 /ADC3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59DD0D6D)
    (at 144.78 99.06 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at -3.81 3.175 180) (layer B.SilkS))
    (fp_text value 2.2K (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 /ADC3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 59DBE068)
    (at 161.29 81.915)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference P10 (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value "M3 Mount" (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 59DF817E)
    (at 150.495 107.95 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at -0.127 -1.524 180) (layer F.SilkS))
    (fp_text value ATTINY84-S (at 0 5.375 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /RED))
    (pad 3 smd rect (at -2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /GREEN))
    (pad 4 smd rect (at -2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /~RST))
    (pad 5 smd rect (at -2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at -2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /BLUE))
    (pad 7 smd rect (at -2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /MOSI))
    (pad 8 smd rect (at 2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /MISO))
    (pad 9 smd rect (at 2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /SCK))
    (pad 10 smd rect (at 2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /OPT))
    (pad 11 smd rect (at 2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /ADC3))
    (pad 12 smd rect (at 2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /ADC2))
    (pad 13 smd rect (at 2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /ADC1))
    (pad 14 smd rect (at 2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59FB2C44)
    (at 162.56 85.725 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P3 (at 0 2.33 90) (layer B.SilkS) hide)
    (fp_text value 1x1 (at 0 -2.33 90) (layer B.Fab))
    (fp_text user %R (at 0 0 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +6V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59FB2C47)
    (at 162.56 90.805 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P4 (at 0 2.33 90) (layer B.SilkS) hide)
    (fp_text value 1x1 (at 0 -2.33 90) (layer B.Fab))
    (fp_text user %R (at 0 0 360) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:pcc-Pin_Header_Straight_1x02 (layer B.Cu) (tedit 59FB2C05)
    (at 163.195 119.38 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at -2.54 -3.175 90) (layer B.SilkS) hide)
    (fp_text value +Vout (at 0 3.1 90) (layer B.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 +6V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lib:pcc_icsp_Pin_Header_Straight_2x03 (layer F.Cu) (tedit 59FB2C1B)
    (at 160.02 110.49)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 0.254 -5.461) (layer F.SilkS) hide)
    (fp_text value ICSP (at 0.381 5.334 180) (layer F.Fab))
    (fp_text user VDD (at 2.921 -3.937 90) (layer B.SilkS))
    (fp_text user MISO (at -2.286 -4.064 90) (layer B.SilkS))
    (fp_text user MOSI (at 2.921 -0.127 90) (layer B.SilkS))
    (fp_text user GND (at 2.921 3.429 90) (layer B.SilkS))
    (fp_text user ~RST (at -2.286 3.429 90) (layer B.SilkS))
    (fp_text user SCK (at -2.286 -0.127 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at -1.016 -2.794) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /MISO))
    (pad 2 thru_hole oval (at 1.524 -2.794) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 3 thru_hole oval (at -1.016 -0.254) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /SCK))
    (pad 4 thru_hole oval (at 1.524 -0.254) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /MOSI))
    (pad 5 thru_hole oval (at -1.016 2.286) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /~RST))
    (pad 6 thru_hole oval (at 1.524 2.286) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 118.11 81.915)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference P11 (at 0 -3.75) (layer F.SilkS))
    (fp_text value "M3 Mount" (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_text "Buck\nConverter" (at 129.032 113.284) (layer F.SilkS))
  (gr_text ICSP (at 160.274 104.775) (layer F.SilkS))
  (gr_text "Portland\nCommunity\nCollege" (at 139.7 89.535) (layer F.SilkS))
  (gr_line (start 164.465 119.38) (end 164.465 80.01) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 114.935 80.01) (end 114.935 119.38) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text -Vout+ (at 118.11 114.3) (layer B.SilkS))
  (gr_text "+\nVout\n-" (at 161.544 88.138) (layer B.SilkS))
  (gr_text "Vin2+\n\n\n\n\n-" (at 115.824 105.664) (layer B.SilkS))
  (gr_text Vin1 (at 117.983 88.265) (layer B.SilkS))
  (gr_text "Bypass\nuC" (at 148.717 81.28) (layer B.SilkS))
  (gr_text "Creative Commons\n(CC BY-SA 4.0)" (at 162.56 93.853) (layer B.SilkS))
  (gr_text PCC (at 151.892 113.411) (layer F.SilkS))
  (gr_text +Vout- (at 118.11 114.3) (layer F.SilkS))
  (gr_line (start 123.825 115.57) (end 155.575 115.57) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 122.555 116.84) (end 122.555 119.38) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 116.205 120.65) (end 121.285 120.65) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 121.285 119.38) (end 122.555 119.38) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 123.825 116.84) (end 122.555 116.84) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 155.575 116.84) (end 155.575 115.57) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 163.195 120.65) (end 158.115 120.65) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 158.115 119.38) (end 158.115 120.65) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 156.845 116.84) (end 156.845 119.38) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 163.195 80.01) (end 163.195 78.74) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 116.205 80.01) (end 114.935 80.01) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 116.205 119.38) (end 116.205 120.65) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 163.195 119.38) (end 164.465 119.38) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 116.205 78.74) (end 163.195 78.74) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text "+\nVout\n-" (at 161.544 88.138) (layer F.SilkS))
  (gr_text "+Vin2\n\n\n\n\n-" (at 115.697 105.664) (layer F.SilkS))
  (gr_text Vin1 (at 118.11 88.265) (layer F.SilkS))
  (gr_text "Goldman\n2018" (at 162.56 101.219) (layer B.Mask))
  (gr_text "Secondary Side\n\nRev 5-2" (at 139.7 93.345) (layer B.SilkS))
  (gr_text "Primary Side\n2 Layer Board\n" (at 139.7 99.695) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 1.016)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 1.27))
    (polygon
      (pts
        (xy 114.935 78.74) (xy 164.465 78.74) (xy 164.465 120.65) (xy 114.935 120.65)
      )
    )
  )
  (zone (net 5) (net_name +6V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 1.016)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 1.27))
    (polygon
      (pts
        (xy 114.935 78.74) (xy 164.465 78.74) (xy 164.465 120.65) (xy 114.935 120.65)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 1.016)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 1.27))
    (polygon
      (pts
        (xy 162.56 103.759) (xy 156.21 103.759) (xy 156.21 98.679) (xy 162.56 98.679) (xy 162.56 103.759)
      )
    )
  )
)
