(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Spectrum Analyzer: Second Mixer - Second Local Oscillator")
    (date "2022-08-06")
    (rev "0")
    (company "Andy McCann KA3KAF Doug McCann KA3KAG")
    (comment 2 "Wes Hayward W7ZOI")
    (comment 3 "Original Design By:")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 101.3968 124.7648)
    (pcbplotparams
      (layerselection 0x0000020_7ffffffe)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits false)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C201-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(C203-Pad1)")
  (net 4 "Net-(C201-Pad2)")
  (net 5 "Net-(C204-Pad1)")
  (net 6 "Net-(C204-Pad2)")
  (net 7 "Net-(C207-Pad2)")
  (net 8 "Net-(C209-Pad1)")
  (net 9 "Net-(C209-Pad2)")
  (net 10 "Net-(C210-Pad1)")
  (net 11 "Net-(C211-Pad1)")
  (net 12 "Net-(C212-Pad1)")
  (net 13 "Net-(C212-Pad2)")
  (net 14 "Net-(C213-Pad2)")
  (net 15 "Net-(J203-Pad1)")
  (net 16 "Net-(C214-Pad2)")
  (net 17 "Net-(L202-Pad2)")
  (net 18 "Net-(J201-Pad1)")
  (net 19 "Net-(L204-Pad1)")
  (net 20 "Net-(L203-Pad1)")
  (net 21 "/+15")
  (net 22 "Net-(Q202-Pad1)")
  (net 23 "Net-(Q202-Pad3)")
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 112.6852 93.7514)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP201" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "Q-Base" (at 3.2512 0.0508 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 1 "Net-(C201-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 161.8596 111.0234)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R217" (at 3.4906 -0.0404) (layer "F.SilkS"))
    (fp_text value "5.1" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(Q202-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C214-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 108.9368 96.6216 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C203" (at 2.5654 -0.0762) (layer "F.SilkS"))
    (fp_text value "470p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C203-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 157.7448 85.5472)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R213" (at 3.4652 -0.0912) (layer "F.SilkS"))
    (fp_text value "2k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(Q202-Pad3)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C212-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 122.769 108.6758 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C205" (at 2.5254 -0.0508 90) (layer "F.SilkS"))
    (fp_text value "33p" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C204-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "2ndmixer-2ndlo:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 116.0634 112.9538 -90)
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C206" (at 2.54615 -1.7018 90) (layer "F.SilkS"))
    (fp_text value "12p-60p" (at 2.67315 2.159 90) (layer "F.SilkS"))
    (fp_text user "*" (at -0.2794 1.3462 90) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 5 "Net-(C204-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0 270) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/Trimmer Cap - Brown.stp"
      (offset (xyz 2.8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/Trimmer Cap - Brown.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 166.33 90.043)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP209" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "Q-Coll" (at 0.127 1.651 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 23 "Net-(Q202-Pad3)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 110.3992 113.8174)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP203" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "Q-Coll" (at 0.0508 1.5494 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 17 "Net-(L202-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 135.0118 86.4362 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R211" (at 3.7338 0.2286 90) (layer "F.SilkS"))
    (fp_text value "220" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C210-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(L203-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 160.4118 117.5512 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R216" (at 3.9878 -0.0762) (layer "F.SilkS"))
    (fp_text value "27" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(Q202-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 130.5414 108.1278)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP204" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "6db Pad In" (at 4.4704 0.2794 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 7 "Net-(C207-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 104.3032 114.6556 90)
    (descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Conn_Coaxial")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr exclude_from_pos_files)
    (fp_text reference "J201" (at 3.8354 2.6924 90) (layer "F.SilkS"))
    (fp_text value "Coax Solder Point" (at 2.3 2.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.3 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 18 "Net-(J201-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.6 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "2ndmixer-2ndlo:691103110002" (layer "F.Cu")
    (tedit 62DE8117)
    (at 106.4622 89.027 90)
    (descr "<b>WR-TBL Serie 1031 - 3.50 mm Horiz. Entry Modular<br></b>Max Height = 8.4mm , Pitch 3.5mm , 2 Pins")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Conn_01x02")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr through_hole)
    (fp_text reference "J202" (at -0.0762 -2.2368 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 4.12 4.865 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -1.75 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "/+15") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.75 0 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/691103110002_1.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/691103110002_1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 170.849 119.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H204" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 124.5724 81.788)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP202" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "+15" (at 2.3114 -0.2286 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 21 "/+15") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 120.1782 122.6312 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R206" (at 3.9878 0.0762) (layer "F.SilkS"))
    (fp_text value "150" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C207-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 136.9676 123.3678)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP206" (at 0.7366 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "MAV-In" (at 3.0734 0.762 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(C209-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 164.5012 107.569)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C212" (at 2.3984 0.0762) (layer "F.SilkS"))
    (fp_text value ".1u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C212-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C212-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 134.072 122.2248 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C209" (at 2.4746 -0.0762 90) (layer "F.SilkS"))
    (fp_text value ".01u" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C209-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C209-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 111.5676 109.8804)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R205" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "510" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(L202-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 115.403 96.1898 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R203" (at 3.7592 -0.127 90) (layer "F.SilkS"))
    (fp_text value "2k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C201-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 107.849 119.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H201" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 160.2594 114.4778 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R214" (at 3.8862 0) (layer "F.SilkS"))
    (fp_text value "390" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C212-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 122.7436 77.7494)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R215" (at 3.8462 -0.269) (layer "F.SilkS"))
    (fp_text value "27" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "/+15") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C213-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 140.3204 108.1278)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP205" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "6db Pad Out" (at 5.1308 0.381 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 8 "Net-(C209-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.6176 122.4788 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R207" (at 3.7996 0.0254) (layer "F.SilkS"))
    (fp_text value "36" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C207-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C209-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 164.6028 121.539 180)
    (descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Conn_Coaxial")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr exclude_from_pos_files)
    (fp_text reference "J203" (at 2.3 -2.25) (layer "F.SilkS"))
    (fp_text value "Coax Solder Point" (at 2.3 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.3 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 15 "Net-(J203-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.6 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 170.849 81)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H203" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 163.536 98.5774)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Field4" "10 turns #28")
    (property "Field5" "T30-6")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L202" (at -0.1016 2.7178) (layer "F.SilkS"))
    (fp_text value "420n" (at 0 8.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(C204-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 "Net-(L202-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/T37-6 IND004.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/T37-6 IND004.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 147.9658 112.141)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP208" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "TUF-Out" (at 0 1.6256 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 19 "Net-(L204-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "2ndmixer-2ndlo:MAV-11BSM&plus_" (layer "F.Cu")
    (tedit 0)
    (at 143.1398 119.9388)
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U201" (at 0 0) (layer "F.SilkS"))
    (fp_text value "MAV-11" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -3.302 -1.27) (layer "F.SilkS"))
    (fp_text user "*" (at -4.064 -1.27) (layer "F.SilkS"))
    (fp_text user "0.058in/1.473mm" (at 7.4295 -3.175) (layer "Cmts.User"))
    (fp_text user "0.25in/6.35mm" (at -7.4295 0) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at 6.604 0) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "0.25in/6.35mm" (at 0 7.874) (layer "Cmts.User"))
    (fp_text user "0.03in/0.762mm" (at 0 -6.604) (layer "Cmts.User"))
    (fp_text user "*" (at -1.4605 0) (layer "F.Fab"))
    (fp_text user "*" (at -1.4605 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.175 0 90) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C209-Pad2)") (pinfunction "RF_In") (pintype "passive"))
    (pad "2" smd rect locked (at 0 3.175) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" smd rect locked (at 3.175 0 90) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "RF_Out") (pintype "passive"))
    (pad "4" smd rect locked (at 0 -3.175) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 112.101 96.266 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R201" (at 3.7592 0.0508 90) (layer "F.SilkS"))
    (fp_text value "3.3k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C203-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C201-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 126.031 117.2972 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C208" (at 2.6016 0.0508) (layer "F.SilkS"))
    (fp_text value "82p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C207-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 108.9114 99.9236 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C201" (at 2.4238 -0.1778) (layer "F.SilkS"))
    (fp_text value "470p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C201-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C201-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "2ndmixer-2ndlo:TUF-1H" (layer "F.Cu")
    (tedit 0)
    (at 135.0118 111.3312)
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U202" (at 4.24 1.66 unlocked) (layer "F.SilkS"))
    (fp_text value "TUF-1H+" (at 3.79 3.01 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.52 -0.54 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.25 1.63 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J201-Pad1)") (pinfunction "RF") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(L204-Pad1)") (pinfunction "IF") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "LO") (pintype "passive"))
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/Body002.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/Body002.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "2ndmixer-2ndlo:TO127P584H533-4N" (layer "F.Cu")
    (tedit 62EBF79A)
    (at 107.3566 104.7349 90)
    (property "MANUFACTURER" "Microchip/Microsemi/Advanced Power Technology")
    (property "MAXIMUM_PACKAGE_HEIGHT" "5.33 mm")
    (property "PARTREV" "N/A")
    (property "STANDARD" "IPC 7351B")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "2ndmixer-2ndlo-spice\\2N5179.LIB")
    (property "Spice_Model" "2N5179")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "Q")
    (attr through_hole)
    (fp_text reference "Q201" (at -0.325 -3.935 90) (layer "F.SilkS"))
    (fp_text value "2N5179" (at 6.66 4.065 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -1.27 0 90) (size 1.11 1.11) (drill 0.71) (layers *.Cu *.Mask)
      (net 17 "Net-(L202-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 1.27 90) (size 1.11 1.11) (drill 0.71) (layers *.Cu *.Mask)
      (net 1 "Net-(C201-Pad1)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 1.27 0 90) (size 1.11 1.11) (drill 0.71) (layers *.Cu *.Mask)
      (net 5 "Net-(C204-Pad1)") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 -1.27 90) (size 1.11 1.11) (drill 0.71) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/to-72.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/to-72.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.0588 118.11 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R208" (at 3.683 0.0508 90) (layer "F.SilkS"))
    (fp_text value "150" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C209-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 107.849 81)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H202" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 149.8708 122.6312)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP207" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "MAV-Out" (at 3.5814 1.3208 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 126.4266 108.5996 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C207" (at 2.5254 -0.127 90) (layer "F.SilkS"))
    (fp_text value "15p" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C204-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C207-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 166.9396 94.3356)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP210" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "Q-Emit" (at 0.0508 1.8542 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 22 "Net-(Q202-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 168.1188 114.3762 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C214" (at 2.3476 -0.2032) (layer "F.SilkS"))
    (fp_text value ".1u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C214-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 162.7086 82.1436 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C213" (at 2.5 0.0762) (layer "F.SilkS"))
    (fp_text value ".1u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C213-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 111.593 106.6292)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R202" (at 3.81 -0.0508) (layer "F.SilkS"))
    (fp_text value "39" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C201-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 112.6598 77.7494)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R210" (at 3.7674 0.0566) (layer "F.SilkS"))
    (fp_text value "47" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "/+15") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C210-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 159.4212 111.125 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C211" (at 2.413 -0.127) (layer "F.SilkS"))
    (fp_text value "120p" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C211-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 154.4174 107.6198)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R212" (at 3.6068 -0.071) (layer "F.SilkS"))
    (fp_text value "51" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(L204-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C211-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_HC49-U_Vertical" (layer "F.Cu")
    (tedit 5A1AD3B8)
    (at 124.9534 97.7138 -90)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y201" (at 2.54 -1.5494 90) (layer "F.SilkS"))
    (fp_text value "100MHz" (at 2.44 3.525 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.44 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(L202-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.88 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C204-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC49-U_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 127.3664 86.8826 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C210" (at 2.5 0.0762 90) (layer "F.SilkS"))
    (fp_text value ".01u" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C210-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 131.1764 86.36 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R209" (at 3.6576 0.0762 90) (layer "F.SilkS"))
    (fp_text value "220" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C210-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(L203-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "2ndmixer-2ndlo:TO127P584H533-4N" (layer "F.Cu")
    (tedit 62EBF79A)
    (at 160.1979 92.0042)
    (property "MANUFACTURER" "Microchip/Microsemi/Advanced Power Technology")
    (property "MAXIMUM_PACKAGE_HEIGHT" "5.33 mm")
    (property "PARTREV" "N/A")
    (property "STANDARD" "IPC 7351B")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "2ndmixer-2ndlo-spice\\2N5179.LIB")
    (property "Spice_Model" "2N5179")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "Q")
    (attr through_hole)
    (fp_text reference "Q202" (at -0.325 -3.935) (layer "F.SilkS"))
    (fp_text value "2N5179" (at 6.66 4.065) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -1.27 0) (size 1.11 1.11) (drill 0.71) (layers *.Cu *.Mask)
      (net 22 "Net-(Q202-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 0 1.27) (size 1.11 1.11) (drill 0.71) (layers *.Cu *.Mask)
      (net 13 "Net-(C212-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 1.27 0) (size 1.11 1.11) (drill 0.71) (layers *.Cu *.Mask)
      (net 23 "Net-(Q202-Pad3)") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 -1.27) (size 1.11 1.11) (drill 0.71) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/to-72.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/to-72.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 149.4136 98.7238)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Field4" "T30-6")
    (property "Field5" "10T #30")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L204" (at -0.6604 2.6416) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 8.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(L204-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(C212-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/T37-6 IND004.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/T37-6 IND004.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 135.342 98.673)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Field4" "T30-6")
    (property "Field5" "10T #30")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L203" (at -0.2794 2.6162) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 8.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(L203-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/T37-6 IND004.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/T37-6 IND004.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Transformer_THT:Autotransformer_Toroid_1Tap_Horizontal_D10.5mm_Amidon-T37" (layer "F.Cu")
    (tedit 5A030845)
    (at 139.2282 87.5538)
    (descr "Autotransformer, Toroid, horizontal, laying, 1 Tap, Diameter 10,5mm, Amidon T37,")
    (tags "Autotransformer Toroid horizontal laying 1 Tap Diameter 10 5mm Amidon T37 ")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "T201" (at 7.4 -3.556) (layer "F.SilkS"))
    (fp_text value "Bifilar_Transformer" (at 7.5 10.2) (layer "F.Fab"))
    (fp_text user "End" (at 15.7 -2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 -3.5) (layer "F.Fab"))
    (fp_text user "Tap1" (at 11.2 6) (layer "F.Fab"))
    (fp_text user "Start" (at -1.1 -2.9) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(C213-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 7.5) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(J203-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 15 0) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(Q202-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/L_Tor_13x8x5_3a_cp.step"
      (offset (xyz 0 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/L_Tor_13x8x5_3a_cp.wrl"
      (offset (xyz 0 -5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 112.736 81.0514)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R204" (at 3.9624 -0.127) (layer "F.SilkS"))
    (fp_text value "100" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "/+15") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C203-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 118.7304 98.8206 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C204" (at 2.5762 0.0508 90) (layer "F.SilkS"))
    (fp_text value "33p" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C204-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C204-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 118.2732 84.3534)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Field4" "4 turns #22")
    (property "Field5" "6-32 screw")
    (property "Sheetfile" "2ndmixer-2ndlo.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L201" (at -0.127 2.7432) (layer "F.SilkS"))
    (fp_text value "40n" (at 0 8.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(C203-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(C204-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/T37-6 IND004.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/T37-6 IND004.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 102.6668 75.2348) (end 175.0568 124.7648) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "+15" (at 105.2938 94.1578) (layer "F.SilkS"))
  (gr_text "In" (at 106.9956 114.6556 90) (layer "F.SilkS"))
  (gr_text "Out" (at 164.2726 118.8212) (layer "F.SilkS"))
  (gr_text "Andy McCann KA3KAF\nDoug McCann KA3KAG" (at 173.2642 100.1268 270) (layer "F.SilkS"))
  (gr_text "Spectrum Analyzer\n2nd Mixer 2nd Local Osc. Rev 0" (at 149.1342 78.5368) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.0568 124.7648)
        (xy 102.6668 124.7648)
        (xy 102.6668 75.2348)
        (xy 175.0568 75.2348)
      )
    )
  )
)
