<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="59.944" width="0.1" layer="20"/>
<wire x1="0" y1="59.944" x2="1.27" y2="61.214" width="0.1" layer="20" curve="-90"/>
<wire x1="1.27" y1="61.214" x2="52.07" y2="61.214" width="0.1" layer="20"/>
<wire x1="52.07" y1="61.214" x2="53.34" y2="59.944" width="0.1" layer="20" curve="-90"/>
<wire x1="53.34" y1="59.944" x2="53.34" y2="1.27" width="0.1" layer="20"/>
<wire x1="53.34" y1="1.27" x2="52.07" y2="0" width="0.1" layer="20" curve="-90"/>
<wire x1="52.07" y1="0" x2="0" y2="0" width="0.1" layer="20"/>
<text>BlinkyTape Test Shield</text>
<text>RevD.1, 07/13</text>
<text>TEST_DUT</text>
<text>OUT_LED</text>
<text>SIG</text>
<text>5V</text>
<text>GND</text>
<text>_A10</text>
<text>_D11</text>
<text>_D7</text>
<text>_D13</text>
<text>OGND</text>
<text>OVCC</text>
<text>DUT USB</text>
<text>HOST USB</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
</package>
<package name="1X03">
</package>
<package name="2X4">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUEMILANOVE_SHIELD_NOHOLES">
</package>
</packages>
</library>
<library name="blinkiverse">
<description>Library of parts that we use for our Blinkiverse designs. Some parts copied (and modified) from the excellent Sparkfun libraries.
</description>
<packages>
<package name="MICRO_USB_FCI_THRUHOLE">
</package>
<package name="RELAY_HK23F-5V">
</package>
<package name="SPARKFUN_ACS712">
</package>
<package name="USB_A_FEMALE_NOSILK_SHIELD">
</package>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SOD-523">
<description>SOD-523 (0.8x1.2mm)

&lt;p&gt;Source: http://www.rohm.com/products/databook/di/pdf/rb751s-40.pdf&lt;/p&gt;</description>
</package>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ICSP_DUT" library="SparkFun-Connectors" package="2X3-NS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT_LED" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-Boards" package="DUEMILANOVE_SHIELD_NOHOLES" value="ARDUINO_SHIELDNOHOLES"/>
<element name="TEST_DUT" library="SparkFun-Connectors" package="2X4" value="M04X2">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="blinkiverse" package="MICRO_USB_FCI_THRUHOLE" value="MICRO_USBSMT+THRUHULE"/>
<element name="U$3" library="blinkiverse" package="RELAY_HK23F-5V" value="RELAY"/>
<element name="U$4" library="blinkiverse" package="RELAY_HK23F-5V" value="RELAY"/>
<element name="U$5" library="blinkiverse" package="RELAY_HK23F-5V" value="RELAY"/>
<element name="U$6" library="blinkiverse" package="RELAY_HK23F-5V" value="RELAY"/>
<element name="U$7" library="blinkiverse" package="RELAY_HK23F-5V" value="RELAY"/>
<element name="U$8" library="blinkiverse" package="RELAY_HK23F-5V" value="RELAY"/>
<element name="U$9" library="blinkiverse" package="RELAY_HK23F-5V" value="RELAY"/>
<element name="U$10" library="blinkiverse" package="RELAY_HK23F-5V" value="RELAY"/>
<element name="R1" library="adafruit" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="adafruit" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="adafruit" package="SOD-523" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="adafruit" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="D2" library="adafruit" package="SOD-523" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="Q3" library="adafruit" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="D3" library="adafruit" package="SOD-523" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="Q4" library="adafruit" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="D4" library="adafruit" package="SOD-523" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="Q5" library="adafruit" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="D5" library="adafruit" package="SOD-523" value="">
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="Q6" library="adafruit" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="D6" library="adafruit" package="SOD-523" value="">
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="Q7" library="adafruit" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="D7" library="adafruit" package="SOD-523" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="R0603" value="1k">
<attribute name="VALUE"/>
</element>
<element name="Q8" library="adafruit" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="D8" library="adafruit" package="SOD-523" value="">
<attribute name="VALUE"/>
</element>
<element name="R9" library="adafruit" package="R1210" value="25">
<attribute name="VALUE"/>
</element>
<element name="U$11" library="blinkiverse" package="SPARKFUN_ACS712" value="SPARKFUN_ACS712"/>
<element name="U$1" library="blinkiverse" package="USB_A_FEMALE_NOSILK_SHIELD" value="USB"/>
<element name="U$12" library="blinkiverse" package="OSHW-LOGO-L" value=""/>
</elements>
<signals>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="ICSP_SCK">
<contactref element="ICSP_DUT" pad="3"/>
</signal>
<signal name="ICSP_MISO">
<contactref element="ICSP_DUT" pad="1"/>
</signal>
<signal name="ICSP_MOSI">
<contactref element="ICSP_DUT" pad="4"/>
</signal>
<signal name="ICSP_RESET">
<contactref element="ICSP_DUT" pad="5"/>
<contactref element="U1" pad="RX"/>
</signal>
<signal name="DUT_A10">
<contactref element="TEST_DUT" pad="1"/>
<contactref element="U1" pad="TX"/>
</signal>
<signal name="DUT_D11">
<contactref element="TEST_DUT" pad="3"/>
<contactref element="U1" pad="D4"/>
</signal>
<signal name="DUT_D7">
<contactref element="TEST_DUT" pad="5"/>
<contactref element="U1" pad="D5"/>
</signal>
<signal name="DUT_D13">
<contactref element="TEST_DUT" pad="7"/>
<contactref element="U$10" pad="P$1"/>
<contactref element="U$10" pad="P$6"/>
<contactref element="U1" pad="D6"/>
</signal>
<signal name="DUT_IN_VCC_NC">
<contactref element="TEST_DUT" pad="2"/>
</signal>
<signal name="DUT_IN_GND_NC">
<contactref element="TEST_DUT" pad="4"/>
</signal>
<signal name="DUT_OUT_GND">
<contactref element="TEST_DUT" pad="8"/>
<contactref element="U$8" pad="P$1"/>
<contactref element="U$8" pad="P$6"/>
<contactref element="U1" pad="A4"/>
</signal>
<signal name="DUT_USB_D+">
<contactref element="U$4" pad="P$1"/>
<contactref element="U$4" pad="P$6"/>
<contactref element="U$1" pad="D+"/>
</signal>
<signal name="DUT_USB_D-">
<contactref element="U$5" pad="P$1"/>
<contactref element="U$5" pad="P$6"/>
<contactref element="U$1" pad="D-"/>
</signal>
<signal name="DUT_USB_GND">
<contactref element="U$6" pad="P$1"/>
<contactref element="U$6" pad="P$6"/>
<contactref element="U1" pad="A1"/>
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="HOST_USB_D-">
<contactref element="U$2" pad="PIN$2"/>
<contactref element="U$5" pad="P$3"/>
</signal>
<signal name="HOST_USB_D+">
<contactref element="U$2" pad="PIN$3"/>
<contactref element="U$4" pad="P$3"/>
</signal>
<signal name="HOST_USB_GND">
<contactref element="U$2" pad="PIN$5"/>
<contactref element="U$6" pad="P$3"/>
</signal>
<signal name="DUT_USB_VCC">
<contactref element="U$3" pad="P$1"/>
<contactref element="U$3" pad="P$6"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="U$7" pad="P$6"/>
<contactref element="U1" pad="A2"/>
<contactref element="U$1" pad="VBUS"/>
</signal>
<signal name="HOST_USB_VCC">
<contactref element="U$2" pad="PIN$1"/>
<contactref element="U$11" pad="IP-"/>
</signal>
<signal name="TAP_USB_D+">
<contactref element="U$4" pad="P$4"/>
<contactref element="U1" pad="D13"/>
</signal>
<signal name="TAP_USB_D-">
<contactref element="U$5" pad="P$4"/>
<contactref element="U1" pad="D12"/>
</signal>
<signal name="LED_OUT_SIG">
<contactref element="U$10" pad="P$3"/>
<contactref element="OUT_LED" pad="1"/>
</signal>
<signal name="LED_OUT_GND">
<contactref element="OUT_LED" pad="3"/>
<contactref element="U$8" pad="P$3"/>
</signal>
<signal name="LED_OUT_VCC">
<contactref element="OUT_LED" pad="2"/>
<contactref element="U$9" pad="P$3"/>
</signal>
<signal name="EN_USB_VCC_LIMIT">
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="D8"/>
</signal>
<signal name="N$14">
<contactref element="Q1" pad="3"/>
<contactref element="U$7" pad="P$2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="Q2" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="U$3" pad="P$2"/>
</signal>
<signal name="N$27">
<contactref element="Q3" pad="3"/>
<contactref element="D3" pad="A"/>
<contactref element="U$4" pad="P$2"/>
</signal>
<signal name="EN_USB_DATA">
<contactref element="Q4" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="Q3" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="D10"/>
</signal>
<signal name="N$31">
<contactref element="Q4" pad="3"/>
<contactref element="D4" pad="A"/>
<contactref element="U$5" pad="P$2"/>
</signal>
<signal name="EN_USB_VCC">
<contactref element="Q2" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="D9"/>
</signal>
<signal name="N$35">
<contactref element="Q5" pad="3"/>
<contactref element="D5" pad="A"/>
<contactref element="U$6" pad="P$2"/>
</signal>
<signal name="N$38">
<contactref element="Q6" pad="3"/>
<contactref element="D6" pad="A"/>
<contactref element="U$8" pad="P$2"/>
</signal>
<signal name="EN_LED_OUT">
<contactref element="Q7" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="Q6" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="Q8" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="A5"/>
</signal>
<signal name="N$42">
<contactref element="Q7" pad="3"/>
<contactref element="D7" pad="A"/>
<contactref element="U$10" pad="P$2"/>
</signal>
<signal name="N$46">
<contactref element="Q8" pad="3"/>
<contactref element="D8" pad="A"/>
<contactref element="U$9" pad="P$2"/>
</signal>
<signal name="5V">
<contactref element="U$3" pad="P$5"/>
<contactref element="U$7" pad="P$5"/>
<contactref element="U1" pad="5V"/>
<contactref element="D2" pad="K"/>
<contactref element="D1" pad="K"/>
<contactref element="D8" pad="K"/>
<contactref element="U$9" pad="P$5"/>
<contactref element="D7" pad="K"/>
<contactref element="U$10" pad="P$5"/>
<contactref element="U$8" pad="P$5"/>
<contactref element="D6" pad="K"/>
<contactref element="D3" pad="K"/>
<contactref element="U$4" pad="P$5"/>
<contactref element="U$6" pad="P$5"/>
<contactref element="U$5" pad="P$5"/>
<contactref element="D5" pad="K"/>
<contactref element="D4" pad="K"/>
<contactref element="U$11" pad="5V"/>
</signal>
<signal name="GND">
<contactref element="R7" pad="1"/>
<contactref element="Q7" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="Q6" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="Q8" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="Q4" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="Q5" pad="2"/>
<contactref element="U1" pad="GND@1"/>
<contactref element="U1" pad="GND@0"/>
<contactref element="U$11" pad="GND"/>
</signal>
<signal name="N$9">
<contactref element="U$7" pad="P$3"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="EN_USB_GND">
<contactref element="Q5" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="D11"/>
</signal>
<signal name="HOST_USB_VCC_M">
<contactref element="U$3" pad="P$3"/>
<contactref element="R9" pad="2"/>
<contactref element="U$11" pad="IP+"/>
</signal>
<signal name="DUT_OUT_VCC">
<contactref element="U$9" pad="P$1"/>
<contactref element="U$9" pad="P$6"/>
<contactref element="TEST_DUT" pad="6"/>
<contactref element="U1" pad="A3"/>
</signal>
<signal name="DUT_CURRENT">
<contactref element="U$11" pad="VOUT"/>
<contactref element="U1" pad="A0"/>
</signal>
<signal name="DUT_USB_SHIELD">
<contactref element="U$1" pad="SHIELD2"/>
<contactref element="U$1" pad="SHIELD1"/>
<contactref element="U1" pad="D7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
