<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<circle x="21.65" y="21.65" radius="21.65" width="0.0001" layer="46"/>
<text>BLF</text>
<text>GT</text>
<text>3V</text>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="testpad" package="TP20R" value="">
<attribute name="VALUE"/>
</element>
<element name="E$2" library="testpad" package="TP20R" value="">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="testpad" package="TP20R" value="">
<attribute name="VALUE"/>
</element>
<element name="E$4" library="testpad" package="TP20R" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="NEG">
<contactref element="E$1" pad="TP"/>
<contactref element="E$2" pad="TP"/>
<contactref element="E$3" pad="TP"/>
<contactref element="E$4" pad="TP"/>
</signal>
<signal name="POS">
</signal>
</signals>
</board>
</drawing>
</eagle>
