(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 267)
    (zones 0)
    (modules 22)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.1)
    (user_trace_width 0.15)
    (trace_clearance 0.2)
    (zone_clearance 0.15)
    (zone_45_only no)
    (trace_min 0.03)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.254)
    (via_min_drill 0.1016)
    (user_via 0.254 0.11)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 BAT+)
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C7-Pad1)")
  (net 8 "Net-(C8-Pad1)")
  (net 9 "Net-(J1-PadB8)")
  (net 10 CC2)
  (net 11 CC1)
  (net 12 "Net-(J1-PadA8)")
  (net 13 DN)
  (net 14 DP)
  (net 15 "Net-(R1-Pad1)")
  (net 16 "Net-(R2-Pad1)")
  (net 17 USBC_5vBoost_Enable)
  (net 18 InputOK)
  (net 19 Status)
  (net 20 USBCharger_SYS)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BAT+)
    (add_net CC1)
    (add_net CC2)
    (add_net DN)
    (add_net DP)
    (add_net GND)
    (add_net InputOK)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(J1-PadA8)")
    (add_net "Net-(J1-PadB8)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net Status)
    (add_net USBC_5vBoost_Enable)
    (add_net USBCharger_SYS)
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5FB8B1AE)
    (at 159.05 109.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 2.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.21 0.58) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module USB4110-GF-A:GCT_USB4110-GF-A (layer F.Cu) (tedit 5FB37D7E)
    (at 157.38 103.98 90)
    (fp_text reference J1 (at -12.58 -1.24 180) (layer F.SilkS))
    (fp_text value USB4110-GF-A (at 5.56 7.265 90) (layer F.Fab) hide)
    (pad A1/B12 smd rect (at -3.2 -1.075 90) (size 0.6 1.15) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad A4/B9 smd rect (at -2.4 -1.075 90) (size 0.6 1.15) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad B4/A9 smd rect (at 2.4 -1.075 90) (size 0.6 1.15) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad B1/A12 smd rect (at 3.2 -1.075 90) (size 0.6 1.15) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad B8 smd rect (at -1.75 -1.075 90) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-PadB8)"))
    (pad B5 smd rect (at 1.75 -1.075 90) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 10 CC2))
    (pad A5 smd rect (at -1.25 -1.075 90) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 11 CC1))
    (pad A8 smd rect (at 1.25 -1.075 90) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-PadA8)"))
    (pad B7 smd rect (at -0.75 -1.075 90) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 13 DN))
    (pad B6 smd rect (at 0.75 -1.075 90) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 14 DP))
    (pad A6 smd rect (at -0.25 -1.075 90) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 14 DP))
    (pad A7 smd rect (at 0.25 -1.075 90) (size 0.3 1.15) (layers F.Cu F.Paste F.Mask)
      (net 13 DN))
    (pad S1 smd rect (at -5.11 -0.5 90) (size 2.18 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad S2 smd rect (at 5.11 -0.5 90) (size 2.18 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad S3 smd rect (at -5.11 3.43 90) (size 2.18 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad S4 smd rect (at 5.11 3.43 90) (size 2.18 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad None np_thru_hole circle (at -2.89 0 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 2.89 0 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (model "C:/Users/RWB/Dropbox/PCB Design Files/Part Footprint Folder/USB4110-GF-A/USB4110-GF-A.step"
      (offset (xyz 0 -6.25 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5FB8AFDB)
    (at 159.05 97.52)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 2.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.2 0.07) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5FB891BF)
    (at 146.77 97.52)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 2.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.2 0.07) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 BAT+))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 5FB892D4)
    (at 142.63 98.94)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x05_Pitch2.54mm (at 0 12.49) (layer F.Fab) hide)
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 5 thru_hole rect (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole rect (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole rect (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 USBCharger_SYS))
    (pad 2 thru_hole rect (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 BAT+))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 BAT+))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5FB8AC85)
    (at 146.57 110.48 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference REF** (at -0.05 -0.03 90) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x04_Pitch2.54mm (at 0 9.95 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 4 thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 Status))
    (pad 3 thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 InputOK))
    (pad 2 thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 USBC_5vBoost_Enable))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5FB8AC85)
    (at 146.57 109.08 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference REF** (at -0.05 -0.03 90) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x04_Pitch2.54mm (at 0 9.95 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 USBC_5vBoost_Enable))
    (pad 3 thru_hole rect (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 InputOK))
    (pad 4 thru_hole rect (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 Status))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5FB891BF)
    (at 146.77 98.91)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 2.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.2 0.07) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 BAT+))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 5FB892D4)
    (at 144.03 98.94)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x05_Pitch2.54mm (at 0 12.49) (layer F.Fab) hide)
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 BAT+))
    (pad 2 thru_hole rect (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 BAT+))
    (pad 3 thru_hole rect (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 USBCharger_SYS))
    (pad 4 thru_hole rect (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole rect (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MAX77751CEFG_:IC_MAX77751CEFG+ (layer F.Cu) (tedit 0)
    (at 151.97 102.12 180)
    (fp_text reference U1 (at 4.63 -13.59 180) (layer F.SilkS))
    (fp_text value MAX77751CEFG+ (at 7.66 3.135 180) (layer F.Fab) hide)
    (pad 18_19 smd rect (at 1.5 -1 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 17 smd rect (at 1.5 -0.6 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 7 "Net-(C7-Pad1)") (solder_mask_margin 0.1016))
    (pad 15_16 smd rect (at 1.5 0 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 20 USBCharger_SYS) (solder_mask_margin 0.1016))
    (pad 13_14 smd rect (at 1.5 0.8 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 5 BAT+) (solder_mask_margin 0.1016))
    (pad 6 smd rect (at -1.5 1 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 14 DP) (solder_mask_margin 0.1016))
    (pad 5 smd rect (at -1.5 0.6 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 11 CC1) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -1.5 0.2 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 10 CC2) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at -1.5 -0.2 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 19 Status) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -1.5 -0.6 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 18 InputOK) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.5 -1 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 4 "Net-(C2-Pad2)") (solder_mask_margin 0.1016))
    (pad 23_24 smd rect (at -0.8 -1.5 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad 22 smd rect (at -0.2 -1.5 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 8 "Net-(C8-Pad1)") (solder_mask_margin 0.1016))
    (pad 20_21 smd rect (at 0.4 -1.5 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
    (pad 12 smd rect (at 1 1.5 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 15 "Net-(R1-Pad1)") (solder_mask_margin 0.1016))
    (pad 11 smd rect (at 0.6 1.5 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 16 "Net-(R2-Pad1)") (solder_mask_margin 0.1016))
    (pad 10 smd rect (at 0.2 1.5 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 6 "Net-(C5-Pad1)") (solder_mask_margin 0.1016))
    (pad 9 smd rect (at -0.2 1.5 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 8 smd rect (at -0.6 1.5 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 17 USBC_5vBoost_Enable) (solder_mask_margin 0.1016))
    (pad 7 smd rect (at -1 1.5 180) (size 0.1 0.1) (layers F.Cu F.Mask)
      (net 13 DN) (solder_mask_margin 0.1016))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm.step
      (offset (xyz 0 0 -0.5))
      (scale (xyz 1.1 1.1 1.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 148.77 102.96 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -12.81 -3.04 90) (layer F.SilkS))
    (fp_text value 22UF (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 USBCharger_SYS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 147.56 102.95 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -12.87 -3.12 90) (layer F.SilkS))
    (fp_text value 22UF (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 USBCharger_SYS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 154.45 106.92 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at -10.89 -5.5 90) (layer F.SilkS))
    (fp_text value 2.2UF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 149.99 106.66 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 11.39 4.12 270) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 148.76 100.09 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -13.83 -4.34 90) (layer F.SilkS))
    (fp_text value 10UF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 BAT+))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 152.55 98.64)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at -3.05 15.17 180) (layer F.SilkS))
    (fp_text value 2.2UF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 146.42 103.56 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 12.74 3.32 90) (layer F.SilkS))
    (fp_text value 2.2UF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 151.77 105.44 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 4.73 -12.18) (layer F.SilkS))
    (fp_text value 10UF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 152.23 106.9 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 4.89 -12.01) (layer F.SilkS))
    (fp_text value 22UF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 149.97 99 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -14.69 -4.41 180) (layer F.SilkS))
    (fp_text value 24.9K (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 150.99 99.01 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -14.71 -3.6 180) (layer F.SilkS))
    (fp_text value 8.06K (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module HMLQ25201T-R47MSR:HMLQ25201T-R47MSR (layer F.Cu) (tedit 5FB4CBBA)
    (at 147.36 105.84)
    (fp_text reference L1 (at -3.19 11.6) (layer F.SilkS))
    (fp_text value 0.47uH (at 0 -3.42) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.2 0) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 20 USBCharger_SYS))
    (pad 2 smd rect (at 1.2 0) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Wuerth_MAPI-2506.step
      (at (xyz 0 0 0))
      (scale (xyz 1.3 1.1 1.4))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "3 Amp USB-C\n1 Cell LiPo Charger" (at 152.76 100 180) (layer B.SilkS))
  (gr_text MAX77751 (at 152.56 101.76 180) (layer B.SilkS))
  (gr_text BAT+ (at 145.33 100.36 90) (layer B.SilkS))
  (gr_text BAT+ (at 146.73 100.44) (layer B.SilkS))
  (gr_text SYS (at 145.54 104.14 90) (layer B.SilkS))
  (gr_text GND (at 145.45 107.33 90) (layer B.SilkS))
  (gr_text GND (at 147.24 107.17 90) (layer B.SilkS))
  (gr_text Status (at 154.15 106.58 90) (layer B.SilkS))
  (gr_text Input_OK (at 151.08 106.23 90) (layer B.SilkS))
  (gr_text USB_OUT_EN (at 148.69 105.72 90) (layer B.SilkS))
  (gr_text GND (at 145.4 107.64 90) (layer F.SilkS))
  (gr_line (start 142.5 97.5) (end 162 97.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.5 110.5) (end 142.5 97.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 162 110.5) (end 142.5 110.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 162 97.5) (end 162 110.5) (layer Edge.Cuts) (width 0.05))
  (gr_text Bat+ (at 145.75 101.03 90) (layer F.SilkS))
  (gr_text VSYS (at 145.51 103.86 90) (layer F.SilkS))
  (zone (net 20) (net_name USBCharger_SYS) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.79 102.41) (xy 150.04 102.41) (xy 149.57 102.73) (xy 146.98 102.73) (xy 146.98 102.51)
        (xy 145.94 102.51) (xy 145.94 104.8) (xy 146.58 104.8) (xy 146.58 106.9) (xy 144.86 106.9)
        (xy 144.86 101.81) (xy 151.79 101.81)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.0254))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.08 104.74) (xy 151.58 105.01) (xy 151.58 105.88) (xy 151.8 106.1) (xy 151.8 107.61)
        (xy 150.58 107.61) (xy 150.58 105.52) (xy 149.53 105.52) (xy 149.53 104.43) (xy 146.14 104.43)
        (xy 146.14 103.74) (xy 147.13 103.74) (xy 147.13 103.26) (xy 149.87 103.26) (xy 150.14 103.02)
        (xy 151.08 103.02)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.3 105.79) (xy 150.24 105.79) (xy 150.24 106.45) (xy 149.3 106.45) (xy 149.3 106.89)
        (xy 148.07 106.89) (xy 148.07 104.8) (xy 149.3 104.8)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.86 104.68) (xy 151.5 104.68) (xy 151.28 104.54) (xy 151.28 102.84) (xy 151.86 102.84)
      )
    )
  )
  (zone (net 8) (net_name "Net-(C8-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.36 104.25) (xy 153.83 106.11) (xy 153.82 107.69) (xy 152.52 107.69) (xy 152.52 106.35)
        (xy 152.07 106.04) (xy 152.06 102.97) (xy 152.32 102.97)
      )
    )
  )
  (zone (net 1) (net_name "Net-(C1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.74 102.85) (xy 153.12 103.41) (xy 154.32 103.41) (xy 154.32 101.24) (xy 156.92 101.24)
        (xy 156.92 101.9) (xy 155.44 101.9) (xy 155.44 105.05) (xy 155.44 106.02) (xy 157.01 106.04)
        (xy 157.01 106.73) (xy 155.54 106.73) (xy 153.96 106.73) (xy 153.96 106.06) (xy 152.47 104.2)
        (xy 152.47 102.85)
      )
    )
  )
  (zone (net 1) (net_name "Net-(C1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.74 102.85) (xy 153.12 103.41) (xy 154.32 103.41) (xy 154.32 101.24) (xy 156.92 101.24)
        (xy 156.92 101.9) (xy 155.44 101.9) (xy 155.44 105.05) (xy 155.44 106.02) (xy 157.01 106.04)
        (xy 157.01 106.73) (xy 155.54 106.73) (xy 153.96 106.73) (xy 153.96 106.06) (xy 152.47 104.2)
        (xy 152.47 102.85)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C2-Pad2)") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.09 103.22) (xy 150.47 107.74) (xy 149.67 107.74) (xy 149.67 106.84) (xy 150.33 106.84)
        (xy 153.19 103.01) (xy 154.09 103.01)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C2-Pad2)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.09 103.22) (xy 150.47 107.74) (xy 149.67 107.74) (xy 149.67 106.84) (xy 150.37 106.84)
        (xy 153.27 103.01) (xy 154.09 103.01)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad1)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.83 104.62) (xy 150.28 106.6) (xy 149.37 106.6) (xy 149.37 106.97) (xy 148.69 106.97)
        (xy 148.69 104.72) (xy 151.29 103.66) (xy 151.83 103.66)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad1)") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.83 104.62) (xy 150.28 106.6) (xy 149.37 106.6) (xy 149.37 106.97) (xy 148.69 106.97)
        (xy 148.69 104.72) (xy 151.29 103.66) (xy 151.83 103.66)
      )
    )
  )
  (zone (net 5) (net_name BAT+) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.08 101.62) (xy 149.38 101.62) (xy 149.19 101.44) (xy 144.87 101.44) (xy 144.87 102.33)
        (xy 142.79 102.325) (xy 142.79 98.055) (xy 147.83 98.06) (xy 147.83 100.36) (xy 150.08 100.36)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162 110.3) (xy 142.68 110.26) (xy 142.68 97.66) (xy 162 97.7)
      )
    )
  )
  (zone (net 5) (net_name BAT+) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.08 101.62) (xy 149.38 101.62) (xy 149.19 101.44) (xy 144.87 101.44) (xy 144.87 102.33)
        (xy 144.1 102.33) (xy 144.1 98.06) (xy 147.83 98.06) (xy 147.83 100.36) (xy 150.08 100.36)
      )
    )
  )
  (zone (net 5) (net_name BAT+) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.08 101.62) (xy 149.38 101.62) (xy 149.19 101.44) (xy 144.87 101.44) (xy 144.87 102.33)
        (xy 144.1 102.33) (xy 144.1 98.06) (xy 147.83 98.06) (xy 147.83 100.36) (xy 150.08 100.36)
      )
    )
  )
  (zone (net 5) (net_name BAT+) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.08 101.62) (xy 149.38 101.62) (xy 149.19 101.44) (xy 144.87 101.44) (xy 144.87 102.33)
        (xy 142.79 102.33) (xy 142.79 97.78) (xy 147.83 97.78) (xy 147.83 100.36) (xy 150.08 100.36)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162 110.3) (xy 142.68 110.26) (xy 142.68 97.66) (xy 162 97.7)
      )
    )
  )
)
