(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-1")
  (general
    (thickness 1.6)
    (drawings 54)
    (tracks 220)
    (zones 0)
    (modules 32)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 CA9)
  (net 5 CA8)
  (net 6 CA7)
  (net 7 CA6)
  (net 8 CA5)
  (net 9 CA4)
  (net 10 CA3)
  (net 11 CA2)
  (net 12 CA1)
  (net 13 CB1)
  (net 14 CB2)
  (net 15 CB3)
  (net 16 CB4)
  (net 17 CB5)
  (net 18 CB6)
  (net 19 CB7)
  (net 20 CB8)
  (net 21 CB9)
  (net 22 SDA)
  (net 23 SCL)
  (net 24 "Net-(R2-Pad1)")
  (net 25 "Net-(R3-Pad1)")
  (net 26 "Net-(R5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CA1)
    (add_net CA2)
    (add_net CA3)
    (add_net CA4)
    (add_net CA5)
    (add_net CA6)
    (add_net CA7)
    (add_net CA8)
    (add_net CA9)
    (add_net CB1)
    (add_net CB2)
    (add_net CB3)
    (add_net CB4)
    (add_net CB5)
    (add_net CB6)
    (add_net CB7)
    (add_net CB8)
    (add_net CB9)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net SCL)
    (add_net SDA)
    (add_net VCC)
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 137.16 119.888 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 10μF (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VCC))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 137.16 121.92 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 10μF (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 141.732 108.712)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 0.1μF (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 137.16 116.332 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 0.1μF (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VCC))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A431)
    (at 129.286 104.14)
    (descr "Through hole straight socket strip, 1x09, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x09 2.54mm single row")
    (fp_text reference J1 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value "A Pins" (at 0 23.09) (layer F.Fab) hide)
    (fp_text user %R (at 0 10.16 90) (layer F.Fab) hide)
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 CA9))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 CA8))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 CA7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 CA6))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 CA5))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 CA4))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 CA3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 CA2))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 CA1))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A431)
    (at 150.114 104.14)
    (descr "Through hole straight socket strip, 1x09, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x09 2.54mm single row")
    (fp_text reference J2 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value "B Pins" (at 0 23.09) (layer F.Fab) hide)
    (fp_text user %R (at 0 10.16 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 CB1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 CB2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 CB3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 CB4))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 CB5))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 CB6))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 CB7))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 CB8))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 CB9))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 138.43 124.714 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.77 90) (layer F.SilkS) hide)
    (fp_text value PWR (at 0 5.31 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 140.97 103.886 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.77 90) (layer F.SilkS) hide)
    (fp_text value I2C (at 0 5.31 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 SDA))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 SCL))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 137.668 106.68 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 20kΩ (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 SCL))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 142.24 121.92)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 20kΩ (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VCC))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 24 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 142.24 117.856)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 20kΩ (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 25 "Net-(R3-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 141.732 106.68)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 20kΩ (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VCC))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 22 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 142.24 119.888)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 20kΩ (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 26 "Net-(R5-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Justins:IS31FL3731 QFN-28" (layer F.Cu) (tedit 5D535070)
    (at 139.7 112.522 90)
    (descr "QFN, 28 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=280), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U1 (at 0 -3.3 90) (layer F.SilkS) hide)
    (fp_text value IS31FL3731 (at 0 3.3 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.025 -1.2 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 CA9))
    (pad 2 smd roundrect (at -2.025 -0.8 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 3 smd roundrect (at -2.025 -0.4 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(R2-Pad1)"))
    (pad 4 smd roundrect (at -2.025 0 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(R5-Pad1)"))
    (pad 5 smd roundrect (at -2.025 0.4 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 6 smd roundrect (at -2.025 0.8 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R3-Pad1)"))
    (pad 7 smd roundrect (at -2.025 1.2 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 CB1))
    (pad 8 smd roundrect (at -1.2 2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 CB2))
    (pad 9 smd roundrect (at -0.8 2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 CB3))
    (pad 10 smd roundrect (at -0.4 2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 CB4))
    (pad 11 smd roundrect (at 0 2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 CB5))
    (pad 12 smd roundrect (at 0.4 2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 CB6))
    (pad 13 smd roundrect (at 0.8 2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 CB7))
    (pad 14 smd roundrect (at 1.2 2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 CB8))
    (pad 15 smd roundrect (at 2.025 1.2 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 CB9))
    (pad 16 smd roundrect (at 2.025 0.8 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C3-Pad1)"))
    (pad 17 smd roundrect (at 2.025 0.4 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 18 smd roundrect (at 2.025 0 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 19 smd roundrect (at 2.025 -0.4 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 SDA))
    (pad 20 smd roundrect (at 2.025 -0.8 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 SCL))
    (pad 21 smd roundrect (at 2.025 -1.2 90) (size 1 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 CA1))
    (pad 22 smd roundrect (at 1.2 -2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 CA2))
    (pad 23 smd roundrect (at 0.8 -2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 CA3))
    (pad 24 smd roundrect (at 0.4 -2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 CA4))
    (pad 25 smd roundrect (at 0 -2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 CA5))
    (pad 26 smd roundrect (at -0.4 -2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 CA6))
    (pad 27 smd roundrect (at -0.8 -2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 CA7))
    (pad 28 smd roundrect (at -1.2 -2.025 90) (size 0.2 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 CA8))
    (pad "" smd roundrect (at 0 0 90) (size 2 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-28-1EP_4x4mm_P0.4mm_EP2.4x2.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 132.334 104.14 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 12 CA1))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 132.334 106.68 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 11 CA2))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 132.334 109.22 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 10 CA3))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 132.334 111.76 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 9 CA4))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 132.334 114.3 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP5 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 8 CA5))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 132.334 116.84 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP6 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 7 CA6))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 132.334 119.38 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP7 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 6 CA7))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 132.334 121.92 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP8 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 5 CA8))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 132.334 124.46 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP9 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 4 CA9))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 147.066 104.14 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP10 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 CB1))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 147.066 106.68 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP11 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 CB2))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 147.066 109.22 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP12 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 15 CB3))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 147.066 111.76 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP13 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 16 CB4))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 147.066 114.3 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP14 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 17 CB5))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 147.066 116.84 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP15 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 18 CB6))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 147.066 119.38 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP16 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 CB7))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 147.066 121.92 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP17 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 CB8))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 147.066 124.46 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP18 (at 0 1.648) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.65) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 CB9))
  )
  (gr_text "Designed by Kredence\nCopyright Black Label Tech\nIS31FL3731 QFN Breakout" (at 139.446 113.792 90) (layer B.SilkS))
  (gr_text VCC (at 135.636 124.587) (layer F.SilkS))
  (gr_text GND (at 143.764 124.714) (layer F.SilkS))
  (gr_text 10μF (at 134.493 122.555) (layer F.SilkS))
  (gr_text 10μF (at 134.493 120.396) (layer F.SilkS))
  (gr_text 0.1μF (at 134.366 116.332) (layer F.SilkS))
  (gr_text SDA (at 143.764 104.013) (layer F.SilkS))
  (gr_text SCL (at 135.636 104.013) (layer F.SilkS))
  (gr_text 20kΩ (at 134.874 106.68) (layer F.SilkS))
  (gr_text 0.1μF (at 144.653 108.712) (layer F.SilkS))
  (gr_text 20kΩ (at 144.653 106.68) (layer F.SilkS))
  (gr_text 20kΩ (at 145.034 122.555) (layer F.SilkS))
  (gr_text 20kΩ (at 145.161 120.523) (layer F.SilkS))
  (gr_text CB1 (at 147.193 104.14) (layer F.SilkS))
  (gr_text CB5 (at 147.193 114.3) (layer F.SilkS))
  (gr_text CB7 (at 147.193 119.507) (layer F.SilkS))
  (gr_text CB2 (at 147.193 106.68) (layer F.SilkS))
  (gr_text CB3 (at 147.193 109.22) (layer F.SilkS))
  (gr_text CB4 (at 147.193 111.76) (layer F.SilkS))
  (gr_text CB6 (at 147.193 116.84) (layer F.SilkS))
  (gr_text CB8 (at 147.193 121.92) (layer F.SilkS))
  (gr_text CB9 (at 147.193 124.46) (layer F.SilkS))
  (gr_text CA5 (at 132.08 114.427) (layer F.SilkS))
  (gr_text CA4 (at 132.08 111.76) (layer F.SilkS))
  (gr_text CA1 (at 132.08 104.14) (layer F.SilkS))
  (gr_text CA3 (at 132.08 109.347) (layer F.SilkS))
  (gr_text CA2 (at 132.08 106.68) (layer F.SilkS))
  (gr_text CA6 (at 132.08 116.84) (layer F.SilkS))
  (gr_text CA8 (at 132.08 121.92) (layer F.SilkS))
  (gr_text CA7 (at 132.08 119.38) (layer F.SilkS))
  (gr_text CA9 (at 132.08 124.46) (layer F.SilkS))
  (gr_text 20kΩ (at 145.161 118.364) (layer F.SilkS))
  (gr_text CA9 (at 134.62 124.587) (layer B.SilkS))
  (gr_text CA3 (at 134.62 109.22) (layer B.SilkS))
  (gr_text CA2 (at 134.62 106.807) (layer B.SilkS))
  (gr_text CA8 (at 134.62 122.047) (layer B.SilkS))
  (gr_text CA7 (at 134.62 119.38) (layer B.SilkS))
  (gr_text CA6 (at 134.62 116.967) (layer B.SilkS))
  (gr_text CA5 (at 134.62 114.3) (layer B.SilkS))
  (gr_text CA4 (at 134.62 111.887) (layer B.SilkS))
  (gr_text CA1 (at 134.62 104.14) (layer B.SilkS))
  (gr_text CB9 (at 144.78 124.587) (layer B.SilkS))
  (gr_text CB7 (at 144.78 119.38) (layer B.SilkS))
  (gr_text CB6 (at 144.78 116.967) (layer B.SilkS))
  (gr_text CB8 (at 144.78 122.047) (layer B.SilkS))
  (gr_text CB5 (at 144.78 114.3) (layer B.SilkS))
  (gr_text CB4 (at 144.78 111.887) (layer B.SilkS))
  (gr_text CB3 (at 144.78 109.22) (layer B.SilkS))
  (gr_text CB2 (at 144.78 106.807) (layer B.SilkS))
  (gr_text CB1 (at 144.78 104.14) (layer B.SilkS))
  (gr_line (start 127 101.6) (end 127 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 101.6) (end 127 101.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 127) (end 152.4 101.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 127) (end 152.4 127) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.255) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127 101.6) (xy 152.4 101.6) (xy 152.4 127) (xy 127 127)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.255) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 127 101.6) (xy 152.4 101.6) (xy 152.4 127) (xy 127 127)
      )
    )
  )
)
