(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 16)
    (no_connects 0)
    (area 141.824999 98.324999 163.475001 115.275001)
    (thickness 1.6)
    (drawings 20)
    (tracks 44)
    (zones 0)
    (modules 3)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad4)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J2-Pad4)")
  (net 10 "Net-(J2-Pad1)")
  (net 11 "Net-(J2-Pad2)")
  (net 12 "Net-(J2-Pad3)")
  (net 13 "Net-(J2-Pad5)")
  (net 14 "Net-(J2-Pad6)")
  (net 15 "Net-(J2-Pad7)")
  (net 16 "Net-(J2-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_8pol (layer B.Cu) (tedit 0)
    (at 143.8 101.8)
    (descr "8-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J1 (at 8.89 4.50088) (layer B.SilkS))
    (fp_text value Screw_Terminal_1x08 (at 8.89 -4.50088) (layer B.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_8pol.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_8pol (layer B.Cu) (tedit 0)
    (at 161.6 111.8 180)
    (descr "8-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J2 (at 8.89 4.50088 180) (layer B.SilkS))
    (fp_text value Screw_Terminal_1x08 (at 8.89 -4.50088 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad4)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad3)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad8)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_8pol.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyConnectors:Gecko16Pin_SMD_Female (layer F.Cu) (tedit 598B7832)
    (at 148.5011 105.0036)
    (fp_text reference J3 (at 0 -9.76) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 -11.54) (layer F.Fab))
    (fp_text user 1 (at 0 -1.9) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 2.5 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 3.75 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 5 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 6.25 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at 7.5 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at 8.75 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at 0 3.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad8)"))
    (pad 10 smd rect (at 1.25 3.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad7)"))
    (pad 11 smd rect (at 2.5 3.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad6)"))
    (pad 12 smd rect (at 3.75 3.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad5)"))
    (pad 13 smd rect (at 5 3.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad4)"))
    (pad 14 smd rect (at 6.25 3.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad3)"))
    (pad 15 smd rect (at 7.5 3.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad2)"))
    (pad 16 smd rect (at 8.75 3.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad1)"))
  )
  (gr_text 16 (at 161.5 108.1) (layer B.SilkS))
  (gr_text 15 (at 158.7 108.1) (layer B.SilkS))
  (gr_text 14 (at 156.3 108.1) (layer B.SilkS))
  (gr_text 13 (at 153.8 108.1) (layer B.SilkS))
  (gr_text 12 (at 151.5 108.1) (layer B.SilkS))
  (gr_text 11 (at 148.9 108.1) (layer B.SilkS))
  (gr_text "10\n" (at 146.1 108.1) (layer B.SilkS))
  (gr_text "9\n" (at 143.6 108.1) (layer B.SilkS))
  (gr_text "8\n" (at 161.6 105.7) (layer B.SilkS))
  (gr_text 7 (at 158.8 105.7) (layer B.SilkS))
  (gr_text 6 (at 156.3 105.7) (layer B.SilkS))
  (gr_text 5 (at 154 105.7) (layer B.SilkS))
  (gr_text 4 (at 151.9 105.6) (layer B.SilkS))
  (gr_text 2 (at 146.3 105.6) (layer B.SilkS))
  (gr_text 1 (at 143.7 105.6) (layer B.SilkS))
  (gr_text 3 (at 149 105.6) (layer B.SilkS))
  (gr_line (start 141.9 98.4) (end 163.4 98.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.9 115.2) (end 141.9 98.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.4 115.2) (end 141.9 115.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.4 98.4) (end 163.4 115.2) (angle 90) (layer Edge.Cuts) (width 0.15))
)
