(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 10)
    (no_connects 0)
    (area 143.924999 100.524999 158.075001 116.875001)
    (thickness 1.6)
    (drawings 15)
    (tracks 20)
    (zones 0)
    (modules 3)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad4)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J2-Pad4)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 "Net-(J2-Pad2)")
  (net 9 "Net-(J2-Pad3)")
  (net 10 "Net-(J2-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_5pol (layer B.Cu) (tedit 598CCDF4)
    (at 146 104)
    (descr "5-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J1 (at 11 4) (layer B.SilkS))
    (fp_text value Screw_Terminal_1x05 (at 5.08 -4.50088) (layer B.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_5pol.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_5pol (layer B.Cu) (tedit 598CCDFD)
    (at 156.2 113.4 180)
    (descr "5-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J2 (at 11.2 4 180) (layer B.SilkS))
    (fp_text value Screw_Terminal_1x05 (at 5.08 -4.50088 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad4)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad3)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad5)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_5pol.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyConnectors:Gecko10Pin_SMD_Female (layer F.Cu) (tedit 598CBB14)
    (at 148.5011 105.0036)
    (fp_text reference J3 (at -1.5 5 90) (layer F.SilkS))
    (fp_text value CONN_01X10 (at -3 -2 90) (layer F.Fab))
    (fp_text user 1 (at 0 -1) (layer F.SilkS))
    (pad 1 smd rect (at 0 2) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 1.25 2) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 2.5 2) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 3.75 2) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 5 2) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 0 5.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad5)"))
    (pad 7 smd rect (at 1.25 5.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad4)"))
    (pad 8 smd rect (at 2.5 5.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad3)"))
    (pad 9 smd rect (at 3.75 5.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 10 smd rect (at 5 5.7) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad1)"))
  )
  (gr_line (start 158 116.8) (end 144 116.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 116.8) (end 158 107.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144 100.6) (end 144 116.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 100.6) (end 144 100.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158 107.4) (end 158 100.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 6 (at 146 109.8) (layer B.SilkS))
  (gr_text 7 (at 148.8 109.8) (layer B.SilkS))
  (gr_text 8 (at 151.2 109.8) (layer B.SilkS))
  (gr_text 9 (at 153.8 109.8) (layer B.SilkS))
  (gr_text 10 (at 156.4 109.8) (layer B.SilkS))
  (gr_text 5 (at 156.2 107.6) (layer B.SilkS))
  (gr_text 4 (at 153.4 107.6) (layer B.SilkS))
  (gr_text 3 (at 151 107.6) (layer B.SilkS))
  (gr_text 2 (at 148.6 107.6) (layer B.SilkS))
  (gr_text 1 (at 146.2 107.6) (layer B.SilkS))
)
