(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 243)
    (no_connects 6)
    (area 115.519999 65.989999 200.710001 104.190001)
    (thickness 1.6)
    (drawings 10)
    (tracks 676)
    (zones 0)
    (modules 39)
    (nets 69)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.89 1.1)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDREF)
  (net 2 +5V)
  (net 3 OutputEnable)
  (net 4 SerialData)
  (net 5 DataLatch)
  (net 6 SerialClock)
  (net 7 12V)
  (net 8 /DP1)
  (net 9 /DP2)
  (net 10 "Net-(P3-Pad4)")
  (net 11 "Net-(P3-Pad5)")
  (net 12 "Net-(P3-Pad1)")
  (net 13 "Net-(P3-Pad2)")
  (net 14 "Net-(R1-Pad1)")
  (net 15 "Net-(R2-Pad1)")
  (net 16 "Net-(R3-Pad1)")
  (net 17 "Net-(R4-Pad1)")
  (net 18 "Net-(U1-Pad22)")
  (net 19 "Net-(U3-Pad22)")
  (net 20 "Net-(P4-Pad4)")
  (net 21 "Net-(P4-Pad1)")
  (net 22 "Net-(P4-Pad2)")
  (net 23 "Net-(P5-Pad4)")
  (net 24 "Net-(P5-Pad5)")
  (net 25 "Net-(P5-Pad1)")
  (net 26 "Net-(P5-Pad2)")
  (net 27 "Net-(P6-Pad4)")
  (net 28 "Net-(P6-Pad1)")
  (net 29 "Net-(P6-Pad2)")
  (net 30 "Net-(P7-Pad4)")
  (net 31 "Net-(P7-Pad5)")
  (net 32 "Net-(P7-Pad1)")
  (net 33 "Net-(P7-Pad2)")
  (net 34 "Net-(P8-Pad1)")
  (net 35 "Net-(P8-Pad2)")
  (net 36 "Net-(P8-Pad4)")
  (net 37 "Net-(P9-Pad1)")
  (net 38 "Net-(P9-Pad2)")
  (net 39 "Net-(P9-Pad4)")
  (net 40 /DP3)
  (net 41 "Net-(P9-Pad5)")
  (net 42 "Net-(P10-Pad1)")
  (net 43 "Net-(P10-Pad2)")
  (net 44 "Net-(P10-Pad4)")
  (net 45 /DP4)
  (net 46 "Net-(P11-Pad1)")
  (net 47 "Net-(P11-Pad2)")
  (net 48 "Net-(P11-Pad4)")
  (net 49 "Net-(P11-Pad5)")
  (net 50 "Net-(P12-Pad1)")
  (net 51 "Net-(P12-Pad2)")
  (net 52 "Net-(P12-Pad4)")
  (net 53 /DP5)
  (net 54 "Net-(P13-Pad1)")
  (net 55 "Net-(P13-Pad2)")
  (net 56 "Net-(P13-Pad4)")
  (net 57 "Net-(P13-Pad5)")
  (net 58 "Net-(P14-Pad1)")
  (net 59 "Net-(P14-Pad2)")
  (net 60 "Net-(P14-Pad4)")
  (net 61 /DP6)
  (net 62 "Net-(C7-Pad1)")
  (net 63 "Net-(R7-Pad2)")
  (net 64 "Net-(C6-Pad1)")
  (net 65 "Net-(D1-Pad1)")
  (net 66 "Net-(R5-Pad1)")
  (net 67 "Net-(R6-Pad1)")
  (net 68 "Net-(U2-Pad22)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DP1)
    (add_net /DP2)
    (add_net /DP3)
    (add_net /DP4)
    (add_net /DP5)
    (add_net /DP6)
    (add_net DataLatch)
    (add_net GNDREF)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P10-Pad2)")
    (add_net "Net-(P10-Pad4)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P11-Pad2)")
    (add_net "Net-(P11-Pad4)")
    (add_net "Net-(P11-Pad5)")
    (add_net "Net-(P12-Pad1)")
    (add_net "Net-(P12-Pad2)")
    (add_net "Net-(P12-Pad4)")
    (add_net "Net-(P13-Pad1)")
    (add_net "Net-(P13-Pad2)")
    (add_net "Net-(P13-Pad4)")
    (add_net "Net-(P13-Pad5)")
    (add_net "Net-(P14-Pad1)")
    (add_net "Net-(P14-Pad2)")
    (add_net "Net-(P14-Pad4)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad4)")
    (add_net "Net-(P5-Pad5)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(P7-Pad5)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(P8-Pad2)")
    (add_net "Net-(P8-Pad4)")
    (add_net "Net-(P9-Pad1)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(P9-Pad4)")
    (add_net "Net-(P9-Pad5)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U3-Pad22)")
    (add_net OutputEnable)
    (add_net SerialClock)
    (add_net SerialData)
  )
  (net_class "12V Bus" ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net 12V)
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 56F0715A)
    (at 122.174 70.144 270)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P1 (at 5 -3.5 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 DataLatch))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 SerialClock))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 SerialData))
    (pad 4 thru_hole circle (at 7.5 0 270) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 5 thru_hole circle (at 10 0 270) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 131.572 85.852 270)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U5 (at 0 -3.55 270) (layer F.SilkS))
    (fp_text value TPS61175 (at 0 3.55 270) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -1.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -2.95 -1.3 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D1-Pad1)"))
    (pad 3 smd rect (at -2.95 -0.65 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 4 smd rect (at -2.95 0 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at -2.95 0.65 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C6-Pad1)"))
    (pad 6 smd rect (at -2.95 1.3 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 7 smd rect (at -2.95 1.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 8 smd rect (at 2.95 1.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R5-Pad1)"))
    (pad 9 smd rect (at 2.95 1.3 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R7-Pad2)"))
    (pad 10 smd rect (at 2.95 0.65 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R6-Pad1)"))
    (pad 11 smd rect (at 2.95 0 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 12 smd rect (at 2.95 -0.65 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 13 smd rect (at 2.95 -1.3 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 14 smd rect (at 2.95 -1.95 270) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (model Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:HTSSOP-24_4.4x7.8mm_Pitch0.65mm_ThermalPad (layer F.Cu) (tedit 59916E65)
    (at 180.086 84.892 90)
    (descr "HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad")
    (tags "TSSOP HTSSOP 0.65 thermal pad")
    (attr smd)
    (fp_text reference U3 (at 0 -5.9 90) (layer F.SilkS))
    (fp_text value TLC5927 (at 0 5.9 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.275 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -2.85 -4.225 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at -2.85 -3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U2-Pad22)"))
    (pad 3 smd rect (at -2.85 -2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 SerialClock))
    (pad 4 smd rect (at -2.85 -2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 DataLatch))
    (pad 5 smd rect (at -2.85 -1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(P12-Pad4)"))
    (pad 6 smd rect (at -2.85 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(P12-Pad2)"))
    (pad 7 smd rect (at -2.85 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(P12-Pad1)"))
    (pad 8 smd rect (at -2.85 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(P11-Pad5)"))
    (pad 9 smd rect (at -2.85 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(P11-Pad4)"))
    (pad 10 smd rect (at -2.85 1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(P11-Pad2)"))
    (pad 11 smd rect (at -2.85 2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(P11-Pad1)"))
    (pad 12 smd rect (at -2.85 2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.85 2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(P14-Pad4)"))
    (pad 14 smd rect (at 2.85 2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(P14-Pad2)"))
    (pad 15 smd rect (at 2.85 1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(P14-Pad1)"))
    (pad 16 smd rect (at 2.85 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(P13-Pad5)"))
    (pad 17 smd rect (at 2.85 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(P13-Pad4)"))
    (pad 18 smd rect (at 2.85 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(P13-Pad2)"))
    (pad 19 smd rect (at 2.85 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(P13-Pad1)"))
    (pad 20 smd rect (at 2.85 -1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 2.85 -2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 OutputEnable))
    (pad 22 smd rect (at 2.85 -2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U3-Pad22)"))
    (pad 23 smd rect (at 2.85 -3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R3-Pad1)"))
    (pad 24 smd rect (at 2.85 -4.225 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Housings_SSOP.3dshapes/HTSSOP-28_4.4x9.7mm_Pitch0.65mm_ThermalPad.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 172.212 84.892 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.021 -0.032857 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 175.514 79.248 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.794 0 180) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 189.484 78.994 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 2.651001 -0.043 180) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 186.436 84.638 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -2.972857 -0.027 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:HTSSOP-24_4.4x7.8mm_Pitch0.65mm_ThermalPad (layer F.Cu) (tedit 59916E65)
    (at 194.071 84.638 90)
    (descr "HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad")
    (tags "TSSOP HTSSOP 0.65 thermal pad")
    (attr smd)
    (fp_text reference U4 (at 0 -5.9 90) (layer F.SilkS))
    (fp_text value TLC5927 (at 0 5.9 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.275 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -2.85 -4.225 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at -2.85 -3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U3-Pad22)"))
    (pad 3 smd rect (at -2.85 -2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 SerialClock))
    (pad 4 smd rect (at -2.85 -2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 DataLatch))
    (pad 5 smd rect (at -2.85 -1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.85 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 61 /DP6))
    (pad 7 smd rect (at -2.85 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 /DP5))
    (pad 8 smd rect (at -2.85 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 /DP4))
    (pad 9 smd rect (at -2.85 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 /DP3))
    (pad 10 smd rect (at -2.85 1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /DP2))
    (pad 11 smd rect (at -2.85 2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /DP1))
    (pad 12 smd rect (at -2.85 2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.85 2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 2.85 2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2.85 1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.85 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 2.85 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 2.85 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 2.85 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 2.85 -1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 2.85 -2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 OutputEnable))
    (pad 22 smd rect (at 2.85 -2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.85 -3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R4-Pad1)"))
    (pad 24 smd rect (at 2.85 -4.225 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Housings_SSOP.3dshapes/HTSSOP-28_4.4x9.7mm_Pitch0.65mm_ThermalPad.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 146.624 79.756 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.86 0 180) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 143.51 85.146 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:HTSSOP-24_4.4x7.8mm_Pitch0.65mm_ThermalPad (layer F.Cu) (tedit 59916E65)
    (at 151.283 85.146 90)
    (descr "HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad")
    (tags "TSSOP HTSSOP 0.65 thermal pad")
    (attr smd)
    (fp_text reference U1 (at 0 -5.9 90) (layer F.SilkS))
    (fp_text value TLC5927 (at 0 5.9 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.275 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -2.85 -4.225 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at -2.85 -3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 SerialData))
    (pad 3 smd rect (at -2.85 -2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 SerialClock))
    (pad 4 smd rect (at -2.85 -2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 DataLatch))
    (pad 5 smd rect (at -2.85 -1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P4-Pad4)"))
    (pad 6 smd rect (at -2.85 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P4-Pad2)"))
    (pad 7 smd rect (at -2.85 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P4-Pad1)"))
    (pad 8 smd rect (at -2.85 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P3-Pad5)"))
    (pad 9 smd rect (at -2.85 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P3-Pad4)"))
    (pad 10 smd rect (at -2.85 1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P3-Pad2)"))
    (pad 11 smd rect (at -2.85 2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P3-Pad1)"))
    (pad 12 smd rect (at -2.85 2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.85 2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P6-Pad4)"))
    (pad 14 smd rect (at 2.85 2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P6-Pad2)"))
    (pad 15 smd rect (at 2.85 1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P6-Pad1)"))
    (pad 16 smd rect (at 2.85 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P5-Pad5)"))
    (pad 17 smd rect (at 2.85 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P5-Pad4)"))
    (pad 18 smd rect (at 2.85 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(P5-Pad2)"))
    (pad 19 smd rect (at 2.85 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P5-Pad1)"))
    (pad 20 smd rect (at 2.85 -1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 2.85 -2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 OutputEnable))
    (pad 22 smd rect (at 2.85 -2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 2.85 -3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R1-Pad1)"))
    (pad 24 smd rect (at 2.85 -4.225 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Housings_SSOP.3dshapes/HTSSOP-28_4.4x9.7mm_Pitch0.65mm_ThermalPad.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 157.988 85.09 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.048 0 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 161.29 79.756 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.54 0 180) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDREF))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:HTSSOP-24_4.4x7.8mm_Pitch0.65mm_ThermalPad (layer F.Cu) (tedit 59916E65)
    (at 165.8895 85.261 90)
    (descr "HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad")
    (tags "TSSOP HTSSOP 0.65 thermal pad")
    (attr smd)
    (fp_text reference U2 (at 0 -5.9 90) (layer F.SilkS))
    (fp_text value TLC5927 (at 0 5.9 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.275 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 2.5125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 1.45625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 0.4 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -0.65625 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -1.7125 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -2.76875 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -1.275 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at -0.425 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 1.275 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 thru_hole rect (at 0.425 -3.825 90) (size 0.89 1.1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -2.85 -4.225 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at -2.85 -3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad22)"))
    (pad 3 smd rect (at -2.85 -2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 SerialClock))
    (pad 4 smd rect (at -2.85 -2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 DataLatch))
    (pad 5 smd rect (at -2.85 -1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(P8-Pad4)"))
    (pad 6 smd rect (at -2.85 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(P8-Pad2)"))
    (pad 7 smd rect (at -2.85 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(P8-Pad1)"))
    (pad 8 smd rect (at -2.85 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P7-Pad5)"))
    (pad 9 smd rect (at -2.85 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P7-Pad4)"))
    (pad 10 smd rect (at -2.85 1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(P7-Pad2)"))
    (pad 11 smd rect (at -2.85 2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P7-Pad1)"))
    (pad 12 smd rect (at -2.85 2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.85 2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(P10-Pad4)"))
    (pad 14 smd rect (at 2.85 2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(P10-Pad2)"))
    (pad 15 smd rect (at 2.85 1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(P10-Pad1)"))
    (pad 16 smd rect (at 2.85 0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(P9-Pad5)"))
    (pad 17 smd rect (at 2.85 0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(P9-Pad4)"))
    (pad 18 smd rect (at 2.85 -0.325 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(P9-Pad2)"))
    (pad 19 smd rect (at 2.85 -0.975 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(P9-Pad1)"))
    (pad 20 smd rect (at 2.85 -1.625 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 2.85 -2.275 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 OutputEnable))
    (pad 22 smd rect (at 2.85 -2.925 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 2.85 -3.575 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R2-Pad1)"))
    (pad 24 smd rect (at 2.85 -4.225 90) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Housings_SSOP.3dshapes/HTSSOP-28_4.4x9.7mm_Pitch0.65mm_ThermalPad.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A279DBB)
    (at 154.9 100.076 180)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P4 (at 5 -3.5 180) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(P4-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 /DP1))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 59C1F822)
    (at 144.646 76.962)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P5 (at 4.96 4.572) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(P5-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(P5-Pad4)"))
    (pad 5 thru_hole circle (at 10 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "Net-(P5-Pad5)"))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 59C1F80D)
    (at 144.606 70.104)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P6 (at 5 4.826) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "Net-(P6-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "Net-(P6-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 "Net-(P6-Pad4)"))
    (pad 5 thru_hole circle (at 10 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 /DP2))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A279DC5)
    (at 171.156 93.218 180)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P7 (at 5 -3.5 180) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(P7-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "Net-(P7-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(P7-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(P7-Pad5)"))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A279DC1)
    (at 171.156 100.076 180)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P8 (at 5 -3.5 180) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "Net-(P8-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(P8-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 "Net-(P8-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 /DP3))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A279DF8)
    (at 160.648 76.962)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P9 (at 4.852 4.118) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 "Net-(P9-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 "Net-(P9-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(P9-Pad4)"))
    (pad 5 thru_hole circle (at 10 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(P9-Pad5)"))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 56F0715A)
    (at 122.174 89.956 270)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P2 (at 5 -3.5 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 OutputEnable))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 7.5 0 270) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 10 0 270) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A279DB1)
    (at 154.9 93.218 180)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P3 (at 5 -3.5 180) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(P3-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(P3-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(P3-Pad5)"))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A279DFE)
    (at 160.568 70.104)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P10 (at 4.932 4.766) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(P10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Net-(P10-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Net-(P10-Pad4)"))
    (pad 5 thru_hole circle (at 10 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 /DP4))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A279DCA)
    (at 187.666 93.218 180)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P11 (at 5 -3.5 180) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "Net-(P11-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 "Net-(P11-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 "Net-(P11-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 "Net-(P11-Pad5)"))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A279DCF)
    (at 187.8 100.076 180)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P12 (at 5 -3.5 180) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "Net-(P12-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "Net-(P12-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 "Net-(P12-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 /DP5))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A279E13)
    (at 176.61 76.962)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P13 (at 4.99 4.228) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 "Net-(P13-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 "Net-(P13-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 "Net-(P13-Pad4)"))
    (pad 5 thru_hole circle (at 10 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 57 "Net-(P13-Pad5)"))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A279E0B)
    (at 176.65 70.104)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P14 (at 4.95 4.866) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 5 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 "Net-(P14-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 59 "Net-(P14-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 12V))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 60 "Net-(P14-Pad4)"))
    (pad 5 thru_hole circle (at 10 0) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 61 /DP6))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 140.716 85.09 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value 10.0µF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 130.81 80.01 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value 47nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 127.508 82.804 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value 33nF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 140.208 91.186 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 2.794 0 270) (layer F.SilkS))
    (fp_text value 10.0µF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 12V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 137.922 91.186 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 2.794 -0.254 270) (layer F.SilkS))
    (fp_text value 10.0µF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 12V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 135.636 91.186 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 3.302 -0.254 270) (layer F.SilkS))
    (fp_text value 10.0µF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 12V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 127.508 88.392 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1.02kΩ (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 131.826 92.202)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -2.794 0) (layer F.SilkS))
    (fp_text value 147kΩ (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 131.826 94.488)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -2.86 0) (layer F.SilkS))
    (fp_text value 88.7kΩ (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 12V))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58307B54)
    (at 131.826 96.774)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -3.048 0) (layer F.SilkS))
    (fp_text value 16.2kΩ (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_1206 (layer F.Cu) (tedit 590CEAF5)
    (at 136.906 85.114 270)
    (descr "Diode SMD 1206, reflow soldering http://datasheets.avx.com/schottky.pdf")
    (tags "Diode 1206")
    (attr smd)
    (fp_text reference D1 (at 3.278 0 270) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 12V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_6.3x6.3_H3 (layer F.Cu) (tedit 5990349C)
    (at 136.652 78.232 90)
    (descr "Choke, SMD, 6.3x6.3mm 3mm height")
    (tags "Choke SMD")
    (attr smd)
    (fp_text reference L1 (at 4.826 0 90) (layer F.SilkS))
    (fp_text value 6.8µH (at 0 4.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.75 0 90) (size 1.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2.75 0 90) (size 1.5 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_6.3x6.3_H3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 5VDC (at 125.984 80.264) (layer F.SilkS))
  (gr_text Ground (at 126.238 77.724) (layer F.SilkS))
  (gr_text "Output Enable" (at 127.762 89.916) (layer F.SilkS))
  (gr_text "Serial Data" (at 128.778 75.184) (layer F.SilkS))
  (gr_text "Serial Clock" (at 129.032 72.644) (layer F.SilkS))
  (gr_text Latch (at 127.762 70.104) (layer F.SilkS))
  (gr_line (start 115.57 104.14) (end 115.57 66.04) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.66 104.14) (end 115.57 104.14) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.66 66.04) (end 200.66 104.14) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.57 66.04) (end 200.66 66.04) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.586 66.802) (xy 199.644 66.802) (xy 199.39 103.378) (xy 116.332 103.632)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.586 66.802) (xy 199.644 66.802) (xy 199.39 103.378) (xy 116.332 103.632)
      )
    )
  )
)
