(kicad_pcb (version 20171130) (host pcbnew 6.0.0-rc1-unknown-51473d9~66~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 1380)
    (zones 0)
    (modules 10)
    (nets 168)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 GND.Cu power)
    (2 PWR.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.12)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 32 32)
    (grid_origin 105.85 32)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(SAS0-PadC2)")
  (net 3 "Net-(SAS1-PadC2)")
  (net 4 +12V)
  (net 5 +5V)
  (net 6 /sas0/T2+)
  (net 7 /sas0/T2-)
  (net 8 /sas0/T0-)
  (net 9 /sas0/T0+)
  (net 10 /sas0/SDAT)
  (net 11 /sas0/SCLK)
  (net 12 /sas0/T3+)
  (net 13 /sas0/T3-)
  (net 14 /sas0/T1-)
  (net 15 /sas0/T1+)
  (net 16 /sas0/ACT)
  (net 17 /sas0/R2+)
  (net 18 /sas0/R2-)
  (net 19 /sas0/R0-)
  (net 20 /sas0/R0+)
  (net 21 /sas0/RST)
  (net 22 /sas0/R3-)
  (net 23 /sas0/R3+)
  (net 24 /sas0/R1-)
  (net 25 /sas0/CLK+)
  (net 26 /sas0/CLK-)
  (net 27 /sas0/R1+)
  (net 28 /sas1/T2+)
  (net 29 /sas1/T2-)
  (net 30 /sas1/T0-)
  (net 31 /sas1/T0+)
  (net 32 /sas1/SDAT)
  (net 33 /sas1/SCLK)
  (net 34 /sas1/T3+)
  (net 35 /sas1/T3-)
  (net 36 /sas1/T1-)
  (net 37 /sas1/T1+)
  (net 38 /sas1/ACT)
  (net 39 /sas1/R2+)
  (net 40 /sas1/R2-)
  (net 41 /sas1/R0-)
  (net 42 /sas1/R0+)
  (net 43 /sas1/RST)
  (net 44 /sas1/R3-)
  (net 45 /sas1/R3+)
  (net 46 /sas1/R1-)
  (net 47 /sas1/CLK+)
  (net 48 /sas1/CLK-)
  (net 49 /sas1/R1+)
  (net 50 /sas2/T2+)
  (net 51 /sas2/T2-)
  (net 52 /sas2/T0-)
  (net 53 /sas2/T0+)
  (net 54 /sas2/SDAT)
  (net 55 /sas2/SCLK)
  (net 56 /sas2/T3+)
  (net 57 /sas2/T3-)
  (net 58 /sas2/T1-)
  (net 59 /sas2/T1+)
  (net 60 /sas2/ACT)
  (net 61 "Net-(SAS2-PadC2)")
  (net 62 /sas2/R2+)
  (net 63 /sas2/R2-)
  (net 64 /sas2/R0-)
  (net 65 /sas2/R0+)
  (net 66 /sas2/RST)
  (net 67 /sas2/R3-)
  (net 68 /sas2/R3+)
  (net 69 /sas2/R1-)
  (net 70 /sas2/CLK+)
  (net 71 /sas2/CLK-)
  (net 72 /sas2/R1+)
  (net 73 /sas3/T2+)
  (net 74 /sas3/T2-)
  (net 75 /sas3/T0-)
  (net 76 /sas3/T0+)
  (net 77 /sas3/SDAT)
  (net 78 /sas3/SCLK)
  (net 79 /sas3/T3+)
  (net 80 /sas3/T3-)
  (net 81 /sas3/T1-)
  (net 82 /sas3/T1+)
  (net 83 /sas3/ACT)
  (net 84 "Net-(SAS3-PadC2)")
  (net 85 /sas3/R2+)
  (net 86 /sas3/R2-)
  (net 87 /sas3/R0-)
  (net 88 /sas3/R0+)
  (net 89 /sas3/RST)
  (net 90 /sas3/R3-)
  (net 91 /sas3/R3+)
  (net 92 /sas3/R1-)
  (net 93 /sas3/CLK+)
  (net 94 /sas3/CLK-)
  (net 95 /sas3/R1+)
  (net 96 "Net-(U.2_0-PadE16)")
  (net 97 "Net-(U.2_0-PadS9)")
  (net 98 "Net-(U.2_0-PadS10)")
  (net 99 "Net-(U.2_0-PadS12)")
  (net 100 "Net-(U.2_0-PadS13)")
  (net 101 "Net-(U.2_0-PadE17)")
  (net 102 "Net-(U.2_0-PadP3)")
  (net 103 "Net-(U.2_0-PadP2)")
  (net 104 "Net-(U.2_0-PadS6)")
  (net 105 "Net-(U.2_0-PadS5)")
  (net 106 "Net-(U.2_0-PadS3)")
  (net 107 "Net-(U.2_0-PadS2)")
  (net 108 "Net-(U.2_0-PadE6)")
  (net 109 "Net-(U.2_0-PadP1)")
  (net 110 "Net-(U.2_0-PadE4)")
  (net 111 "Net-(U.2_0-PadE3)")
  (net 112 "Net-(U.2_0-PadE2)")
  (net 113 "Net-(U.2_0-PadE1)")
  (net 114 "Net-(U.2_1-PadE16)")
  (net 115 "Net-(U.2_1-PadS9)")
  (net 116 "Net-(U.2_1-PadS10)")
  (net 117 "Net-(U.2_1-PadS12)")
  (net 118 "Net-(U.2_1-PadS13)")
  (net 119 "Net-(U.2_1-PadE17)")
  (net 120 "Net-(U.2_1-PadP3)")
  (net 121 "Net-(U.2_1-PadP2)")
  (net 122 "Net-(U.2_1-PadS6)")
  (net 123 "Net-(U.2_1-PadS5)")
  (net 124 "Net-(U.2_1-PadS3)")
  (net 125 "Net-(U.2_1-PadS2)")
  (net 126 "Net-(U.2_1-PadE6)")
  (net 127 "Net-(U.2_1-PadP1)")
  (net 128 "Net-(U.2_1-PadE4)")
  (net 129 "Net-(U.2_1-PadE3)")
  (net 130 "Net-(U.2_1-PadE2)")
  (net 131 "Net-(U.2_1-PadE1)")
  (net 132 "Net-(U.2_2-PadE1)")
  (net 133 "Net-(U.2_2-PadE2)")
  (net 134 "Net-(U.2_2-PadE3)")
  (net 135 "Net-(U.2_2-PadE4)")
  (net 136 "Net-(U.2_2-PadP1)")
  (net 137 "Net-(U.2_2-PadE6)")
  (net 138 "Net-(U.2_2-PadS2)")
  (net 139 "Net-(U.2_2-PadS3)")
  (net 140 "Net-(U.2_2-PadS5)")
  (net 141 "Net-(U.2_2-PadS6)")
  (net 142 "Net-(U.2_2-PadP2)")
  (net 143 "Net-(U.2_2-PadP3)")
  (net 144 "Net-(U.2_2-PadE17)")
  (net 145 "Net-(U.2_2-PadS13)")
  (net 146 "Net-(U.2_2-PadS12)")
  (net 147 "Net-(U.2_2-PadS10)")
  (net 148 "Net-(U.2_2-PadS9)")
  (net 149 "Net-(U.2_2-PadE16)")
  (net 150 "Net-(U.2_3-PadE1)")
  (net 151 "Net-(U.2_3-PadE2)")
  (net 152 "Net-(U.2_3-PadE3)")
  (net 153 "Net-(U.2_3-PadE4)")
  (net 154 "Net-(U.2_3-PadP1)")
  (net 155 "Net-(U.2_3-PadE6)")
  (net 156 "Net-(U.2_3-PadS2)")
  (net 157 "Net-(U.2_3-PadS3)")
  (net 158 "Net-(U.2_3-PadS5)")
  (net 159 "Net-(U.2_3-PadS6)")
  (net 160 "Net-(U.2_3-PadP2)")
  (net 161 "Net-(U.2_3-PadP3)")
  (net 162 "Net-(U.2_3-PadE17)")
  (net 163 "Net-(U.2_3-PadS13)")
  (net 164 "Net-(U.2_3-PadS12)")
  (net 165 "Net-(U.2_3-PadS10)")
  (net 166 "Net-(U.2_3-PadS9)")
  (net 167 "Net-(U.2_3-PadE16)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net /sas0/ACT)
    (add_net /sas0/CLK+)
    (add_net /sas0/CLK-)
    (add_net /sas0/R0+)
    (add_net /sas0/R0-)
    (add_net /sas0/R1+)
    (add_net /sas0/R1-)
    (add_net /sas0/R2+)
    (add_net /sas0/R2-)
    (add_net /sas0/R3+)
    (add_net /sas0/R3-)
    (add_net /sas0/RST)
    (add_net /sas0/SCLK)
    (add_net /sas0/SDAT)
    (add_net /sas0/T0+)
    (add_net /sas0/T0-)
    (add_net /sas0/T1+)
    (add_net /sas0/T1-)
    (add_net /sas0/T2+)
    (add_net /sas0/T2-)
    (add_net /sas0/T3+)
    (add_net /sas0/T3-)
    (add_net /sas1/ACT)
    (add_net /sas1/CLK+)
    (add_net /sas1/CLK-)
    (add_net /sas1/R0+)
    (add_net /sas1/R0-)
    (add_net /sas1/R1+)
    (add_net /sas1/R1-)
    (add_net /sas1/R2+)
    (add_net /sas1/R2-)
    (add_net /sas1/R3+)
    (add_net /sas1/R3-)
    (add_net /sas1/RST)
    (add_net /sas1/SCLK)
    (add_net /sas1/SDAT)
    (add_net /sas1/T0+)
    (add_net /sas1/T0-)
    (add_net /sas1/T1+)
    (add_net /sas1/T1-)
    (add_net /sas1/T2+)
    (add_net /sas1/T2-)
    (add_net /sas1/T3+)
    (add_net /sas1/T3-)
    (add_net /sas2/ACT)
    (add_net /sas2/CLK+)
    (add_net /sas2/CLK-)
    (add_net /sas2/R0+)
    (add_net /sas2/R0-)
    (add_net /sas2/R1+)
    (add_net /sas2/R1-)
    (add_net /sas2/R2+)
    (add_net /sas2/R2-)
    (add_net /sas2/R3+)
    (add_net /sas2/R3-)
    (add_net /sas2/RST)
    (add_net /sas2/SCLK)
    (add_net /sas2/SDAT)
    (add_net /sas2/T0+)
    (add_net /sas2/T0-)
    (add_net /sas2/T1+)
    (add_net /sas2/T1-)
    (add_net /sas2/T2+)
    (add_net /sas2/T2-)
    (add_net /sas2/T3+)
    (add_net /sas2/T3-)
    (add_net /sas3/ACT)
    (add_net /sas3/CLK+)
    (add_net /sas3/CLK-)
    (add_net /sas3/R0+)
    (add_net /sas3/R0-)
    (add_net /sas3/R1+)
    (add_net /sas3/R1-)
    (add_net /sas3/R2+)
    (add_net /sas3/R2-)
    (add_net /sas3/R3+)
    (add_net /sas3/R3-)
    (add_net /sas3/RST)
    (add_net /sas3/SCLK)
    (add_net /sas3/SDAT)
    (add_net /sas3/T0+)
    (add_net /sas3/T0-)
    (add_net /sas3/T1+)
    (add_net /sas3/T1-)
    (add_net /sas3/T2+)
    (add_net /sas3/T2-)
    (add_net /sas3/T3+)
    (add_net /sas3/T3-)
    (add_net GND)
    (add_net "Net-(SAS0-PadC2)")
    (add_net "Net-(SAS1-PadC2)")
    (add_net "Net-(SAS2-PadC2)")
    (add_net "Net-(SAS3-PadC2)")
    (add_net "Net-(U.2_0-PadE1)")
    (add_net "Net-(U.2_0-PadE16)")
    (add_net "Net-(U.2_0-PadE17)")
    (add_net "Net-(U.2_0-PadE2)")
    (add_net "Net-(U.2_0-PadE3)")
    (add_net "Net-(U.2_0-PadE4)")
    (add_net "Net-(U.2_0-PadE6)")
    (add_net "Net-(U.2_0-PadP1)")
    (add_net "Net-(U.2_0-PadP2)")
    (add_net "Net-(U.2_0-PadP3)")
    (add_net "Net-(U.2_0-PadS10)")
    (add_net "Net-(U.2_0-PadS12)")
    (add_net "Net-(U.2_0-PadS13)")
    (add_net "Net-(U.2_0-PadS2)")
    (add_net "Net-(U.2_0-PadS3)")
    (add_net "Net-(U.2_0-PadS5)")
    (add_net "Net-(U.2_0-PadS6)")
    (add_net "Net-(U.2_0-PadS9)")
    (add_net "Net-(U.2_1-PadE1)")
    (add_net "Net-(U.2_1-PadE16)")
    (add_net "Net-(U.2_1-PadE17)")
    (add_net "Net-(U.2_1-PadE2)")
    (add_net "Net-(U.2_1-PadE3)")
    (add_net "Net-(U.2_1-PadE4)")
    (add_net "Net-(U.2_1-PadE6)")
    (add_net "Net-(U.2_1-PadP1)")
    (add_net "Net-(U.2_1-PadP2)")
    (add_net "Net-(U.2_1-PadP3)")
    (add_net "Net-(U.2_1-PadS10)")
    (add_net "Net-(U.2_1-PadS12)")
    (add_net "Net-(U.2_1-PadS13)")
    (add_net "Net-(U.2_1-PadS2)")
    (add_net "Net-(U.2_1-PadS3)")
    (add_net "Net-(U.2_1-PadS5)")
    (add_net "Net-(U.2_1-PadS6)")
    (add_net "Net-(U.2_1-PadS9)")
    (add_net "Net-(U.2_2-PadE1)")
    (add_net "Net-(U.2_2-PadE16)")
    (add_net "Net-(U.2_2-PadE17)")
    (add_net "Net-(U.2_2-PadE2)")
    (add_net "Net-(U.2_2-PadE3)")
    (add_net "Net-(U.2_2-PadE4)")
    (add_net "Net-(U.2_2-PadE6)")
    (add_net "Net-(U.2_2-PadP1)")
    (add_net "Net-(U.2_2-PadP2)")
    (add_net "Net-(U.2_2-PadP3)")
    (add_net "Net-(U.2_2-PadS10)")
    (add_net "Net-(U.2_2-PadS12)")
    (add_net "Net-(U.2_2-PadS13)")
    (add_net "Net-(U.2_2-PadS2)")
    (add_net "Net-(U.2_2-PadS3)")
    (add_net "Net-(U.2_2-PadS5)")
    (add_net "Net-(U.2_2-PadS6)")
    (add_net "Net-(U.2_2-PadS9)")
    (add_net "Net-(U.2_3-PadE1)")
    (add_net "Net-(U.2_3-PadE16)")
    (add_net "Net-(U.2_3-PadE17)")
    (add_net "Net-(U.2_3-PadE2)")
    (add_net "Net-(U.2_3-PadE3)")
    (add_net "Net-(U.2_3-PadE4)")
    (add_net "Net-(U.2_3-PadE6)")
    (add_net "Net-(U.2_3-PadP1)")
    (add_net "Net-(U.2_3-PadP2)")
    (add_net "Net-(U.2_3-PadP3)")
    (add_net "Net-(U.2_3-PadS10)")
    (add_net "Net-(U.2_3-PadS12)")
    (add_net "Net-(U.2_3-PadS13)")
    (add_net "Net-(U.2_3-PadS2)")
    (add_net "Net-(U.2_3-PadS3)")
    (add_net "Net-(U.2_3-PadS5)")
    (add_net "Net-(U.2_3-PadS6)")
    (add_net "Net-(U.2_3-PadS9)")
  )
  (module SATA:ATA_FLOPPY_POWER_4 (layer B.Cu) (tedit 5B98213B)
    (at 96.71 99.99 180)
    (descr "Molex ATA Power Connector")
    (attr smd)
    (fp_text reference POWER0 (at 0 4.165 180) (layer B.SilkS))
    (fp_text value ATA_FLOPPY_POWER_4 (at 0 3.5 180) (layer B.Fab))
    (pad 1 thru_hole rect (at -3.75 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 +12V))
    (pad 2 thru_hole oval (at -1.25 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 1.25 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 3.75 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 +5V))
    (model ${KIPRJMOD}/lib/SATA/ATA_FLOPPY_POWER_4.stp
      (offset (xyz 0 0 10.4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SATA:U2_COMBINED_68 (layer F.Cu) (tedit 5B801FC3)
    (at 74 90.3)
    (attr smd)
    (fp_text reference U.2_3 (at 0 8) (layer F.SilkS))
    (fp_text value U2_COMBINED_68 (at 0 -4) (layer F.Fab))
    (pad E1 smd rect (at -7.08 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(U.2_3-PadE1)"))
    (pad E2 smd rect (at -6.28 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(U.2_3-PadE2)"))
    (pad E3 smd rect (at -5.48 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(U.2_3-PadE3)"))
    (pad E4 smd rect (at -4.68 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(U.2_3-PadE4)"))
    (pad E5 smd rect (at -3.88 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 89 /sas3/RST))
    (pad P1 smd rect (at -1.905 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(U.2_3-PadP1)"))
    (pad E6 smd rect (at -3.08 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(U.2_3-PadE6)"))
    (pad S1 smd rect (at -15.875 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S2 smd rect (at -14.605 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(U.2_3-PadS2)"))
    (pad S3 smd rect (at -13.335 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(U.2_3-PadS3)"))
    (pad S4 smd rect (at -12.065 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S5 smd rect (at -10.795 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(U.2_3-PadS5)"))
    (pad S6 smd rect (at -9.525 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(U.2_3-PadS6)"))
    (pad S7 smd rect (at -8.255 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P2 smd rect (at -0.635 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(U.2_3-PadP2)"))
    (pad P3 smd rect (at 0.635 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(U.2_3-PadP3)"))
    (pad P4 smd rect (at 1.905 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P5 smd rect (at 3.175 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P6 smd rect (at 4.445 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P7 smd rect (at 5.715 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P8 smd rect (at 6.985 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P9 smd rect (at 8.255 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P10 smd rect (at 9.525 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P11 smd rect (at 10.795 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 83 /sas3/ACT))
    (pad P12 smd rect (at 12.065 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P13 smd rect (at 13.335 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad P14 smd rect (at 14.605 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad P15 smd rect (at 15.875 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad "" connect rect (at -19.095 -1.14) (size 3.36 3) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at -19.365 2.26) (size 2.6 2.6) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 19.365 2.26) (size 2.6 2.6) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" connect rect (at 19.095 -1.14) (size 3.36 3) (layers F.Cu F.Mask))
    (pad E39 smd rect (at 15.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E38 smd rect (at 14.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 77 /sas3/SDAT))
    (pad E37 smd rect (at 14.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 78 /sas3/SCLK))
    (pad E36 smd rect (at 13.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E35 smd rect (at 12.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 91 /sas3/R3+))
    (pad E34 smd rect (at 11.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 90 /sas3/R3-))
    (pad E33 smd rect (at 10.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E32 smd rect (at 10.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 80 /sas3/T3-))
    (pad E31 smd rect (at 9.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 79 /sas3/T3+))
    (pad E30 smd rect (at 8.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E29 smd rect (at 7.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 85 /sas3/R2+))
    (pad E28 smd rect (at 6.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 86 /sas3/R2-))
    (pad E27 smd rect (at 6.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E26 smd rect (at 5.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 74 /sas3/T2-))
    (pad E25 smd rect (at 4.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 73 /sas3/T2+))
    (pad E24 smd rect (at 3.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E23 smd rect (at 2.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 95 /sas3/R1+))
    (pad E22 smd rect (at 2.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 92 /sas3/R1-))
    (pad E21 smd rect (at 1.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E20 smd rect (at 0.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 81 /sas3/T1-))
    (pad E19 smd rect (at -0.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 82 /sas3/T1+))
    (pad E18 smd rect (at -1.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E17 smd rect (at -1.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(U.2_3-PadE17)"))
    (pad S14 smd rect (at -2.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S13 smd rect (at -3.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(U.2_3-PadS13)"))
    (pad S12 smd rect (at -4.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(U.2_3-PadS12)"))
    (pad S11 smd rect (at -5.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S10 smd rect (at -5.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(U.2_3-PadS10)"))
    (pad S9 smd rect (at -6.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(U.2_3-PadS9)"))
    (pad S8 smd rect (at -7.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E16 smd rect (at -8.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(U.2_3-PadE16)"))
    (pad E15 smd rect (at -9.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E14 smd rect (at -9.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 88 /sas3/R0+))
    (pad E13 smd rect (at -10.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 87 /sas3/R0-))
    (pad E12 smd rect (at -11.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E11 smd rect (at -12.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 75 /sas3/T0-))
    (pad E10 smd rect (at -13.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 76 /sas3/T0+))
    (pad E9 smd rect (at -13.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E8 smd rect (at -14.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 94 /sas3/CLK-))
    (pad E7 smd rect (at -15.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 93 /sas3/CLK+))
    (model ${KIPRJMOD}/lib/SATA/U2_COMBINED_68.stp
      (offset (xyz 41.32 45.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SATA:MINI_SAS_DATA_36 (layer B.Cu) (tedit 5B9A7F65)
    (at 42.12 91.7 180)
    (attr smd)
    (fp_text reference SAS3 (at -10.38 0 90) (layer B.SilkS))
    (fp_text value MINI_SAS_DATA_36 (at 0 8.89 180) (layer B.Fab))
    (pad A4 thru_hole circle (at 4.7 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 95 /sas3/R1+))
    (pad A3 thru_hole circle (at 5.4 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A2 thru_hole circle (at 6.1 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 94 /sas3/CLK-))
    (pad A1 thru_hole circle (at 4.7 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 93 /sas3/CLK+))
    (pad A5 thru_hole circle (at 6.1 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 92 /sas3/R1-))
    (pad A7 thru_hole circle (at 4.7 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 91 /sas3/R3+))
    (pad A6 thru_hole circle (at 5.4 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A9 thru_hole circle (at 5.4 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A8 thru_hole circle (at 6.1 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 90 /sas3/R3-))
    (pad B2 thru_hole circle (at 2.3 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B6 thru_hole circle (at 1.6 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B1 thru_hole circle (at 0.9 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 89 /sas3/RST))
    (pad B4 thru_hole circle (at 0.9 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 88 /sas3/R0+))
    (pad B9 thru_hole circle (at 1.6 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B3 thru_hole circle (at 1.6 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B5 thru_hole circle (at 2.3 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 87 /sas3/R0-))
    (pad B8 thru_hole circle (at 2.3 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 86 /sas3/R2-))
    (pad B7 thru_hole circle (at 0.9 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 85 /sas3/R2+))
    (pad C2 thru_hole circle (at -1.5 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 84 "Net-(SAS3-PadC2)"))
    (pad C6 thru_hole circle (at -2.2 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C1 thru_hole circle (at -2.9 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 83 /sas3/ACT))
    (pad C4 thru_hole circle (at -2.9 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 82 /sas3/T1+))
    (pad C9 thru_hole circle (at -2.2 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C3 thru_hole circle (at -2.2 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C5 thru_hole circle (at -1.5 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 81 /sas3/T1-))
    (pad C8 thru_hole circle (at -1.5 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 80 /sas3/T3-))
    (pad C7 thru_hole circle (at -2.9 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 79 /sas3/T3+))
    (pad D2 thru_hole circle (at -5.3 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 78 /sas3/SCLK))
    (pad D6 thru_hole circle (at -6 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D1 thru_hole circle (at -6.7 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 77 /sas3/SDAT))
    (pad D4 thru_hole circle (at -6.7 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 76 /sas3/T0+))
    (pad D9 thru_hole circle (at -6 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D3 thru_hole circle (at -6 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D5 thru_hole circle (at -5.3 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 75 /sas3/T0-))
    (pad D8 thru_hole circle (at -5.3 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 74 /sas3/T2-))
    (pad D7 thru_hole circle (at -6.7 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 73 /sas3/T2+))
    (pad "" connect circle (at -6 6 180) (size 2.2 2.2) (layers *.SilkS))
    (pad "" np_thru_hole circle (at -6 -6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6 -6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6 6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/lib/SATA/MINI_SAS_DATA_36.stp
      (offset (xyz -0.3 0 14.15))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module SATA:U2_COMBINED_68 (layer F.Cu) (tedit 5B801FC3)
    (at 74 74.3)
    (attr smd)
    (fp_text reference U.2_2 (at 0 8) (layer F.SilkS))
    (fp_text value U2_COMBINED_68 (at 0 -4) (layer F.Fab))
    (pad E1 smd rect (at -7.08 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(U.2_2-PadE1)"))
    (pad E2 smd rect (at -6.28 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(U.2_2-PadE2)"))
    (pad E3 smd rect (at -5.48 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(U.2_2-PadE3)"))
    (pad E4 smd rect (at -4.68 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(U.2_2-PadE4)"))
    (pad E5 smd rect (at -3.88 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 66 /sas2/RST))
    (pad P1 smd rect (at -1.905 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(U.2_2-PadP1)"))
    (pad E6 smd rect (at -3.08 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(U.2_2-PadE6)"))
    (pad S1 smd rect (at -15.875 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S2 smd rect (at -14.605 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(U.2_2-PadS2)"))
    (pad S3 smd rect (at -13.335 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(U.2_2-PadS3)"))
    (pad S4 smd rect (at -12.065 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S5 smd rect (at -10.795 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(U.2_2-PadS5)"))
    (pad S6 smd rect (at -9.525 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(U.2_2-PadS6)"))
    (pad S7 smd rect (at -8.255 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P2 smd rect (at -0.635 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(U.2_2-PadP2)"))
    (pad P3 smd rect (at 0.635 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(U.2_2-PadP3)"))
    (pad P4 smd rect (at 1.905 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P5 smd rect (at 3.175 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P6 smd rect (at 4.445 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P7 smd rect (at 5.715 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P8 smd rect (at 6.985 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P9 smd rect (at 8.255 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P10 smd rect (at 9.525 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P11 smd rect (at 10.795 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 60 /sas2/ACT))
    (pad P12 smd rect (at 12.065 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P13 smd rect (at 13.335 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad P14 smd rect (at 14.605 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad P15 smd rect (at 15.875 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad "" connect rect (at -19.095 -1.14) (size 3.36 3) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at -19.365 2.26) (size 2.6 2.6) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 19.365 2.26) (size 2.6 2.6) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" connect rect (at 19.095 -1.14) (size 3.36 3) (layers F.Cu F.Mask))
    (pad E39 smd rect (at 15.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E38 smd rect (at 14.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 54 /sas2/SDAT))
    (pad E37 smd rect (at 14.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 55 /sas2/SCLK))
    (pad E36 smd rect (at 13.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E35 smd rect (at 12.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 68 /sas2/R3+))
    (pad E34 smd rect (at 11.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 67 /sas2/R3-))
    (pad E33 smd rect (at 10.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E32 smd rect (at 10.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 57 /sas2/T3-))
    (pad E31 smd rect (at 9.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 56 /sas2/T3+))
    (pad E30 smd rect (at 8.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E29 smd rect (at 7.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 62 /sas2/R2+))
    (pad E28 smd rect (at 6.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 63 /sas2/R2-))
    (pad E27 smd rect (at 6.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E26 smd rect (at 5.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 51 /sas2/T2-))
    (pad E25 smd rect (at 4.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 50 /sas2/T2+))
    (pad E24 smd rect (at 3.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E23 smd rect (at 2.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 72 /sas2/R1+))
    (pad E22 smd rect (at 2.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 69 /sas2/R1-))
    (pad E21 smd rect (at 1.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E20 smd rect (at 0.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 58 /sas2/T1-))
    (pad E19 smd rect (at -0.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 59 /sas2/T1+))
    (pad E18 smd rect (at -1.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E17 smd rect (at -1.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(U.2_2-PadE17)"))
    (pad S14 smd rect (at -2.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S13 smd rect (at -3.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(U.2_2-PadS13)"))
    (pad S12 smd rect (at -4.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(U.2_2-PadS12)"))
    (pad S11 smd rect (at -5.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S10 smd rect (at -5.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(U.2_2-PadS10)"))
    (pad S9 smd rect (at -6.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(U.2_2-PadS9)"))
    (pad S8 smd rect (at -7.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E16 smd rect (at -8.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(U.2_2-PadE16)"))
    (pad E15 smd rect (at -9.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E14 smd rect (at -9.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 65 /sas2/R0+))
    (pad E13 smd rect (at -10.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 64 /sas2/R0-))
    (pad E12 smd rect (at -11.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E11 smd rect (at -12.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 52 /sas2/T0-))
    (pad E10 smd rect (at -13.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 53 /sas2/T0+))
    (pad E9 smd rect (at -13.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E8 smd rect (at -14.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 71 /sas2/CLK-))
    (pad E7 smd rect (at -15.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 70 /sas2/CLK+))
    (model ${KIPRJMOD}/lib/SATA/U2_COMBINED_68.stp
      (offset (xyz 41.32 45.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SATA:MINI_SAS_DATA_36 (layer B.Cu) (tedit 5B9A7F65)
    (at 42.12 75.7 180)
    (attr smd)
    (fp_text reference SAS2 (at -10.38 0 90) (layer B.SilkS))
    (fp_text value MINI_SAS_DATA_36 (at 0 8.89 180) (layer B.Fab))
    (pad A4 thru_hole circle (at 4.7 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 72 /sas2/R1+))
    (pad A3 thru_hole circle (at 5.4 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A2 thru_hole circle (at 6.1 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 71 /sas2/CLK-))
    (pad A1 thru_hole circle (at 4.7 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 70 /sas2/CLK+))
    (pad A5 thru_hole circle (at 6.1 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 69 /sas2/R1-))
    (pad A7 thru_hole circle (at 4.7 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 68 /sas2/R3+))
    (pad A6 thru_hole circle (at 5.4 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A9 thru_hole circle (at 5.4 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A8 thru_hole circle (at 6.1 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 67 /sas2/R3-))
    (pad B2 thru_hole circle (at 2.3 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B6 thru_hole circle (at 1.6 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B1 thru_hole circle (at 0.9 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 66 /sas2/RST))
    (pad B4 thru_hole circle (at 0.9 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 65 /sas2/R0+))
    (pad B9 thru_hole circle (at 1.6 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B3 thru_hole circle (at 1.6 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B5 thru_hole circle (at 2.3 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 64 /sas2/R0-))
    (pad B8 thru_hole circle (at 2.3 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 63 /sas2/R2-))
    (pad B7 thru_hole circle (at 0.9 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 62 /sas2/R2+))
    (pad C2 thru_hole circle (at -1.5 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 61 "Net-(SAS2-PadC2)"))
    (pad C6 thru_hole circle (at -2.2 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C1 thru_hole circle (at -2.9 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 60 /sas2/ACT))
    (pad C4 thru_hole circle (at -2.9 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 59 /sas2/T1+))
    (pad C9 thru_hole circle (at -2.2 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C3 thru_hole circle (at -2.2 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C5 thru_hole circle (at -1.5 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 58 /sas2/T1-))
    (pad C8 thru_hole circle (at -1.5 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 57 /sas2/T3-))
    (pad C7 thru_hole circle (at -2.9 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 56 /sas2/T3+))
    (pad D2 thru_hole circle (at -5.3 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 55 /sas2/SCLK))
    (pad D6 thru_hole circle (at -6 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D1 thru_hole circle (at -6.7 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 54 /sas2/SDAT))
    (pad D4 thru_hole circle (at -6.7 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 53 /sas2/T0+))
    (pad D9 thru_hole circle (at -6 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D3 thru_hole circle (at -6 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D5 thru_hole circle (at -5.3 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 52 /sas2/T0-))
    (pad D8 thru_hole circle (at -5.3 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 51 /sas2/T2-))
    (pad D7 thru_hole circle (at -6.7 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 50 /sas2/T2+))
    (pad "" connect circle (at -6 6 180) (size 2.2 2.2) (layers *.SilkS))
    (pad "" np_thru_hole circle (at -6 -6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6 -6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6 6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/lib/SATA/MINI_SAS_DATA_36.stp
      (offset (xyz -0.3 0 14.15))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module SATA:U2_COMBINED_68 (layer F.Cu) (tedit 5B801FC3)
    (at 74 58.3)
    (attr smd)
    (fp_text reference U.2_1 (at 0 8) (layer F.SilkS))
    (fp_text value U2_COMBINED_68 (at 0 -4) (layer F.Fab))
    (pad E7 smd rect (at -15.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 47 /sas1/CLK+))
    (pad E8 smd rect (at -14.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 48 /sas1/CLK-))
    (pad E9 smd rect (at -13.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E10 smd rect (at -13.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 31 /sas1/T0+))
    (pad E11 smd rect (at -12.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 30 /sas1/T0-))
    (pad E12 smd rect (at -11.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E13 smd rect (at -10.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 41 /sas1/R0-))
    (pad E14 smd rect (at -9.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 42 /sas1/R0+))
    (pad E15 smd rect (at -9.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E16 smd rect (at -8.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(U.2_1-PadE16)"))
    (pad S8 smd rect (at -7.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S9 smd rect (at -6.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(U.2_1-PadS9)"))
    (pad S10 smd rect (at -5.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(U.2_1-PadS10)"))
    (pad S11 smd rect (at -5.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S12 smd rect (at -4.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(U.2_1-PadS12)"))
    (pad S13 smd rect (at -3.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(U.2_1-PadS13)"))
    (pad S14 smd rect (at -2.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E17 smd rect (at -1.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(U.2_1-PadE17)"))
    (pad E18 smd rect (at -1.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E19 smd rect (at -0.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 37 /sas1/T1+))
    (pad E20 smd rect (at 0.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 36 /sas1/T1-))
    (pad E21 smd rect (at 1.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E22 smd rect (at 2.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 46 /sas1/R1-))
    (pad E23 smd rect (at 2.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 49 /sas1/R1+))
    (pad E24 smd rect (at 3.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E25 smd rect (at 4.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 28 /sas1/T2+))
    (pad E26 smd rect (at 5.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 29 /sas1/T2-))
    (pad E27 smd rect (at 6.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E28 smd rect (at 6.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 40 /sas1/R2-))
    (pad E29 smd rect (at 7.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 39 /sas1/R2+))
    (pad E30 smd rect (at 8.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E31 smd rect (at 9.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 34 /sas1/T3+))
    (pad E32 smd rect (at 10.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 35 /sas1/T3-))
    (pad E33 smd rect (at 10.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E34 smd rect (at 11.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 44 /sas1/R3-))
    (pad E35 smd rect (at 12.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 45 /sas1/R3+))
    (pad E36 smd rect (at 13.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E37 smd rect (at 14.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 33 /sas1/SCLK))
    (pad E38 smd rect (at 14.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 32 /sas1/SDAT))
    (pad E39 smd rect (at 15.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad "" connect rect (at 19.095 -1.14) (size 3.36 3) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at 19.365 2.26) (size 2.6 2.6) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -19.365 2.26) (size 2.6 2.6) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" connect rect (at -19.095 -1.14) (size 3.36 3) (layers F.Cu F.Mask))
    (pad P15 smd rect (at 15.875 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad P14 smd rect (at 14.605 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad P13 smd rect (at 13.335 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad P12 smd rect (at 12.065 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P11 smd rect (at 10.795 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 38 /sas1/ACT))
    (pad P10 smd rect (at 9.525 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P9 smd rect (at 8.255 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P8 smd rect (at 6.985 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P7 smd rect (at 5.715 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P6 smd rect (at 4.445 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P5 smd rect (at 3.175 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P4 smd rect (at 1.905 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P3 smd rect (at 0.635 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(U.2_1-PadP3)"))
    (pad P2 smd rect (at -0.635 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(U.2_1-PadP2)"))
    (pad S7 smd rect (at -8.255 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S6 smd rect (at -9.525 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(U.2_1-PadS6)"))
    (pad S5 smd rect (at -10.795 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(U.2_1-PadS5)"))
    (pad S4 smd rect (at -12.065 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S3 smd rect (at -13.335 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(U.2_1-PadS3)"))
    (pad S2 smd rect (at -14.605 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(U.2_1-PadS2)"))
    (pad S1 smd rect (at -15.875 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E6 smd rect (at -3.08 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(U.2_1-PadE6)"))
    (pad P1 smd rect (at -1.905 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(U.2_1-PadP1)"))
    (pad E5 smd rect (at -3.88 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 43 /sas1/RST))
    (pad E4 smd rect (at -4.68 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(U.2_1-PadE4)"))
    (pad E3 smd rect (at -5.48 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(U.2_1-PadE3)"))
    (pad E2 smd rect (at -6.28 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(U.2_1-PadE2)"))
    (pad E1 smd rect (at -7.08 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(U.2_1-PadE1)"))
    (model ${KIPRJMOD}/lib/SATA/U2_COMBINED_68.stp
      (offset (xyz 41.32 45.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SATA:MINI_SAS_DATA_36 (layer B.Cu) (tedit 5B9A7F72)
    (at 42.12 43.7 180)
    (attr smd)
    (fp_text reference SAS0 (at -10.38 0 90) (layer B.SilkS))
    (fp_text value MINI_SAS_DATA_36 (at 0 8.89 180) (layer B.Fab))
    (pad A4 thru_hole circle (at 4.7 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 27 /sas0/R1+))
    (pad A3 thru_hole circle (at 5.4 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A2 thru_hole circle (at 6.1 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 26 /sas0/CLK-))
    (pad A1 thru_hole circle (at 4.7 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 25 /sas0/CLK+))
    (pad A5 thru_hole circle (at 6.1 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 24 /sas0/R1-))
    (pad A7 thru_hole circle (at 4.7 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 23 /sas0/R3+))
    (pad A6 thru_hole circle (at 5.4 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A9 thru_hole circle (at 5.4 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A8 thru_hole circle (at 6.1 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 22 /sas0/R3-))
    (pad B2 thru_hole circle (at 2.3 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B6 thru_hole circle (at 1.6 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B1 thru_hole circle (at 0.9 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 21 /sas0/RST))
    (pad B4 thru_hole circle (at 0.9 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 20 /sas0/R0+))
    (pad B9 thru_hole circle (at 1.6 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B3 thru_hole circle (at 1.6 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B5 thru_hole circle (at 2.3 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 19 /sas0/R0-))
    (pad B8 thru_hole circle (at 2.3 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 18 /sas0/R2-))
    (pad B7 thru_hole circle (at 0.9 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 17 /sas0/R2+))
    (pad C2 thru_hole circle (at -1.5 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 2 "Net-(SAS0-PadC2)"))
    (pad C6 thru_hole circle (at -2.2 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C1 thru_hole circle (at -2.9 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 16 /sas0/ACT))
    (pad C4 thru_hole circle (at -2.9 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 15 /sas0/T1+))
    (pad C9 thru_hole circle (at -2.2 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C3 thru_hole circle (at -2.2 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C5 thru_hole circle (at -1.5 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 14 /sas0/T1-))
    (pad C8 thru_hole circle (at -1.5 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 13 /sas0/T3-))
    (pad C7 thru_hole circle (at -2.9 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 12 /sas0/T3+))
    (pad D2 thru_hole circle (at -5.3 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 11 /sas0/SCLK))
    (pad D6 thru_hole circle (at -6 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D1 thru_hole circle (at -6.7 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 10 /sas0/SDAT))
    (pad D4 thru_hole circle (at -6.7 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 9 /sas0/T0+))
    (pad D9 thru_hole circle (at -6 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D3 thru_hole circle (at -6 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D5 thru_hole circle (at -5.3 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 8 /sas0/T0-))
    (pad D8 thru_hole circle (at -5.3 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 7 /sas0/T2-))
    (pad D7 thru_hole circle (at -6.7 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 6 /sas0/T2+))
    (pad "" connect circle (at -6 6 180) (size 2.2 2.2) (layers *.SilkS))
    (pad "" np_thru_hole circle (at -6 -6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6 -6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6 6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/lib/SATA/MINI_SAS_DATA_36.stp
      (offset (xyz -0.3 0 14.15))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module SATA:MINI_SAS_DATA_36 (layer B.Cu) (tedit 5B9A7F65)
    (at 42.12 59.7 180)
    (attr smd)
    (fp_text reference SAS1 (at -10.38 0 90) (layer B.SilkS))
    (fp_text value MINI_SAS_DATA_36 (at 0 8.89 180) (layer B.Fab))
    (pad "" np_thru_hole circle (at 6 6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6 -6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6 -6 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" connect circle (at -6 6 180) (size 2.2 2.2) (layers *.SilkS))
    (pad D7 thru_hole circle (at -6.7 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 28 /sas1/T2+))
    (pad D8 thru_hole circle (at -5.3 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 29 /sas1/T2-))
    (pad D5 thru_hole circle (at -5.3 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 30 /sas1/T0-))
    (pad D3 thru_hole circle (at -6 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D9 thru_hole circle (at -6 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D4 thru_hole circle (at -6.7 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 31 /sas1/T0+))
    (pad D1 thru_hole circle (at -6.7 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 32 /sas1/SDAT))
    (pad D6 thru_hole circle (at -6 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D2 thru_hole circle (at -5.3 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 33 /sas1/SCLK))
    (pad C7 thru_hole circle (at -2.9 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 34 /sas1/T3+))
    (pad C8 thru_hole circle (at -1.5 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 35 /sas1/T3-))
    (pad C5 thru_hole circle (at -1.5 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 36 /sas1/T1-))
    (pad C3 thru_hole circle (at -2.2 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C9 thru_hole circle (at -2.2 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C4 thru_hole circle (at -2.9 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 37 /sas1/T1+))
    (pad C1 thru_hole circle (at -2.9 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 38 /sas1/ACT))
    (pad C6 thru_hole circle (at -2.2 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C2 thru_hole circle (at -1.5 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 3 "Net-(SAS1-PadC2)"))
    (pad B7 thru_hole circle (at 0.9 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 39 /sas1/R2+))
    (pad B8 thru_hole circle (at 2.3 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 40 /sas1/R2-))
    (pad B5 thru_hole circle (at 2.3 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 41 /sas1/R0-))
    (pad B3 thru_hole circle (at 1.6 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B9 thru_hole circle (at 1.6 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B4 thru_hole circle (at 0.9 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 42 /sas1/R0+))
    (pad B1 thru_hole circle (at 0.9 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 43 /sas1/RST))
    (pad B6 thru_hole circle (at 1.6 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B2 thru_hole circle (at 2.3 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A8 thru_hole circle (at 6.1 2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 44 /sas1/R3-))
    (pad A9 thru_hole circle (at 5.4 3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A6 thru_hole circle (at 5.4 0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A7 thru_hole circle (at 4.7 1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 45 /sas1/R3+))
    (pad A5 thru_hole circle (at 6.1 0 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 46 /sas1/R1-))
    (pad A1 thru_hole circle (at 4.7 -3 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 47 /sas1/CLK+))
    (pad A2 thru_hole circle (at 6.1 -2.25 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 48 /sas1/CLK-))
    (pad A3 thru_hole circle (at 5.4 -1.5 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A4 thru_hole circle (at 4.7 -0.75 180) (size 0.37 0.37) (drill 0.32) (layers *.Cu *.Mask)
      (net 49 /sas1/R1+))
    (model ${KIPRJMOD}/lib/SATA/MINI_SAS_DATA_36.stp
      (offset (xyz -0.3 0 14.15))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module SATA:U2_COMBINED_68 (layer F.Cu) (tedit 5B801FC3)
    (at 74 42.3)
    (attr smd)
    (fp_text reference U.2_0 (at 0 8) (layer F.SilkS))
    (fp_text value U2_COMBINED_68 (at 0 -4) (layer F.Fab))
    (pad E7 smd rect (at -15.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 25 /sas0/CLK+))
    (pad E8 smd rect (at -14.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 26 /sas0/CLK-))
    (pad E9 smd rect (at -13.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E10 smd rect (at -13.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 9 /sas0/T0+))
    (pad E11 smd rect (at -12.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /sas0/T0-))
    (pad E12 smd rect (at -11.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E13 smd rect (at -10.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 19 /sas0/R0-))
    (pad E14 smd rect (at -9.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 20 /sas0/R0+))
    (pad E15 smd rect (at -9.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E16 smd rect (at -8.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(U.2_0-PadE16)"))
    (pad S8 smd rect (at -7.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S9 smd rect (at -6.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U.2_0-PadS9)"))
    (pad S10 smd rect (at -5.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(U.2_0-PadS10)"))
    (pad S11 smd rect (at -5.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S12 smd rect (at -4.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(U.2_0-PadS12)"))
    (pad S13 smd rect (at -3.48 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(U.2_0-PadS13)"))
    (pad S14 smd rect (at -2.68 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E17 smd rect (at -1.88 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(U.2_0-PadE17)"))
    (pad E18 smd rect (at -1.08 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E19 smd rect (at -0.28 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 15 /sas0/T1+))
    (pad E20 smd rect (at 0.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 14 /sas0/T1-))
    (pad E21 smd rect (at 1.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E22 smd rect (at 2.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /sas0/R1-))
    (pad E23 smd rect (at 2.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 27 /sas0/R1+))
    (pad E24 smd rect (at 3.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E25 smd rect (at 4.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 /sas0/T2+))
    (pad E26 smd rect (at 5.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /sas0/T2-))
    (pad E27 smd rect (at 6.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E28 smd rect (at 6.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 18 /sas0/R2-))
    (pad E29 smd rect (at 7.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 /sas0/R2+))
    (pad E30 smd rect (at 8.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E31 smd rect (at 9.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 /sas0/T3+))
    (pad E32 smd rect (at 10.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 13 /sas0/T3-))
    (pad E33 smd rect (at 10.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E34 smd rect (at 11.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 22 /sas0/R3-))
    (pad E35 smd rect (at 12.52 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 23 /sas0/R3+))
    (pad E36 smd rect (at 13.32 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E37 smd rect (at 14.12 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 11 /sas0/SCLK))
    (pad E38 smd rect (at 14.92 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 10 /sas0/SDAT))
    (pad E39 smd rect (at 15.72 0) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad "" connect rect (at 19.095 -1.14) (size 3.36 3) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at 19.365 2.26) (size 2.6 2.6) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -19.365 2.26) (size 2.6 2.6) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" connect rect (at -19.095 -1.14) (size 3.36 3) (layers F.Cu F.Mask))
    (pad P15 smd rect (at 15.875 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad P14 smd rect (at 14.605 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad P13 smd rect (at 13.335 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad P12 smd rect (at 12.065 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P11 smd rect (at 10.795 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 16 /sas0/ACT))
    (pad P10 smd rect (at 9.525 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P9 smd rect (at 8.255 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P8 smd rect (at 6.985 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P7 smd rect (at 5.715 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad P6 smd rect (at 4.445 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P5 smd rect (at 3.175 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P4 smd rect (at 1.905 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P3 smd rect (at 0.635 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(U.2_0-PadP3)"))
    (pad P2 smd rect (at -0.635 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(U.2_0-PadP2)"))
    (pad S7 smd rect (at -8.255 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S6 smd rect (at -9.525 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(U.2_0-PadS6)"))
    (pad S5 smd rect (at -10.795 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(U.2_0-PadS5)"))
    (pad S4 smd rect (at -12.065 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S3 smd rect (at -13.335 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U.2_0-PadS3)"))
    (pad S2 smd rect (at -14.605 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U.2_0-PadS2)"))
    (pad S1 smd rect (at -15.875 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad E6 smd rect (at -3.08 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(U.2_0-PadE6)"))
    (pad P1 smd rect (at -1.905 3.97) (size 0.7 1.8) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U.2_0-PadP1)"))
    (pad E5 smd rect (at -3.88 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 21 /sas0/RST))
    (pad E4 smd rect (at -4.68 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U.2_0-PadE4)"))
    (pad E3 smd rect (at -5.48 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(U.2_0-PadE3)"))
    (pad E2 smd rect (at -6.28 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(U.2_0-PadE2)"))
    (pad E1 smd rect (at -7.08 4.59) (size 0.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(U.2_0-PadE1)"))
    (model ${KIPRJMOD}/lib/SATA/U2_COMBINED_68.stp
      (offset (xyz 41.32 45.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Logo:System76 (layer B.Cu) (tedit 0)
    (at 87.945 37 180)
    (attr virtual)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_line (start 109.05 50.4) (end 109.05 85.4) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 107.45 50.4) (end 109.05 50.4) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 105.85 48.8) (end 107.45 48.8) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 105.85 87) (end 107.45 87) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 107.45 85.4) (end 107.45 87) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 102.65 35.2) (end 105.85 35.2) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 102.65 100.6) (end 102.65 103.8) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.85 48.8) (end 105.85 35.2) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 105.85 87) (end 105.85 100.6) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 30.4 50.4) (end 30.4 48.8) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 32 48.8) (end 30.4 48.8) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 32 87) (end 30.4 87) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 30.4 85.4) (end 28.8 85.4) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 28.8 85.4) (end 28.8 50.4) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 32 48.8) (end 32 35.2) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 32 87) (end 32 100.6) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 35.2 32) (end 102.65 32) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 35.2 35.2) (end 35.2 32) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 102.65 103.8) (end 35.2 103.8) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 35.2 100.6) (end 32 100.6) (angle -90) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name GND) (layer GND.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32 32) (xy 105.85 32) (xy 105.85 104) (xy 32 104)
      )
    )
  )
  (zone (net 4) (net_name +12V) (layer PWR.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68 32) (xy 105.85 32) (xy 105.85 104) (xy 68 104)
      )
    )
  )
)
