(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 146)
    (no_connects 2)
    (area 29.924999 19.924999 92.575001 73.575001)
    (thickness 1.6)
    (drawings 64)
    (tracks 1408)
    (zones 0)
    (modules 49)
    (nets 83)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 12 12)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 AGND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 +Vdd)
  (net 5 +AVdd)
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(C8-Pad1)")
  (net 8 "Net-(CON1-Pad1)")
  (net 9 /SPI1_CS1)
  (net 10 /SPI1_MOSI)
  (net 11 /SPI1_CLK)
  (net 12 /SPI1_MISO)
  (net 13 "Net-(CON1-Pad8)")
  (net 14 "Net-(D2-Pad2)")
  (net 15 "Net-(D4-Pad2)")
  (net 16 /PMODE0)
  (net 17 /PMODE1)
  (net 18 /PMODE2)
  (net 19 /SWCLK)
  (net 20 "Net-(P2-Pad1)")
  (net 21 "Net-(P3-Pad1)")
  (net 22 "Net-(P4-Pad1)")
  (net 23 "Net-(P5-Pad1)")
  (net 24 "Net-(P6-Pad1)")
  (net 25 "Net-(P7-Pad1)")
  (net 26 "Net-(P8-Pad1)")
  (net 27 "Net-(P8-Pad2)")
  (net 28 "Net-(P8-Pad3)")
  (net 29 "Net-(P8-Pad4)")
  (net 30 /I2C1_SCL)
  (net 31 /I2C1_SDA)
  (net 32 /I2C2_SCL)
  (net 33 /I2C2_SDA)
  (net 34 "Net-(P14-Pad4)")
  (net 35 "Net-(P14-Pad5)")
  (net 36 "Net-(P14-Pad6)")
  (net 37 "Net-(P14-Pad11)")
  (net 38 "Net-(P14-Pad13)")
  (net 39 "Net-(R2-Pad1)")
  (net 40 "Net-(R3-Pad1)")
  (net 41 "Net-(R4-Pad1)")
  (net 42 "Net-(R5-Pad1)")
  (net 43 "Net-(R6-Pad1)")
  (net 44 /W5500_RST)
  (net 45 /W5500_INT)
  (net 46 "Net-(U1-Pad28)")
  (net 47 "Net-(U1-Pad29)")
  (net 48 "Net-(U1-Pad30)")
  (net 49 "Net-(U1-Pad33)")
  (net 50 "Net-(U1-Pad55)")
  (net 51 "Net-(U1-Pad56)")
  (net 52 /SPI1_CS2)
  (net 53 "Net-(U1-Pad59)")
  (net 54 "Net-(U1-Pad60)")
  (net 55 "Net-(U1-Pad61)")
  (net 56 "Net-(U1-Pad62)")
  (net 57 "Net-(U2-Pad4)")
  (net 58 "Net-(U3-Pad4)")
  (net 59 "Net-(U4-Pad7)")
  (net 60 "Net-(U4-Pad12)")
  (net 61 "Net-(U4-Pad13)")
  (net 62 "Net-(U4-Pad18)")
  (net 63 "Net-(U4-Pad22)")
  (net 64 "Net-(U4-Pad23)")
  (net 65 "Net-(U4-Pad38)")
  (net 66 "Net-(U4-Pad39)")
  (net 67 "Net-(U4-Pad40)")
  (net 68 "Net-(U4-Pad41)")
  (net 69 "Net-(U4-Pad42)")
  (net 70 "Net-(U4-Pad46)")
  (net 71 "Net-(U4-Pad47)")
  (net 72 /TX+)
  (net 73 /TX-)
  (net 74 /RX+)
  (net 75 /RX-)
  (net 76 /SWDIO)
  (net 77 /STM32-OO)
  (net 78 /STM32-OI)
  (net 79 /NRST)
  (net 80 "Net-(C9-Pad1)")
  (net 81 /+12V-Digital)
  (net 82 /+12V-Analog)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+12V-Analog)
    (add_net /+12V-Digital)
    (add_net /I2C1_SCL)
    (add_net /I2C1_SDA)
    (add_net /I2C2_SCL)
    (add_net /I2C2_SDA)
    (add_net /NRST)
    (add_net /PMODE0)
    (add_net /PMODE1)
    (add_net /PMODE2)
    (add_net /SPI1_CLK)
    (add_net /SPI1_CS1)
    (add_net /SPI1_CS2)
    (add_net /SPI1_MISO)
    (add_net /SPI1_MOSI)
    (add_net /STM32-OI)
    (add_net /STM32-OO)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /W5500_INT)
    (add_net /W5500_RST)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad8)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(P14-Pad11)")
    (add_net "Net-(P14-Pad13)")
    (add_net "Net-(P14-Pad4)")
    (add_net "Net-(P14-Pad5)")
    (add_net "Net-(P14-Pad6)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(P8-Pad2)")
    (add_net "Net-(P8-Pad3)")
    (add_net "Net-(P8-Pad4)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad55)")
    (add_net "Net-(U1-Pad56)")
    (add_net "Net-(U1-Pad59)")
    (add_net "Net-(U1-Pad60)")
    (add_net "Net-(U1-Pad61)")
    (add_net "Net-(U1-Pad62)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad13)")
    (add_net "Net-(U4-Pad18)")
    (add_net "Net-(U4-Pad22)")
    (add_net "Net-(U4-Pad23)")
    (add_net "Net-(U4-Pad38)")
    (add_net "Net-(U4-Pad39)")
    (add_net "Net-(U4-Pad40)")
    (add_net "Net-(U4-Pad41)")
    (add_net "Net-(U4-Pad42)")
    (add_net "Net-(U4-Pad46)")
    (add_net "Net-(U4-Pad47)")
    (add_net "Net-(U4-Pad7)")
  )
  (net_class Differential ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /RX+)
    (add_net /RX-)
    (add_net /TX+)
    (add_net /TX-)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +AVdd)
    (add_net +Vdd)
    (add_net AGND)
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 67 31.5)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U4 (at 0 -6) (layer F.SilkS))
    (fp_text value W5500 (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 73 /TX-))
    (pad 2 smd rect (at -4.35 -2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 /TX+))
    (pad 3 smd rect (at -4.35 -1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 4 smd rect (at -4.35 -1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +AVdd))
    (pad 5 smd rect (at -4.35 -0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 75 /RX-))
    (pad 6 smd rect (at -4.35 -0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 74 /RX+))
    (pad 7 smd rect (at -4.35 0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U4-Pad7)"))
    (pad 8 smd rect (at -4.35 0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +AVdd))
    (pad 9 smd rect (at -4.35 1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 10 smd rect (at -4.35 1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R2-Pad1)"))
    (pad 11 smd rect (at -4.35 2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +AVdd))
    (pad 12 smd rect (at -4.35 2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U4-Pad12)"))
    (pad 13 smd rect (at -2.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U4-Pad13)"))
    (pad 14 smd rect (at -2.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 15 smd rect (at -1.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +AVdd))
    (pad 16 smd rect (at -1.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 17 smd rect (at -0.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +AVdd))
    (pad 18 smd rect (at -0.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U4-Pad18)"))
    (pad 19 smd rect (at 0.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 20 smd rect (at 0.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C9-Pad1)"))
    (pad 21 smd rect (at 1.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +AVdd))
    (pad 22 smd rect (at 1.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U4-Pad22)"))
    (pad 23 smd rect (at 2.25 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U4-Pad23)"))
    (pad 24 smd rect (at 2.75 4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R5-Pad1)"))
    (pad 25 smd rect (at 4.35 2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R3-Pad1)"))
    (pad 26 smd rect (at 4.35 2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R6-Pad1)"))
    (pad 27 smd rect (at 4.35 1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R4-Pad1)"))
    (pad 28 smd rect (at 4.35 1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 29 smd rect (at 4.35 0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 30 smd rect (at 4.35 0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 31 smd rect (at 4.35 -0.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 32 smd rect (at 4.35 -0.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 /SPI1_CS2))
    (pad 33 smd rect (at 4.35 -1.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /SPI1_CLK))
    (pad 34 smd rect (at 4.35 -1.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /SPI1_MISO))
    (pad 35 smd rect (at 4.35 -2.25) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /SPI1_MOSI))
    (pad 36 smd rect (at 4.35 -2.75) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 /W5500_INT))
    (pad 37 smd rect (at 2.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 /W5500_RST))
    (pad 38 smd rect (at 2.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U4-Pad38)"))
    (pad 39 smd rect (at 1.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U4-Pad39)"))
    (pad 40 smd rect (at 1.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U4-Pad40)"))
    (pad 41 smd rect (at 0.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U4-Pad41)"))
    (pad 42 smd rect (at 0.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U4-Pad42)"))
    (pad 43 smd rect (at -0.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /PMODE2))
    (pad 44 smd rect (at -0.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /PMODE1))
    (pad 45 smd rect (at -1.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /PMODE0))
    (pad 46 smd rect (at -1.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U4-Pad46)"))
    (pad 47 smd rect (at -2.25 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U4-Pad47)"))
    (pad 48 smd rect (at -2.75 -4.35 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 57.5 44.5 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 77 /STM32-OO))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 57.5 59 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 78 /STM32-OI))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 47.5 61.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 81 /+12V-Digital))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 47.5 64)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 78.5 54.5 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 82 /+12V-Analog))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 82 54.5 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +AVdd))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 76.5 34 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 18uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 76.5 28.5 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 18uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 57 38.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 57 36)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module microSD:microSD-5031821852 (layer F.Cu) (tedit 589FE667)
    (at 39 50 90)
    (fp_text reference CON1 (at 0.3 5.9 90) (layer F.SilkS))
    (fp_text value Micro_SD_Card (at -0.1 -9.8 90) (layer F.Fab))
    (pad 1 smd rect (at 4.249994 -7 90) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(CON1-Pad1)"))
    (pad 2 smd rect (at 3.142852 -7 90) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 9 /SPI1_CS1))
    (pad 3 smd rect (at 2.03571 -7 90) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 10 /SPI1_MOSI))
    (pad 4 smd rect (at 0.928568 -7 90) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 5 smd rect (at -0.178574 -7 90) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 11 /SPI1_CLK))
    (pad 6 smd rect (at -1.285716 -7 90) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 7 smd rect (at -2.392858 -7 90) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 12 /SPI1_MISO))
    (pad 8 smd rect (at -3.5 -7 90) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CON1-Pad8)"))
    (pad 9 smd rect (at 7 -7 90) (size 0.8 1.24) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 9 smd rect (at 3.9 5.7 90) (size 1.5 1.15) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 9 smd rect (at -3.9 5.7 90) (size 1.5 1.15) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 9 smd rect (at -8.2 5 90) (size 1.15 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 9 smd rect (at -8.3 -6.4 90) (size 0.95 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 62 38.5 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 71.5 38.5 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 64 23.5)
    (fp_text reference JP1 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /PMODE0))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 68 23.5)
    (fp_text reference JP2 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /PMODE1))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 72 23.5)
    (fp_text reference JP3 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /PMODE2))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 76.12 62.5 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 +Vdd))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 /SWDIO))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /SWCLK))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 /NRST))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 90.5 21.96 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 90.5 29.868 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 90.5 37.776 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 90.5 45.684 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P5 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 90.5 53.592 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P6 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(P6-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 90.5 61.5 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P7 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(P7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 56.88 71.5)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P8 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(P8-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(P8-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(P8-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 80.46 71.5)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P9 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /I2C1_SCL))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /I2C1_SDA))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 88 71.5)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P10 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /I2C2_SCL))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /I2C2_SDA))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 31.5 62.96 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P11 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 /+12V-Digital))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 42 72)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P12 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 +Vdd))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 31.5 69.46 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P13 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 /+12V-Analog))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 AGND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Custom_Footprints:8p8c-RB1-125BAG1A (layer F.Cu) (tedit 58A22CC4)
    (at 45 31.5 270)
    (fp_text reference P14 (at 0 6.5 270) (layer F.SilkS))
    (fp_text value CNT-RJ45 (at -0.25 -8.5 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -4.45 -2.7 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 72 /TX+))
    (pad 2 thru_hole circle (at -3.15 -5.3 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 73 /TX-))
    (pad 3 thru_hole circle (at -1.916667 -2.7 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 +Vdd))
    (pad 4 thru_hole circle (at -0.616667 -5.3 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "Net-(P14-Pad4)"))
    (pad 5 thru_hole circle (at 0.616666 -2.7 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(P14-Pad5)"))
    (pad 6 thru_hole circle (at 1.916666 -5.3 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 "Net-(P14-Pad6)"))
    (pad 7 thru_hole circle (at 3.149999 -2.7 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 74 /RX+))
    (pad 8 thru_hole circle (at 4.449999 -5.3 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 75 /RX-))
    (pad 9 thru_hole circle (at 7.9 0.6 270) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 10 thru_hole circle (at -7.6 0.6 270) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 11 thru_hole circle (at -3.85 6.85 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 "Net-(P14-Pad11)"))
    (pad 12 thru_hole circle (at -6.4 8.35 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad 13 thru_hole circle (at 6.3 6.85 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 "Net-(P14-Pad13)"))
    (pad 14 thru_hole circle (at 3.8 8.35 270) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 AGND))
    (pad "" np_thru_hole circle (at 6.2 3.7 270) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.7 3.7 270) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 74 28.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 1M (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 61 24 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 12K4 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 47.5 41.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 390K (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(P14-Pad11)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 38 41 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 390K (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(P14-Pad13)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 68.5 40 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 499 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 65 40 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 499 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 56.85 33)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 49R9 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 74 /RX+))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 56.85 30.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 49R9 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 75 /RX-))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 56.85 25.3)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 49R9 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 73 /TX-))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 56.85 27.9)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 49R9 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 72 /TX+))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-64_10x10mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 66.5 50 90)
    (descr "64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -7.2 90) (layer F.SilkS))
    (fp_text value STM32F030R8T6 (at 0 7.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -3.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 2 smd rect (at -5.7 -3.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -5.7 -2.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -5.7 -2.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -5.7 -1.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 /STM32-OI))
    (pad 6 smd rect (at -5.7 -1.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 77 /STM32-OO))
    (pad 7 smd rect (at -5.7 -0.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 /NRST))
    (pad 8 smd rect (at -5.7 -0.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -5.7 0.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -5.7 0.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -5.7 1.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -5.7 1.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 13 smd rect (at -5.7 2.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 14 smd rect (at -5.7 2.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P2-Pad1)"))
    (pad 15 smd rect (at -5.7 3.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P3-Pad1)"))
    (pad 16 smd rect (at -5.7 3.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P4-Pad1)"))
    (pad 17 smd rect (at -3.75 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P5-Pad1)"))
    (pad 18 smd rect (at -3.25 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -2.75 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at -2.25 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P6-Pad1)"))
    (pad 21 smd rect (at -1.75 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P7-Pad1)"))
    (pad 22 smd rect (at -1.25 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(P8-Pad1)"))
    (pad 23 smd rect (at -0.75 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P8-Pad2)"))
    (pad 24 smd rect (at -0.25 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 0.25 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 0.75 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 /W5500_RST))
    (pad 27 smd rect (at 1.25 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 /W5500_INT))
    (pad 28 smd rect (at 1.75 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at 2.25 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 2.75 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at 3.25 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 32 smd rect (at 3.75 5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 33 smd rect (at 5.7 3.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-Pad33)"))
    (pad 34 smd rect (at 5.7 3.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /SPI1_CLK))
    (pad 35 smd rect (at 5.7 2.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /SPI1_MISO))
    (pad 36 smd rect (at 5.7 2.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /SPI1_MOSI))
    (pad 37 smd rect (at 5.7 1.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 5.7 1.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 5.7 0.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 5.7 0.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 5.7 -0.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P8-Pad3)"))
    (pad 42 smd rect (at 5.7 -0.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /I2C1_SCL))
    (pad 43 smd rect (at 5.7 -1.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /I2C1_SDA))
    (pad 44 smd rect (at 5.7 -1.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 /I2C2_SCL))
    (pad 45 smd rect (at 5.7 -2.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 /I2C2_SDA))
    (pad 46 smd rect (at 5.7 -2.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 /SWDIO))
    (pad 47 smd rect (at 5.7 -3.25 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 48 smd rect (at 5.7 -3.75 90) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (pad 49 smd rect (at 3.75 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /SWCLK))
    (pad 50 smd rect (at 3.25 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P8-Pad4)"))
    (pad 51 smd rect (at 2.75 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 52 smd rect (at 2.25 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 53 smd rect (at 1.75 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 54 smd rect (at 1.25 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 55 smd rect (at 0.75 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad55)"))
    (pad 56 smd rect (at 0.25 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-Pad56)"))
    (pad 57 smd rect (at -0.25 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /SPI1_CS1))
    (pad 58 smd rect (at -0.75 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 /SPI1_CS2))
    (pad 59 smd rect (at -1.25 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U1-Pad59)"))
    (pad 60 smd rect (at -1.75 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U1-Pad60)"))
    (pad 61 smd rect (at -2.25 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U1-Pad61)"))
    (pad 62 smd rect (at -2.75 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-Pad62)"))
    (pad 63 smd rect (at -3.25 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 64 smd rect (at -3.75 -5.7 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (model Housings_QFP.3dshapes/LQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 583F3A3F)
    (at 42.5 62.5)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0 -2.9) (layer F.SilkS))
    (fp_text value LD3985M (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 81 /+12V-Digital))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 81 /+12V-Digital))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +Vdd))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 583F3A3F)
    (at 80.175 49.710952 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 0 -2.9 270) (layer F.SilkS))
    (fp_text value LD3985M (at 0 2.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 82 /+12V-Analog))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 82 /+12V-Analog))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 +AVdd))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_HC49-SD_HandSoldering (layer F.Cu) (tedit 5873B462)
    (at 53 51.5 90)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, hand-soldering, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at 0 -3.55 90) (layer F.SilkS))
    (fp_text value Crystal (at 0 3.55 90) (layer F.Fab))
    (pad 1 smd rect (at -5.9375 0 90) (size 7.875 2) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 5.9375 0 90) (size 7.875 2) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model Crystals.3dshapes/Crystal_SMD_HC49-SD_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_HC49-SD_HandSoldering (layer F.Cu) (tedit 5873B462)
    (at 81 33 90)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, hand-soldering, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y2 (at 0 -3.55 90) (layer F.SilkS))
    (fp_text value 25MHz (at 0 3.55 90) (layer F.Fab))
    (pad 1 smd rect (at -5.9375 0 90) (size 7.875 2) (layers F.Cu F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 5.9375 0 90) (size 7.875 2) (layers F.Cu F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (model Crystals.3dshapes/Crystal_SMD_HC49-SD_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 74 34 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 71.5 66.75)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 79 /NRST))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_B3S-1000 (layer F.Cu) (tedit 56EDA1C6)
    (at 55 65.5)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value SW_Push (at 0 4.5) (layer F.Fab))
    (pad 1 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 1 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 AGND))
    (pad 2 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 79 /NRST))
    (pad 2 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 79 /NRST))
  )
  (gr_text SPD (at 72 42) (layer F.SilkS))
  (gr_text DUP (at 61.25 42) (layer F.SilkS))
  (gr_text PA5 (at 87 61.5) (layer B.SilkS))
  (gr_text PA4 (at 86.75 53.5) (layer B.SilkS))
  (gr_text PA3 (at 86.75 45.75) (layer B.SilkS))
  (gr_text PA2 (at 86.75 38) (layer B.SilkS))
  (gr_text PA1 (at 86.5 29.75) (layer B.SilkS))
  (gr_text PA0 (at 86.5 22) (layer B.SilkS))
  (gr_text GND (at 87 64) (layer B.SilkS))
  (gr_text GND (at 86.75 56) (layer B.SilkS))
  (gr_text GND (at 87 48.25) (layer B.SilkS))
  (gr_text GND (at 86.75 40.5) (layer B.SilkS))
  (gr_text GND (at 86.5 32.5) (layer B.SilkS))
  (gr_text GND (at 86.5 24.5) (layer B.SilkS))
  (gr_text "Revision A" (at 53 51.75) (layer B.SilkS))
  (gr_text "David Lenfesty" (at 50.75 47.5) (layer B.SilkS))
  (gr_text STM32F030-Ethernet (at 47 44) (layer B.SilkS))
  (gr_text GND (at 44.5 67.75 90) (layer F.SilkS))
  (gr_text Vdd (at 42 67.75 90) (layer F.SilkS))
  (gr_text GND (at 37.5 72.25) (layer F.SilkS))
  (gr_text 12VA (at 37.75 69.25) (layer F.SilkS))
  (gr_text GND (at 37.75 66) (layer F.SilkS))
  (gr_text 12VD (at 37.5 63) (layer F.SilkS))
  (gr_text PA5 (at 84.75 62.5 90) (layer F.SilkS))
  (gr_text PA4 (at 84.75 55.25 90) (layer F.SilkS))
  (gr_text PA3 (at 84.75 47.25 90) (layer F.SilkS))
  (gr_text PA2 (at 84.75 39 90) (layer F.SilkS))
  (gr_text PA1 (at 84.75 31.25 90) (layer F.SilkS))
  (gr_text PA0 (at 84.75 23.25 90) (layer F.SilkS))
  (gr_text 15 (at 64.5 68.25 90) (layer F.SilkS))
  (gr_text 8 (at 62 69 90) (layer F.SilkS))
  (gr_text 7 (at 59.5 69 90) (layer F.SilkS))
  (gr_text 6 (at 56.75 69 90) (layer F.SilkS))
  (gr_text "Port A" (at 55.75 64.25) (layer F.SilkS))
  (gr_text NRST (at 68.5 58.25 90) (layer F.SilkS))
  (gr_text SWCLK (at 71.25 57.5 90) (layer F.SilkS))
  (gr_text SWDIO (at 73.75 57.5 90) (layer F.SilkS))
  (gr_text Vdd (at 76.25 58.75 90) (layer F.SilkS))
  (gr_text GND (at 68.5 67.5) (layer F.SilkS))
  (gr_text 2 (at 85.8 67.8) (layer F.SilkS))
  (gr_text 1 (at 78.6 67.8) (layer F.SilkS))
  (gr_text SCL (at 80.6 67.8 90) (layer F.SilkS))
  (gr_text SDA (at 90.6 68 90) (layer F.SilkS))
  (gr_text SCL (at 88.1 67.9 90) (layer F.SilkS))
  (gr_text SDA (at 83.1 67.7 90) (layer F.SilkS))
  (gr_text I2C (at 74.25 66.25) (layer F.SilkS))
  (gr_text 2 (at 72 21.1) (layer F.SilkS))
  (gr_text 0 (at 64 21.1) (layer F.SilkS))
  (gr_text 1 (at 68 21.1) (layer F.SilkS))
  (gr_text PMODE (at 79.1 21.6) (layer F.SilkS))
  (gr_text PMODE (at 76.5 22.6) (layer F.Cu))
  (gr_line (start 30 20) (end 92.5 20) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 30 73.5) (end 30 20) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.5 73.5) (end 30 73.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.5 20) (end 92.5 73.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name AGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 20.5) (xy 92 20.5) (xy 92 73) (xy 30.5 73)
      )
    )
  )
)
