(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 598)
    (no_connects 1)
    (area 57.771558 99.809499 182.228443 175.190501)
    (thickness 1.6002)
    (drawings 148)
    (tracks 1273)
    (zones 0)
    (modules 152)
    (nets 204)
  )
  (page A4)
  (layers
    (0 C1F signal)
    (1 C2 signal hide)
    (2 C3 signal hide)
    (31 C4B signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.4572)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2032)
    (edge_width 0.381)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.7874 0.4064)
    (user_via 0.9398 0.508)
    (user_via 1.0668 0.635)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.254)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.1905)
    (pcb_text_size 0.762 1.016)
    (mod_edge_width 0.2032)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 0.8 0.24)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0762)
    (pad_to_paste_clearance_ratio -0.12)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f8_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(C1-Pad1)")
  (net 5 "Net-(C2-Pad2)")
  (net 6 "Net-(C2-Pad1)")
  (net 7 "Net-(C3-Pad2)")
  (net 8 "Net-(C3-Pad1)")
  (net 9 "Net-(C4-Pad2)")
  (net 10 "Net-(C4-Pad1)")
  (net 11 "Net-(C5-Pad2)")
  (net 12 "Net-(C5-Pad1)")
  (net 13 "Net-(C6-Pad2)")
  (net 14 "Net-(C6-Pad1)")
  (net 15 "Net-(C7-Pad2)")
  (net 16 "Net-(C7-Pad1)")
  (net 17 "Net-(C8-Pad2)")
  (net 18 "Net-(C8-Pad1)")
  (net 19 "Net-(C9-Pad2)")
  (net 20 "Net-(C9-Pad1)")
  (net 21 "Net-(C10-Pad2)")
  (net 22 "Net-(C10-Pad1)")
  (net 23 "Net-(C11-Pad2)")
  (net 24 "Net-(C11-Pad1)")
  (net 25 "Net-(C12-Pad2)")
  (net 26 "Net-(C12-Pad1)")
  (net 27 "Net-(DA0-Pad1)")
  (net 28 /U2V3)
  (net 29 "Net-(DAG1-Pad1)")
  (net 30 /U2V1)
  (net 31 /U2V2)
  (net 32 /U2V4)
  (net 33 "Net-(DAY1-Pad1)")
  (net 34 "Net-(DB0-Pad1)")
  (net 35 /U3V3)
  (net 36 "Net-(DBG1-Pad1)")
  (net 37 /U3V1)
  (net 38 /U3V2)
  (net 39 /U3V4)
  (net 40 "Net-(DBY1-Pad1)")
  (net 41 /EXT_U3CTRL1)
  (net 42 /EXT_U2CTRL1)
  (net 43 /EXT_U3CTRL0)
  (net 44 /EXT_U2CTRL0)
  (net 45 /EXT_U1CTRL)
  (net 46 /SDA)
  (net 47 /SCL)
  (net 48 /A0)
  (net 49 /A1)
  (net 50 /A2)
  (net 51 "Net-(R1-Pad2)")
  (net 52 "Net-(R2-Pad2)")
  (net 53 /!LED_EN)
  (net 54 /!RESET)
  (net 55 /!OE)
  (net 56 /U2CTRL1)
  (net 57 /U2CTRL0)
  (net 58 /U3CTRL1)
  (net 59 /U3CTRL0)
  (net 60 /U1CTRL)
  (net 61 /LED_EN2)
  (net 62 /U1VC1)
  (net 63 /U1VC2)
  (net 64 "Net-(J1-Pad3)")
  (net 65 "Net-(J1-Pad4)")
  (net 66 "Net-(J1-Pad5)")
  (net 67 "Net-(J1-Pad6)")
  (net 68 "Net-(J1-Pad7)")
  (net 69 "Net-(J1-Pad8)")
  (net 70 "Net-(J1-Pad9)")
  (net 71 "Net-(J1-Pad10)")
  (net 72 "Net-(J1-Pad11)")
  (net 73 "Net-(J1-Pad12)")
  (net 74 "Net-(J1-Pad13)")
  (net 75 "Net-(J1-Pad14)")
  (net 76 "Net-(J1-Pad15)")
  (net 77 "Net-(J1-Pad16)")
  (net 78 "Net-(J1-Pad17)")
  (net 79 "Net-(J1-Pad18)")
  (net 80 "Net-(J1-Pad19)")
  (net 81 "Net-(J1-Pad20)")
  (net 82 "Net-(J1-Pad21)")
  (net 83 "Net-(J1-Pad22)")
  (net 84 "Net-(J1-Pad23)")
  (net 85 "Net-(J1-Pad24)")
  (net 86 "Net-(J1-Pad25)")
  (net 87 "Net-(J1-Pad26)")
  (net 88 "Net-(J1-Pad27)")
  (net 89 "Net-(J1-Pad28)")
  (net 90 "Net-(J1-Pad29)")
  (net 91 "Net-(J1-Pad30)")
  (net 92 "Net-(J1-Pad31)")
  (net 93 "Net-(J1-Pad32)")
  (net 94 "Net-(J1-Pad33)")
  (net 95 "Net-(J1-Pad34)")
  (net 96 "Net-(J1-Pad35)")
  (net 97 "Net-(J1-Pad36)")
  (net 98 "Net-(J1-Pad37)")
  (net 99 "Net-(J1-Pad38)")
  (net 100 "Net-(J1-Pad39)")
  (net 101 "Net-(J1-Pad40)")
  (net 102 "Net-(J2-Pad2)")
  (net 103 "Net-(J2-Pad3)")
  (net 104 "Net-(J2-Pad4)")
  (net 105 "Net-(J2-Pad5)")
  (net 106 "Net-(J2-Pad11)")
  (net 107 "Net-(J2-Pad12)")
  (net 108 "Net-(J2-Pad13)")
  (net 109 "Net-(J2-Pad14)")
  (net 110 "Net-(J2-Pad15)")
  (net 111 "Net-(J2-Pad16)")
  (net 112 "Net-(J2-Pad17)")
  (net 113 "Net-(J2-Pad18)")
  (net 114 "Net-(J2-Pad19)")
  (net 115 "Net-(J2-Pad20)")
  (net 116 "Net-(J2-Pad21)")
  (net 117 "Net-(J2-Pad22)")
  (net 118 "Net-(J2-Pad23)")
  (net 119 "Net-(J2-Pad24)")
  (net 120 "Net-(J2-Pad25)")
  (net 121 "Net-(J2-Pad26)")
  (net 122 "Net-(J2-Pad27)")
  (net 123 "Net-(J2-Pad28)")
  (net 124 "Net-(J2-Pad29)")
  (net 125 "Net-(J2-Pad30)")
  (net 126 "Net-(J2-Pad31)")
  (net 127 "Net-(J2-Pad32)")
  (net 128 "Net-(J2-Pad33)")
  (net 129 "Net-(J2-Pad34)")
  (net 130 "Net-(J2-Pad35)")
  (net 131 "Net-(J2-Pad36)")
  (net 132 "Net-(J2-Pad37)")
  (net 133 "Net-(J2-Pad38)")
  (net 134 "Net-(P9-Pad4)")
  (net 135 "Net-(P9-Pad5)")
  (net 136 "Net-(P9-Pad6)")
  (net 137 "Net-(P9-Pad7)")
  (net 138 "Net-(P9-Pad10)")
  (net 139 "Net-(P9-Pad11)")
  (net 140 "Net-(P9-Pad12)")
  (net 141 "Net-(P9-Pad13)")
  (net 142 "Net-(P20-Pad1)")
  (net 143 "Net-(P20-Pad2)")
  (net 144 "Net-(P20-Pad4)")
  (net 145 "Net-(P20-Pad6)")
  (net 146 "Net-(P20-Pad7)")
  (net 147 "Net-(P20-Pad8)")
  (net 148 "Net-(P20-Pad14)")
  (net 149 "Net-(P20-Pad16)")
  (net 150 "Net-(P20-Pad17)")
  (net 151 "Net-(P20-Pad18)")
  (net 152 "Net-(P20-Pad20)")
  (net 153 "Net-(P20-Pad21)")
  (net 154 "Net-(P20-Pad22)")
  (net 155 "Net-(P22-Pad1)")
  (net 156 "Net-(P22-Pad2)")
  (net 157 "Net-(P22-Pad3)")
  (net 158 "Net-(P22-Pad5)")
  (net 159 "Net-(P22-Pad6)")
  (net 160 "Net-(P22-Pad7)")
  (net 161 "Net-(P22-Pad8)")
  (net 162 "Net-(P22-Pad9)")
  (net 163 "Net-(P22-Pad12)")
  (net 164 "Net-(P22-Pad13)")
  (net 165 "Net-(P22-Pad14)")
  (net 166 "Net-(P22-Pad15)")
  (net 167 "Net-(P22-Pad16)")
  (net 168 "Net-(P22-Pad17)")
  (net 169 "Net-(P22-Pad19)")
  (net 170 "Net-(P22-Pad20)")
  (net 171 "Net-(P22-Pad21)")
  (net 172 "Net-(P22-Pad22)")
  (net 173 "Net-(P22-Pad23)")
  (net 174 "Net-(P22-Pad25)")
  (net 175 "Net-(P28-Pad3)")
  (net 176 "Net-(P28-Pad4)")
  (net 177 "Net-(P28-Pad5)")
  (net 178 "Net-(P28-Pad6)")
  (net 179 "Net-(P28-Pad7)")
  (net 180 "Net-(P28-Pad8)")
  (net 181 "Net-(P28-Pad9)")
  (net 182 "Net-(P28-Pad10)")
  (net 183 "Net-(P28-Pad11)")
  (net 184 "Net-(P28-Pad13)")
  (net 185 "Net-(P28-Pad14)")
  (net 186 "Net-(P28-Pad15)")
  (net 187 "Net-(P28-Pad16)")
  (net 188 "Net-(P28-Pad17)")
  (net 189 "Net-(P28-Pad18)")
  (net 190 "Net-(P28-Pad19)")
  (net 191 "Net-(P28-Pad20)")
  (net 192 "Net-(P28-Pad21)")
  (net 193 "Net-(P28-Pad22)")
  (net 194 "Net-(U2-Pad3)")
  (net 195 "Net-(U3-Pad3)")
  (net 196 "Net-(U5-Pad1)")
  (net 197 "Net-(U5-Pad7)")
  (net 198 "Net-(U5-Pad8)")
  (net 199 "Net-(U5-Pad9)")
  (net 200 "Net-(U5-Pad11)")
  (net 201 "Net-(U5-Pad12)")
  (net 202 "Net-(U5-Pad13)")
  (net 203 "Net-(P20-Pad13)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2794)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /!LED_EN)
    (add_net /!OE)
    (add_net /!RESET)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /EXT_U1CTRL)
    (add_net /EXT_U2CTRL0)
    (add_net /EXT_U2CTRL1)
    (add_net /EXT_U3CTRL0)
    (add_net /EXT_U3CTRL1)
    (add_net /LED_EN2)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /U1CTRL)
    (add_net /U1VC1)
    (add_net /U1VC2)
    (add_net /U2CTRL0)
    (add_net /U2CTRL1)
    (add_net /U2V1)
    (add_net /U2V2)
    (add_net /U2V3)
    (add_net /U2V4)
    (add_net /U3CTRL0)
    (add_net /U3CTRL1)
    (add_net /U3V1)
    (add_net /U3V2)
    (add_net /U3V3)
    (add_net /U3V4)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(DA0-Pad1)")
    (add_net "Net-(DAG1-Pad1)")
    (add_net "Net-(DAY1-Pad1)")
    (add_net "Net-(DB0-Pad1)")
    (add_net "Net-(DBG1-Pad1)")
    (add_net "Net-(DBY1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad27)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J1-Pad29)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(J1-Pad31)")
    (add_net "Net-(J1-Pad32)")
    (add_net "Net-(J1-Pad33)")
    (add_net "Net-(J1-Pad34)")
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J1-Pad37)")
    (add_net "Net-(J1-Pad38)")
    (add_net "Net-(J1-Pad39)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad40)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad25)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad30)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad34)")
    (add_net "Net-(J2-Pad35)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad37)")
    (add_net "Net-(J2-Pad38)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(P20-Pad1)")
    (add_net "Net-(P20-Pad13)")
    (add_net "Net-(P20-Pad14)")
    (add_net "Net-(P20-Pad16)")
    (add_net "Net-(P20-Pad17)")
    (add_net "Net-(P20-Pad18)")
    (add_net "Net-(P20-Pad2)")
    (add_net "Net-(P20-Pad20)")
    (add_net "Net-(P20-Pad21)")
    (add_net "Net-(P20-Pad22)")
    (add_net "Net-(P20-Pad4)")
    (add_net "Net-(P20-Pad6)")
    (add_net "Net-(P20-Pad7)")
    (add_net "Net-(P20-Pad8)")
    (add_net "Net-(P22-Pad1)")
    (add_net "Net-(P22-Pad12)")
    (add_net "Net-(P22-Pad13)")
    (add_net "Net-(P22-Pad14)")
    (add_net "Net-(P22-Pad15)")
    (add_net "Net-(P22-Pad16)")
    (add_net "Net-(P22-Pad17)")
    (add_net "Net-(P22-Pad19)")
    (add_net "Net-(P22-Pad2)")
    (add_net "Net-(P22-Pad20)")
    (add_net "Net-(P22-Pad21)")
    (add_net "Net-(P22-Pad22)")
    (add_net "Net-(P22-Pad23)")
    (add_net "Net-(P22-Pad25)")
    (add_net "Net-(P22-Pad3)")
    (add_net "Net-(P22-Pad5)")
    (add_net "Net-(P22-Pad6)")
    (add_net "Net-(P22-Pad7)")
    (add_net "Net-(P22-Pad8)")
    (add_net "Net-(P22-Pad9)")
    (add_net "Net-(P28-Pad10)")
    (add_net "Net-(P28-Pad11)")
    (add_net "Net-(P28-Pad13)")
    (add_net "Net-(P28-Pad14)")
    (add_net "Net-(P28-Pad15)")
    (add_net "Net-(P28-Pad16)")
    (add_net "Net-(P28-Pad17)")
    (add_net "Net-(P28-Pad18)")
    (add_net "Net-(P28-Pad19)")
    (add_net "Net-(P28-Pad20)")
    (add_net "Net-(P28-Pad21)")
    (add_net "Net-(P28-Pad22)")
    (add_net "Net-(P28-Pad3)")
    (add_net "Net-(P28-Pad4)")
    (add_net "Net-(P28-Pad5)")
    (add_net "Net-(P28-Pad6)")
    (add_net "Net-(P28-Pad7)")
    (add_net "Net-(P28-Pad8)")
    (add_net "Net-(P28-Pad9)")
    (add_net "Net-(P9-Pad10)")
    (add_net "Net-(P9-Pad11)")
    (add_net "Net-(P9-Pad12)")
    (add_net "Net-(P9-Pad13)")
    (add_net "Net-(P9-Pad4)")
    (add_net "Net-(P9-Pad5)")
    (add_net "Net-(P9-Pad6)")
    (add_net "Net-(P9-Pad7)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad13)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U5-Pad9)")
    (add_net VCC)
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 176.775 154.675)
    (solder_mask_margin 0.1016)
    (fp_text reference DBG1 (at 0.7112 0) (layer F.SilkS))
    (fp_text value LED (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 39 /U3V4) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 36 "Net-(DBG1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 176.775 155.9)
    (solder_mask_margin 0.1016)
    (fp_text reference DBY1 (at 0.7112 0) (layer F.SilkS))
    (fp_text value LED (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 39 /U3V4) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 40 "Net-(DBY1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 176.775 117.55)
    (solder_mask_margin 0.1016)
    (fp_text reference DBG4 (at 0.7112 0) (layer F.SilkS))
    (fp_text value LED (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 35 /U3V3) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 36 "Net-(DBG1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 176.775 118.775)
    (solder_mask_margin 0.1016)
    (fp_text reference DBY4 (at 0.7112 0) (layer F.SilkS))
    (fp_text value LED (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 35 /U3V3) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 40 "Net-(DBY1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 176.775 129.925)
    (solder_mask_margin 0.1016)
    (fp_text reference DBG3 (at 0.7112 0) (layer F.SilkS))
    (fp_text value LED (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 37 /U3V1) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 36 "Net-(DBG1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 176.775 131.15)
    (solder_mask_margin 0.1016)
    (fp_text reference DBY3 (at 0.7112 0) (layer F.SilkS))
    (fp_text value LED (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 37 /U3V1) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 40 "Net-(DBY1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 63.225 118.775 180)
    (solder_mask_margin 0.1016)
    (fp_text reference DAY4 (at 0.7112 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 32 /U2V4) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 33 "Net-(DAY1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 63.225 117.55 180)
    (solder_mask_margin 0.1016)
    (fp_text reference DAG4 (at 0.7112 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 32 /U2V4) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 29 "Net-(DAG1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 67.5 136.75 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C1 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 67.5 112 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C2 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 6 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 167.5 136.75)
    (solder_mask_margin 0.1016)
    (fp_text reference C3 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 7 "Net-(C3-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 "Net-(C3-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 172.5 112)
    (solder_mask_margin 0.1016)
    (fp_text reference C4 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 9 "Net-(C4-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 10 "Net-(C4-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 67.5 149.125 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C5 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 11 "Net-(C5-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 12 "Net-(C5-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 67.5 124.375 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C6 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 14 "Net-(C6-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 167.5 149.525)
    (solder_mask_margin 0.1016)
    (fp_text reference C7 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 15 "Net-(C7-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 16 "Net-(C7-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 172.5 124.375)
    (solder_mask_margin 0.1016)
    (fp_text reference C8 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 17 "Net-(C8-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 18 "Net-(C8-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 115.09248 165.8874 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C9 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 19 "Net-(C9-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 20 "Net-(C9-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 123.87072 165.36416 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C10 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 21 "Net-(C10-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 22 "Net-(C10-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 67.5 161.5 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C11 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 23 "Net-(C11-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 24 "Net-(C11-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 172.475 161.5)
    (solder_mask_margin 0.1016)
    (fp_text reference C12 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 25 "Net-(C12-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 26 "Net-(C12-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 69.1 136.2 90)
    (solder_mask_margin 0.1016)
    (fp_text reference D1 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value GSG-DIODE-TVS-BI (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 69.1 111.5 90)
    (solder_mask_margin 0.1016)
    (fp_text reference D2 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value GSG-DIODE-TVS-BI (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 6 "Net-(C2-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 165.9 136.3 90)
    (solder_mask_margin 0.1016)
    (fp_text reference D3 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value GSG-DIODE-TVS-BI (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 8 "Net-(C3-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 170.9 111.5 90)
    (solder_mask_margin 0.1016)
    (fp_text reference D4 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value GSG-DIODE-TVS-BI (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 10 "Net-(C4-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 69.1 148.6 90)
    (solder_mask_margin 0.1016)
    (fp_text reference D5 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value GSG-DIODE-TVS-BI (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 12 "Net-(C5-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 69.1 123.9 90)
    (solder_mask_margin 0.1016)
    (fp_text reference D6 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value GSG-DIODE-TVS-BI (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 14 "Net-(C6-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 165.9 149 90)
    (solder_mask_margin 0.1016)
    (fp_text reference D7 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value GSG-DIODE-TVS-BI (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 16 "Net-(C7-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 170.9 123.9 90)
    (solder_mask_margin 0.1016)
    (fp_text reference D8 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value GSG-DIODE-TVS-BI (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 18 "Net-(C8-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 69.1 161 90)
    (solder_mask_margin 0.1016)
    (fp_text reference D9 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value GSG-DIODE-TVS-BI (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 24 "Net-(C11-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 170.9 161 90)
    (solder_mask_margin 0.1016)
    (fp_text reference D10 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value GSG-DIODE-TVS-BI (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 26 "Net-(C12-Pad1)") (solder_mask_margin 0.1016))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 63.225 167.05 180)
    (solder_mask_margin 0.1016)
    (fp_text reference DA0 (at 0.7112 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 27 "Net-(DA0-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 63.225 154.675 180)
    (solder_mask_margin 0.1016)
    (fp_text reference DAG1 (at 0.7112 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 28 /U2V3) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 29 "Net-(DAG1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 63.225 142.3 180)
    (solder_mask_margin 0.1016)
    (fp_text reference DAG2 (at 0.7112 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 30 /U2V1) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 29 "Net-(DAG1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 63.225 129.925 180)
    (solder_mask_margin 0.1016)
    (fp_text reference DAG3 (at 0.7112 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 31 /U2V2) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 29 "Net-(DAG1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 63.225 155.9 180)
    (solder_mask_margin 0.1016)
    (fp_text reference DAY1 (at 0.7112 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 28 /U2V3) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 33 "Net-(DAY1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 63.225 143.525 180)
    (solder_mask_margin 0.1016)
    (fp_text reference DAY2 (at 0.7112 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 30 /U2V1) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 33 "Net-(DAY1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 63.225 131.15 180)
    (solder_mask_margin 0.1016)
    (fp_text reference DAY3 (at 0.7112 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 31 /U2V2) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 33 "Net-(DAY1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 176.775 167.05)
    (solder_mask_margin 0.1016)
    (fp_text reference DB0 (at 0.7112 0) (layer F.SilkS))
    (fp_text value LED (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 34 "Net-(DB0-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 176.775 142.3)
    (solder_mask_margin 0.1016)
    (fp_text reference DBG2 (at 0.7112 0) (layer F.SilkS))
    (fp_text value LED (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 38 /U3V2) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 36 "Net-(DBG1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603D (layer C1F) (tedit 56030F0A)
    (at 176.775 143.525)
    (solder_mask_margin 0.1016)
    (fp_text reference DBY2 (at 0.7112 0) (layer F.SilkS))
    (fp_text value LED (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 38 /U3V2) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 40 "Net-(DBY1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:HOLE126MIL-COPPER (layer C1F) (tedit 528F8568)
    (at 64 104)
    (fp_text reference MH1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTING_HOLE (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2004) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module gsg-modules:HOLE126MIL-COPPER (layer C1F) (tedit 528F8568)
    (at 64 171)
    (fp_text reference MH2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTING_HOLE (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2004) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module gsg-modules:HOLE126MIL-COPPER (layer C1F) (tedit 528F8568)
    (at 176 171)
    (fp_text reference MH3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTING_HOLE (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2004) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module gsg-modules:HOLE126MIL-COPPER (layer C1F) (tedit 528F8568)
    (at 176 104)
    (fp_text reference MH4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTING_HOLE (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2004) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module gsg-modules:HOLE126MIL-COPPER (layer C1F) (tedit 528F8568)
    (at 126 104)
    (fp_text reference MH5 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTING_HOLE (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2004) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module gsg-modules:HOLE126MIL-COPPER (layer C1F) (tedit 528F8568)
    (at 131 144)
    (fp_text reference MH6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTING_HOLE (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2004) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 2.2) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.2 0) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 -1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.55 1.55) (size 0.6 0.6) (drill 0.381) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module gsg-modules:HEADER-2x3 (layer C1F) (tedit 4F8A5FD1)
    (at 152.71 154.68)
    (tags CONN)
    (fp_text reference P1 (at 0 0) (layer F.SilkS))
    (fp_text value ADDRESS (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /A0))
    (pad 3 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 4 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /A1))
    (pad 5 thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 6 thru_hole circle (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /A2))
  )
  (module gsg-modules:HEADER-2x8 (layer C1F) (tedit 4F8A6071)
    (at 98.1 129.28 180)
    (tags CONN)
    (fp_text reference P9 (at 0 0 180) (layer F.SilkS))
    (fp_text value BASEBAND (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -8.89 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -8.89 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at -6.35 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at -6.35 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(P9-Pad4)"))
    (pad 5 thru_hole circle (at -3.81 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 135 "Net-(P9-Pad5)"))
    (pad 6 thru_hole circle (at -3.81 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 136 "Net-(P9-Pad6)"))
    (pad 7 thru_hole circle (at -1.27 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 137 "Net-(P9-Pad7)"))
    (pad 8 thru_hole circle (at -1.27 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole circle (at 1.27 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole circle (at 1.27 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 138 "Net-(P9-Pad10)"))
    (pad 11 thru_hole circle (at 3.81 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 139 "Net-(P9-Pad11)"))
    (pad 12 thru_hole circle (at 3.81 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 140 "Net-(P9-Pad12)"))
    (pad 13 thru_hole circle (at 6.35 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 141 "Net-(P9-Pad13)"))
    (pad 14 thru_hole circle (at 6.35 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole circle (at 8.89 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 16 thru_hole circle (at 8.89 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module gsg-modules:HEADER-2x11 (layer C1F) (tedit 52878E74)
    (at 171.76 143.25 90)
    (tags CONN)
    (fp_text reference P20 (at 0 0 90) (layer F.SilkS))
    (fp_text value GPIO (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -12.7 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 142 "Net-(P20-Pad1)"))
    (pad 2 thru_hole circle (at -12.7 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 143 "Net-(P20-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 4 thru_hole circle (at -10.16 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 144 "Net-(P20-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /EXT_U1CTRL))
    (pad 6 thru_hole circle (at -7.62 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 145 "Net-(P20-Pad6)"))
    (pad 7 thru_hole circle (at -5.08 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 146 "Net-(P20-Pad7)"))
    (pad 8 thru_hole circle (at -5.08 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 147 "Net-(P20-Pad8)"))
    (pad 9 thru_hole circle (at -2.54 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /EXT_U2CTRL0))
    (pad 10 thru_hole circle (at -2.54 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /EXT_U2CTRL1))
    (pad 11 thru_hole circle (at 0 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /EXT_U3CTRL0))
    (pad 12 thru_hole circle (at 0 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /EXT_U3CTRL1))
    (pad 13 thru_hole circle (at 2.54 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 203 "Net-(P20-Pad13)"))
    (pad 14 thru_hole circle (at 2.54 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 148 "Net-(P20-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 16 thru_hole circle (at 5.08 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 149 "Net-(P20-Pad16)"))
    (pad 17 thru_hole circle (at 7.62 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 150 "Net-(P20-Pad17)"))
    (pad 18 thru_hole circle (at 7.62 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 151 "Net-(P20-Pad18)"))
    (pad 19 thru_hole circle (at 10.16 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 20 thru_hole circle (at 10.16 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 152 "Net-(P20-Pad20)"))
    (pad 21 thru_hole circle (at 12.7 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 153 "Net-(P20-Pad21)"))
    (pad 22 thru_hole circle (at 12.7 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 154 "Net-(P20-Pad22)"))
  )
  (module gsg-modules:HEADER-2x13 (layer C1F) (tedit 527F1853)
    (at 152.71 164.84 180)
    (tags CONN)
    (fp_text reference P22 (at 0 0 180) (layer F.SilkS))
    (fp_text value I2S (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -15.24 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 155 "Net-(P22-Pad1)"))
    (pad 2 thru_hole circle (at -15.24 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 156 "Net-(P22-Pad2)"))
    (pad 3 thru_hole circle (at -12.7 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 157 "Net-(P22-Pad3)"))
    (pad 4 thru_hole circle (at -12.7 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at -10.16 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 158 "Net-(P22-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 159 "Net-(P22-Pad6)"))
    (pad 7 thru_hole circle (at -7.62 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 160 "Net-(P22-Pad7)"))
    (pad 8 thru_hole circle (at -7.62 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 161 "Net-(P22-Pad8)"))
    (pad 9 thru_hole circle (at -5.08 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 162 "Net-(P22-Pad9)"))
    (pad 10 thru_hole circle (at -5.08 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 11 thru_hole circle (at -2.54 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 12 thru_hole circle (at -2.54 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 163 "Net-(P22-Pad12)"))
    (pad 13 thru_hole circle (at 0 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 164 "Net-(P22-Pad13)"))
    (pad 14 thru_hole circle (at 0 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 165 "Net-(P22-Pad14)"))
    (pad 15 thru_hole circle (at 2.54 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 166 "Net-(P22-Pad15)"))
    (pad 16 thru_hole circle (at 2.54 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 167 "Net-(P22-Pad16)"))
    (pad 17 thru_hole circle (at 5.08 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 168 "Net-(P22-Pad17)"))
    (pad 18 thru_hole circle (at 5.08 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 19 thru_hole circle (at 7.62 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 169 "Net-(P22-Pad19)"))
    (pad 20 thru_hole circle (at 7.62 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 170 "Net-(P22-Pad20)"))
    (pad 21 thru_hole circle (at 10.16 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 171 "Net-(P22-Pad21)"))
    (pad 22 thru_hole circle (at 10.16 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 172 "Net-(P22-Pad22)"))
    (pad 23 thru_hole circle (at 12.7 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 173 "Net-(P22-Pad23)"))
    (pad 24 thru_hole circle (at 12.7 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /SDA))
    (pad 25 thru_hole circle (at 15.24 1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 174 "Net-(P22-Pad25)"))
    (pad 26 thru_hole circle (at 15.24 -1.27 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /SCL))
  )
  (module gsg-modules:HEADER-2x11 (layer C1F) (tedit 52878E74)
    (at 123.5 143.25 90)
    (tags CONN)
    (fp_text reference P28 (at 0 0 90) (layer F.SilkS))
    (fp_text value SD (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -12.7 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole circle (at -12.7 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at -10.16 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 175 "Net-(P28-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 176 "Net-(P28-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 177 "Net-(P28-Pad5)"))
    (pad 6 thru_hole circle (at -7.62 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 178 "Net-(P28-Pad6)"))
    (pad 7 thru_hole circle (at -5.08 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 179 "Net-(P28-Pad7)"))
    (pad 8 thru_hole circle (at -5.08 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 180 "Net-(P28-Pad8)"))
    (pad 9 thru_hole circle (at -2.54 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 181 "Net-(P28-Pad9)"))
    (pad 10 thru_hole circle (at -2.54 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 182 "Net-(P28-Pad10)"))
    (pad 11 thru_hole circle (at 0 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 183 "Net-(P28-Pad11)"))
    (pad 12 thru_hole circle (at 0 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 13 thru_hole circle (at 2.54 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 184 "Net-(P28-Pad13)"))
    (pad 14 thru_hole circle (at 2.54 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 185 "Net-(P28-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 186 "Net-(P28-Pad15)"))
    (pad 16 thru_hole circle (at 5.08 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 187 "Net-(P28-Pad16)"))
    (pad 17 thru_hole circle (at 7.62 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 188 "Net-(P28-Pad17)"))
    (pad 18 thru_hole circle (at 7.62 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 189 "Net-(P28-Pad18)"))
    (pad 19 thru_hole circle (at 10.16 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 190 "Net-(P28-Pad19)"))
    (pad 20 thru_hole circle (at 10.16 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 191 "Net-(P28-Pad20)"))
    (pad 21 thru_hole circle (at 12.7 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 192 "Net-(P28-Pad21)"))
    (pad 22 thru_hole circle (at 12.7 -1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 193 "Net-(P28-Pad22)"))
  )
  (module hackrf:GSG-SMA-73251-2120 (layer C1F) (tedit 52DD8040)
    (at 61.02 161.5)
    (fp_text reference PA0 (at 1.99898 0) (layer F.SilkS))
    (fp_text value GSG-RF-CONN (at 1.99898 4.0005) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.095 0) (size 4.19 1.78) (layers C1F F.Mask)
      (net 23 "Net-(C11-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 2.095 -3.4925) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND) (die_length 509.13792))
    (pad 2 smd rect (at 2.095 -3.4925) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND) (die_length 483.12832))
    (pad 2 thru_hole circle (at 3.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
  )
  (module hackrf:GSG-SMA-73251-2120 (layer C1F) (tedit 52DD8040)
    (at 61.02 149.125)
    (fp_text reference PA1 (at 1.99898 0) (layer F.SilkS))
    (fp_text value GSG-RF-CONN (at 1.99898 4.0005) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.095 0) (size 4.19 1.78) (layers C1F F.Mask)
      (net 11 "Net-(C5-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 2.095 -3.4925) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND) (die_length 509.13792))
    (pad 2 smd rect (at 2.095 -3.4925) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND) (die_length 483.12832))
    (pad 2 thru_hole circle (at 3.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
  )
  (module hackrf:GSG-SMA-73251-2120 (layer C1F) (tedit 52DD8040)
    (at 61.02 136.75)
    (fp_text reference PA2 (at 1.99898 0) (layer F.SilkS))
    (fp_text value GSG-RF-CONN (at 1.99898 4.0005) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.095 0) (size 4.19 1.78) (layers C1F F.Mask)
      (net 3 "Net-(C1-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 2.095 -3.4925) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND) (die_length 509.13792))
    (pad 2 smd rect (at 2.095 -3.4925) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND) (die_length 483.12832))
    (pad 2 thru_hole circle (at 3.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
  )
  (module hackrf:GSG-SMA-73251-2120 (layer C1F) (tedit 52DD8040)
    (at 61.02 124.375)
    (fp_text reference PA3 (at 1.99898 0) (layer F.SilkS))
    (fp_text value GSG-RF-CONN (at 1.99898 4.0005) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.095 0) (size 4.19 1.78) (layers C1F F.Mask)
      (net 13 "Net-(C6-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 2.095 -3.4925) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND) (die_length 509.13792))
    (pad 2 smd rect (at 2.095 -3.4925) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND) (die_length 483.12832))
    (pad 2 thru_hole circle (at 3.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
  )
  (module hackrf:GSG-SMA-73251-2120 (layer C1F) (tedit 52DD8040)
    (at 61.02 112)
    (fp_text reference PA4 (at 1.99898 0) (layer F.SilkS))
    (fp_text value GSG-RF-CONN (at 1.99898 4.0005) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.095 0) (size 4.19 1.78) (layers C1F F.Mask)
      (net 5 "Net-(C2-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 2.095 -3.4925) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND) (die_length 509.13792))
    (pad 2 smd rect (at 2.095 -3.4925) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND) (die_length 483.12832))
    (pad 2 thru_hole circle (at 3.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -2.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -3.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -4.5) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
  )
  (module hackrf:GSG-SMA-73251-2120 (layer C1F) (tedit 52DD8040)
    (at 178.98 161.5 180)
    (fp_text reference PB0 (at 1.99898 0 180) (layer F.SilkS))
    (fp_text value GSG-RF-CONN (at 1.99898 4.0005 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.095 0 180) (size 4.19 1.78) (layers C1F F.Mask)
      (net 25 "Net-(C12-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 2.095 -3.4925 180) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925 180) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND) (die_length 509.13792))
    (pad 2 smd rect (at 2.095 -3.4925 180) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925 180) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND) (die_length 483.12832))
    (pad 2 thru_hole circle (at 3.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
  )
  (module hackrf:GSG-SMA-73251-2120 (layer C1F) (tedit 52DD8040)
    (at 178.98 149.125 180)
    (fp_text reference PB1 (at 1.99898 0 180) (layer F.SilkS))
    (fp_text value GSG-RF-CONN (at 1.99898 4.0005 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.095 0 180) (size 4.19 1.78) (layers C1F F.Mask)
      (net 15 "Net-(C7-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 2.095 -3.4925 180) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925 180) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND) (die_length 509.13792))
    (pad 2 smd rect (at 2.095 -3.4925 180) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925 180) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND) (die_length 483.12832))
    (pad 2 thru_hole circle (at 3.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
  )
  (module hackrf:GSG-SMA-73251-2120 (layer C1F) (tedit 52DD8040)
    (at 178.98 136.75 180)
    (fp_text reference PB2 (at 1.99898 0 180) (layer F.SilkS))
    (fp_text value GSG-RF-CONN (at 1.99898 4.0005 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.095 0 180) (size 4.19 1.78) (layers C1F F.Mask)
      (net 7 "Net-(C3-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 2.095 -3.4925 180) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925 180) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND) (die_length 509.13792))
    (pad 2 smd rect (at 2.095 -3.4925 180) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925 180) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND) (die_length 483.12832))
    (pad 2 thru_hole circle (at 3.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
  )
  (module hackrf:GSG-SMA-73251-2120 (layer C1F) (tedit 52DD8040)
    (at 178.98 124.375 180)
    (fp_text reference PB3 (at 1.99898 0 180) (layer F.SilkS))
    (fp_text value GSG-RF-CONN (at 1.99898 4.0005 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.095 0 180) (size 4.19 1.78) (layers C1F F.Mask)
      (net 17 "Net-(C8-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 2.095 -3.4925 180) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925 180) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND) (die_length 509.13792))
    (pad 2 smd rect (at 2.095 -3.4925 180) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925 180) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND) (die_length 483.12832))
    (pad 2 thru_hole circle (at 3.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
  )
  (module hackrf:GSG-SMA-73251-2120 (layer C1F) (tedit 52DD8040)
    (at 178.98 112 180)
    (fp_text reference PB4 (at 1.99898 0 180) (layer F.SilkS))
    (fp_text value GSG-RF-CONN (at 1.99898 4.0005 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.095 0 180) (size 4.19 1.78) (layers C1F F.Mask)
      (net 9 "Net-(C4-Pad2)") (die_length -2147.483648))
    (pad 2 smd rect (at 2.095 -3.4925 180) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925 180) (size 4.19 2.665) (layers C1F F.Mask)
      (net 1 GND) (die_length 509.13792))
    (pad 2 smd rect (at 2.095 -3.4925 180) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.095 3.4925 180) (size 4.19 2.665) (layers C4B B.Mask)
      (net 1 GND) (die_length 483.12832))
    (pad 2 thru_hole circle (at 3.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -2.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -3.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.5 -4.5 180) (size 0.6 0.6) (drill 0.381) (layers *.Cu)
      (net 1 GND))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 112.3188 130.048 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 330 (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 51 "Net-(R1-Pad2)") (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 29 "Net-(DAG1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 112.4966 124.968 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 330 (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 52 "Net-(R2-Pad2)") (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 33 "Net-(DAY1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 110.49 123.4694 270)
    (solder_mask_margin 0.1016)
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 270) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 52 "Net-(R2-Pad2)") (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 270) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 36 "Net-(DBG1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 110.4646 128.5748 270)
    (solder_mask_margin 0.1016)
    (fp_text reference R4 (at 0 0 270) (layer F.SilkS))
    (fp_text value 330 (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 270) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 51 "Net-(R1-Pad2)") (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 270) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 40 "Net-(DBY1-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 134.5 140.5 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R5 (at 0 0 90) (layer F.SilkS))
    (fp_text value 330 (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 53 /!LED_EN) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 27 "Net-(DA0-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 136.5 140.5 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R6 (at 0 0 90) (layer F.SilkS))
    (fp_text value 330 (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 53 /!LED_EN) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 34 "Net-(DB0-Pad1)") (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 134 166.1)
    (solder_mask_margin 0.1016)
    (fp_text reference R7 (at 0 0) (layer F.SilkS))
    (fp_text value 1k8 (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 47 /SCL) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 140.8 168.6 180)
    (solder_mask_margin 0.1016)
    (fp_text reference R8 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1k8 (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 46 /SDA) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 131.5 139.5)
    (solder_mask_margin 0.1016)
    (fp_text reference R9 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 53 /!LED_EN) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 130.74396 133.91388)
    (solder_mask_margin 0.1016)
    (fp_text reference R10 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 54 /!RESET) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 140.589 128.79324)
    (solder_mask_margin 0.1016)
    (fp_text reference R11 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 55 /!OE) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 130.77 106.8236)
    (solder_mask_margin 0.1016)
    (fp_text reference R12 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 56 /U2CTRL1) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 125.5 126 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R13 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 57 /U2CTRL0) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 134.77 106.8236)
    (solder_mask_margin 0.1016)
    (fp_text reference R14 (at 0 0) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 58 /U3CTRL1) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 138.7 121.7 180)
    (solder_mask_margin 0.1016)
    (fp_text reference R15 (at 0 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 59 /U3CTRL0) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 117.336777 136.475619 180)
    (solder_mask_margin 0.1016)
    (fp_text reference R16 (at 0 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 180) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 60 /U1CTRL) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 150.2 149.6 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R17 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 48 /A0) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 152.7 149.6 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R18 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 49 /A1) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 155.2 149.6 90)
    (solder_mask_margin 0.1016)
    (fp_text reference R19 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 90) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 50 /A2) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:0603 (layer C1F) (tedit 5605D54C)
    (at 128.1 135.8 270)
    (solder_mask_margin 0.1016)
    (fp_text reference R20 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0 270) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016) (clearance 0.1778))
    (pad 1 smd rect (at -0.762 0 270) (size 0.8636 0.8636) (layers C1F F.Paste F.Mask)
      (net 61 /LED_EN2) (solder_mask_margin 0.1016) (clearance 0.1778))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 149 129.8)
    (fp_text reference TP1 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 42 /EXT_U2CTRL1))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 163.11372 144.19834)
    (fp_text reference TP2 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 44 /EXT_U2CTRL0))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 151.2 128.3)
    (fp_text reference TP3 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 41 /EXT_U3CTRL1))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 153.5 127)
    (fp_text reference TP4 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 43 /EXT_U3CTRL0))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 163.5 148)
    (fp_text reference TP5 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 45 /EXT_U1CTRL))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 139.4 141.1)
    (fp_text reference TP6 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 53 /!LED_EN))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 134.4 131.3)
    (fp_text reference TP7 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 54 /!RESET))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 140.5 130.5)
    (fp_text reference TP8 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 55 /!OE))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 118.2 136.5 90)
    (fp_text reference TP9 (at 0 0 90) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0 90) (size 1.27 1.27) (layers C4B B.Mask)
      (net 60 /U1CTRL))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 129.6 131.9)
    (fp_text reference TP10 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 57 /U2CTRL0))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 138.6 124.1)
    (fp_text reference TP11 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 56 /U2CTRL1))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 138.2 120.5)
    (fp_text reference TP12 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 59 /U3CTRL0))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 133.77 104.3236)
    (fp_text reference TP13 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 58 /U3CTRL1))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 111 128)
    (fp_text reference TP14 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 1 GND))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 122.3 125.2)
    (fp_text reference TP15 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 2 VCC))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 115.8 151 90)
    (fp_text reference TP16 (at 0 0 90) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0 90) (size 1.27 1.27) (layers C4B B.Mask)
      (net 62 /U1VC1))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 113.1062 156.2862)
    (fp_text reference TP17 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 63 /U1VC2))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 67.9 142.9)
    (fp_text reference TP18 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 30 /U2V1))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 73.5 130.5)
    (fp_text reference TP19 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 31 /U2V2))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 85.3 140.7)
    (fp_text reference TP20 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 28 /U2V3))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 82.4 124)
    (fp_text reference TP21 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 32 /U2V4))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 168.2 129.6)
    (fp_text reference TP22 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 37 /U3V1))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 162.03168 133.72592)
    (fp_text reference TP23 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 38 /U3V2))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 162 118.2)
    (fp_text reference TP24 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 35 /U3V3))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 153 140.667998)
    (fp_text reference TP25 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 39 /U3V4))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 133.5 162)
    (fp_text reference TP26 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 46 /SDA))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 131 164)
    (fp_text reference TP27 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 47 /SCL))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 146.7 155.1)
    (fp_text reference TP28 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 48 /A0))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 140.6 135.7)
    (fp_text reference TP29 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 49 /A1))
  )
  (module gsg-modules:TESTPOINT-50MIL (layer C4B) (tedit 50997FDC)
    (at 140.44 138.6)
    (fp_text reference TP30 (at 0 0) (layer B.SilkS))
    (fp_text value CONN_1 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.27 1.27) (layers C4B B.Mask)
      (net 50 /A2))
  )
  (module gsg-modules:QFN12-3 (layer C1F) (tedit 57F1C708)
    (at 120 169 180)
    (solder_mask_margin 0.07112)
    (clearance 0.1524)
    (fp_text reference U1 (at 0 0 180) (layer F.SilkS))
    (fp_text value MASWSS0129 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd oval (at -1.7 -0.5 180) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd oval (at -1.7 0 180) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd oval (at -1.7 0.5 180) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 62 /U1VC1))
    (pad 4 smd oval (at -0.5 1.7 270) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 21 "Net-(C10-Pad2)"))
    (pad 5 smd oval (at 0 1.7 270) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd oval (at 0.5 1.7 270) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 20 "Net-(C9-Pad1)"))
    (pad 7 smd oval (at 1.7 0.5 180) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 63 /U1VC2))
    (pad 8 smd oval (at 1.7 0 180) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd oval (at 1.7 -0.5 180) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd oval (at 0.5 -1.7 270) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 24 "Net-(C11-Pad1)"))
    (pad 11 smd oval (at 0 -1.7 270) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd oval (at -0.5 -1.7 270) (size 1.2 0.32) (layers C1F F.Paste F.Mask)
      (net 26 "Net-(C12-Pad1)"))
    (pad 0 smd rect (at 0 0 180) (size 1 1) (layers C1F F.Mask)
      (net 1 GND) (solder_mask_margin -0.09906))
    (pad 0 thru_hole circle (at -0.25 -0.25 180) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu B.Mask)
      (net 1 GND))
    (pad 0 thru_hole circle (at 0.25 -0.25 180) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu B.Mask)
      (net 1 GND))
    (pad 0 thru_hole circle (at 0.25 0.25 180) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu B.Mask)
      (net 1 GND))
    (pad 0 thru_hole circle (at -0.25 0.25 180) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu B.Mask)
      (net 1 GND))
    (pad 0 smd rect (at -0.25 -0.25 180) (size 0.5 0.5) (layers C1F F.Paste)
      (net 1 GND))
    (pad 0 smd rect (at 0.25 -0.25 180) (size 0.5 0.5) (layers C1F F.Paste)
      (net 1 GND))
    (pad 0 smd rect (at -0.25 0.25 180) (size 0.5 0.5) (layers C1F F.Paste)
      (net 1 GND))
    (pad 0 smd rect (at 0.25 0.25 180) (size 0.5 0.5) (layers C1F F.Paste)
      (net 1 GND))
  )
  (module gsg-modules:SKY13322-375LF (layer C1F) (tedit 57F1C8D1)
    (at 83 130.5625)
    (fp_text reference U2 (at 0 0.5) (layer F.SilkS))
    (fp_text value SKY13322 (at 0 -0.5) (layer F.Fab) hide)
    (pad 0 smd rect (at 0 0) (size 0.76 2.4) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -1) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 14 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at -1 -0.5) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 31 /U2V2))
    (pad 3 smd rect (at -1 0) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 194 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -1 0.5) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 30 /U2V1))
    (pad 5 smd rect (at -1 1) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 6 smd rect (at 1 1) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 12 "Net-(C5-Pad1)"))
    (pad 7 smd rect (at 1 0.5) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 28 /U2V3))
    (pad 8 smd rect (at 1 0) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 19 "Net-(C9-Pad2)"))
    (pad 9 smd rect (at 1 -0.5) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 32 /U2V4))
    (pad 10 smd rect (at 1 -1) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 6 "Net-(C2-Pad1)"))
    (pad 0 thru_hole circle (at 0 -0.3) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at 0 -0.9) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at 0 0.3) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at 0 0.9) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module gsg-modules:SKY13322-375LF (layer C1F) (tedit 57F1C8D1)
    (at 157 130.5625 180)
    (fp_text reference U3 (at 0 0.5 180) (layer F.SilkS))
    (fp_text value SKY13322 (at 0 -0.5 180) (layer F.Fab) hide)
    (pad 0 smd rect (at 0 0 180) (size 0.76 2.4) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -1 180) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 8 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at -1 -0.5 180) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 38 /U3V2))
    (pad 3 smd rect (at -1 0 180) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 195 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at -1 0.5 180) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 37 /U3V1))
    (pad 5 smd rect (at -1 1 180) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 18 "Net-(C8-Pad1)"))
    (pad 6 smd rect (at 1 1 180) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 10 "Net-(C4-Pad1)"))
    (pad 7 smd rect (at 1 0.5 180) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 35 /U3V3))
    (pad 8 smd rect (at 1 0 180) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 22 "Net-(C10-Pad1)"))
    (pad 9 smd rect (at 1 -0.5 180) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 39 /U3V4))
    (pad 10 smd rect (at 1 -1 180) (size 0.8 0.25) (layers C1F F.Paste F.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (pad 0 thru_hole circle (at 0 -0.3 180) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at 0 -0.9 180) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at 0 0.3 180) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at 0 0.9 180) (size 0.4572 0.4572) (drill 0.254) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module gsg-modules:TSSOP16 (layer C1F) (tedit 5605DC3A)
    (at 136 134 90)
    (fp_text reference U4 (at 1.3 0 180) (layer F.SilkS))
    (fp_text value PCA9557 (at -0.4 -0.1 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.925 -2.275 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 47 /SCL))
    (pad 2 smd rect (at -2.925 -1.625 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 46 /SDA))
    (pad 3 smd rect (at -2.925 -0.975 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 48 /A0))
    (pad 4 smd rect (at -2.925 -0.325 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 49 /A1))
    (pad 5 smd rect (at -2.925 0.325 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 50 /A2))
    (pad 6 smd rect (at -2.925 0.975 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 53 /!LED_EN))
    (pad 7 smd rect (at -2.925 1.625 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 61 /LED_EN2))
    (pad 8 smd rect (at -2.925 2.275 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.925 2.275 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 60 /U1CTRL))
    (pad 10 smd rect (at 2.925 1.625 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 59 /U3CTRL0))
    (pad 11 smd rect (at 2.925 0.975 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 58 /U3CTRL1))
    (pad 12 smd rect (at 2.925 0.325 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 57 /U2CTRL0))
    (pad 13 smd rect (at 2.925 -0.325 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 56 /U2CTRL1))
    (pad 14 smd rect (at 2.925 -0.975 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 55 /!OE))
    (pad 15 smd rect (at 2.925 -1.625 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 54 /!RESET))
    (pad 16 smd rect (at 2.925 -2.275 90) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
  )
  (module gsg-modules:TSSOP20 (layer C1F) (tedit 57F1CC68)
    (at 145 122 180)
    (fp_text reference U5 (at 1.3 0 270) (layer F.SilkS))
    (fp_text value TC7MBL3245CFT (at -0.4 -0.1 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.925 -2.925 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 196 "Net-(U5-Pad1)"))
    (pad 2 smd rect (at -2.925 -2.275 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 42 /EXT_U2CTRL1))
    (pad 3 smd rect (at -2.925 -1.625 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 44 /EXT_U2CTRL0))
    (pad 4 smd rect (at -2.925 -0.975 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 41 /EXT_U3CTRL1))
    (pad 5 smd rect (at -2.925 -0.325 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 43 /EXT_U3CTRL0))
    (pad 6 smd rect (at -2.925 0.325 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 45 /EXT_U1CTRL))
    (pad 7 smd rect (at -2.925 0.975 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 197 "Net-(U5-Pad7)"))
    (pad 8 smd rect (at -2.925 1.625 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 198 "Net-(U5-Pad8)"))
    (pad 9 smd rect (at -2.925 2.275 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 199 "Net-(U5-Pad9)"))
    (pad 10 smd rect (at -2.925 2.925 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.925 2.925 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 200 "Net-(U5-Pad11)"))
    (pad 12 smd rect (at 2.925 2.275 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 201 "Net-(U5-Pad12)"))
    (pad 13 smd rect (at 2.925 1.625 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 202 "Net-(U5-Pad13)"))
    (pad 14 smd rect (at 2.925 0.975 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 60 /U1CTRL))
    (pad 15 smd rect (at 2.925 0.325 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 59 /U3CTRL0))
    (pad 16 smd rect (at 2.925 -0.325 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 58 /U3CTRL1))
    (pad 17 smd rect (at 2.925 -0.975 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 57 /U2CTRL0))
    (pad 18 smd rect (at 2.925 -1.625 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 56 /U2CTRL1))
    (pad 19 smd rect (at 2.925 -2.275 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 55 /!OE))
    (pad 20 smd rect (at 2.925 -2.925 180) (size 1.05 0.32) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
  )
  (module gsg-modules:SOT363 (layer C1F) (tedit 5099C1B1)
    (at 117.336777 128.975619 90)
    (fp_text reference U6 (at 0 -0.18 90) (layer F.SilkS))
    (fp_text value 74LVC1G58 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 61 /LED_EN2))
    (pad 2 smd rect (at 0 1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.65 1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at 0.65 -1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 51 "Net-(R1-Pad2)"))
    (pad 5 smd rect (at 0 -1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at -0.65 -1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 63 /U1VC2))
  )
  (module gsg-modules:SOT363 (layer C1F) (tedit 5099C1B1)
    (at 117.336777 123.975619 90)
    (fp_text reference U7 (at 0 -0.18 90) (layer F.SilkS))
    (fp_text value 74LVC1G58 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 61 /LED_EN2))
    (pad 2 smd rect (at 0 1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.65 1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at 0.65 -1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 52 "Net-(R2-Pad2)"))
    (pad 5 smd rect (at 0 -1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at -0.65 -1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 62 /U1VC1))
  )
  (module gsg-modules:SOT353-1 (layer C1F) (tedit 57E1C050)
    (at 127.7506 109.5596 90)
    (fp_text reference U8 (at 0 -0.18 90) (layer F.SilkS))
    (fp_text value 74AHC1G08 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 0.95 90) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 56 /U2CTRL1))
    (pad 2 smd rect (at 0 0.95 90) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 57 /U2CTRL0))
    (pad 3 smd rect (at 0.65 0.95 90) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -0.95 90) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 32 /U2V4))
    (pad 5 smd rect (at -0.65 -0.95 90) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
  )
  (module gsg-modules:SOT353-1 (layer C1F) (tedit 57E1C050)
    (at 134.5298 109.4778 270)
    (fp_text reference U9 (at 0 -0.18 270) (layer F.SilkS))
    (fp_text value 74AHC1G08 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 0.95 270) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 58 /U3CTRL1))
    (pad 2 smd rect (at 0 0.95 270) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 59 /U3CTRL0))
    (pad 3 smd rect (at 0.65 0.95 270) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -0.95 270) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 35 /U3V3))
    (pad 5 smd rect (at -0.65 -0.95 270) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
  )
  (module gsg-modules:SOT363 (layer C1F) (tedit 5099C1B1)
    (at 127.95504 113.32464 180)
    (fp_text reference U10 (at 0 -0.18 180) (layer F.SilkS))
    (fp_text value 74LVC1G58 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 57 /U2CTRL0))
    (pad 2 smd rect (at 0 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.65 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 31 /U2V2))
    (pad 5 smd rect (at 0 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at -0.65 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 56 /U2CTRL1))
  )
  (module gsg-modules:SOT363 (layer C1F) (tedit 5099C1B1)
    (at 132.05968 113.3856 180)
    (fp_text reference U11 (at 0 -0.18 180) (layer F.SilkS))
    (fp_text value 74LVC1G58 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 59 /U3CTRL0))
    (pad 2 smd rect (at 0 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.65 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 37 /U3V1))
    (pad 5 smd rect (at 0 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at -0.65 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 58 /U3CTRL1))
  )
  (module gsg-modules:SOT363 (layer C1F) (tedit 5099C1B1)
    (at 127.83312 119.60352 180)
    (fp_text reference U12 (at 0 -0.18 180) (layer F.SilkS))
    (fp_text value 74LVC1G58 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 56 /U2CTRL1))
    (pad 2 smd rect (at 0 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.65 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 30 /U2V1))
    (pad 5 smd rect (at 0 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at -0.65 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 57 /U2CTRL0))
  )
  (module gsg-modules:SOT363 (layer C1F) (tedit 5099C1B1)
    (at 132.0546 119.61876 180)
    (fp_text reference U13 (at 0 -0.18 180) (layer F.SilkS))
    (fp_text value 74LVC1G58 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 58 /U3CTRL1))
    (pad 2 smd rect (at 0 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.65 1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 38 /U3V2))
    (pad 5 smd rect (at 0 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at -0.65 -1 180) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 59 /U3CTRL0))
  )
  (module gsg-modules:SOT353-1 (layer C1F) (tedit 57E1C050)
    (at 128 127 180)
    (fp_text reference U14 (at 0 -0.18 180) (layer F.SilkS))
    (fp_text value 74AHC1G02 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 0.95 180) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 56 /U2CTRL1))
    (pad 2 smd rect (at 0 0.95 180) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 57 /U2CTRL0))
    (pad 3 smd rect (at 0.65 0.95 180) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -0.95 180) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 28 /U2V3))
    (pad 5 smd rect (at -0.65 -0.95 180) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
  )
  (module gsg-modules:SOT353-1 (layer C1F) (tedit 57E1C050)
    (at 132 127 180)
    (fp_text reference U15 (at 0 -0.18 180) (layer F.SilkS))
    (fp_text value 74AHC1G02 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 0.95 180) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 58 /U3CTRL1))
    (pad 2 smd rect (at 0 0.95 180) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 59 /U3CTRL0))
    (pad 3 smd rect (at 0.65 0.95 180) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -0.95 180) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 39 /U3V4))
    (pad 5 smd rect (at -0.65 -0.95 180) (size 0.42 0.6) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
  )
  (module gsg-modules:SOT363 (layer C1F) (tedit 5099C1B1)
    (at 117.336777 133.975619 90)
    (fp_text reference U16 (at 0 -0.18 90) (layer F.SilkS))
    (fp_text value 74LVC1G19 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 60 /U1CTRL))
    (pad 2 smd rect (at 0 1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.65 1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 62 /U1VC1))
    (pad 5 smd rect (at 0 -1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at -0.65 -1 90) (size 0.45 1) (layers C1F F.Paste F.Mask)
      (net 63 /U1VC2))
  )
  (module gsg-modules:HEADER-2x20-REVERSE (layer C1F) (tedit 57F3E589)
    (at 96.322 116.58)
    (tags CONN)
    (fp_text reference J1 (at 0 0) (layer F.SilkS))
    (fp_text value CONN_02X20 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -24.13 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -24.13 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J1-Pad12)"))
    (pad 13 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J1-Pad13)"))
    (pad 14 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(J1-Pad15)"))
    (pad 16 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(J1-Pad16)"))
    (pad 17 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(J1-Pad17)"))
    (pad 18 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(J1-Pad18)"))
    (pad 19 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(J1-Pad19)"))
    (pad 20 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(J1-Pad20)"))
    (pad 21 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(J1-Pad21)"))
    (pad 22 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(J1-Pad22)"))
    (pad 23 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J1-Pad23)"))
    (pad 24 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J1-Pad24)"))
    (pad 25 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J1-Pad25)"))
    (pad 26 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(J1-Pad26)"))
    (pad 27 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(J1-Pad27)"))
    (pad 28 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(J1-Pad28)"))
    (pad 29 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(J1-Pad29)"))
    (pad 30 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(J1-Pad30)"))
    (pad 31 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(J1-Pad31)"))
    (pad 32 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(J1-Pad32)"))
    (pad 33 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(J1-Pad33)"))
    (pad 34 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(J1-Pad34)"))
    (pad 35 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(J1-Pad35)"))
    (pad 36 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(J1-Pad36)"))
    (pad 37 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(J1-Pad37)"))
    (pad 38 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(J1-Pad38)"))
    (pad 39 thru_hole circle (at 24.13 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(J1-Pad39)"))
    (pad 40 thru_hole circle (at 24.13 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(J1-Pad40)"))
  )
  (module gsg-modules:HEADER-2x20-REVERSE (layer C1F) (tedit 57F3E589)
    (at 96.322 162.3)
    (tags CONN)
    (fp_text reference J2 (at 0 0) (layer F.SilkS))
    (fp_text value CONN_02X20 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -24.13 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -24.13 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at -21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /EXT_U1CTRL))
    (pad 7 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /EXT_U3CTRL0))
    (pad 8 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /EXT_U3CTRL1))
    (pad 9 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /EXT_U2CTRL0))
    (pad 10 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /EXT_U2CTRL1))
    (pad 11 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(J2-Pad11)"))
    (pad 12 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(J2-Pad12)"))
    (pad 13 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(J2-Pad13)"))
    (pad 14 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(J2-Pad14)"))
    (pad 15 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(J2-Pad15)"))
    (pad 16 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(J2-Pad16)"))
    (pad 17 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(J2-Pad17)"))
    (pad 18 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(J2-Pad18)"))
    (pad 19 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(J2-Pad19)"))
    (pad 20 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(J2-Pad20)"))
    (pad 21 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(J2-Pad21)"))
    (pad 22 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(J2-Pad22)"))
    (pad 23 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(J2-Pad23)"))
    (pad 24 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(J2-Pad24)"))
    (pad 25 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(J2-Pad25)"))
    (pad 26 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(J2-Pad26)"))
    (pad 27 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(J2-Pad27)"))
    (pad 28 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(J2-Pad28)"))
    (pad 29 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(J2-Pad29)"))
    (pad 30 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(J2-Pad30)"))
    (pad 31 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(J2-Pad31)"))
    (pad 32 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 127 "Net-(J2-Pad32)"))
    (pad 33 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 128 "Net-(J2-Pad33)"))
    (pad 34 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 129 "Net-(J2-Pad34)"))
    (pad 35 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 130 "Net-(J2-Pad35)"))
    (pad 36 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 131 "Net-(J2-Pad36)"))
    (pad 37 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(J2-Pad37)"))
    (pad 38 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 133 "Net-(J2-Pad38)"))
    (pad 39 thru_hole circle (at 24.13 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /SDA))
    (pad 40 thru_hole circle (at 24.13 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /SCL))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 595A86A8)
    (at 85.344 132.588 270)
    (fp_text reference C13 (at 0 0 270) (layer F.SilkS))
    (fp_text value 33pF (at 0 0.0508 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 28 /U2V3))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 80.1116 131.7244 270)
    (fp_text reference C14 (at 0 0.0508 270) (layer F.SilkS))
    (fp_text value 33pF (at 0 0.0508 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 30 /U2V1))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 80.0862 129.4638 270)
    (fp_text reference C15 (at 0 0.0508 270) (layer F.SilkS))
    (fp_text value 33pF (at 0 0.0508 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 31 /U2V2))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 85.598 128.9558 180)
    (fp_text reference C16 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value 33pF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 32 /U2V4))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 116.4082 167.7416 270)
    (fp_text reference C17 (at 0 0.0508 270) (layer F.SilkS))
    (fp_text value 33pF (at 0 0.0508 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 63 /U1VC2))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 123.5964 167.6908 270)
    (fp_text reference C18 (at 0 0.0508 270) (layer F.SilkS))
    (fp_text value 33pF (at 0 0.0508 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 62 /U1VC1))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 154.13736 129.3114 90)
    (fp_text reference C19 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value 33pF (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 35 /U3V3))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 159.6136 129.4638 90)
    (fp_text reference C20 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value 33pF (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 37 /U3V1))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 159.6136 131.7244 90)
    (fp_text reference C21 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value 33pF (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 38 /U3V2))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 154.1526 131.79552 90)
    (fp_text reference C22 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value 33pF (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 39 /U3V4))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 113.87328 129.32664 90)
    (fp_text reference C23 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 124.41174 110.74146 90)
    (fp_text reference C24 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 127.3556 116.8527)
    (fp_text reference C25 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 127.29972 123.18492)
    (fp_text reference C26 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 128.1684 130.302)
    (fp_text reference C27 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 113.9571 123.72594 270)
    (fp_text reference C28 (at 0 0.0508 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 137.8077 108.28782 270)
    (fp_text reference C29 (at 0 0.0508 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0 270) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 131.76504 117.30228)
    (fp_text reference C30 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 132.52704 123.14428 180)
    (fp_text reference C31 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 132.02412 129.98196)
    (fp_text reference C32 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 113.67262 134.69112 90)
    (fp_text reference C33 (at 0 0.0508 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0 90) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 132.03936 131.38912)
    (fp_text reference C34 (at 0 0.0508) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (module gsg-modules:0402 (layer C1F) (tedit 4FB6CFE4)
    (at 141.53388 126.49962 180)
    (fp_text reference C35 (at 0 0.0508 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0.0508 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.5334 0 180) (size 0.508 0.5588) (layers C1F F.Paste F.Mask)
      (net 1 GND))
  )
  (gr_text P1 (at 158.3 154.8) (layer F.SilkS))
  (gr_text A2 (at 155.3 158.7) (layer F.SilkS))
  (gr_text A1 (at 152.7 158.7) (layer F.SilkS))
  (gr_text A0 (at 150.2 158.7) (layer F.SilkS))
  (gr_text PB4 (at 173 113.725) (layer F.SilkS))
  (gr_text PB3 (at 173 126.1) (layer F.SilkS))
  (gr_text PB2 (at 167.5 138.475) (layer F.SilkS))
  (gr_text PB1 (at 167.5 150.85) (layer F.SilkS))
  (gr_text PB0 (at 173 163.25) (layer F.SilkS))
  (gr_text PA4 (at 67 113.75) (layer F.SilkS))
  (gr_text PA3 (at 67 126.125) (layer F.SilkS))
  (gr_text PA2 (at 67 138.5) (layer F.SilkS))
  (gr_text PA1 (at 67 150.875) (layer F.SilkS))
  (gr_text PA0 (at 67 163.25) (layer F.SilkS))
  (gr_text J2 (at 96.25 167) (layer F.SilkS))
  (gr_text J1 (at 96.25 120.25) (layer F.SilkS))
  (gr_line (start 60 104) (end 60 105) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60 105) (end 61.02 108.75) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 61.02 108.75) (end 61.02 115.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 61.02 115.25) (end 60.75 116.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60.75 116.25) (end 60.75 120.125) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60.75 120.125) (end 61.02 121.125) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 61.02 121.125) (end 61.02 127.625) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 61.02 127.625) (end 60.75 128.625) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60.75 128.625) (end 60.75 132.5) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60.75 132.5) (end 61.02 133.5) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 61.02 133.5) (end 61.02 140) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 61.02 140) (end 60.75 141) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60.75 141) (end 60.75 144.875) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60.75 144.875) (end 61.02 145.875) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 61.02 145.875) (end 61.02 152.375) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 61.02 152.375) (end 60.75 153.375) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60.75 153.375) (end 60.75 157.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60.75 157.25) (end 61.02 158.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 61.02 158.25) (end 61.02 164.75) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 61.02 164.75) (end 60 168.5) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 60 168.5) (end 60 171) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 180 104) (end 180 105) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 180 105) (end 178.98 108.75) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.98 108.75) (end 178.98 115.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.98 115.25) (end 179.25 116.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 179.25 116.25) (end 179.25 120.125) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 179.25 120.125) (end 178.98 121.125) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.98 121.125) (end 178.98 127.625) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.98 127.625) (end 179.25 128.625) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 179.25 128.625) (end 179.25 132.5) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 179.25 132.5) (end 178.98 133.5) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.98 133.5) (end 178.98 140) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.98 140) (end 179.25 141) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 179.25 141) (end 179.25 144.875) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 179.25 144.875) (end 178.98 145.875) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.98 145.875) (end 178.98 152.375) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.98 152.375) (end 179.25 153.375) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 179.25 153.375) (end 179.25 157.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 179.25 157.25) (end 178.98 158.25) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.98 158.25) (end 178.98 164.75) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.98 164.75) (end 180 168.5) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 180 168.5) (end 180 171) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_text "Install GreatFET One on opposite side." (at 96.28 142.89) (layer B.SilkS))
  (gr_text "Optional: Install GreatFET One upside-down instead of connecting to HackRF." (at 96.25 158.5) (layer F.SilkS))
  (gr_text 4 (at 167.7 101.3) (layer C4B))
  (gr_text 3 (at 166.8 101.3) (layer C3))
  (gr_text 2 (at 165.8 101.3) (layer C2))
  (gr_text 1 (at 164.9 101.3) (layer C1F))
  (gr_text "4 October 2016" (at 113.58 111.17) (layer F.SilkS))
  (gr_text P9 (at 98.1 125.47) (layer F.SilkS))
  (gr_text "Opera Cake" (at 89.2 107.6) (layer F.SilkS))
  (gr_line (start 176 100) (end 64 100) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 64 175) (end 176 175) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 176 171) (end 180 171) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 176 104) (end 176 100) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 64 171) (end 64 175) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 64 104) (end 60 104) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_text P20 (at 167.8 143.25 90) (layer F.SilkS))
  (gr_text P22 (at 152.7608 168.7516) (layer F.SilkS))
  (gr_text P28 (at 119.5 143.25 90) (layer F.SilkS))
  (gr_text http://greatscottgadgets.com/hackrf/ (at 152.8878 171.2154) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer C2) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60 100) (xy 60 175) (xy 180 175) (xy 180 100) (xy 168.5 100)
        (xy 168.5 102.5) (xy 164.1 102.5) (xy 164.1 100)
      )
    )
  )
  (zone (net 2) (net_name VCC) (layer C3) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122 175) (xy 180 175) (xy 180 100) (xy 168.5 100) (xy 168.5 102.5)
        (xy 164.1 102.5) (xy 164.1 100) (xy 60 100) (xy 60 146) (xy 60 175)
      )
    )
  )
)
