(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 80)
    (no_connects 0)
    (area 59.789287 67.15 206.275715 139.225001)
    (thickness 1.6002)
    (drawings 24)
    (tracks 602)
    (zones 0)
    (modules 36)
    (nets 22)
  )
  (page A)
  (title_block
    (title "Interactive Rainbow")
    (date 2017-03-29)
    (rev 1.0.1)
    (company "Sembazuru Circuits (for Barrel of Makers)")
    (comment 1 "1.0.0 Initial layout.")
    (comment 2 "1.0.1 Correct pinout for U1 (7555 timer). Add KiCad logo. Isolate unused gate input for future modification.")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 0.889)
    (user_trace_width 1.016)
    (trace_clearance 0.254)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 76.2 127)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.076200)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 /~IR_Osc+)
  (net 5 /~IR_Osc-)
  (net 6 /~SS+)
  (net 7 /~SS-)
  (net 8 /MISO+)
  (net 9 /MOSI+)
  (net 10 /MOSI-)
  (net 11 /MISO-)
  (net 12 /SCK+)
  (net 13 /SCK-)
  (net 14 /IR_Osc)
  (net 15 /~IR_Osc)
  (net 16 "Net-(R1-Pad2)")
  (net 17 /IR_Enable)
  (net 18 /~SS)
  (net 19 /MOSI)
  (net 20 /MISO)
  (net 21 /SCK)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /IR_Enable)
    (add_net /IR_Osc)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net /~IR_Osc)
    (add_net /~SS)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (net_class 3A_Power ""
    (clearance 0.1524)
    (trace_width 0.889)
    (via_dia 0.889)
    (via_drill 0.4572)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class 5A_Power ""
    (clearance 0.1524)
    (trace_width 1.778)
    (via_dia 1.778)
    (via_drill 0.889)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net GND)
  )
  (net_class Differential ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.7874)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /MISO+)
    (add_net /MISO-)
    (add_net /MOSI+)
    (add_net /MOSI-)
    (add_net /SCK+)
    (add_net /SCK-)
    (add_net /~IR_Osc+)
    (add_net /~IR_Osc-)
    (add_net /~SS+)
    (add_net /~SS-)
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P placed (layer F.Cu) (tedit 58157E65)
    (at 186.70539 93.98527 180)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C1 (at 0.01539 2.54527 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 3.82539 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P placed (layer F.Cu) (tedit 58157E65)
    (at 185.43539 107.95527 180)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C2 (at 5.09539 0.64027 180) (layer F.SilkS))
    (fp_text value 0.001µF (at 1.27 -1.26473 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPPRD254W50D500H850 placed (layer F.Cu) (tedit 58157DD8)
    (at 104.15539 116.21027)
    (descr "Capacitor, Polarized, Radial (Dipped, Round); 2.54 mm C X 5.00 mm Dia X 8.50 mm H body")
    (fp_text reference C3 (at -1.28539 -3.18027) (layer F.SilkS))
    (fp_text value 10µF (at 2.52461 -3.18027) (layer F.Fab))
    (fp_text user + (at -1.778 -1.016) (layer F.SilkS))
    (fp_text user + (at -1.778 -1.016) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.05 0 0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P placed (layer F.Cu) (tedit 58157E65)
    (at 104.15539 120.02027)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C4 (at -0.65039 2.53473) (layer F.SilkS))
    (fp_text value 0.1µF (at 3.15961 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P placed (layer F.Cu) (tedit 58157E65)
    (at 153.68539 121.29027 90)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C5 (at -2.53473 -0.01539 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 5.08527 -0.01539 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPPRD254W50D500H850 placed (layer F.Cu) (tedit 58157DD8)
    (at 157.49539 121.29027 90)
    (descr "Capacitor, Polarized, Radial (Dipped, Round); 2.54 mm C X 5.00 mm Dia X 8.50 mm H body")
    (fp_text reference C6 (at -2.53473 1.25461 180) (layer F.SilkS))
    (fp_text value 10µF (at 4.45027 0.61961 180) (layer F.Fab))
    (fp_text user + (at -1.778 -1.016 90) (layer F.SilkS))
    (fp_text user + (at -1.778 -1.016 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.05 0 0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P placed (layer F.Cu) (tedit 58157E65)
    (at 140.98539 93.98527 270)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C7 (at -2.54527 0.01539 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 5.07473 0.01539 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPPRD254W50D500H850 placed (layer F.Cu) (tedit 58157DD8)
    (at 137.17539 93.98527 270)
    (descr "Capacitor, Polarized, Radial (Dipped, Round); 2.54 mm C X 5.00 mm Dia X 8.50 mm H body")
    (fp_text reference C8 (at -2.54527 0.65039 360) (layer F.SilkS))
    (fp_text value 10µF (at 4.43973 0.65039 360) (layer F.Fab))
    (fp_text user + (at -1.778 -1.016 270) (layer F.SilkS))
    (fp_text user + (at -1.778 -1.016 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.05 0 0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P placed (layer F.Cu) (tedit 58157E65)
    (at 163.84539 99.06527)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C9 (at -0.01539 -2.54) (layer F.SilkS))
    (fp_text value 0.1µF (at 6.33461 -0.00527) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P placed (layer F.Cu) (tedit 58157E65)
    (at 106.69539 83.82527 270)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C10 (at -2.16427 -0.49261 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.27 -2.52461 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P placed (layer F.Cu) (tedit 58157E65)
    (at 106.69539 96.52527 270)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C11 (at -2.16427 -0.49261 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 1.26473 -2.52461 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-connectors:KYCON_KLDVHCX-0202-x_CirHole placed (layer F.Cu) (tedit 587EDFE8)
    (at 94.17539 120.02027 180)
    (descr "DC Power Jack Kycon# KLDVHCX-0202-x")
    (tags "PWR DC")
    (fp_text reference J1 (at -1.905 -5.715 180) (layer F.SilkS))
    (fp_text value KLDVHCX-0202-A (at 0 -8.24973 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -4.9 0 270) (size 4.5 4.5) (drill 3.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at -1.4 5.6 180) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 1.4 2.8 180) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ipc-7251TH-connectors.3dshapes/KYCON_KLDVHCX-0202-x.wrl
      (at (xyz 0 -0.255906 0.562992))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-connectors:KYCON_KLDVHCX-0202-x_CirHole placed (layer F.Cu) (tedit 587EDFE8)
    (at 143.70539 120.02027 180)
    (descr "DC Power Jack Kycon# KLDVHCX-0202-x")
    (tags "PWR DC")
    (fp_text reference J2 (at -1.905 -5.715 180) (layer F.SilkS))
    (fp_text value KLDVHCX-0202-A (at 0 -8.24973 360) (layer F.Fab))
    (pad 1 thru_hole rect (at -4.9 0 270) (size 4.5 4.5) (drill 3.5) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at -1.4 5.6 180) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 1.4 2.8 180) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ipc-7251TH-connectors.3dshapes/KYCON_KLDVHCX-0202-x.wrl
      (at (xyz 0 -0.255906 0.562992))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 placed (layer F.Cu) (tedit 581580AA)
    (at 156.22539 90.17527 270)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J3 (at -4.45027 -2.52461 360) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.43973 -4.42961 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /~IR_Osc+))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /~IR_Osc-))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 270) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 270) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 placed (layer F.Cu) (tedit 581580AA)
    (at 88.91539 90.17527 270)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J4 (at -4.45027 -2.52461 360) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 3.80473 13.98539 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 /~SS+))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /~SS-))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 /MISO+))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 /MOSI+))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 /MOSI-))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 /MISO-))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 /SCK+))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 /SCK-))
    (pad "" np_thru_hole circle (at 10.165 6.35 270) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 270) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.183071 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module ipc-7251TH-standard:TO92184P520H734-3 placed (layer F.Cu) (tedit 58157AC6)
    (at 175.74364 106.11543 270)
    (descr "TO-92, 1.8415 mm pitch; 3 pin, 5.207 mm W X 7.341 mm H body")
    (tags "TO92 TO-92")
    (fp_text reference Q1 (at -1.97543 0.48364 360) (layer F.SilkS))
    (fp_text value VN3205 (at 1.83457 2.00764 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -0.00166 -0.0015 270) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 1.83984 -2.07175 270) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 14 /IR_Osc))
    (pad 3 thru_hole circle (at 3.68134 -0.0015 270) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 15 /~IR_Osc))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Wide.wrl
      (at (xyz 0.072435 -0.000315 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 -90))
    )
  )
  (module ipc-7251TH-standard:RESAD1016W56L681D259 placed (layer F.Cu) (tedit 5815799F)
    (at 189.24539 104.14527 270)
    (descr "Resistor, Axial; 400 mil C X 22 mil W 268 mil L X 102 mil Dia body - Standard 1/4W Resistor")
    (tags "RES 0.25 1/4")
    (fp_text reference R1 (at -0.00527 -2.14361 360) (layer F.SilkS))
    (fp_text value 15kΩ (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.53 1.53) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.53 1.53) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 "Net-(R1-Pad2)"))
    (model unused_3d.3dshapes/discret.resistors.horizontal.r_h_15K.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESAD1016W56L681D259 placed (layer F.Cu) (tedit 5815799F)
    (at 166.38539 113.03527)
    (descr "Resistor, Axial; 400 mil C X 22 mil W 268 mil L X 102 mil Dia body - Standard 1/4W Resistor")
    (tags "RES 0.25 1/4")
    (fp_text reference R3 (at -0.01539 1.89973) (layer F.SilkS))
    (fp_text value 15kΩ (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.53 1.53) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.53 1.53) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 /~IR_Osc))
    (model unused_3d.3dshapes/discret.resistors.horizontal.r_h_15K.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 placed (layer F.Cu) (tedit 588192A7)
    (at 104.15539 106.68527 180)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R4 (at -2.52461 0 180) (layer F.SilkS))
    (fp_text value 100Ω (at 1.27 -1.89973 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 8 /MISO+))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 11 /MISO-))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100r.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L1003H508Q8 placed (layer F.Cu) (tedit 587D45C5)
    (at 179.08539 96.52 270)
    (descr "DIPS, 300 mil lead span, 100 mil pitch; 8 pin, 395 mil L X 400 mil W X 200 mil H body")
    (fp_text reference U1 (at 0 2.55539 360) (layer F.SilkS))
    (fp_text value ICM7555 (at 3.81 -3.81 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 14 /IR_Osc))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 17 /IR_Enable))
    (pad 5 thru_hole circle (at 7.62 -7.62 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 5.08 -7.62 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 7 thru_hole circle (at 2.54 -7.62 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 0 -7.62 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model dil/sockets/dil_socket_8.wrl
      (at (xyz 0.15 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module arduino_shields:ARDUINO_Pro-MiniU placed (layer F.Cu) (tedit 0)
    (at 121.93539 109.22527 180)
    (fp_text reference U2 (at -10.77961 -12.69473 360) (layer F.SilkS))
    (fp_text value "ARDUINO_Pro-Mini 5v" (at 0.01539 17.78527 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 -12.7) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -7.62 -10.16) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -7.62 -7.62) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -7.62 -5.08) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at -7.62 -2.54) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -7.62 0) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at -7.62 2.54) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -7.62 5.08) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at -7.62 7.62) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -7.62 10.16) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at -7.62 12.7) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -7.62 15.24) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask)
      (net 17 /IR_Enable))
    (pad 13 thru_hole oval (at 7.62 15.24 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask)
      (net 18 /~SS))
    (pad 14 thru_hole oval (at 7.62 12.7 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask)
      (net 19 /MOSI))
    (pad 15 thru_hole oval (at 7.62 10.16 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask)
      (net 20 /MISO))
    (pad 16 thru_hole oval (at 7.62 7.62 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask)
      (net 21 /SCK))
    (pad 17 thru_hole oval (at 7.62 5.08 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 7.62 2.54 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 7.62 0 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 7.62 -2.54 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 7.62 -5.08 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 22 thru_hole oval (at 7.62 -7.62 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 7.62 -10.16 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 24 thru_hole oval (at 7.62 -12.7 180) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad A4 thru_hole oval (at 4.699 -1.397) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad A5 thru_hole oval (at 4.699 -3.937) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad A6 thru_hole oval (at 4.699 9.0678) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (pad A7 thru_hole oval (at 4.699 6.5278) (size 2.12 1.7) (drill 1.05 (offset 0.21 0)) (layers *.Cu *.Mask))
    (model arduino/Arduino-Pro-Mini.wrl
      (at (xyz -0.35 -0.65 0.135))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 0.6 0.17))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0.3 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz -0.3 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L1003H508Q8 placed (layer F.Cu) (tedit 587D45C5)
    (at 163.84539 101.60527 270)
    (descr "DIPS, 300 mil lead span, 100 mil pitch; 8 pin, 395 mil L X 400 mil W X 200 mil H body")
    (fp_text reference U3 (at -0.00527 2.55539 360) (layer F.SilkS))
    (fp_text value uA9638C (at 3.81 -3.81 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 15 /~IR_Osc))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 7.62 -7.62 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 5.08 -7.62 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 2.54 -7.62 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 5 /~IR_Osc-))
    (pad 8 thru_hole circle (at 0 -7.62 270) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 4 /~IR_Osc+))
    (model dil/sockets/dil_socket_8.wrl
      (at (xyz 0.15 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L1003H508Q8 placed (layer F.Cu) (tedit 587D45C5)
    (at 104.15539 83.82527 180)
    (descr "DIPS, 300 mil lead span, 100 mil pitch; 8 pin, 395 mil L X 400 mil W X 200 mil H body")
    (fp_text reference U4 (at 0.52339 2.16427 180) (layer F.SilkS))
    (fp_text value uA9638C (at 3.81 -3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 18 /~SS))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 21 /SCK))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 7.62 -7.62 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 13 /SCK-))
    (pad 6 thru_hole circle (at 5.08 -7.62 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 12 /SCK+))
    (pad 7 thru_hole circle (at 2.54 -7.62 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 7 /~SS-))
    (pad 8 thru_hole circle (at 0 -7.62 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 6 /~SS+))
    (model dil/sockets/dil_socket_8.wrl
      (at (xyz 0.15 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L1003H508Q8 placed (layer F.Cu) (tedit 587D45C5)
    (at 104.15539 96.52527 180)
    (descr "DIPS, 300 mil lead span, 100 mil pitch; 8 pin, 395 mil L X 400 mil W X 200 mil H body")
    (fp_text reference U5 (at 0.52339 2.16427 180) (layer F.SilkS))
    (fp_text value DS8921 (at 3.81 -3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 20 /MISO))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 19 /MOSI))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 7.62 -7.62 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 10 /MOSI-))
    (pad 6 thru_hole circle (at 5.08 -7.62 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 9 /MOSI+))
    (pad 7 thru_hole circle (at 2.54 -7.62 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 11 /MISO-))
    (pad 8 thru_hole circle (at 0 -7.62 180) (size 1.05664 1.05664) (drill 0.65024) (layers *.Cu *.Mask)
      (net 8 /MISO+))
    (model dil/sockets/dil_socket_8.wrl
      (at (xyz 0.15 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS762W45P254L1016H508Q8 placed (layer F.Cu) (tedit 587D1F93)
    (at 179.07 96.52527 270)
    (descr "DIP for Socket, 300 mil lead span, 100 mil pitch; 8 pin, 400 mil L X 255.9 mil W X 200 mil H body")
    (fp_text reference XU1 (at 0.62973 -2.54 360) (layer F.SilkS))
    (fp_text value IC_Socket08 (at 6.34473 -3.81 360) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-8__300.wrl
      (at (xyz 0.15 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS762W45P254L1016H508Q8 placed (layer F.Cu) (tedit 587D1F93)
    (at 163.83 101.6 270)
    (descr "DIP for Socket, 300 mil lead span, 100 mil pitch; 8 pin, 400 mil L X 255.9 mil W X 200 mil H body")
    (fp_text reference XU3 (at 0.635 -2.54 360) (layer F.SilkS))
    (fp_text value IC_Socket08 (at 6.35 -3.81 360) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-8__300.wrl
      (at (xyz 0.15 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS762W45P254L1016H508Q8 placed (layer F.Cu) (tedit 587D1F93)
    (at 104.15539 83.82527 180)
    (descr "DIP for Socket, 300 mil lead span, 100 mil pitch; 8 pin, 400 mil L X 255.9 mil W X 200 mil H body")
    (fp_text reference XU4 (at 1.28539 -1.89973 180) (layer F.SilkS))
    (fp_text value IC_Socket08 (at 3.82539 -5.70973 180) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-8__300.wrl
      (at (xyz 0.15 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS762W45P254L1016H508Q8 placed (layer F.Cu) (tedit 587D1F93)
    (at 104.15539 96.52527 180)
    (descr "DIP for Socket, 300 mil lead span, 100 mil pitch; 8 pin, 400 mil L X 255.9 mil W X 200 mil H body")
    (fp_text reference XU5 (at 1.28539 -1.89973 180) (layer F.SilkS))
    (fp_text value IC_Socket08 (at 3.82539 -5.70973 180) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-8__300.wrl
      (at (xyz 0.15 0.15 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-non-standard:TRIM_Bourns3296WA (layer F.Cu) (tedit 5892AC34)
    (at 182.89539 113.03527 180)
    (tags TRIM_Bourns3296W)
    (fp_text reference R2 (at -3.15961 -3.16973 180) (layer F.SilkS))
    (fp_text value 5kΩ (at 1.28539 -3.16973 180) (layer F.Fab))
    (fp_text user "CW -->" (at 0.1905 1.7145 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 1.46 1.46) (drill 0.76) (layers *.Cu *.Mask)
      (net 16 "Net-(R1-Pad2)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.46 1.46) (drill 0.76) (layers *.Cu *.Mask)
      (net 14 /IR_Osc))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.46 1.46) (drill 0.76) (layers *.Cu *.Mask)
      (net 14 /IR_Osc))
    (model discret/potentiometer/Bourns_3296W_Inline_ScrewUp.wrl
      (at (xyz -0.1 0 0))
      (scale (xyz -1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module logos:OSHW_03mm_copper_noMask (layer B.Cu) (tedit 0)
    (at 121.92 83.185 180)
    (fp_text reference G*** (at 0 -1.77038 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 1.77038 180) (layer B.SilkS) hide)
  )
  (module logos:crane_0.40in_silkscreen (layer B.Cu) (tedit 0)
    (at 131.445 80.645 180)
    (fp_text reference G*** (at 0 -3.64236 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 3.64236 180) (layer B.SilkS) hide)
  )
  (module Symbols:Symbol_KiCAD-Logo_CopperAndSilkScreenTop (layer B.Cu) (tedit 58DB3416)
    (at 121.92 90.17 180)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference REF** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "KiCAD Logo" (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module ipc-7251TH-standard:MTGP794H326V8P (layer F.Cu) (tedit 549A50E1)
    (at 81.28 121.92 180)
    (descr "Mounting Hole, Plated, #4 Free Fit")
    (tags MTGP#4Free)
    (fp_text reference MH1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value "#4 PTH" (at 0 0 180) (layer F.SilkS) hide)
    (pad 0 thru_hole rect (at 0 0 180) (size 7.94 7.94) (drill 3.26) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at 0 3.556 180) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at 3.556 3.556 180) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at 3.556 0 180) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at 3.556 -3.556 180) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at 0 -3.556 180) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at -3.556 -3.556 180) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at -3.556 0 180) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at -3.556 3.556 180) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module ipc-7251TH-standard:MTGNP794H326Z794P (layer F.Cu) (tedit 549A53B9)
    (at 187.96 121.92 180)
    (descr "Mounting Hole, Not Plated, #4 Free Fit")
    (tags MTGNP#4Free)
    (fp_text reference MH2 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value "#4 NPTH" (at 0 0 180) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 3.26 3.26) (drill 3.26) (layers *.Cu *.Mask)
      (clearance 2.34))
  )
  (module ipc-7251TH-standard:MTGNP794H326Z794P (layer F.Cu) (tedit 549A53B9)
    (at 187.96 81.28 180)
    (descr "Mounting Hole, Not Plated, #4 Free Fit")
    (tags MTGNP#4Free)
    (fp_text reference MH3 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value "#4 NPTH" (at 0 0 180) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 3.26 3.26) (drill 3.26) (layers *.Cu *.Mask)
      (clearance 2.34))
  )
  (module ipc-7251TH-standard:MTGNP794H326Z794P (layer F.Cu) (tedit 549A53B9)
    (at 81.28 81.28 180)
    (descr "Mounting Hole, Not Plated, #4 Free Fit")
    (tags MTGNP#4Free)
    (fp_text reference MH4 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value "#4 NPTH" (at 0 0 180) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0 180) (size 3.26 3.26) (drill 3.26) (layers *.Cu *.Mask)
      (clearance 2.34))
  )
  (gr_text "Adjust R2 for 38kHz @ R3-2\n(R2-1 to R2-2 about 3.797kΩ)" (at 174.625 118.11) (layer F.SilkS))
  (dimension 45.72 (width 0.3) (layer Dwgs.User)
    (gr_text "1.8000 in" (at 65.325 104.14 90) (layer Dwgs.User))
    (feature1 (pts (xy 75.565 81.28) (xy 63.975 81.28)))
    (feature2 (pts (xy 75.565 127) (xy 63.975 127)))
    (crossbar (pts (xy 66.675 127) (xy 66.675 81.28)))
    (arrow1a (pts (xy 66.675 81.28) (xy 67.261421 82.406504)))
    (arrow1b (pts (xy 66.675 81.28) (xy 66.088579 82.406504)))
    (arrow2a (pts (xy 66.675 127) (xy 67.261421 125.873496)))
    (arrow2b (pts (xy 66.675 127) (xy 66.088579 125.873496)))
  )
  (dimension 5.08 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 71.04 78.74 90) (layer Dwgs.User))
    (feature1 (pts (xy 75.565 76.2) (xy 69.69 76.2)))
    (feature2 (pts (xy 75.565 81.28) (xy 69.69 81.28)))
    (crossbar (pts (xy 72.39 81.28) (xy 72.39 76.2)))
    (arrow1a (pts (xy 72.39 76.2) (xy 72.976421 77.326504)))
    (arrow1b (pts (xy 72.39 76.2) (xy 71.803579 77.326504)))
    (arrow2a (pts (xy 72.39 81.28) (xy 72.976421 80.153496)))
    (arrow2b (pts (xy 72.39 81.28) (xy 71.803579 80.153496)))
  )
  (dimension 40.64 (width 0.3) (layer Dwgs.User)
    (gr_text "1.6000 in" (at 71.04 101.6 90) (layer Dwgs.User))
    (feature1 (pts (xy 75.565 81.28) (xy 69.69 81.28)))
    (feature2 (pts (xy 75.565 121.92) (xy 69.69 121.92)))
    (crossbar (pts (xy 72.39 121.92) (xy 72.39 81.28)))
    (arrow1a (pts (xy 72.39 81.28) (xy 72.976421 82.406504)))
    (arrow1b (pts (xy 72.39 81.28) (xy 71.803579 82.406504)))
    (arrow2a (pts (xy 72.39 121.92) (xy 72.976421 120.793496)))
    (arrow2b (pts (xy 72.39 121.92) (xy 71.803579 120.793496)))
  )
  (dimension 5.08 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 190.5 132.16) (layer Dwgs.User))
    (feature1 (pts (xy 193.04 127.635) (xy 193.04 133.51)))
    (feature2 (pts (xy 187.96 127.635) (xy 187.96 133.51)))
    (crossbar (pts (xy 187.96 130.81) (xy 193.04 130.81)))
    (arrow1a (pts (xy 193.04 130.81) (xy 191.913496 131.396421)))
    (arrow1b (pts (xy 193.04 130.81) (xy 191.913496 130.223579)))
    (arrow2a (pts (xy 187.96 130.81) (xy 189.086504 131.396421)))
    (arrow2b (pts (xy 187.96 130.81) (xy 189.086504 130.223579)))
  )
  (dimension 5.08 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 71.04 124.46 90) (layer Dwgs.User))
    (feature1 (pts (xy 75.565 121.92) (xy 69.69 121.92)))
    (feature2 (pts (xy 75.565 127) (xy 69.69 127)))
    (crossbar (pts (xy 72.39 127) (xy 72.39 121.92)))
    (arrow1a (pts (xy 72.39 121.92) (xy 72.976421 123.046504)))
    (arrow1b (pts (xy 72.39 121.92) (xy 71.803579 123.046504)))
    (arrow2a (pts (xy 72.39 127) (xy 72.976421 125.873496)))
    (arrow2b (pts (xy 72.39 127) (xy 71.803579 125.873496)))
  )
  (dimension 111.76 (width 0.3) (layer Dwgs.User)
    (gr_text "4.4000 in" (at 132.08 137.875) (layer Dwgs.User))
    (feature1 (pts (xy 187.96 127.635) (xy 187.96 139.225)))
    (feature2 (pts (xy 76.2 127.635) (xy 76.2 139.225)))
    (crossbar (pts (xy 76.2 136.525) (xy 187.96 136.525)))
    (arrow1a (pts (xy 187.96 136.525) (xy 186.833496 137.111421)))
    (arrow1b (pts (xy 187.96 136.525) (xy 186.833496 135.938579)))
    (arrow2a (pts (xy 76.2 136.525) (xy 77.326504 137.111421)))
    (arrow2b (pts (xy 76.2 136.525) (xy 77.326504 135.938579)))
  )
  (dimension 106.68 (width 0.3) (layer Dwgs.User)
    (gr_text "4.2000 in" (at 134.62 132.159999) (layer Dwgs.User))
    (feature1 (pts (xy 187.96 127.635) (xy 187.96 133.509999)))
    (feature2 (pts (xy 81.28 127.635) (xy 81.28 133.509999)))
    (crossbar (pts (xy 81.28 130.809999) (xy 187.96 130.809999)))
    (arrow1a (pts (xy 187.96 130.809999) (xy 186.833496 131.39642)))
    (arrow1b (pts (xy 187.96 130.809999) (xy 186.833496 130.223578)))
    (arrow2a (pts (xy 81.28 130.809999) (xy 82.406504 131.39642)))
    (arrow2b (pts (xy 81.28 130.809999) (xy 82.406504 130.223578)))
  )
  (dimension 5.08 (width 0.3) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 78.74 132.16) (layer Dwgs.User))
    (feature1 (pts (xy 81.28 127.635) (xy 81.28 133.51)))
    (feature2 (pts (xy 76.2 127.635) (xy 76.2 133.51)))
    (crossbar (pts (xy 76.2 130.81) (xy 81.28 130.81)))
    (arrow1a (pts (xy 81.28 130.81) (xy 80.153496 131.396421)))
    (arrow1b (pts (xy 81.28 130.81) (xy 80.153496 130.223579)))
    (arrow2a (pts (xy 76.2 130.81) (xy 77.326504 131.396421)))
    (arrow2b (pts (xy 76.2 130.81) (xy 77.326504 130.223579)))
  )
  (dimension 50.8 (width 0.3) (layer Dwgs.User)
    (gr_text "2.0000 in" (at 200.74 101.6 90) (layer Dwgs.User))
    (feature1 (pts (xy 193.675 76.2) (xy 202.09 76.2)))
    (feature2 (pts (xy 193.675 127) (xy 202.09 127)))
    (crossbar (pts (xy 199.39 127) (xy 199.39 76.2)))
    (arrow1a (pts (xy 199.39 76.2) (xy 199.976421 77.326504)))
    (arrow1b (pts (xy 199.39 76.2) (xy 198.803579 77.326504)))
    (arrow2a (pts (xy 199.39 127) (xy 199.976421 125.873496)))
    (arrow2b (pts (xy 199.39 127) (xy 198.803579 125.873496)))
  )
  (dimension 116.84 (width 0.3) (layer Dwgs.User)
    (gr_text "4.6000 in" (at 134.62 68.5) (layer Dwgs.User))
    (feature1 (pts (xy 193.04 75.565) (xy 193.04 67.15)))
    (feature2 (pts (xy 76.2 75.565) (xy 76.2 67.15)))
    (crossbar (pts (xy 76.2 69.85) (xy 193.04 69.85)))
    (arrow1a (pts (xy 193.04 69.85) (xy 191.913496 70.436421)))
    (arrow1b (pts (xy 193.04 69.85) (xy 191.913496 69.263579)))
    (arrow2a (pts (xy 76.2 69.85) (xy 77.326504 70.436421)))
    (arrow2b (pts (xy 76.2 69.85) (xy 77.326504 69.263579)))
  )
  (gr_text "+5V DC\nMaster Power" (at 143.51 109.855) (layer F.SilkS))
  (gr_text "LED Pwr" (at 93.98 111.125) (layer F.SilkS))
  (gr_text "Osc Out" (at 151.13 83.82) (layer F.SilkS))
  (gr_text "SPI\nOut" (at 88.9 81.915) (layer F.SilkS))
  (gr_text "Sch V2.0.3\nPcb V1.0.1" (at 127 85.09) (layer F.SilkS))
  (gr_text "TrippyRGB\nLogic & Oscillator" (at 127 80.01) (layer F.SilkS))
  (gr_text "Sembazuru\nCircuits" (at 131.445 85.725) (layer B.SilkS))
  (gr_text "DIY DE" (at 113.665 85.725) (layer B.SilkS))
  (gr_text BoM (at 113.665 82.55) (layer B.SilkS))
  (gr_line (start 76.21539 127.00527) (end 193.05539 127.00527) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 76.21539 127.00527) (end 76.21539 76.20527) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 193.05539 127.00527) (end 193.05539 76.20527) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 193.05539 76.20527) (end 76.21539 76.20527) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 192.80139 126.75127) (xy 76.46939 126.75127) (xy 76.46939 76.45927) (xy 192.80139 76.45927)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 192.80139 126.75127) (xy 76.46939 126.75127) (xy 76.46939 76.45927) (xy 192.80139 76.45927)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.52 117.475) (xy 101.6 117.475) (xy 101.6 122.555) (xy 96.52 122.555)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.251 119.126) (xy 105.029 119.126) (xy 105.029 120.904) (xy 103.251 120.904)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.251 95.631) (xy 105.029 95.631) (xy 105.029 97.409) (xy 103.251 97.409)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.251 82.931) (xy 105.029 82.931) (xy 105.029 84.709) (xy 103.251 84.709)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.081 93.091) (xy 141.859 93.091) (xy 141.859 94.869) (xy 140.081 94.869)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.194 89.154) (xy 157.226 89.154) (xy 157.226 91.186) (xy 155.194 91.186)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.242 90.424) (xy 159.258 90.424) (xy 159.766 90.932) (xy 159.766 91.948) (xy 159.258 92.456)
        (xy 158.242 92.456) (xy 157.734 91.948) (xy 157.734 90.932)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.194 92.202) (xy 155.702 91.694) (xy 156.718 91.694) (xy 157.226 92.202) (xy 157.226 93.218)
        (xy 156.718 93.726) (xy 155.702 93.726) (xy 155.194 93.218)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.941 100.711) (xy 164.719 100.711) (xy 164.719 102.489) (xy 162.941 102.489)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.309 95.631) (xy 187.071 95.631) (xy 187.579 96.139) (xy 187.579 96.901) (xy 187.071 97.409)
        (xy 186.309 97.409) (xy 185.801 96.901) (xy 185.801 96.139)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.05 117.475) (xy 151.13 117.475) (xy 151.13 122.555) (xy 146.05 122.555)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.781 120.396) (xy 154.559 120.396) (xy 154.559 122.174) (xy 152.781 122.174)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.462 95.631) (xy 141.478 95.631) (xy 141.859 96.012) (xy 141.859 97.028) (xy 141.478 97.409)
        (xy 140.462 97.409) (xy 140.081 97.028) (xy 140.081 96.012)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.702 96.774) (xy 156.718 96.774) (xy 157.226 97.282) (xy 157.226 98.298) (xy 156.718 98.806)
        (xy 155.829 98.806) (xy 155.194 98.298) (xy 155.194 97.282)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.242 95.504) (xy 159.258 95.504) (xy 159.766 96.012) (xy 159.766 97.028) (xy 159.258 97.536)
        (xy 158.242 97.536) (xy 157.734 97.028) (xy 157.734 96.012)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.734 98.552) (xy 158.242 98.044) (xy 159.258 98.044) (xy 159.766 98.552) (xy 159.766 99.568)
        (xy 159.258 100.076) (xy 158.242 100.076) (xy 157.734 99.568)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.719 106.172) (xy 164.719 107.188) (xy 164.338 107.569) (xy 163.322 107.569) (xy 162.941 107.188)
        (xy 162.941 106.172) (xy 163.322 105.791) (xy 164.338 105.791)
      )
    )
  )
)
