(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 2934)
    (tracks 1659)
    (zones 0)
    (modules 117)
    (nets 58)
  )
  (page A)
  (title_block
    (title "DEC PC3XX RAM Board (5016233-01-A1), Reverse Engineered")
    (date 2021-03-09)
    (rev A1)
    (company "Bjoren Davis")
    (comment 2 http://bitsavers.org/pdf/dec/pdp11/pro3xx/MP-01394_PC350_Field_Maintenance_Print_Set_.pdf)
    (comment 3 "additional information from the schematic in the DEC PC350 Field Maintenance Print Set")
    (comment 4 "This is reverse engineered from an actual instance of the board, SN ZG71912329, with")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 76.2 76.2)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "production_output/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 /~MUXA1)
  (net 4 /~MUXA7)
  (net 5 /~MUXA2)
  (net 6 /~MUXA0)
  (net 7 /~MUXA4)
  (net 8 /~MUXA3)
  (net 9 /~LCAS)
  (net 10 /D07)
  (net 11 /~RASD0)
  (net 12 /D06)
  (net 13 /D05)
  (net 14 /D04)
  (net 15 /CAS)
  (net 16 /~MUXA6)
  (net 17 /MWLB)
  (net 18 /~MUXA8)
  (net 19 /~MUXA5)
  (net 20 /MWHB)
  (net 21 /D15)
  (net 22 /D14)
  (net 23 /D13)
  (net 24 /~P256KD)
  (net 25 /D12)
  (net 26 /D11)
  (net 27 /D10)
  (net 28 /D09)
  (net 29 /D08)
  (net 30 /D00)
  (net 31 /D01)
  (net 32 /D02)
  (net 33 /D03)
  (net 34 /LMUXA1)
  (net 35 /LMUXA2)
  (net 36 /LMUXA6)
  (net 37 /LMUXA0)
  (net 38 /LMUXA3)
  (net 39 /LMUXA4)
  (net 40 /LMUXA5)
  (net 41 /LMUXA7)
  (net 42 /LMUXA8)
  (net 43 /~LMWHB)
  (net 44 /~LMWLB)
  (net 45 "Net-(R21-Pad1)")
  (net 46 "Net-(E9-Pad6)")
  (net 47 "Net-(E9-Pad12)")
  (net 48 "Net-(E9-Pad4)")
  (net 49 "Net-(E9-Pad10)")
  (net 50 "Net-(E9-Pad2)")
  (net 51 "Net-(E9-Pad8)")
  (net 52 "Net-(E18-Pad6)")
  (net 53 "Net-(E18-Pad12)")
  (net 54 "Net-(E18-Pad4)")
  (net 55 "Net-(E18-Pad10)")
  (net 56 "Net-(E18-Pad2)")
  (net 57 "Net-(E18-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /CAS)
    (add_net /D00)
    (add_net /D01)
    (add_net /D02)
    (add_net /D03)
    (add_net /D04)
    (add_net /D05)
    (add_net /D06)
    (add_net /D07)
    (add_net /D08)
    (add_net /D09)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D14)
    (add_net /D15)
    (add_net /LMUXA0)
    (add_net /LMUXA1)
    (add_net /LMUXA2)
    (add_net /LMUXA3)
    (add_net /LMUXA4)
    (add_net /LMUXA5)
    (add_net /LMUXA6)
    (add_net /LMUXA7)
    (add_net /LMUXA8)
    (add_net /MWHB)
    (add_net /MWLB)
    (add_net /~LCAS)
    (add_net /~LMWHB)
    (add_net /~LMWLB)
    (add_net /~MUXA0)
    (add_net /~MUXA1)
    (add_net /~MUXA2)
    (add_net /~MUXA3)
    (add_net /~MUXA4)
    (add_net /~MUXA5)
    (add_net /~MUXA6)
    (add_net /~MUXA7)
    (add_net /~MUXA8)
    (add_net /~P256KD)
    (add_net /~RASD0)
    (add_net GND)
    (add_net "Net-(E18-Pad10)")
    (add_net "Net-(E18-Pad12)")
    (add_net "Net-(E18-Pad2)")
    (add_net "Net-(E18-Pad4)")
    (add_net "Net-(E18-Pad6)")
    (add_net "Net-(E18-Pad8)")
    (add_net "Net-(E9-Pad10)")
    (add_net "Net-(E9-Pad12)")
    (add_net "Net-(E9-Pad2)")
    (add_net "Net-(E9-Pad4)")
    (add_net "Net-(E9-Pad6)")
    (add_net "Net-(E9-Pad8)")
    (add_net "Net-(R21-Pad1)")
  )
  (module ramboard_footprint_library:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 101.6 139.7 180)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E18 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74S04 (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 14 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /CAS))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(E18-Pad6)"))
    (pad 12 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(E18-Pad12)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /~MUXA6))
    (pad 11 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /MWLB))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(E18-Pad4)"))
    (pad 10 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(E18-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /~MUXA8))
    (pad 9 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /~MUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(E18-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(E18-Pad8)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /MWHB))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 132.08 139.7 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E17 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /D15))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /~LMWHB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /D15))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 142.24 139.7 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E16 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /D14))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /~LMWHB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /D14))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 152.4 139.7 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E15 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /D13))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /~LMWHB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /D13))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 162.56 139.7 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E14 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /D12))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /~LMWHB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /D12))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 172.72 139.7 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E13 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /D11))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /~LMWHB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /D11))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 182.88 139.7 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E12 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /D10))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /~LMWHB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /D10))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 193.04 139.7 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E11 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /D09))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /~LMWHB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /D09))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 203.2 139.7 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E10 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /D08))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /~LMWHB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /D08))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 101.6 109.22 180)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E9 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 74S04 (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 14 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /~MUXA7))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(E9-Pad6)"))
    (pad 12 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(E9-Pad12)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /~MUXA2))
    (pad 11 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /~MUXA0))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(E9-Pad4)"))
    (pad 10 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(E9-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /~MUXA4))
    (pad 9 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /~MUXA1))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(E9-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(E9-Pad8)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /~MUXA3))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 132.08 106.68 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E8 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /D07))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /~LMWLB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /D07))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 142.24 106.68 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E7 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /D06))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /~LMWLB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /D06))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 152.4 106.68 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E6 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /D05))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /~LMWLB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /D05))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 162.56 106.68 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E5 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /D04))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /~LMWLB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /D04))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 172.72 106.68 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E4 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /D03))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /~LMWLB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /D03))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 182.88 106.68 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E3 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /D02))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /~LMWLB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /D02))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 193.04 106.68 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /D01))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /~LMWLB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /D01))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 203.2 106.68 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference E1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value M5M4256AP (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /D00))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /~LMWLB))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /D00))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dec_strokefont_library:Sym2 (layer B.Cu) (tedit 604662EE)
    (at 151.7396 81.6356)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymBlank (layer B.Cu) (tedit 604664A7)
    (at 148.1836 81.6356)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymE (layer B.Cu) (tedit 604665CD)
    (at 144.6276 81.6356)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymD (layer B.Cu) (tedit 60466583)
    (at 141.0716 81.6356)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymI (layer B.Cu) (tedit 60466554)
    (at 137.5156 81.6356)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymS (layer B.Cu) (tedit 60466519)
    (at 133.9596 81.6356)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymM (layer B.Cu) (tedit 6046687F)
    (at 148.5392 85.6234)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymA (layer B.Cu) (tedit 604667E3)
    (at 144.9832 85.6234)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymR (layer B.Cu) (tedit 60466905)
    (at 141.4272 85.6234)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymBlank (layer B.Cu) (tedit 604664A7)
    (at 137.8712 85.6234)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym0 (layer B.Cu) (tedit 604662FE)
    (at 134.3152 85.6234)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym0 (layer B.Cu) (tedit 604662FE)
    (at 130.7592 85.6234)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym3 (layer B.Cu) (tedit 604662E2)
    (at 127.2032 85.6234)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymC (layer B.Cu) (tedit 60466BED)
    (at 123.6472 85.6234)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymP (layer B.Cu) (tedit 604668D2)
    (at 120.0912 85.6234)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym4 (layer B.Cu) (tedit 604662D2)
    (at 186.7916 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymL (layer B.Cu) (tedit 60466824)
    (at 183.2356 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym1 (layer B.Cu) (tedit 604662F5)
    (at 167.2336 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:SymA (layer B.Cu) (tedit 604667E3)
    (at 163.6776 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym- (layer B.Cu) (tedit 60466457)
    (at 160.1216 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym1 (layer B.Cu) (tedit 604662F5)
    (at 156.5656 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym0 (layer B.Cu) (tedit 604662FE)
    (at 153.0096 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym- (layer B.Cu) (tedit 60466457)
    (at 149.4536 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym3 (layer B.Cu) (tedit 604662E2)
    (at 145.8976 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym3 (layer B.Cu) (tedit 604662E2)
    (at 142.3416 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym2 (layer B.Cu) (tedit 604662EE)
    (at 138.7856 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym6 (layer B.Cu) (tedit 604662DB)
    (at 135.2296 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym1 (layer B.Cu) (tedit 604662F5)
    (at 131.6736 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym0 (layer B.Cu) (tedit 604662FE)
    (at 128.1176 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym5 (layer B.Cu) (tedit 604662C6)
    (at 124.5616 117.1702)
    (fp_text reference " " (at 0.4 3.29) (layer B.SilkS) hide)
    (fp_text value " " (at 0.7 1.66) (layer B.Fab) hide)
  )
  (module dec_strokefont_library:Sym1 (layer F.Cu) (tedit 604662F5)
    (at 199.4662 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:SymBlank (layer F.Cu) (tedit 604664A7)
    (at 195.9102 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:SymE (layer F.Cu) (tedit 604665CD)
    (at 192.3542 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:SymD (layer F.Cu) (tedit 60466583)
    (at 188.7982 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:SymI (layer F.Cu) (tedit 60466554)
    (at 185.2422 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:SymS (layer F.Cu) (tedit 60466519)
    (at 181.6862 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:SymBlank (layer F.Cu) (tedit 604664A7)
    (at 178.1302 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:SymBlank (layer F.Cu) (tedit 604664A7)
    (at 174.5742 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:SymBlank (layer F.Cu) (tedit 604664A7)
    (at 171.0182 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:Sym1 (layer F.Cu) (tedit 604662F5)
    (at 167.4622 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:Sym0 (layer F.Cu) (tedit 604662FE)
    (at 163.9062 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:Sym- (layer F.Cu) (tedit 60466457)
    (at 160.3502 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:Sym4 (layer F.Cu) (tedit 604662D2)
    (at 156.7942 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:Sym3 (layer F.Cu) (tedit 604662E2)
    (at 153.2382 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:Sym2 (layer F.Cu) (tedit 604662EE)
    (at 149.6822 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:Sym6 (layer F.Cu) (tedit 604662DB)
    (at 146.1262 114.7953)
    (fp_text reference " " (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:Sym1 (layer F.Cu) (tedit 604662F5)
    (at 142.5702 114.7953)
    (fp_text reference "" (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:Sym4 (layer F.Cu) (tedit 604662D2)
    (at 139.0142 114.7953)
    (fp_text reference "" (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module dec_strokefont_library:Sym5 (layer F.Cu) (tedit 604662C6)
    (at 135.4582 114.7953)
    (fp_text reference "" (at 0.4 -3.29) (layer F.SilkS) hide)
    (fp_text value " " (at 0.7 -1.66) (layer F.Fab) hide)
  )
  (module ramboard_footprint_library:MountingHole_OctagonalOutline (layer F.Cu) (tedit 60464AD6)
    (at 203.2 81.28)
    (fp_text reference REF** (at 0 -0.127) (layer F.SilkS) hide)
    (fp_text value MountingHole_SquareOutline (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.81) (layers *.Cu *.Mask))
  )
  (module ramboard_footprint_library:PinSocket_2x24_P2.54mm_Vertical_Mirror_MinusOuter8 (layer F.Cu) (tedit 5E88B279)
    (at 83.82 86.36)
    (descr "Through hole straight socket strip, 2x24, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated with outer 8 pins missing")
    (tags "Through hole socket strip THT 2x24 2.54mm double row")
    (fp_text reference J1 (at 3.2385 -2.54) (layer F.SilkS))
    (fp_text value Conn_02x24_Odd_Even_MinusOuter8 (at 1.27 61.19) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 29.21 90) (layer F.Fab) hide)
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /~P256KD))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /MWHB))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /CAS))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /~RASD0))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /MWLB))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /~MUXA8))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /D12))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /~MUXA5))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /D11))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /~MUXA6))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /D10))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /D13))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /D09))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /D14))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D08))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /D15))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D00))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /D07))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D01))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /D06))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D02))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /D05))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /D03))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /D04))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /~MUXA3))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /~MUXA7))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /~MUXA4))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /~MUXA0))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /~MUXA2))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /~MUXA1))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x24_P2.54mm_Vertical.wrl
      (offset (xyz 2.54 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 93.98 149.86)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference W2 (at 3.8735 2.0955) (layer F.Cu))
    (fp_text value 0Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 /~P256KD))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 93.98 119.38)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference W1 (at 7.747 0.0635 90) (layer F.Cu))
    (fp_text value 0Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 54 "Net-(E18-Pad4)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 45 "Net-(R21-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 149.86)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R10 (at 12.827 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 53 "Net-(E18-Pad12)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 147.32)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R22 (at 12.827 0) (layer F.SilkS))
    (fp_text value 10Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 53 "Net-(E18-Pad12)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 /~LCAS))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 144.78)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R12 (at 12.827 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 56 "Net-(E18-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 142.24)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R24 (at 12.827 0) (layer F.SilkS))
    (fp_text value 33Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 56 "Net-(E18-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 43 /~LMWHB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 139.7)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R19 (at 12.827 0) (layer F.SilkS))
    (fp_text value 22Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 52 "Net-(E18-Pad6)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 /LMUXA6))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 137.16)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R7 (at 12.350809 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 52 "Net-(E18-Pad6)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 134.62)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R18 (at 12.827 0) (layer F.SilkS))
    (fp_text value 22Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 57 "Net-(E18-Pad8)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 /LMUXA5))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 132.08)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R6 (at 12.350809 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 57 "Net-(E18-Pad8)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 129.54)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R20 (at 12.827 0) (layer F.SilkS))
    (fp_text value 22Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "Net-(E9-Pad12)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 41 /LMUXA7))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 127)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R8 (at 12.350809 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "Net-(E9-Pad12)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 124.46)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R21 (at 12.827 0) (layer F.SilkS))
    (fp_text value 22Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 45 "Net-(R21-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 /LMUXA8))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 121.92)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R9 (at 12.350809 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 45 "Net-(R21-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 119.38)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R11 (at 12.827 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 55 "Net-(E18-Pad10)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 116.84)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R23 (at 12.827 0) (layer F.SilkS))
    (fp_text value 33Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 55 "Net-(E18-Pad10)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 /~LMWLB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 114.3)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R4 (at 12.350809 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 50 "Net-(E9-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 111.76)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R16 (at 12.827 0) (layer F.SilkS))
    (fp_text value 22Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 50 "Net-(E9-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 38 /LMUXA3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 109.22)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R1 (at 12.350809 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 49 "Net-(E9-Pad10)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 106.68)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R13 (at 12.827 0) (layer F.SilkS))
    (fp_text value 22Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 49 "Net-(E9-Pad10)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 37 /LMUXA0))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 104.14)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R5 (at 12.350809 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 48 "Net-(E9-Pad4)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 101.6)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R17 (at 12.827 0) (layer F.SilkS))
    (fp_text value 22Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 48 "Net-(E9-Pad4)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 39 /LMUXA4))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 99.06)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R3 (at 12.350809 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 46 "Net-(E9-Pad6)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 96.52)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R15 (at 12.827 0) (layer F.SilkS))
    (fp_text value 22Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 46 "Net-(E9-Pad6)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 /LMUXA2))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 93.98)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R2 (at 12.350809 0) (layer F.SilkS))
    (fp_text value 1kΩ (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 51 "Net-(E9-Pad8)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:R_Axial_US_0.25W_0.40in (layer F.Cu) (tedit 5E88A231)
    (at 106.68 91.44)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial US 1/4W ")
    (fp_text reference R14 (at 12.827 0) (layer F.SilkS))
    (fp_text value 22Ω (at 4.9276 2.032) (layer F.Fab))
    (fp_text user %R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 51 "Net-(E9-Pad8)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 34 /LMUXA1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1.33 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 203.2 144.78 180)
    (fp_text reference C9 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 193.04 144.78 180)
    (fp_text reference C10 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 182.88 144.78 180)
    (fp_text reference C11 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 172.72 144.78 180)
    (fp_text reference C12 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 162.56 144.78 180)
    (fp_text reference C13 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 152.4 144.78 180)
    (fp_text reference C14 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 142.24 144.78 180)
    (fp_text reference C15 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 132.08 144.78 180)
    (fp_text reference C16 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 94 144.78)
    (fp_text reference C17 (at 9.378 1.8415) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 94 114.3)
    (fp_text reference C18 (at 8.362 2.3495) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 203.2 111.76 180)
    (fp_text reference C1 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 193.04 111.76 180)
    (fp_text reference C2 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 182.88 111.76 180)
    (fp_text reference C3 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 172.72 111.76 180)
    (fp_text reference C4 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 162.56 111.76 180)
    (fp_text reference C5 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 152.4 111.76 180)
    (fp_text reference C6 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 142.24 111.76 180)
    (fp_text reference C7 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:Capacitor_CX (layer F.Cu) (tedit 60463419)
    (at 132.08 111.76 180)
    (fp_text reference C8 (at 2.9464 -2.3368) (layer F.SilkS))
    (fp_text value "0.22μF 50V" (at 3.81 2.413) (layer F.Fab))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:CapacitorPolar_C1 (layer F.Cu) (tedit 5E88A081)
    (at 96.52 86.36)
    (tags CapacitorPolar_C1)
    (fp_text reference C19 (at 7.6708 -4.1148) (layer F.SilkS))
    (fp_text value "10μF 35V" (at 7.4168 4.2164) (layer F.Fab))
    (fp_text user %R (at 7.5 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 20.32 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.35 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ramboard_footprint_library:MountingHole_SquareOutline (layer F.Cu) (tedit 60464AE8)
    (at 81.28 81.28)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_SquareOutline (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.81) (layers *.Cu *.Mask))
  )
  (module ramboard_footprint_library:MountingHole_SquareOutline (layer F.Cu) (tedit 60464AE8)
    (at 203.2 152.4)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_SquareOutline (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.81) (layers *.Cu *.Mask))
  )
  (module ramboard_footprint_library:MountingHole_SquareOutline (layer F.Cu) (tedit 60464AE8)
    (at 81.28 152.4)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_SquareOutline (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.81) (layers *.Cu *.Mask))
  )
  (dimension 132.08 (width 0.15) (layer Cmts.User)
    (gr_text "5.2000 in" (at 142.24 165.003) (layer Cmts.User))
    (feature1 (pts (xy 208.28 157.48) (xy 208.28 164.289421)))
    (feature2 (pts (xy 76.2 157.48) (xy 76.2 164.289421)))
    (crossbar (pts (xy 76.2 163.703) (xy 208.28 163.703)))
    (arrow1a (pts (xy 208.28 163.703) (xy 207.153496 164.289421)))
    (arrow1b (pts (xy 208.28 163.703) (xy 207.153496 163.116579)))
    (arrow2a (pts (xy 76.2 163.703) (xy 77.326504 164.289421)))
    (arrow2b (pts (xy 76.2 163.703) (xy 77.326504 163.116579)))
  )
  (dimension 121.92 (width 0.15) (layer Cmts.User)
    (gr_text "4.8000 in" (at 142.24 162.9075) (layer Cmts.User))
    (feature1 (pts (xy 203.2 152.4) (xy 203.2 162.193921)))
    (feature2 (pts (xy 81.28 152.4) (xy 81.28 162.193921)))
    (crossbar (pts (xy 81.28 161.6075) (xy 203.2 161.6075)))
    (arrow1a (pts (xy 203.2 161.6075) (xy 202.073496 162.193921)))
    (arrow1b (pts (xy 203.2 161.6075) (xy 202.073496 161.021079)))
    (arrow2a (pts (xy 81.28 161.6075) (xy 82.406504 162.193921)))
    (arrow2b (pts (xy 81.28 161.6075) (xy 82.406504 161.021079)))
  )
  (dimension 81.28 (width 0.15) (layer Cmts.User)
    (gr_text "3.2000 in" (at 223.2325 116.84 90) (layer Cmts.User))
    (feature1 (pts (xy 208.28 76.2) (xy 222.518921 76.2)))
    (feature2 (pts (xy 208.28 157.48) (xy 222.518921 157.48)))
    (crossbar (pts (xy 221.9325 157.48) (xy 221.9325 76.2)))
    (arrow1a (pts (xy 221.9325 76.2) (xy 222.518921 77.326504)))
    (arrow1b (pts (xy 221.9325 76.2) (xy 221.346079 77.326504)))
    (arrow2a (pts (xy 221.9325 157.48) (xy 222.518921 156.353496)))
    (arrow2b (pts (xy 221.9325 157.48) (xy 221.346079 156.353496)))
  )
  (dimension 71.12 (width 0.15) (layer Cmts.User)
    (gr_text "2.8000 in" (at 218.216 116.9162 90) (layer Cmts.User))
    (feature1 (pts (xy 203.2 81.3562) (xy 217.502421 81.3562)))
    (feature2 (pts (xy 203.2 152.4762) (xy 217.502421 152.4762)))
    (crossbar (pts (xy 216.916 152.4762) (xy 216.916 81.3562)))
    (arrow1a (pts (xy 216.916 81.3562) (xy 217.502421 82.482704)))
    (arrow1b (pts (xy 216.916 81.3562) (xy 216.329579 82.482704)))
    (arrow2a (pts (xy 216.916 152.4762) (xy 217.502421 151.349696)))
    (arrow2b (pts (xy 216.916 152.4762) (xy 216.329579 151.349696)))
  )
  (dimension 15.24 (width 0.15) (layer Cmts.User)
    (gr_text "0.6000 in" (at 65.375 83.82 90) (layer Cmts.User))
    (feature1 (pts (xy 83.82 76.2) (xy 66.088579 76.2)))
    (feature2 (pts (xy 83.82 91.44) (xy 66.088579 91.44)))
    (crossbar (pts (xy 66.675 91.44) (xy 66.675 76.2)))
    (arrow1a (pts (xy 66.675 76.2) (xy 67.261421 77.326504)))
    (arrow1b (pts (xy 66.675 76.2) (xy 66.088579 77.326504)))
    (arrow2a (pts (xy 66.675 91.44) (xy 67.261421 90.313496)))
    (arrow2b (pts (xy 66.675 91.44) (xy 66.088579 90.313496)))
  )
  (dimension 17.78 (width 0.15) (layer Cmts.User)
    (gr_text "0.7000 in" (at 64.486 148.59 270) (layer Cmts.User))
    (feature1 (pts (xy 83.82 157.48) (xy 65.199579 157.48)))
    (feature2 (pts (xy 83.82 139.7) (xy 65.199579 139.7)))
    (crossbar (pts (xy 65.786 139.7) (xy 65.786 157.48)))
    (arrow1a (pts (xy 65.786 157.48) (xy 65.199579 156.353496)))
    (arrow1b (pts (xy 65.786 157.48) (xy 66.372421 156.353496)))
    (arrow2a (pts (xy 65.786 139.7) (xy 65.199579 140.826504)))
    (arrow2b (pts (xy 65.786 139.7) (xy 66.372421 140.826504)))
  )
  (dimension 7.62 (width 0.15) (layer Cmts.User)
    (gr_text "0.3000 in" (at 80.01 67.661) (layer Cmts.User))
    (feature1 (pts (xy 76.2 91.44) (xy 76.2 68.374579)))
    (feature2 (pts (xy 83.82 91.44) (xy 83.82 68.374579)))
    (crossbar (pts (xy 83.82 68.961) (xy 76.2 68.961)))
    (arrow1a (pts (xy 76.2 68.961) (xy 77.326504 68.374579)))
    (arrow1b (pts (xy 76.2 68.961) (xy 77.326504 69.547421)))
    (arrow2a (pts (xy 83.82 68.961) (xy 82.693496 68.374579)))
    (arrow2b (pts (xy 83.82 68.961) (xy 82.693496 69.547421)))
  )
  (dimension 2.54 (width 0.15) (layer Cmts.User)
    (gr_text "0.1000 in" (at 82.55 74.138) (layer Cmts.User))
    (feature1 (pts (xy 81.28 91.44) (xy 81.28 74.851579)))
    (feature2 (pts (xy 83.82 91.44) (xy 83.82 74.851579)))
    (crossbar (pts (xy 83.82 75.438) (xy 81.28 75.438)))
    (arrow1a (pts (xy 81.28 75.438) (xy 82.406504 74.851579)))
    (arrow1b (pts (xy 81.28 75.438) (xy 82.406504 76.024421)))
    (arrow2a (pts (xy 83.82 75.438) (xy 82.693496 74.851579)))
    (arrow2b (pts (xy 83.82 75.438) (xy 82.693496 76.024421)))
  )
  (dimension 10.16 (width 0.15) (layer Cmts.User)
    (gr_text "0.4000 in" (at 74.0745 86.36 90) (layer Cmts.User))
    (feature1 (pts (xy 83.82 81.28) (xy 74.788079 81.28)))
    (feature2 (pts (xy 83.82 91.44) (xy 74.788079 91.44)))
    (crossbar (pts (xy 75.3745 91.44) (xy 75.3745 81.28)))
    (arrow1a (pts (xy 75.3745 81.28) (xy 75.960921 82.406504)))
    (arrow1b (pts (xy 75.3745 81.28) (xy 74.788079 82.406504)))
    (arrow2a (pts (xy 75.3745 91.44) (xy 75.960921 90.313496)))
    (arrow2b (pts (xy 75.3745 91.44) (xy 74.788079 90.313496)))
  )
  (dimension 71.12 (width 0.15) (layer Cmts.User)
    (gr_text "2.8000 in" (at 69.82 116.84 270) (layer Cmts.User))
    (feature1 (pts (xy 81.28 152.4) (xy 70.533579 152.4)))
    (feature2 (pts (xy 81.28 81.28) (xy 70.533579 81.28)))
    (crossbar (pts (xy 71.12 81.28) (xy 71.12 152.4)))
    (arrow1a (pts (xy 71.12 152.4) (xy 70.533579 151.273496)))
    (arrow1b (pts (xy 71.12 152.4) (xy 71.706421 151.273496)))
    (arrow2a (pts (xy 71.12 81.28) (xy 70.533579 82.406504)))
    (arrow2b (pts (xy 71.12 81.28) (xy 71.706421 82.406504)))
  )
  (dimension 121.92 (width 0.15) (layer Cmts.User)
    (gr_text "4.8000 in" (at 142.24 71.471) (layer Cmts.User))
    (feature1 (pts (xy 203.2 81.28) (xy 203.2 72.184579)))
    (feature2 (pts (xy 81.28 81.28) (xy 81.28 72.184579)))
    (crossbar (pts (xy 81.28 72.771) (xy 203.2 72.771)))
    (arrow1a (pts (xy 203.2 72.771) (xy 202.073496 73.357421)))
    (arrow1b (pts (xy 203.2 72.771) (xy 202.073496 72.184579)))
    (arrow2a (pts (xy 81.28 72.771) (xy 82.406504 73.357421)))
    (arrow2b (pts (xy 81.28 72.771) (xy 82.406504 72.184579)))
  )
  (dimension 81.28 (width 0.15) (layer Cmts.User)
    (gr_text "3.2000 in" (at 67.3435 116.84 270) (layer Cmts.User))
    (feature1 (pts (xy 76.2 157.48) (xy 68.057079 157.48)))
    (feature2 (pts (xy 76.2 76.2) (xy 68.057079 76.2)))
    (crossbar (pts (xy 68.6435 76.2) (xy 68.6435 157.48)))
    (arrow1a (pts (xy 68.6435 157.48) (xy 68.057079 156.353496)))
    (arrow1b (pts (xy 68.6435 157.48) (xy 69.229921 156.353496)))
    (arrow2a (pts (xy 68.6435 76.2) (xy 68.057079 77.326504)))
    (arrow2b (pts (xy 68.6435 76.2) (xy 69.229921 77.326504)))
  )
  (dimension 132.08 (width 0.15) (layer Cmts.User)
    (gr_text "5.2000 in" (at 142.24 69.2485) (layer Cmts.User))
    (feature1 (pts (xy 208.28 76.2) (xy 208.28 69.962079)))
    (feature2 (pts (xy 76.2 76.2) (xy 76.2 69.962079)))
    (crossbar (pts (xy 76.2 70.5485) (xy 208.28 70.5485)))
    (arrow1a (pts (xy 208.28 70.5485) (xy 207.153496 71.134921)))
    (arrow1b (pts (xy 208.28 70.5485) (xy 207.153496 69.962079)))
    (arrow2a (pts (xy 76.2 70.5485) (xy 77.326504 71.134921)))
    (arrow2b (pts (xy 76.2 70.5485) (xy 77.326504 69.962079)))
  )
  (gr_text "DEC Professional 3XX 128 KiB/512 KiB RAM\nDaughtercard (Replica), Revision A1\nBjoren Davis, March 9, 2021 " (at 152.5905 152.4635 180) (layer B.SilkS))
  (gr_line (start 76.2 157.48) (end 76.2 76.2) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 208.28 157.48) (end 76.2 157.48) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 208.28 76.2) (end 208.28 157.48) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 76.2 76.2) (end 208.28 76.2) (layer Edge.Cuts) (width 0.0254))
  (zone (net 2) (net_name +5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.628 85.852) (xy 207.772 85.852) (xy 207.772 147.828) (xy 198.628 147.828) (xy 198.628 156.972)
        (xy 85.852 156.972) (xy 85.852 147.828) (xy 76.708 147.828) (xy 76.708 85.852) (xy 85.852 85.852)
        (xy 85.852 76.708) (xy 198.628 76.708)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.628 85.852) (xy 207.772 85.852) (xy 207.772 147.828) (xy 198.628 147.828) (xy 198.628 156.972)
        (xy 85.852 156.972) (xy 85.852 147.828) (xy 76.708 147.828) (xy 76.708 85.852) (xy 85.852 85.852)
        (xy 85.852 76.708) (xy 198.628 76.708)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.4455 81.5975) (xy 135.4455 86.868) (xy 134.9375 87.376) (xy 129.032 87.376) (xy 129.032 110.5535)
        (xy 129.54 111.0615) (xy 130.556 112.0775) (xy 130.556 118.872) (xy 130.2385 119.1895) (xy 127.4445 119.1895)
        (xy 127.4445 121.4755) (xy 126.1745 121.4755) (xy 126.1745 119.1895) (xy 125.095 119.1895) (xy 124.7775 118.872)
        (xy 124.7775 116.5225) (xy 123.444 115.189) (xy 123.444 105.8545) (xy 123.825 105.4735) (xy 125.73 105.4735)
        (xy 125.73 87.376) (xy 113.7285 87.376) (xy 113.7285 90.424) (xy 104.8385 90.3605) (xy 104.8385 113.157)
        (xy 104.5845 113.411) (xy 104.013 113.411) (xy 102.0445 115.3795) (xy 98.679 115.3795) (xy 98.679 110.617)
        (xy 103.3145 110.617) (xy 103.3145 95.1865) (xy 98.7425 95.1865) (xy 98.7425 81.0895) (xy 134.9375 81.0895)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.648 132.1435) (xy 104.648 140.7795) (xy 105.3465 141.478) (xy 105.3465 147.0025) (xy 100.6475 147.0025)
        (xy 100.6475 142.24) (xy 99.5045 142.24) (xy 99.314 141.986) (xy 99.314 141.1605) (xy 99.568 140.9065)
        (xy 102.87 140.9065) (xy 102.87 132.1435) (xy 103.0605 131.953) (xy 104.4575 131.953)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.923 80.899) (xy 145.923 87.122) (xy 145.6055 87.4395) (xy 139.7635 87.4395) (xy 139.446 87.757)
        (xy 139.446 113.157) (xy 139.2555 113.3475) (xy 133.858 113.3475) (xy 133.6675 113.157) (xy 133.6675 112.903)
        (xy 133.6675 105.7275) (xy 133.985 105.41) (xy 135.255 105.41) (xy 136.4615 104.2035) (xy 136.4615 80.9625)
        (xy 137.0965 80.3275) (xy 145.3515 80.3275)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.083 80.391) (xy 156.083 87.122) (xy 155.7655 87.4395) (xy 149.9235 87.4395) (xy 149.606 87.757)
        (xy 149.606 113.157) (xy 149.4155 113.3475) (xy 144.018 113.3475) (xy 143.8275 113.157) (xy 143.8275 112.903)
        (xy 143.8275 105.7275) (xy 144.145 105.41) (xy 145.415 105.41) (xy 146.6215 104.2035) (xy 146.685 80.391)
        (xy 147.2565 79.8195) (xy 155.5115 79.8195)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.243 79.9465) (xy 166.243 87.122) (xy 165.9255 87.4395) (xy 160.0835 87.4395) (xy 159.766 87.757)
        (xy 159.766 113.157) (xy 159.5755 113.3475) (xy 154.178 113.3475) (xy 153.9875 113.157) (xy 153.9875 112.903)
        (xy 153.9875 105.7275) (xy 154.305 105.41) (xy 155.575 105.41) (xy 156.7815 104.2035) (xy 156.7815 80.01)
        (xy 157.4165 79.375) (xy 165.6715 79.375)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.403 79.375) (xy 176.403 87.122) (xy 176.0855 87.4395) (xy 170.2435 87.4395) (xy 169.926 87.757)
        (xy 169.926 113.157) (xy 169.7355 113.3475) (xy 164.338 113.3475) (xy 164.1475 113.157) (xy 164.1475 112.903)
        (xy 164.1475 105.7275) (xy 164.465 105.41) (xy 165.735 105.41) (xy 166.9415 104.2035) (xy 166.9415 79.4385)
        (xy 167.5765 78.8035) (xy 175.8315 78.8035)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.563 78.867) (xy 186.563 87.122) (xy 186.2455 87.4395) (xy 180.4035 87.4395) (xy 180.086 87.757)
        (xy 180.086 113.157) (xy 179.8955 113.3475) (xy 174.498 113.3475) (xy 174.3075 113.157) (xy 174.3075 112.903)
        (xy 174.3075 105.7275) (xy 174.625 105.41) (xy 175.895 105.41) (xy 177.1015 104.2035) (xy 177.1015 78.9305)
        (xy 177.7365 78.2955) (xy 185.9915 78.2955)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.723 78.359) (xy 196.723 87.122) (xy 196.4055 87.4395) (xy 190.5635 87.4395) (xy 190.246 87.757)
        (xy 190.246 113.157) (xy 190.0555 113.3475) (xy 184.658 113.3475) (xy 184.4675 113.157) (xy 184.4675 112.903)
        (xy 184.4675 105.7275) (xy 184.785 105.41) (xy 186.055 105.41) (xy 187.2615 104.2035) (xy 187.2615 78.359)
        (xy 187.8965 77.7875) (xy 196.1515 77.7875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.7145 141.0335) (xy 128.7145 143.764) (xy 129.667 144.7165) (xy 129.667 151.8285) (xy 129.4765 152.019)
        (xy 125.9205 152.019) (xy 125.73 151.8285) (xy 125.73 141.0335) (xy 125.857 140.843) (xy 128.524 140.843)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.479 119.1895) (xy 149.479 144.0815) (xy 151.384 145.9865) (xy 152.908 145.9865) (xy 153.289 146.2405)
        (xy 153.289 152.7175) (xy 152.8445 153.035) (xy 144.2085 153.035) (xy 143.8275 152.5905) (xy 143.8275 138.938)
        (xy 144.0815 138.684) (xy 145.415 138.684) (xy 145.8595 138.303) (xy 145.8595 119.126) (xy 146.2405 118.745)
        (xy 149.0345 118.745)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.639 119.1895) (xy 159.639 144.0815) (xy 161.544 145.9865) (xy 163.068 145.9865) (xy 163.449 146.33575)
        (xy 163.449 153.13025) (xy 163.0045 153.543) (xy 154.3685 153.543) (xy 153.9875 153.035) (xy 153.9875 138.938)
        (xy 154.2415 138.684) (xy 155.575 138.684) (xy 156.0195 138.303) (xy 156.0195 119.126) (xy 156.4005 118.745)
        (xy 159.1945 118.745)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.799 119.1895) (xy 169.799 144.0815) (xy 171.704 145.9865) (xy 173.228 145.9865) (xy 173.609 146.2405)
        (xy 173.609 153.543) (xy 173.1645 154.051) (xy 164.5285 154.051) (xy 164.1475 153.543) (xy 164.1475 138.938)
        (xy 164.4015 138.684) (xy 165.735 138.684) (xy 166.1795 138.303) (xy 166.1795 119.126) (xy 166.5605 118.745)
        (xy 169.3545 118.745)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.959 119.1895) (xy 179.959 144.0815) (xy 181.864 145.9865) (xy 183.388 145.9865) (xy 183.769 146.2405)
        (xy 183.769 154.051) (xy 183.3245 154.559) (xy 174.6885 154.559) (xy 174.3075 154.051) (xy 174.3075 138.938)
        (xy 174.5615 138.684) (xy 175.895 138.684) (xy 176.3395 138.303) (xy 176.3395 119.126) (xy 176.7205 118.745)
        (xy 179.5145 118.745)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190.119 119.1895) (xy 190.119 144.0815) (xy 192.024 145.9865) (xy 193.548 145.9865) (xy 193.929 146.33575)
        (xy 193.929 154.65425) (xy 193.4845 155.067) (xy 184.8485 155.067) (xy 184.4675 154.559) (xy 184.4675 138.938)
        (xy 184.7215 138.684) (xy 186.055 138.684) (xy 186.4995 138.303) (xy 186.4995 119.126) (xy 186.8805 118.745)
        (xy 189.6745 118.745)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.319 119.1895) (xy 139.319 144.0815) (xy 141.224 145.9865) (xy 142.748 145.9865) (xy 143.129 146.2405)
        (xy 143.129 152.146) (xy 142.621 152.527) (xy 133.985 152.527) (xy 133.6675 152.2095) (xy 133.6675 138.938)
        (xy 133.9215 138.684) (xy 135.255 138.684) (xy 135.6995 138.303) (xy 135.6995 119.126) (xy 136.0805 118.745)
        (xy 138.8745 118.745)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.279 119.1895) (xy 200.279 144.0815) (xy 200.279 147.1295) (xy 198.34225 147.1295) (xy 198.02475 147.47875)
        (xy 198.0565 155.92425) (xy 197.612 156.4005) (xy 195.072 156.4005) (xy 194.6275 155.92425) (xy 194.6275 138.938)
        (xy 194.8815 138.684) (xy 196.215 138.684) (xy 196.6595 138.303) (xy 196.6595 119.126) (xy 197.0405 118.745)
        (xy 199.8345 118.745)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 200.406 86.106) (xy 200.406 113.157) (xy 200.2155 113.3475) (xy 194.818 113.3475) (xy 194.6275 113.157)
        (xy 194.6275 112.903) (xy 194.6275 105.7275) (xy 194.945 105.41) (xy 196.215 105.41) (xy 197.4215 104.2035)
        (xy 197.4215 95.15475) (xy 197.4215 86.36) (xy 197.6755 86.106)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 197.739 156.083) (xy 178.816 156.083) (xy 178.816 153.4795) (xy 175.387 153.4795) (xy 175.387 148.336)
        (xy 197.739 148.336)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 182.245 120.015) (xy 148.7805 120.015) (xy 148.7805 117.9195) (xy 182.245 117.9195)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.682 141.224) (xy 122.682 148.5265) (xy 122.3645 148.844) (xy 119.8245 148.844) (xy 119.507 148.5265)
        (xy 119.507 141.2875) (xy 119.8245 140.97) (xy 122.428 140.97)
      )
    )
  )
)
