(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 41)
    (no_connects 0)
    (area 83.693 55.626 178.435 123.19)
    (thickness 1.6)
    (drawings 36)
    (tracks 138)
    (zones 0)
    (modules 37)
    (nets 40)
  )
  (page A4)
  (title_block
    (title "Project Title")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3302)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2352 2.2352)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEDF7D)
    (pcbplotparams
      (layerselection 0x000fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(CAP1-Pad1)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(J1-Pad0)")
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 "Net-(J1-Pad4)")
  (net 10 "Net-(J1-Pad5)")
  (net 11 "Net-(J1-Pad6)")
  (net 12 "Net-(J1-Pad7)")
  (net 13 "Net-(J1-Pad8)")
  (net 14 "Net-(J1-Pad9)")
  (net 15 "Net-(J1-Pad10)")
  (net 16 "Net-(J1-Pad11)")
  (net 17 "Net-(J1-Pad12)")
  (net 18 "Net-(J1-Pad17A)")
  (net 19 "Net-(J1-Pad3V1)")
  (net 20 "Net-(J1-PadG2)")
  (net 21 "Net-(J1-PadPGM)")
  (net 22 "Net-(J1-PadDAC)")
  (net 23 "Net-(J1-Pad13)")
  (net 24 "Net-(J1-Pad3V2)")
  (net 25 "Net-(J1-Pad18)")
  (net 26 "Net-(J1-Pad17)")
  (net 27 "Net-(J1-PadG3)")
  (net 28 "Net-(J1-Pad22)")
  (net 29 "Net-(J1-PadVIN)")
  (net 30 "Net-(J1-Pad21)")
  (net 31 "Net-(J1-Pad20)")
  (net 32 "Net-(J1-Pad19)")
  (net 33 "Net-(J1-Pad23)")
  (net 34 "Net-(J1-Pad14)")
  (net 35 "Net-(J1-Pad15)")
  (net 36 "Net-(J28-Pad1)")
  (net 37 "Net-(J29-Pad1)")
  (net 38 "Net-(J30-Pad1)")
  (net 39 "Net-(J31-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(CAP1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad17A)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad3V1)")
    (add_net "Net-(J1-Pad3V2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadG2)")
    (add_net "Net-(J1-PadG3)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVIN)")
    (add_net "Net-(J28-Pad1)")
    (add_net "Net-(J29-Pad1)")
    (add_net "Net-(J30-Pad1)")
    (add_net "Net-(J31-Pad1)")
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 578EC0CD)
    (at 143.002 93.218)
    (fp_text reference CAP16 (at 0.1778 -0.0508) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 1 "Net-(CAP1-Pad1)") (clearance 0.508))
  )
  (module Wickerlib:LED-3MM-2PIN (layer F.Cu) (tedit 578EC0BC)
    (at 128.524 101.6 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference LED15 (at -0.1524 -2.9464 90) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:LED-3MM-2PIN (layer F.Cu) (tedit 578EC0AE)
    (at 133.2992 101.4984 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference LED14 (at -0.2794 3.1496 90) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:TEENSY-LC (layer F.Cu) (tedit 578EC060)
    (at 114.503201 70.307201)
    (fp_text reference J1 (at -0.279401 2.387599 180) (layer F.SilkS))
    (fp_text value TEENSY-LC (at -2.54 20.32 180) (layer F.Fab))
    (fp_text user "TEENSY LC" (at -2.082801 0.253999) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 0 thru_hole circle (at -10.16 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad0)"))
    (pad 1 thru_hole circle (at -10.16 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -10.16 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -10.16 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at -10.16 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad12)"))
    (pad 17A thru_hole circle (at -7.62 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-Pad17A)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J1-Pad3V1)"))
    (pad G2 thru_hole circle (at -2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J1-PadG2)"))
    (pad PGM thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad13)"))
    (pad 16 thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(CAP1-Pad1)"))
    (pad 3V2 thru_hole circle (at 5.08 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J1-Pad3V2)"))
    (pad 18 thru_hole circle (at 5.08 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 5.08 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J1-Pad17)"))
    (pad G3 thru_hole circle (at 5.08 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J1-PadG3)"))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J1-Pad19)"))
    (pad 23 thru_hole circle (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J1-Pad23)"))
    (pad 14 thru_hole circle (at 5.08 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J1-Pad15)"))
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2AE)
    (at 100.584 67.691)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 2 (at -0.1524 -2.4638) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2B2)
    (at 96.266 70.231)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 3 (at -0.1016 -2.3368) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2BB)
    (at 100.457 72.898)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 4 (at -0.1016 -2.2352) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2BF)
    (at 96.139 75.438)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 5 (at 0.0254 -2.3368) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad5)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2C6)
    (at 100.203 77.978)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 6 (at 0.0254 -2.2606) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad6)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2CB)
    (at 96.139 80.518)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 7 (at 0.0254 -2.3622) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad7)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2D3)
    (at 100.203 83.058)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 8 (at -0.0508 -2.3114) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2E7)
    (at 96.012 85.598)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 9 (at -0.0254 -2.3876) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad9)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2E2)
    (at 100.076 88.011)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 10 (at 0.0508 -2.3114) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad10)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2EA)
    (at 96.012 90.5764)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 11 (at 0.1016 -2.3368) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad11)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC2F0)
    (at 100.2284 92.8624)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 12 (at -0.1016 -2.3622) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad12)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC23C)
    (at 121.285 97.282)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 13 (at 0 2.2352) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad13)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC25A)
    (at 124.968 82.931)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 17 (at -0.2286 -2.3876) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J1-Pad17)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC25E)
    (at 129.159 80.391)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 18 (at 0.0254 -2.3368) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J1-Pad18)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC262)
    (at 124.841 77.978)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 19 (at -0.0254 -2.4384) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J1-Pad19)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC28D)
    (at 129.159 75.438)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 20 (at 0 -2.3368) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J1-Pad20)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC280)
    (at 124.841 72.771)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 21 (at -0.2032 -2.5908) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J1-Pad21)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC285)
    (at 129.159 70.358)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 22 (at -0.127 -2.5146) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J1-Pad22)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC276)
    (at 124.841 67.691)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 23 (at -0.127 -2.413) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J1-Pad23)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC22E)
    (at 109.728 97.155)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference G2 (at -0.0254 2.3114) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J1-PadG2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC29A)
    (at 129.1336 62.6872)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference G3 (at 0.0254 -2.667) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J1-PadG3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC29F)
    (at 125.0442 60.2488)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference VIN (at -0.0762 -2.6162) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J1-PadVIN)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC220)
    (at 105.664 97.155)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 3V1 (at 0 2.4638) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J1-Pad3V1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC20F)
    (at 101.6 97.155)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 17A (at -0.127 2.413) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-Pad17A)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC238)
    (at 117.475 97.282)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference DAC (at 0.1016 2.3114) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J1-PadDAC)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC234)
    (at 113.665 97.155)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference PGM (at 0.0508 2.3114) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J1-PadPGM)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC0EF)
    (at 140.2588 59.9948)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J28 (at 0.1016 -2.4892) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J28-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 140.6144 80.264)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J29 (at 0 -5.1) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J29-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 578EC0EC)
    (at 145.288 60.0456)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J30 (at 0 -2.4384) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J30-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 145.1356 80.4164)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J31 (at 0 -5.1) (layer F.SilkS))
    (fp_text value HEADER-MALE-1POS-TH-1x01 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J31-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 578EC092)
    (at 128.0668 95.3516 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 3.683 -2.3622 90) (layer F.SilkS))
    (fp_text value R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 35 "Net-(J1-Pad15)"))
  )
  (module Wickerlib:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 578EC095)
    (at 133.2992 95.25 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 3.5306 -2.1844 90) (layer F.SilkS))
    (fp_text value R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 34 "Net-(J1-Pad14)"))
  )
  (module ESP8266:ESP-01 (layer F.Cu) (tedit 578EC409)
    (at 141.1605 66.5099)
    (descr "Module, ESP-8266, ESP-01, 8 pin")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference ESP-01 (at 5.6896 3.5052 90) (layer F.SilkS))
    (fp_text value ESP-01v090 (at 12.192 3.556) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad0)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J28-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J30-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J29-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J31-Pad1)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J1-Pad3V2)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad1)"))
  )
  (gr_text "DREW FUSTINI\ndrew@oshpark.com" (at 111.9251 77.4319 90) (layer B.SilkS))
  (gr_text "drew@oshpark.com\n" (at 111.6711 57.0738) (layer F.Mask))
  (gr_text "drew@oshpark.com\n" (at 111.6711 57.0738) (layer F.Cu))
  (gr_text "DREW FUSTINI\n" (at 111.0234 102.3112) (layer F.Cu))
  (gr_text "DREW FUSTINI\n" (at 111.0234 102.3112) (layer F.Mask))
  (gr_line (start 92.329 57.7088) (end 92.3036 57.7088) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.234 55.8038) (end 92.329 57.7088) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.1738 55.8038) (end 94.234 55.8038) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.4636 55.8038) (end 95.1738 55.8038) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.622 58.6232) (end 150.622 58.8264) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.828 55.8292) (end 150.622 58.6232) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.8628 55.8292) (end 147.828 55.8292) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.304 55.8292) (end 146.8628 55.8292) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.3112 55.8292) (end 146.304 55.8292) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.3544 96.9264) (end 92.3544 57.6072) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.076 104.648) (end 92.3544 96.9264) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.6624 104.648) (end 100.076 104.648) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.622 97.6884) (end 143.6624 104.648) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.622 58.8772) (end 150.622 97.6884) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(D1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.599 94.488) (xy 93.4974 57.5056) (xy 102.7176 56.2102) (xy 106.2736 56.388) (xy 142.7734 56.4388)
        (xy 146.0246 56.3372) (xy 147.701 57.0992) (xy 149.3774 58.9534) (xy 149.8092 94.1832) (xy 149.098 97.536)
        (xy 145.9738 100.8126) (xy 142.5194 103.6574) (xy 125.2474 103.8352) (xy 100.7364 103.8352) (xy 93.6752 96.7232)
        (xy 93.599 94.488)
      )
    )
  )
)
