(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 40)
    (tracks 206)
    (zones 0)
    (modules 52)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.35)
    (user_trace_width 0.609)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 139.04 131.02)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(R9-Pad2)")
  (net 5 "Net-(J7-Pad2)")
  (net 6 "Net-(J8-Pad1)")
  (net 7 "Net-(C10-Pad1)")
  (net 8 "Net-(C18-Pad1)")
  (net 9 "Net-(C1-Pad2)")
  (net 10 "Net-(C2-Pad1)")
  (net 11 "Net-(C2-Pad2)")
  (net 12 "Net-(C10-Pad2)")
  (net 13 "Net-(C17-Pad1)")
  (net 14 "Net-(R10-Pad2)")
  (net 15 "Net-(R13-Pad1)")
  (net 16 "Net-(C32-Pad1)")
  (net 17 "Net-(C31-Pad2)")
  (net 18 "Net-(C32-Pad2)")
  (net 19 "Net-(C31-Pad1)")
  (net 20 "Net-(J6-Pad1)")
  (net 21 "Net-(J6-Pad3)")
  (net 22 "Net-(R3-Pad1)")
  (net 23 "Net-(R4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class SMD ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class grounds ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
  )
  (net_class power ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.762)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (net_class signal ""
    (clearance 0.2)
    (trace_width 0.6096)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C31-Pad2)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(C32-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R9-Pad2)")
  )
  (net_class soic ""
    (clearance 0.1524)
    (trace_width 0.4)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
  )
  (module SMC_generic:mkds_1,5-3 (layer F.Cu) (tedit 5FB7ECF6)
    (at 122.04 126.02)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J5 (at 0 -5.4) (layer F.Fab))
    (fp_text value Power (at -0.05 3.55) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND) (thermal_width 1))
    (pad 1 thru_hole circle (at -5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 3 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/pxc_1935174_03_PT-1-5-3-5-0-H_3D.stp
      (offset (xyz -30.09899954795837 -44.70399932861328 -38.86199941635132))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (module SMC_generic:LMH6321D (layer F.Cu) (tedit 5FB7E4BD)
    (at 97.44 107.62 180)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-7-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-7 TO-263-7 SOT-427")
    (attr smd)
    (fp_text reference U2 (at 3.2 6.8) (layer F.SilkS))
    (fp_text value LMH6321 (at -1.9 0 90) (layer F.SilkS))
    (fp_text user 1 (at -3 -3.8 90 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 thru_hole circle (at 5.4 -4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 -4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 -4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 -1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 -3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 -4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 -1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 -1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 -1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 -1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 -1.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 -3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 -3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 -3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 -3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 -3 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 -4.55 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 -4.5 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad "" smd rect (at 0.95 2.775 180) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775 180) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775 180) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 2.775 180) (size 4.55 5.25) (layers F.Paste))
    (pad 4 smd rect (at 3.375 0 180) (size 9.4 10.8) (layers F.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 7 smd rect (at -5.775 3.81 180) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R10-Pad2)"))
    (pad 6 smd rect (at -5.775 2.54 180) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R13-Pad1)"))
    (pad 5 smd rect (at -5.775 1.27 180) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 4 smd rect (at -5.775 0 180) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 3 smd rect (at -5.775 -1.27 180) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J6-Pad1)"))
    (pad 2 smd rect (at -5.775 -2.54 180) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -5.775 -3.81 180) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C32-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-7_TabPin4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:LMH6321D (layer F.Cu) (tedit 5FB7E4BD)
    (at 180.665 107.52)
    (descr "TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-7-1/")
    (tags "D2PAK DDPAK TO-263 D2PAK-7 TO-263-7 SOT-427")
    (attr smd)
    (fp_text reference U3 (at 2.775 -6.7) (layer F.SilkS))
    (fp_text value LMH6321 (at -1.925 0 270 unlocked) (layer F.SilkS))
    (fp_text user 1 (at -3 -3.8 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at -1.55 -0.05 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 5.4 -4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 -4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 -4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 3) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 -3) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 -4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 3) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 3) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 3) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 3) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 3) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 -1.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 5.4 -3) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 3.9 -3) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 2.4 -3) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 0.9 -3) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 -3) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at 6.9 -4.55) (size 0.6 0.6) (drill 0.3) (layers *.Cu F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 4 thru_hole circle (at -0.6 -4.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad "" smd rect (at 0.95 2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 -2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 0.95 -2.775) (size 4.55 5.25) (layers F.Paste))
    (pad "" smd rect (at 5.8 2.775) (size 4.55 5.25) (layers F.Paste))
    (pad 4 smd rect (at 3.375 0) (size 9.4 10.8) (layers F.Cu)
      (net 12 "Net-(C10-Pad2)"))
    (pad 7 smd rect (at -5.775 3.81) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R9-Pad2)"))
    (pad 6 smd rect (at -5.775 2.54) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R13-Pad1)"))
    (pad 5 smd rect (at -5.775 1.27) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 4 smd rect (at -5.775 0) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 3 smd rect (at -5.775 -1.27) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J6-Pad3)"))
    (pad 2 smd rect (at -5.775 -2.54) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -5.775 -3.81) (size 4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C31-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-263-7_TabPin4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_Capacitors:CP_5x11mm_WP (layer F.Cu) (tedit 5FB7DEF7)
    (at 146.04 118.12 180)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C20 (at -3.5 0 90) (layer F.SilkS))
    (fp_text value 10u (at -1.8 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 1 180) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 "Net-(C18-Pad1)"))
    (model ${SMC_3D}/Capacitor_THT.3dshapes/cp_5x11mm_WP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_Capacitors:CP_5x11mm_WP (layer F.Cu) (tedit 5FB7DEF7)
    (at 132.04 118.12)
    (descr "Capacitor, pol, cyl 5x11mm")
    (fp_text reference C19 (at -3.4 0 270) (layer F.SilkS))
    (fp_text value 10u (at -1.8 0 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "Net-(C17-Pad1)"))
    (pad 1 thru_hole rect (at 0 1) (size 1.5 1.5) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${SMC_3D}/Capacitor_THT.3dshapes/cp_5x11mm_WP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5FB7DE41)
    (at 175.74 96.92 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C13 (at -3.2 0 180) (layer F.SilkS))
    (fp_text value 100u (at 1.1 -2 270) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5FB7DE41)
    (at 102.34 99.52 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C14 (at 5.6 0.1 180) (layer F.SilkS))
    (fp_text value 100u (at 1.1 -2 90) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5FB7DE41)
    (at 175.74 116.82 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C15 (at 5.5 -0.1 180) (layer F.SilkS))
    (fp_text value 100u (at 1.1 -2 270) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5FB7DE41)
    (at 102.34 118.27 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C16 (at -3.1 0.1 180) (layer F.SilkS))
    (fp_text value 100u (at 1.2 -2 90) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:Molex_KK_1x03_P3.96mm_Plain (layer F.Cu) (tedit 5F7C9437)
    (at 150.08 126.02)
    (descr "JST VH series connector, B3P-VH (http://www.jst-mfg.com/product/pdf/eng/eVH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST VH side entry")
    (fp_text reference J6 (at 3.96 -4.9) (layer F.SilkS) hide)
    (fp_text value Output (at 3.9 5.1) (layer F.Fab))
    (fp_text user %R (at 4.5 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad1)"))
    (pad 2 thru_hole circle (at 3.96 0) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 7.92 0) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_VH_B3P-VH_1x03_P3.96mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 136.94 117.32 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 5.2 2.1 90) (layer F.SilkS))
    (fp_text value 10 (at 5.6 0 270) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 148.04 113.22)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.2 2.3) (layer F.SilkS))
    (fp_text value 510 (at 5.25 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 146.04 108.12 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C18 (at 6.9 0) (layer F.SilkS))
    (fp_text value 100n (at 2 0 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C18-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 134.74 100.42 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 4.8 -2.3 90) (layer F.SilkS))
    (fp_text value 220k (at 4.9 -0.1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 132.04 108.12 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C17 (at 6.9 0) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5F94A867)
    (at 93.04 127.02 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2.5))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5F94A879)
    (at 185.04 127.02 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2.5))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5F94A83C)
    (at 93.04 88.02 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2.5))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5F94A88A)
    (at 185.04 88.02 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2.5))
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 141.14 127.52 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 5.1 2.2 90) (layer F.SilkS))
    (fp_text value 10 (at 5.3 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C18-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 114.14 110.32 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 8.2 2.2 270) (layer F.SilkS))
    (fp_text value 18k (at 5.15 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R10-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 117.44 108.62)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 5.1 2.2) (layer F.SilkS))
    (fp_text value 510 (at 5.2 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 108.84 101.52 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C8 (at 7.02 0.11 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 -0.05 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5F6DFAAC)
    (at 108.84 113.82 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C12 (at 7.18 -0.02 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0.05 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)") (zone_connect 0))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm placed (layer F.Cu) (tedit 5D56008B)
    (at 118.04 87.02)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J2 (at 0 -2.148) (layer F.Fab))
    (fp_text value Top (at 0 2.4 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm placed (layer F.Cu) (tedit 5D56008B)
    (at 123.04 87.02 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J3 (at 0 -2.148) (layer F.Fab))
    (fp_text value IN (at 0 2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C2-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 128.04 87.02 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J4 (at 0 -2.148) (layer F.Fab))
    (fp_text value Bottom (at 0 -2.4) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 129.24 113.22 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5 -2.3 180) (layer F.SilkS))
    (fp_text value 510 (at 4.7 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_Capacitors:C_Rect_L13mm_W6.5mm_P10mm_Panasonic (layer F.Cu) (tedit 5F6A0B8D)
    (at 118.44 94.77)
    (descr "C, Rect series, Radial, pin pitch=7.50mm 10.00mm, , length*width=13*6.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 7.50mm 10.00mm  length 13mm width 6.5mm Capacitor")
    (fp_text reference C2 (at -2.7 -0.05 90) (layer F.SilkS))
    (fp_text value 470n (at 5.3 -0.2 -180) (layer F.SilkS))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 10 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C2-Pad2)"))
    (model ${SMC_3D}/Capacitor_THT.3dshapes/C_Rect_L13mm_W6.5mm_P10mm_Panasonic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 169.24 113.82 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C11 (at 7.16 0 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 -0.05 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_Capacitors:C_Rect_L13mm_W6.5mm_P10mm_Panasonic (layer F.Cu) (tedit 5F6A0B8D)
    (at 159.64 94.77 180)
    (descr "C, Rect series, Radial, pin pitch=7.50mm 10.00mm, , length*width=13*6.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 7.50mm 10.00mm  length 13mm width 6.5mm Capacitor")
    (fp_text reference C1 (at -2.8 0 90) (layer F.SilkS))
    (fp_text value 470n (at 5 -0.01 180) (layer F.SilkS))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad2)"))
    (model ${SMC_3D}/Capacitor_THT.3dshapes/C_Rect_L13mm_W6.5mm_P10mm_Panasonic.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5F6DFC43)
    (at 169.24 101.52 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C7 (at 7.35 -0.38 180) (layer F.SilkS))
    (fp_text value 100n (at 2.5 0.05 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)") (zone_connect 0))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 163.94 104.52 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 7.5 2.2 90) (layer F.SilkS))
    (fp_text value 18k (at 5 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 160.64 108.62 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5.3 -2.2) (layer F.SilkS))
    (fp_text value 510 (at 5.1 -0.05) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 143.44 100.52 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.2 2.3 90) (layer F.SilkS))
    (fp_text value 220k (at 5.25 0 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 160.04 87.02)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J9 (at 0 -2.148) (layer F.Fab))
    (fp_text value Top (at 0 2.4) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(J8-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 155.04 87.02 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J10 (at 0 -2.148) (layer F.Fab))
    (fp_text value IN (at 0 2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 150.04 87.02)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J11 (at 0 -2.148) (layer F.Fab))
    (fp_text value Bottom (at 0 2.4) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:SO-LOMC (layer F.Cu) (tedit 5E18F70F)
    (at 139.04 105.52)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0 3.4) (layer F.SilkS))
    (fp_text value OPA1656 (at 0 0.2 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (fp_text user 1 (at -4.25 -1.9 unlocked) (layer F.SilkS))
    (pad 1 smd roundrect (at -2.725 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C32-Pad1)"))
    (pad 2 smd roundrect (at -2.725 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(R4-Pad1)"))
    (pad 3 smd roundrect (at -2.725 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C2-Pad2)"))
    (pad 4 smd roundrect (at -2.725 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C17-Pad1)"))
    (pad 5 smd roundrect (at 2.725 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C1-Pad2)"))
    (pad 6 smd roundrect (at 2.725 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(R3-Pad1)"))
    (pad 7 smd roundrect (at 2.725 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(C31-Pad1)"))
    (pad 8 smd roundrect (at 2.725 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C18-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 112.04 87.02 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J1 (at 0 -2.148) (layer F.Fab))
    (fp_text value Volume (at 0 -2.25 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 166.04 87.02 180)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J8 (at 0 -2.148) (layer F.Fab))
    (fp_text value Volume (at 0 -2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(J8-Pad1)"))
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 117.44 104.92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5 -2.05) (layer F.SilkS))
    (fp_text value 10k (at 5.1 0) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C32-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C32-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 160.64 104.92 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.2 2.1) (layer F.SilkS))
    (fp_text value 10k (at 5.1 -0.1) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C31-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C31-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 137.74 87.12 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.Fab))
    (fp_text value LED (at 2.1 1.3 180) (layer F.SilkS))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J7-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:R_Axial__L6.3mm_D2.5mm_P10.16mm_custom (layer F.Cu) (tedit 5D5348AB)
    (at 139.14 100.42 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 4.9 -2 270) (layer F.SilkS))
    (fp_text value 10k (at 5.224999 0.074999 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R13-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 108.84 105.12 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C10 (at 5.9 -3.4 90) (layer F.SilkS))
    (fp_text value 100n (at 2.45 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 141.54 112.82 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C21 (at 2.5 -3.4) (layer F.SilkS))
    (fp_text value 100n (at 2.324999 0.024999 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C17-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C18-Pad1)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima (layer F.Cu) (tedit 5D53486E)
    (at 169.24 110.12 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (fp_text reference C9 (at 5.3 -3.3 90) (layer F.SilkS))
    (fp_text value 100n (at 2.55 0.1) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (model ${KIPRJMOD}/Lib/3D/C_Rect_L7.2mm_W5.0mm_P5.00mm_Wima.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 125.34 100.22 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C32 (at 2.55 -0.05) (layer F.SilkS))
    (fp_text value 1n (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C32-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C32-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 152.54 100.42)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C31 (at 2.5 0) (layer F.SilkS))
    (fp_text value 1n (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(C31-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C31-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 107.04 87.02)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J12 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module SMC_generic:IO_Pad_D2.5mm_Drill1.2mm (layer F.Cu) (tedit 5D56008B)
    (at 171.04 87.02)
    (descr "THT pad as test Point, diameter 2.5mm, hole diameter 1.2mm ")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J13 (at 0 -2.148) (layer F.Fab))
    (fp_text value gnd (at 0 2.25) (layer F.SilkS))
    (fp_text user %R (at 0 -2.15) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_text IN (at 166.04 90.72) (layer F.SilkS))
  (gr_text IN (at 112.04 90.72) (layer F.SilkS))
  (gr_text gnd (at 130.24 87.02 90) (layer F.SilkS))
  (gr_text gnd (at 147.84 87.02 270) (layer F.SilkS))
  (gr_text + (at 135.54 87.12) (layer F.SilkS))
  (gr_text - (at 142.44 87.12) (layer F.SilkS))
  (gr_text Right (at 157.94 128.52) (layer B.SilkS))
  (gr_text Left (at 150.14 128.52) (layer B.SilkS))
  (gr_text V+ (at 130.79 126.02) (layer B.SilkS))
  (gr_text V- (at 113.54 126.02) (layer B.SilkS))
  (gr_text gnd (at 154.04 123.52) (layer F.SilkS))
  (gr_text Right (at 157.94 123.52) (layer F.SilkS))
  (gr_text Left (at 150.14 123.52) (layer F.SilkS))
  (gr_text Output (at 154.04 128.62) (layer F.SilkS))
  (gr_text "LMH6321 Heaphone Amp\nv1.1 Oct. 2020" (at 139.04 93.77) (layer B.SilkS))
  (gr_text Wiper (at 155.04 89.42) (layer F.SilkS))
  (gr_text Wiper (at 123.04 89.42) (layer F.SilkS))
  (gr_text Left (at 94.69 97.32) (layer F.SilkS))
  (gr_text Right (at 183.74 97.12) (layer F.SilkS))
  (gr_text V- (at 112.64 126.02) (layer F.SilkS))
  (gr_text V+ (at 131.14 126.02) (layer F.SilkS))
  (gr_line (start 189.04 84.02) (end 189.04 131.02) (layer Edge.Cuts) (width 0.025))
  (gr_line (start 89.04 84.02) (end 189.04 84.02) (layer Edge.Cuts) (width 0.025))
  (gr_line (start 89.04 131.02) (end 89.04 84.02) (layer Edge.Cuts) (width 0.025))
  (gr_line (start 189.04 131.02) (end 89.04 131.02) (layer Edge.Cuts) (width 0.025))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.94 122.82) (xy 110.84 120.92) (xy 100.14 120.92) (xy 100.14 94.27) (xy 104.79 94.27)
        (xy 104.79 84.52) (xy 173.29 84.52) (xy 173.29 94.27) (xy 177.79 94.27) (xy 177.79 121.944986)
        (xy 162.14 121.92) (xy 153.54 130.52) (xy 112.94 130.52)
      )
    )
  )
  (zone (net 12) (net_name "Net-(C10-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.04 84.52) (xy 104.04 93.52) (xy 99.54 93.52) (xy 99.54 121.62) (xy 110.14 121.62)
        (xy 112.24 123.42) (xy 112.24 130.52) (xy 89.54 130.52) (xy 89.54 84.52)
      )
    )
  )
  (zone (net 12) (net_name "Net-(C10-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188.54 84.52) (xy 188.54 130.52) (xy 162.64 130.52) (xy 162.64 122.52) (xy 178.54 122.52)
        (xy 178.54 93.52) (xy 174.04 93.52) (xy 174.04 84.52)
      )
    )
  )
  (zone (net 12) (net_name "Net-(C10-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.54 130.52) (xy 114.54 123.02) (xy 103.54 112.27) (xy 103.54 103.02) (xy 114.54 100.02)
        (xy 114.54 84.52) (xy 89.54 84.52) (xy 89.54 130.52)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.74 98.77) (xy 177.79 117.52) (xy 174.54 117.52) (xy 174.64 98.77)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.29 98.77) (xy 100.29 116.52) (xy 103.29 116.52) (xy 103.24 98.77)
      )
    )
  )
  (zone (net 12) (net_name "Net-(C10-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188.54 84.52) (xy 163.54 84.52) (xy 163.54 101.52) (xy 169.24 101.52) (xy 173.04 102.77)
        (xy 173.04 112.27) (xy 163.54 121.77) (xy 163.54 130.52) (xy 188.54 130.52)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.34 123.62) (xy 128.54 123.72) (xy 122.04 130.52) (xy 160.34 130.52)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.79 84.52) (xy 138.79 114.77) (xy 137.04 117.02) (xy 135.94 118.22) (xy 136.44 118.62)
        (xy 137.29 117.52) (xy 139.29 115.02) (xy 139.29 84.52)
      )
    )
  )
)
