(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 90)
    (zones 0)
    (modules 15)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.635)
    (user_trace_width 0.1778)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.1778)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.8636 0.508)
    (user_via 1.1176 0.762)
    (user_via 1.3716 1.016)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.381 0.381)
    (mod_text_width 0.09525)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.1016)
    (aux_axis_origin 139.065 111.125)
    (visible_elements 7FFDDF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(L1-Pad1)")
  (net 5 "Net-(L1-Pad2)")
  (net 6 "Net-(R3-Pad1)")
  (net 7 "Net-(C2-Pad1)")
  (net 8 "Net-(J4-Pad1)")
  (net 9 "Net-(R2-Pad1)")
  (net 10 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
  )
  (module PJS-icons:metroid (layer B.Cu) (tedit 5A0106A6)
    (at 217.17 102.87 90)
    (fp_text reference icon1 (at 0 -2.54 90) (layer B.Fab) hide)
    (fp_text value Metroid (at 0 2.54 90) (layer B.SilkS) hide)
    (pad "" smd circle (at -0.635 0 90) (size 0.635 0.635) (layers B.Cu B.Paste B.Mask))
    (pad "" smd circle (at 0.635 0 90) (size 0.635 0.635) (layers B.Cu B.Paste B.Mask))
    (pad "" smd circle (at 0 0.635 90) (size 0.635 0.635) (layers B.Cu B.Paste B.Mask))
  )
  (module Degson:DG301-5.002P-12 (layer F.Cu) (tedit 5B763123)
    (at 194.945 111.76 270)
    (tags terminal)
    (fp_text reference J1 (at 4.445 -4.953 270) (layer F.SilkS))
    (fp_text value Vin (at 3.683 4.318 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.5 0 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Degson:DG301-5.002P-12 (layer F.Cu) (tedit 5B76311A)
    (at 215.9 109.26 90)
    (tags terminal)
    (fp_text reference J3 (at 4.739 -4.953 90) (layer F.SilkS))
    (fp_text value Vout (at -5.04 4.826 90) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 2.5 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -2.5 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C3-Pad1)"))
  )
  (module PJS_smt_parts:SMT_passive_1008 (layer F.Cu) (tedit 5B761EF4)
    (at 204.851 114.681 180)
    (fp_text reference L1 (at 0 -1.397 180) (layer F.SilkS))
    (fp_text value 1.5uH (at -0.1 -2 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(L1-Pad2)"))
  )
  (module PJS_smt_parts:TI_VQFN_12 (layer F.Cu) (tedit 5B7621B8)
    (at 205.105 110.871 90)
    (solder_mask_margin 0.0254)
    (zone_connect 2)
    (fp_text reference U1 (at -1.016 -1.651 90) (layer F.SilkS))
    (fp_text value TPS63051 (at 0 -2.25 90) (layer F.Fab))
    (pad 1 smd rect (at -1.15 -0.75 180) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(L1-Pad2)") (zone_connect 2))
    (pad 2 smd rect (at -1.15 -0.25 180) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 3 smd rect (at -1.15 0.25 180) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(L1-Pad1)") (zone_connect 2))
    (pad 4 smd rect (at -1.15 0.75 180) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)") (zone_connect 2))
    (pad 5 smd rect (at -0.25 1.15 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)") (zone_connect 2))
    (pad 6 smd rect (at 0.25 1.15 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R3-Pad1)") (zone_connect 2))
    (pad 7 smd rect (at 1.15 0.75) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad1)") (zone_connect 2))
    (pad 8 smd rect (at 1.15 0.25 180) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J4-Pad1)") (zone_connect 2))
    (pad 9 smd rect (at 1.15 -0.25 180) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 10 smd rect (at 1.15 -0.75 180) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad1)") (zone_connect 2))
    (pad 11 smd rect (at 0.25 -1.15 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad1)") (zone_connect 2))
    (pad 12 smd rect (at -0.25 -1.15 270) (size 0.25 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)") (zone_connect 2))
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 201.93 112.395 270)
    (fp_text reference C1 (at 0 1.016 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 208.28 107.315)
    (fp_text reference C2 (at -1.524 0 90) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.7 0) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 210.185 112.395 270)
    (fp_text reference C3 (at -1.524 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 208.28 112.395 270)
    (fp_text reference C4 (at 0 1.016 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 198.12 102.87 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 -2.159 270) (layer F.SilkS))
    (fp_text value EN (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 205.74 102.87 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.159 270) (layer F.SilkS))
    (fp_text value Pgood (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 200.66 106.68 90)
    (fp_text reference R1 (at 0 1.016 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad1)"))
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 202.692 108.712 180)
    (fp_text reference R2 (at 1.524 0 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 595EA1C0)
    (at 208.28 109.22)
    (fp_text reference R3 (at -1.524 0 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.7 0) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R3-Pad1)"))
  )
  (module digikey-footprints:0603 (layer F.Cu) (tedit 5B762DBF)
    (at 208.28 105.537 180)
    (fp_text reference R4 (at 1.524 0 270) (layer F.SilkS))
    (fp_text value 1M (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J4-Pad1)"))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
  )
  (gr_text Pgood (at 204.4065 105.283) (layer F.SilkS))
  (gr_text EN (at 192.9765 102.87 90) (layer F.SilkS))
  (gr_text "2.5V to 5.5Vin to \n3.3V @ 0.5A out" (at 203.708 114.3) (layer B.SilkS))
  (gr_text "Vin +" (at 194.818 105.664) (layer F.SilkS))
  (gr_text "Vout +" (at 215.265 115.443) (layer F.SilkS))
  (gr_text "TPS63051 breakout\nPJS 16AUG2018\nMIT License " (at 205.105 108.966) (layer B.SilkS))
  (gr_line (start 191.77 116.84) (end 191.77 100.965) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 219.075 116.84) (end 191.77 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 219.075 100.965) (end 219.075 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.77 100.965) (end 219.075 100.965) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.77 100.965) (xy 219.075 100.965) (xy 219.075 116.84) (xy 191.77 116.84)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.77 100.965) (xy 219.075 100.965) (xy 219.075 116.84) (xy 191.77 116.84)
      )
    )
  )
)
