(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 353)
    (no_connects 0)
    (area 35.484999 57.074999 158.825001 162.635001)
    (thickness 1.6)
    (drawings 46)
    (tracks 1397)
    (zones 0)
    (modules 68)
    (nets 137)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.4)
    (via_drill 0.7)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF3F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /D7)
  (net 3 /D6)
  (net 4 /D5)
  (net 5 /D4)
  (net 6 /D3)
  (net 7 /D2)
  (net 8 /D1)
  (net 9 /D0)
  (net 10 "Net-(U1-Pad26)")
  (net 11 "Net-(U1-Pad27)")
  (net 12 "Net-(U1-Pad30)")
  (net 13 "Net-(U1-Pad34)")
  (net 14 VCC)
  (net 15 "Net-(U3-Pad12)")
  (net 16 "Net-(U3-Pad13)")
  (net 17 "Net-(U3-Pad15)")
  (net 18 "Net-(U5-Pad15)")
  (net 19 "Net-(U5-Pad17)")
  (net 20 "Net-(U5-Pad23)")
  (net 21 "Net-(U5-Pad24)")
  (net 22 "Net-(U5-Pad29)")
  (net 23 "Net-(U5-Pad31)")
  (net 24 "Net-(U5-Pad32)")
  (net 25 "Net-(U5-Pad33)")
  (net 26 "Net-(U5-Pad34)")
  (net 27 /A14)
  (net 28 /A13)
  (net 29 /A12)
  (net 30 /A11)
  (net 31 /A10)
  (net 32 /A9)
  (net 33 /A8)
  (net 34 /AS19)
  (net 35 /AS18)
  (net 36 /AS17)
  (net 37 /AS16)
  (net 38 /A15)
  (net 39 /ALE)
  (net 40 /A0)
  (net 41 /A1)
  (net 42 /A2)
  (net 43 /A3)
  (net 44 /A4)
  (net 45 /A5)
  (net 46 /A6)
  (net 47 /A7)
  (net 48 /A19)
  (net 49 /A18)
  (net 50 /A17)
  (net 51 /A16)
  (net 52 "Net-(U7-Pad1)")
  (net 53 //RD)
  (net 54 //WR)
  (net 55 /CLK)
  (net 56 /RESET)
  (net 57 /INTR)
  (net 58 /INTA)
  (net 59 /INT4)
  (net 60 /INT5)
  (net 61 /INT7)
  (net 62 /IO/M)
  (net 63 /PIC_CS)
  (net 64 /UART_CS)
  (net 65 "Net-(U11-Pad9)")
  (net 66 "Net-(U11-Pad10)")
  (net 67 "Net-(U11-Pad11)")
  (net 68 /ROM_CS)
  (net 69 /RAML_CS)
  (net 70 /RAMH_CS)
  (net 71 "Net-(U12-Pad4)")
  (net 72 "Net-(U12-Pad5)")
  (net 73 "Net-(U12-Pad6)")
  (net 74 "Net-(U12-Pad12)")
  (net 75 "Net-(C1-Pad1)")
  (net 76 "Net-(C1-Pad2)")
  (net 77 "Net-(C2-Pad1)")
  (net 78 "Net-(C2-Pad2)")
  (net 79 "Net-(C3-Pad1)")
  (net 80 "Net-(C4-Pad2)")
  (net 81 "Net-(U13-Pad12)")
  (net 82 "Net-(U13-Pad13)")
  (net 83 "Net-(J1-Pad1)")
  (net 84 "Net-(J1-Pad4)")
  (net 85 "Net-(J1-Pad9)")
  (net 86 "Net-(J1-Pad8)")
  (net 87 "Net-(J1-Pad7)")
  (net 88 "Net-(J1-Pad6)")
  (net 89 /RXD)
  (net 90 /TXD)
  (net 91 /UART_RXD)
  (net 92 /UART_TXD)
  (net 93 "Net-(C20-Pad2)")
  (net 94 "Net-(C21-Pad2)")
  (net 95 "Net-(U11-Pad15)")
  (net 96 "Net-(R5-Pad2)")
  (net 97 /PORT_CS)
  (net 98 /IO0)
  (net 99 /IO1)
  (net 100 /IO2)
  (net 101 /IO3)
  (net 102 /9V)
  (net 103 "Net-(IC1-Pad1)")
  (net 104 "Net-(IC1-Pad2)")
  (net 105 "Net-(IC1-Pad4)")
  (net 106 "Net-(IC1-Pad5)")
  (net 107 "Net-(IC1-Pad6)")
  (net 108 "Net-(IC1-Pad7)")
  (net 109 "Net-(IC1-Pad9)")
  (net 110 "Net-(IC1-Pad10)")
  (net 111 "Net-(IC1-Pad13)")
  (net 112 "Net-(IC1-Pad14)")
  (net 113 "Net-(U6-Pad16)")
  (net 114 "Net-(U6-Pad14)")
  (net 115 "Net-(U6-Pad15)")
  (net 116 /CPU_A15)
  (net 117 "Net-(C22-Pad2)")
  (net 118 "Net-(C23-Pad2)")
  (net 119 /IO4)
  (net 120 /IO5)
  (net 121 /IO6)
  (net 122 /IO7)
  (net 123 +3V3)
  (net 124 "Net-(J1-Pad2)")
  (net 125 "Net-(J1-Pad3)")
  (net 126 "Net-(D1-Pad2)")
  (net 127 "Net-(D2-Pad2)")
  (net 128 "Net-(U12-Pad14)")
  (net 129 "Net-(U11-Pad7)")
  (net 130 "Net-(U10-Pad4)")
  (net 131 "Net-(U10-Pad12)")
  (net 132 "Net-(R3-Pad2)")
  (net 133 "Net-(C24-Pad1)")
  (net 134 "Net-(P3-Pad2)")
  (net 135 "Net-(R10-Pad1)")
  (net 136 "Net-(J1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 1.4)
    (via_drill 0.7)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net //RD)
    (add_net //WR)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /ALE)
    (add_net /AS16)
    (add_net /AS17)
    (add_net /AS18)
    (add_net /AS19)
    (add_net /CLK)
    (add_net /CPU_A15)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /INT4)
    (add_net /INT5)
    (add_net /INT7)
    (add_net /INTA)
    (add_net /INTR)
    (add_net /IO/M)
    (add_net /IO0)
    (add_net /IO1)
    (add_net /IO2)
    (add_net /IO3)
    (add_net /IO4)
    (add_net /IO5)
    (add_net /IO6)
    (add_net /IO7)
    (add_net /PIC_CS)
    (add_net /PORT_CS)
    (add_net /RAMH_CS)
    (add_net /RAML_CS)
    (add_net /RESET)
    (add_net /ROM_CS)
    (add_net /RXD)
    (add_net /TXD)
    (add_net /UART_CS)
    (add_net /UART_RXD)
    (add_net /UART_TXD)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U10-Pad12)")
    (add_net "Net-(U10-Pad4)")
    (add_net "Net-(U11-Pad10)")
    (add_net "Net-(U11-Pad11)")
    (add_net "Net-(U11-Pad15)")
    (add_net "Net-(U11-Pad7)")
    (add_net "Net-(U11-Pad9)")
    (add_net "Net-(U12-Pad12)")
    (add_net "Net-(U12-Pad14)")
    (add_net "Net-(U12-Pad4)")
    (add_net "Net-(U12-Pad5)")
    (add_net "Net-(U12-Pad6)")
    (add_net "Net-(U13-Pad12)")
    (add_net "Net-(U13-Pad13)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad17)")
    (add_net "Net-(U5-Pad23)")
    (add_net "Net-(U5-Pad24)")
    (add_net "Net-(U5-Pad29)")
    (add_net "Net-(U5-Pad31)")
    (add_net "Net-(U5-Pad32)")
    (add_net "Net-(U5-Pad33)")
    (add_net "Net-(U5-Pad34)")
    (add_net "Net-(U6-Pad14)")
    (add_net "Net-(U6-Pad15)")
    (add_net "Net-(U6-Pad16)")
    (add_net "Net-(U7-Pad1)")
    (add_net VCC)
  )
  (net_class POWER ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1.4)
    (via_drill 0.7)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /9V)
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5CA8EF58)
    (at 128.27 90.17 180)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U11 (at 2.54 0 360) (layer F.SilkS))
    (fp_text value 74HC138 (at 0 -3.72 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /A5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /A6))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /IO/M))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 "Net-(U11-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(U11-Pad9)"))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(U11-Pad10)"))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(U11-Pad11)"))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /PORT_CS))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 /PIC_CS))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /UART_CS))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(U11-Pad15)"))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5CA8EF5C)
    (at 156.21 90.17 180)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U10 (at 2.54 0 360) (layer F.SilkS))
    (fp_text value 74HCU04 (at 0 -3.72 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(R10-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /RESET))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 "Net-(C24-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 "Net-(U10-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 "Net-(U10-Pad4)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(R10-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(R3-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "Net-(C20-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /CLK))
    (pad 11 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(R3-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "Net-(U10-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /A19))
    (pad 14 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W15.24mm (layer F.Cu) (tedit 5CA8DEDF)
    (at 77.47 77.47)
    (descr "28-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U3 (at 2.54 0) (layer F.SilkS))
    (fp_text value 82C59 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 /PIC_CS))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 //RD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 //WR))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /D7))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D6))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D5))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D4))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D1))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U3-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U3-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U3-Pad15)"))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "Net-(R5-Pad2)"))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /INTR))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /INT4))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /INT5))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /INT7))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /INTA))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A0))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5CA8DDDC)
    (at 140.97 64.77)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R4 (at -3.81 0) (layer F.SilkS))
    (fp_text value 1k (at -1.143 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 94 "Net-(C21-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 132 "Net-(R3-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-40_W15.24mm (layer F.Cu) (tedit 5CA8DE38)
    (at 140.97 110.49)
    (descr "40-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 8088_Min_Mode (at 0 -3.81) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /A14))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /A13))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /A12))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /A11))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /A10))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /A9))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /A8))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /D7))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D6))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D5))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D4))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D1))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /INTR))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /CLK))
    (pad 20 thru_hole oval (at 0 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 15.24 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /RESET))
    (pad 22 thru_hole oval (at 15.24 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 23 thru_hole oval (at 15.24 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole oval (at 15.24 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /INTA))
    (pad 25 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /ALE))
    (pad 26 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad26)"))
    (pad 27 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad27)"))
    (pad 28 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /IO/M))
    (pad 29 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 //WR))
    (pad 30 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad30)"))
    (pad 31 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 32 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 //RD))
    (pad 33 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 34 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad34)"))
    (pad 35 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /AS19))
    (pad 36 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /AS18))
    (pad 37 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /AS17))
    (pad 38 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /AS16))
    (pad 39 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 /CPU_A15))
    (pad 40 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-40_W15.24mm (layer F.Cu) (tedit 5CA8DEF5)
    (at 99.06 62.23)
    (descr "40-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U5 (at 2.54 0) (layer F.SilkS))
    (fp_text value 16C550 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D1))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D4))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D5))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D6))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /D7))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(U5-Pad15)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 /UART_RXD))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 /UART_TXD))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /UART_CS))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(U5-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /CLK))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(U5-Pad17)"))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 //WR))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 0 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 15.24 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 //RD))
    (pad 22 thru_hole oval (at 15.24 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 23 thru_hole oval (at 15.24 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(U5-Pad23)"))
    (pad 24 thru_hole oval (at 15.24 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(U5-Pad24)"))
    (pad 25 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /A2))
    (pad 27 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /A1))
    (pad 28 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A0))
    (pad 29 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U5-Pad29)"))
    (pad 30 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /INT7))
    (pad 31 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(U5-Pad31)"))
    (pad 32 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(U5-Pad32)"))
    (pad 33 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U5-Pad33)"))
    (pad 34 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(U5-Pad34)"))
    (pad 35 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /RESET))
    (pad 36 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 37 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 38 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 39 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5CA8DED9)
    (at 54.61 68.58 90)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U13 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value MAX232 (at 0 -3.72 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(C3-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(C1-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(C2-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(C2-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(C4-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 /TXD))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 /RXD))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 /UART_RXD))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 /UART_TXD))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(U13-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(U13-Pad13)"))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(U13-Pad13)"))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-32_W15.24mm (layer F.Cu) (tedit 5CA8DE6E)
    (at 77.47 120.65)
    (descr "32-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U8 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value AS6C4008 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /A18))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /A16))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /A14))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /A12))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /A7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /A6))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /A5))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /A4))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /A3))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /A2))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /A1))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A0))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D1))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 18 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D4))
    (pad 19 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D5))
    (pad 20 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D6))
    (pad 21 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /D7))
    (pad 22 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 /RAMH_CS))
    (pad 23 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /A10))
    (pad 24 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 //RD))
    (pad 25 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /A11))
    (pad 26 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /A9))
    (pad 27 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /A8))
    (pad 28 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /A13))
    (pad 29 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 //WR))
    (pad 30 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /A17))
    (pad 31 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /A15))
    (pad 32 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-32_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-32_W15.24mm (layer F.Cu) (tedit 5CA8DE66)
    (at 99.06 120.65)
    (descr "32-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U9 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value AS6C4008 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /A18))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /A16))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /A14))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /A12))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /A7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /A6))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /A5))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /A4))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /A3))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /A2))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /A1))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A0))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D1))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 18 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D4))
    (pad 19 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D5))
    (pad 20 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D6))
    (pad 21 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /D7))
    (pad 22 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 /RAML_CS))
    (pad 23 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /A10))
    (pad 24 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 //RD))
    (pad 25 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /A11))
    (pad 26 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /A9))
    (pad 27 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /A8))
    (pad 28 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /A13))
    (pad 29 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 //WR))
    (pad 30 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /A17))
    (pad 31 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /A15))
    (pad 32 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-32_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 58.42 74.93)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -3.8) (layer F.SilkS))
    (fp_text value 2u2 (at 1.25 3.8) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 64.77 74.93)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at 1.25 -3.8) (layer F.SilkS))
    (fp_text value 2u2 (at 1.25 3.8) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 52.07 74.93)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 1.25 -3.8) (layer F.SilkS))
    (fp_text value 2u2 (at 1.25 3.8) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 71.12 74.93)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C4 (at 1.25 -3.8) (layer F.SilkS))
    (fp_text value 2u2 (at 1.25 3.8) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(C4-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8DEFE)
    (at 74.93 116.84)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 5.08 0) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8DF04)
    (at 90.17 116.84)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at -2.54 0) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5C985E45)
    (at 99.06 116.84)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 5.08 0) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5C985E7E)
    (at 156.21 105.41 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5C985E8D)
    (at 118.11 62.23 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C9 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5C9860C5)
    (at 87.63 72.39 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C10 (at 5.715 0 180) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5C985E67)
    (at 66.04 92.71)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C11 (at 5.08 0) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5C985E6E)
    (at 132.08 156.21 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C12 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5C985E85)
    (at 132.08 118.11 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C13 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CAAE844)
    (at 117.475 90.17 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C14 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8DF5B)
    (at 114.3 116.84 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C15 (at 1.27 2.54 90) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8DE5A)
    (at 148.59 95.25)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C16 (at 5.08 0) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8DE86)
    (at 41.91 132.08 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C17 (at 1.27 2.54 90) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA9779A)
    (at 60.96 116.84 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C18 (at 1.27 2.54 90) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5CA8EF4D)
    (at 128.27 156.21 180)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 2.54 0 360) (layer F.SilkS))
    (fp_text value 74HC573 (at 0 -3.72 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D1))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D4))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D5))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D6))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /D7))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /ALE))
    (pad 12 thru_hole oval (at 7.62 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /A7))
    (pad 13 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /A6))
    (pad 14 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /A5))
    (pad 15 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /A4))
    (pad 16 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /A3))
    (pad 17 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /A2))
    (pad 18 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /A1))
    (pad 19 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A0))
    (pad 20 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5CA8EF53)
    (at 128.27 123.19 180)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U6 (at 2.54 0 360) (layer F.SilkS))
    (fp_text value 74HC573 (at 0 -3.72 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /AS16))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /AS17))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /AS18))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 /CPU_A15))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /AS19))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /ALE))
    (pad 12 thru_hole oval (at 7.62 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /A19))
    (pad 13 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /A15))
    (pad 14 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "Net-(U6-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "Net-(U6-Pad15)"))
    (pad 16 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "Net-(U6-Pad16)"))
    (pad 17 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /A18))
    (pad 18 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /A17))
    (pad 19 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /A16))
    (pad 20 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-32_W15.24mm (layer F.Cu) (tedit 5CA8DE72)
    (at 55.88 120.65)
    (descr "32-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U7 (at 2.54 0) (layer F.SilkS))
    (fp_text value 39SF010 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(U7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /A16))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /A15))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /A12))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /A7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /A6))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /A5))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /A4))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /A3))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /A2))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /A1))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /A0))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D1))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 18 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D4))
    (pad 19 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D5))
    (pad 20 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D6))
    (pad 21 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /D7))
    (pad 22 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /ROM_CS))
    (pad 23 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /A10))
    (pad 24 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 //RD))
    (pad 25 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /A11))
    (pad 26 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /A9))
    (pad 27 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /A8))
    (pad 28 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /A13))
    (pad 29 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /A14))
    (pad 30 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 31 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 //WR))
    (pad 32 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-32_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5CA8EF5B)
    (at 142.24 90.17 180)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U12 (at 2.54 0 360) (layer F.SilkS))
    (fp_text value 74HC139 (at 0 -3.72 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "Net-(U10-Pad12)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /A17))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /A18))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(U12-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(U12-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(U12-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 "Net-(U12-Pad14)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 /RAMH_CS))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /ROM_CS))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 /RAML_CS))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(U12-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /A19))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 "Net-(U12-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /IO/M))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8DDE6)
    (at 142.24 59.69 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C20 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 22p (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 93 "Net-(C20-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8DDE4)
    (at 142.24 67.31 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C21 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 47p (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 94 "Net-(C21-Pad2)"))
  )
  (module Discret:R1 (layer F.Cu) (tedit 5CA8DDE1)
    (at 140.97 62.23)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R3 (at -3.81 0) (layer F.SilkS))
    (fp_text value 330k (at -1.143 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 93 "Net-(C20-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 132 "Net-(R3-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 5CA8DDE8)
    (at 132.08 63.5 90)
    (descr "Crystal Quarz HC49/U vertical stehend")
    (tags "Crystal Quarz HC49/U vertical stehend")
    (fp_text reference Y1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 2.4576MHz (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.44094 0 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 94 "Net-(C21-Pad2)"))
    (pad 2 thru_hole circle (at 2.44094 0 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 93 "Net-(C20-Pad2)"))
  )
  (module Discret:R1 (layer F.Cu) (tedit 5CA8DF09)
    (at 96.52 117.475 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R5 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 4k7 (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 96 "Net-(R5-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-20_W7.62mm (layer F.Cu) (tedit 5CA8DE82)
    (at 41.91 135.89)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U14 (at 2.54 0) (layer F.SilkS))
    (fp_text value 74HCT541 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 //RD))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 /IO7))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 /IO6))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 /IO0))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 /IO5))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 /IO1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 /IO4))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 /IO2))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 /IO3))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D4))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D1))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D5))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D6))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /D7))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /PORT_CS))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5CA8DE99)
    (at 41.91 107.95)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U15 (at 2.54 0) (layer F.SilkS))
    (fp_text value 74HC173 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 /IO3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 /IO2))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 /IO1))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 /IO0))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 //WR))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /PORT_CS))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D1))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D2))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D3))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8DEF2)
    (at 93.98 59.69 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C19 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 102 /9V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connect:BARREL_JACK (layer F.Cu) (tedit 5CA8DF37)
    (at 82.55 60.96 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at 2.54 -3.81 450) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -5.99948 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 6.20014 0 270) (size 3.50012 3.50012) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask)
      (net 102 /9V))
    (pad 2 thru_hole rect (at 0.20066 0 270) (size 3.50012 3.50012) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole rect (at 3.2004 4.699 270) (size 3.50012 3.50012) (drill oval 2.99974 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 5CAA4625)
    (at 92.71 67.31 270)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference U16 (at 6.35 -2.54 540) (layer F.SilkS))
    (fp_text value 7805 (at 0 3.81 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 102 /9V))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5CA8DEAA)
    (at 55.88 92.71)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference IC1 (at 2.54 0) (layer F.SilkS))
    (fp_text value 4060N (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 /INT4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "Net-(IC1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "Net-(IC1-Pad9)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(IC1-Pad10)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "Net-(C23-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(IC1-Pad13)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(IC1-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /INT5))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8EA4D)
    (at 66.04 110.49)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C22 (at 5.715 0) (layer F.SilkS))
    (fp_text value 22p (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 117 "Net-(C22-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8EA47)
    (at 66.04 102.87)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C23 (at 5.715 0) (layer F.SilkS))
    (fp_text value 22p (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 118 "Net-(C23-Pad2)"))
  )
  (module Discret:R1 (layer F.Cu) (tedit 5CA8EA4B)
    (at 67.31 107.95 180)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R1 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 330k (at -1.143 2.54 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 117 "Net-(C22-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 110 "Net-(IC1-Pad10)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5CA8EA4A)
    (at 67.31 105.41 180)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R2 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 1M (at -1.143 2.54 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 118 "Net-(C23-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 110 "Net-(IC1-Pad10)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_Round_Vertical_3mm (layer F.Cu) (tedit 5CA8DEC3)
    (at 67.31 99.06 180)
    (descr "Crystal, Quarz, Rundgehaeuse, round, vertical, stehend, Uhrenquarz, Diam. 3mm,")
    (tags "Crystal Quarz Rundgehaeuse round vertical stehend Uhrenquarz Diam. 3mm")
    (fp_text reference Y2 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value 32.768kHz (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.7493 0 180) (size 1.00076 1.00076) (drill 0.59944) (layers *.Cu *.Mask)
      (net 117 "Net-(C22-Pad2)"))
    (pad 2 thru_hole circle (at 0.7493 0 180) (size 1.00076 1.00076) (drill 0.59944) (layers *.Cu *.Mask)
      (net 118 "Net-(C23-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Array_SIP5 (layer F.Cu) (tedit 5CA8DE8F)
    (at 38.1 113.03 270)
    (descr "5-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 13.97 0 270) (layer F.SilkS))
    (fp_text value 47k (at 6.35 2.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 /IO4))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 /IO5))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 /IO6))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 /IO7))
    (model Resistors_ThroughHole.3dshapes/Resistor_Array_SIP5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12 (layer F.Cu) (tedit 5CA8DE7B)
    (at 38.1 158.75 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value CONN_01X12 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 101 /IO3))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 100 /IO2))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 119 /IO4))
    (pad 5 thru_hole oval (at 10.16 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 99 /IO1))
    (pad 6 thru_hole oval (at 12.7 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 120 /IO5))
    (pad 7 thru_hole oval (at 15.24 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 98 /IO0))
    (pad 8 thru_hole oval (at 17.78 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 121 /IO6))
    (pad 9 thru_hole oval (at 20.32 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 122 /IO7))
    (pad 10 thru_hole oval (at 22.86 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 11 thru_hole oval (at 25.4 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 123 +3V3))
    (pad 12 thru_hole oval (at 27.94 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0.55 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5CAAEBB3)
    (at 41.91 95.25 180)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D1 (at 4.445 -3.175 180) (layer F.SilkS))
    (fp_text value LED (at 1.524 -3.937 180) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 126 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5CAAEBA4)
    (at 39.37 101.6 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R6 (at 0 2.54 270) (layer F.SilkS))
    (fp_text value R (at -1.143 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 126 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 101 /IO3))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5CAA40C7)
    (at 49.53 95.25 180)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D2 (at -1.27 -3.81 180) (layer F.SilkS))
    (fp_text value LED (at 1.524 -3.937 180) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask)
      (net 127 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5CAA3FD4)
    (at 46.99 101.6 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R7 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value R (at -1.143 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 127 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 VCC))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CA8DDAF)
    (at 153.67 66.04)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C24 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 133 "Net-(C24-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Discret:D3 (layer F.Cu) (tedit 0)
    (at 125.73 63.5 90)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D3 (at 0 0 90) (layer F.SilkS))
    (fp_text value D (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 133 "Net-(C24-Pad1)"))
    (model Discret.3dshapes/D3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 5CA8EAC6)
    (at 156.21 59.69 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 3.175 -2.54 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.54 -2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 134 "Net-(P3-Pad2)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5CA8EC9C)
    (at 149.86 64.77 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R8 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value 100 (at -1.143 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 133 "Net-(C24-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 134 "Net-(P3-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5CA8DDEC)
    (at 121.92 63.5 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R9 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 10k (at -1.143 2.54 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 133 "Net-(C24-Pad1)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 5CA8DDB3)
    (at 154.94 69.85 180)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R10 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 100k (at -1.143 2.54 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 135 "Net-(R10-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 133 "Net-(C24-Pad1)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CAAE3C6)
    (at 143.51 95.25)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C25 (at -2.54 0) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module db9:DB_9M (layer F.Cu) (tedit 5CAA3A2D)
    (at 39.37 73.406 270)
    (descr "D-SUB 9 pin plug, Tyco P/N 4-338168-2")
    (fp_text reference J1 (at 0 -2.286 450) (layer F.SilkS))
    (fp_text value DB9 (at -0.254 9.652 270) (layer F.SilkS))
    (pad "" thru_hole circle (at 12.49426 -7.112 270) (size 5.00126 5.00126) (drill 3.2004) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -8.382 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 -0.24892)) (layers *.Cu *.Mask)
      (net 125 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.77114 -8.382 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 -0.24892)) (layers *.Cu *.Mask)
      (net 84 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 5.53974 -8.382 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 -0.24892)) (layers *.Cu *.Mask)
      (net 136 "Net-(J1-Pad5)"))
    (pad 2 thru_hole oval (at -2.77114 -8.382 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 -0.24892)) (layers *.Cu *.Mask)
      (net 124 "Net-(J1-Pad2)"))
    (pad 1 thru_hole oval (at -5.53974 -8.382 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 -0.24892)) (layers *.Cu *.Mask)
      (net 83 "Net-(J1-Pad1)"))
    (pad 6 thru_hole oval (at -4.15544 -5.842 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 0.24892)) (layers *.Cu *.Mask)
      (net 88 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at -1.3843 -5.842 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 0.24892)) (layers *.Cu *.Mask)
      (net 87 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 1.3843 -5.842 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 0.24892)) (layers *.Cu *.Mask)
      (net 86 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 4.15544 -5.842 270) (size 1.50114 1.99898) (drill 0.89916 (offset 0 0.24892)) (layers *.Cu *.Mask)
      (net 85 "Net-(J1-Pad9)"))
    (pad "" thru_hole circle (at -12.49426 -7.112 270) (size 5.00126 5.00126) (drill 3.2004) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/pcb libs/packages3d/conn_d-sub/db_9m.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03 (layer F.Cu) (tedit 5CAAEC41)
    (at 60.96 80.645)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at -9.525 0) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 84 "Net-(J1-Pad4)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 90 /TXD))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 125 "Net-(J1-Pad3)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03 (layer F.Cu) (tedit 5CAAEC43)
    (at 60.96 83.82)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at -9.525 0) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 125 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 89 /RXD))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 124 "Net-(J1-Pad2)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03 (layer F.Cu) (tedit 5CAAEC45)
    (at 60.96 86.995)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P5 (at -9.525 0) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 136 "Net-(J1-Pad5)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 54F24281)
    (at 38.1 108.585 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U4 (at 0 -4 90) (layer F.SilkS))
    (fp_text value REG33 (at 0 3 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 1 thru_hole oval (at 0 0 270) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask)
      (net 123 +3V3))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 0)
    (at 134.62 100.33 180)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C26 (at 1.25 -2.5 180) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CAAE8C2)
    (at 117.475 92.71 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C27 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value C (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 5CAAEBBA)
    (at 43.18 102.87 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C28 (at 4.445 1.27 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 123 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_text "COM\n(M)" (at 70.485 83.82 90) (layer F.SilkS))
  (gr_text "modem\n(F)" (at 56.515 83.82 270) (layer F.SilkS))
  (gr_text "DC\nin" (at 78.105 71.12) (layer F.SilkS))
  (gr_text 32.768k (at 68.58 96.52) (layer F.SilkS))
  (gr_text 7805 (at 89.535 67.31 270) (layer F.SilkS))
  (gr_text gnd (at 45.72 130.81) (layer B.SilkS))
  (gr_text +3.3v (at 46.355 133.35) (layer B.SilkS))
  (gr_text +5v (at 45.72 135.89) (layer B.SilkS))
  (gr_text iP7 (at 45.72 138.43) (layer B.SilkS))
  (gr_text iP6 (at 45.72 140.97) (layer B.SilkS))
  (gr_text oP0 (at 45.72 143.51) (layer B.SilkS))
  (gr_text iP5 (at 45.72 146.05) (layer B.SilkS))
  (gr_text oP1 (at 45.72 148.59) (layer B.SilkS))
  (gr_text iP4 (at 45.72 151.13) (layer B.SilkS))
  (gr_text oP2 (at 45.72 153.67) (layer B.SilkS))
  (gr_text oP3 (at 45.72 156.21) (layer B.SilkS))
  (gr_text gnd (at 45.72 158.75) (layer B.SilkS))
  (gr_text oP3 (at 40.64 90.805) (layer F.SilkS))
  (gr_text power (at 48.26 90.805) (layer F.SilkS))
  (gr_text reset (at 147.955 59.69) (layer F.SilkS))
  (gr_text "Rev. 1.0" (at 142.24 104.775) (layer F.SilkS))
  (gr_line (start 158.75 57.15) (end 35.56 57.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.75 162.56) (end 158.75 57.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 35.56 162.56) (end 35.56 57.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 4060 (at 59.69 101.6 270) (layer F.SilkS))
  (gr_text 9-12V (at 86.36 64.77 90) (layer B.SilkS))
  (gr_text "x86 light" (at 106.045 107.95 90) (layer B.SilkS))
  (gr_text MAX232 (at 63.5 64.77) (layer F.SilkS))
  (gr_text 74HCT541 (at 45.72 147.32 270) (layer F.SilkS))
  (gr_text 74HC173 (at 45.72 116.84 270) (layer F.SilkS))
  (gr_text 74HCU04 (at 152.4 82.55 90) (layer F.SilkS))
  (gr_text 74HC139 (at 138.43 81.28 90) (layer F.SilkS))
  (gr_text 74HC138 (at 124.46 81.28 90) (layer F.SilkS))
  (gr_text 74HC573 (at 124.46 111.76 90) (layer F.SilkS))
  (gr_text 74HC573 (at 124.46 144.78 90) (layer F.SilkS))
  (gr_text "80C88 / NEC V20\nCPU" (at 148.59 134.62 270) (layer F.SilkS))
  (gr_text "16C550\nUART" (at 106.68 86.36 270) (layer F.SilkS))
  (gr_text "82C59\nPIC" (at 85.09 93.98 270) (layer F.SilkS))
  (gr_text "29F010\nFlash ROM" (at 63.5 139.7 270) (layer F.SilkS))
  (gr_text "AS6C4008\nSRAM low" (at 85.09 139.7 270) (layer F.SilkS))
  (gr_text "AS6C4008\nSRAM high" (at 106.68 139.7 270) (layer F.SilkS))
  (gr_text "x86 light" (at 146.05 100.33) (layer F.SilkS))
  (gr_line (start 158.75 162.56) (end 35.56 162.56) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 14) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.29 163.83) (xy 160.02 163.83) (xy 160.02 53.34) (xy 34.29 53.34)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 163.83) (xy 34.29 163.83) (xy 34.29 53.34) (xy 160.02 53.34)
      )
    )
  )
)
