(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 111)
    (tracks 2066)
    (zones 0)
    (modules 138)
    (nets 140)
  )
  (page A4)
  (title_block
    (date "mar. 31 mars 2015")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power hide)
    (2 In2.Cu power hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.15)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.1)
    (mod_text_size 0.75 0.75)
    (mod_text_width 0.1)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 103.378 121.666)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 /IOREF)
  (net 4 /Reset)
  (net 5 /Vin)
  (net 6 /A12)
  (net 7 /A13)
  (net 8 /A14)
  (net 9 /A15)
  (net 10 /SCL)
  (net 11 /SDA)
  (net 12 "/7(**)")
  (net 13 "/4(**)")
  (net 14 "/3(**)")
  (net 15 "/2(**)")
  (net 16 "Net-(P8-Pad1)")
  (net 17 "Net-(P10-Pad1)")
  (net 18 "Net-(P11-Pad1)")
  (net 19 "Net-(P12-Pad1)")
  (net 20 "Net-(P2-Pad1)")
  (net 21 +3V3)
  (net 22 "/1(Tx0)")
  (net 23 "/0(Rx0)")
  (net 24 +12V)
  (net 25 "Net-(D1-Pad2)")
  (net 26 /TEMP_1)
  (net 27 /TEMP_2)
  (net 28 /TEMP_3)
  (net 29 /TEMP_4)
  (net 30 /TEMP_5)
  (net 31 /TEMP_6)
  (net 32 /ENC_1)
  (net 33 /ENC_2)
  (net 34 /ENC_3)
  (net 35 /ENC_4)
  (net 36 /ENC_5)
  (net 37 /ENC_6)
  (net 38 /ENC_7)
  (net 39 /ENC_8)
  (net 40 /ENC_9)
  (net 41 /ENC_10)
  (net 42 /ENC_11)
  (net 43 /ENC_12)
  (net 44 /ENC_13)
  (net 45 /ENC_14)
  (net 46 /ENC_15)
  (net 47 /ENC_16)
  (net 48 /ENC_17)
  (net 49 /ENC_18)
  (net 50 /MB9)
  (net 51 /MA9)
  (net 52 /MB8)
  (net 53 /MA8)
  (net 54 /MB7)
  (net 55 /MA7)
  (net 56 /MB6)
  (net 57 /MA6)
  (net 58 /MB5)
  (net 59 /MA5)
  (net 60 /MB4)
  (net 61 /MA4)
  (net 62 /MB3)
  (net 63 /MA3)
  (net 64 /MB2)
  (net 65 /MA2)
  (net 66 /MB1)
  (net 67 /MA1)
  (net 68 /MA10)
  (net 69 /MB10)
  (net 70 /MA11)
  (net 71 /MB11)
  (net 72 /MA12)
  (net 73 /MB12)
  (net 74 /MA13)
  (net 75 /MB13)
  (net 76 /MA14)
  (net 77 /MB14)
  (net 78 /MA15)
  (net 79 /MB15)
  (net 80 /MA16)
  (net 81 /MB16)
  (net 82 /MA17)
  (net 83 /MB17)
  (net 84 /MA18)
  (net 85 /MB18)
  (net 86 /M17)
  (net 87 /M18)
  (net 88 /M15)
  (net 89 /M16)
  (net 90 /M13)
  (net 91 /M14)
  (net 92 /M11)
  (net 93 /M12)
  (net 94 /M9)
  (net 95 /M10)
  (net 96 /M7)
  (net 97 /M8)
  (net 98 /M5)
  (net 99 /M6)
  (net 100 /M3)
  (net 101 /M4)
  (net 102 /M1)
  (net 103 /M2)
  (net 104 /TEMP_D1)
  (net 105 /TEMP_D2)
  (net 106 /TEMP_D3)
  (net 107 /TEMP_D4)
  (net 108 /TEMP_D5)
  (net 109 /TEMP_D6)
  (net 110 /DIR)
  (net 111 /PWM)
  (net 112 /SOL_V)
  (net 113 /FAULT)
  (net 114 "Net-(Q1-Pad1)")
  (net 115 "Net-(R29-Pad1)")
  (net 116 "Net-(R30-Pad1)")
  (net 117 "Net-(R31-Pad1)")
  (net 118 "Net-(R32-Pad1)")
  (net 119 "Net-(R41-Pad1)")
  (net 120 "Net-(R42-Pad1)")
  (net 121 "Net-(R43-Pad1)")
  (net 122 "Net-(R44-Pad1)")
  (net 123 "Net-(R53-Pad1)")
  (net 124 "Net-(R54-Pad1)")
  (net 125 "Net-(R55-Pad1)")
  (net 126 "Net-(R56-Pad1)")
  (net 127 "Net-(R63-Pad1)")
  (net 128 "Net-(R64-Pad1)")
  (net 129 "Net-(R65-Pad1)")
  (net 130 "Net-(R72-Pad1)")
  (net 131 "Net-(R73-Pad1)")
  (net 132 "Net-(R74-Pad1)")
  (net 133 "Net-(J9-Pad8)")
  (net 134 "Net-(J12-Pad8)")
  (net 135 "Net-(J15-Pad16)")
  (net 136 "Net-(P1-Pad8)")
  (net 137 "Net-(P1-Pad10)")
  (net 138 "Net-(J15-Pad2)")
  (net 139 +5VA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net +5VA)
    (add_net "/0(Rx0)")
    (add_net "/1(Tx0)")
    (add_net "/2(**)")
    (add_net "/3(**)")
    (add_net "/4(**)")
    (add_net "/7(**)")
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /ENC_1)
    (add_net /ENC_10)
    (add_net /ENC_11)
    (add_net /ENC_12)
    (add_net /ENC_13)
    (add_net /ENC_14)
    (add_net /ENC_15)
    (add_net /ENC_16)
    (add_net /ENC_17)
    (add_net /ENC_18)
    (add_net /ENC_2)
    (add_net /ENC_3)
    (add_net /ENC_4)
    (add_net /ENC_5)
    (add_net /ENC_6)
    (add_net /ENC_7)
    (add_net /ENC_8)
    (add_net /ENC_9)
    (add_net /IOREF)
    (add_net /M1)
    (add_net /M10)
    (add_net /M11)
    (add_net /M12)
    (add_net /M13)
    (add_net /M14)
    (add_net /M15)
    (add_net /M16)
    (add_net /M17)
    (add_net /M18)
    (add_net /M2)
    (add_net /M3)
    (add_net /M4)
    (add_net /M5)
    (add_net /M6)
    (add_net /M7)
    (add_net /M8)
    (add_net /M9)
    (add_net /MA1)
    (add_net /MA10)
    (add_net /MA11)
    (add_net /MA12)
    (add_net /MA13)
    (add_net /MA14)
    (add_net /MA15)
    (add_net /MA16)
    (add_net /MA17)
    (add_net /MA18)
    (add_net /MA2)
    (add_net /MA3)
    (add_net /MA4)
    (add_net /MA5)
    (add_net /MA6)
    (add_net /MA7)
    (add_net /MA8)
    (add_net /MA9)
    (add_net /MB1)
    (add_net /MB10)
    (add_net /MB11)
    (add_net /MB12)
    (add_net /MB13)
    (add_net /MB14)
    (add_net /MB15)
    (add_net /MB16)
    (add_net /MB17)
    (add_net /MB18)
    (add_net /MB2)
    (add_net /MB3)
    (add_net /MB4)
    (add_net /MB5)
    (add_net /MB6)
    (add_net /MB7)
    (add_net /MB8)
    (add_net /MB9)
    (add_net /Reset)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SOL_V)
    (add_net /TEMP_1)
    (add_net /TEMP_2)
    (add_net /TEMP_3)
    (add_net /TEMP_4)
    (add_net /TEMP_5)
    (add_net /TEMP_6)
    (add_net /TEMP_D1)
    (add_net /TEMP_D2)
    (add_net /TEMP_D3)
    (add_net /TEMP_D4)
    (add_net /TEMP_D5)
    (add_net /TEMP_D6)
    (add_net /Vin)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J12-Pad8)")
    (add_net "Net-(J15-Pad16)")
    (add_net "Net-(J15-Pad2)")
    (add_net "Net-(J9-Pad8)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P12-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R29-Pad1)")
    (add_net "Net-(R30-Pad1)")
    (add_net "Net-(R31-Pad1)")
    (add_net "Net-(R32-Pad1)")
    (add_net "Net-(R41-Pad1)")
    (add_net "Net-(R42-Pad1)")
    (add_net "Net-(R43-Pad1)")
    (add_net "Net-(R44-Pad1)")
    (add_net "Net-(R53-Pad1)")
    (add_net "Net-(R54-Pad1)")
    (add_net "Net-(R55-Pad1)")
    (add_net "Net-(R56-Pad1)")
    (add_net "Net-(R63-Pad1)")
    (add_net "Net-(R64-Pad1)")
    (add_net "Net-(R65-Pad1)")
    (add_net "Net-(R72-Pad1)")
    (add_net "Net-(R73-Pad1)")
    (add_net "Net-(R74-Pad1)")
  )
  (net_class PWM/FAULT ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DIR)
    (add_net /FAULT)
    (add_net /PWM)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Right (layer B.Cu) (tedit 59FED5CC)
    (at 125.984 70.866 270)
    (descr "surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x04 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference P5 (at 0 6.14 270) (layer B.SilkS))
    (fp_text value PWM (at 0 -6.14 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 3 smd rect (at 1.655 -1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 21 +3V3))
    (pad 1 smd rect (at 1.655 3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 10 /SCL))
    (pad 4 smd rect (at -1.655 -3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.655 1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 11 /SDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 169.8117 92.3925)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP1 (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value PWM (at 0 2.75) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 111 /PWM))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 114.5654 62.1124 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0.22 2.82) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R29-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 67 /MA1))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R29-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 102 /M1))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 /MB1))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R29-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 149.8679 79.1811 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U2 (at -0.032 2.236) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R30-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 /MA6))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R30-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 99 /M6))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 /MB6))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(R30-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 113.7539 104.5972 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U3 (at 0 2.286) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R31-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 /MA11))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R31-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 92 /M11))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 71 /MB11))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(R31-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 169.4066 105.2468 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U4 (at -0.028 2.354) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R32-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 80 /MA16))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R32-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 89 /M16))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 81 /MB16))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R32-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 114.3296 79.5032 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U5 (at 0 -2.65) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R41-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 65 /MA2))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R41-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 103 /M2))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 /MB2))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R41-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 159.7844 62.1665 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U6 (at -0.034 2.316 180) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R42-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 /MA7))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R42-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 96 /M7))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 /MB7))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R42-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 134.0184 104.9327 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U7 (at 0.008 2.304) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R43-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 /MA12))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R43-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 /M12))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 /MB12))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R43-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 168.9633 114.7947 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U8 (at 0.0787 2.4251) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R44-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 82 /MA17))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R44-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 /M17))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 83 /MB17))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R44-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 129.5654 62.1124 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U9 (at -0.07 2.36) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(R53-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 63 /MA3))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(R53-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 100 /M3))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 62 /MB3))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(R53-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 166.6658 79.4189 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U10 (at -0.004 2.332) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R54-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 /MA8))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R54-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 97 /M8))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 /MB8))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(R54-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 134.1022 113.1463 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U11 (at 0.046 2.348) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R55-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 /MA13))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R55-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 90 /M13))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 /MB13))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(R55-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 184.9642 104.6129 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U12 (at -0.352 2.454) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(R56-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 84 /MA18))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(R56-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 87 /M18))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 85 /MB18))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(R56-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 132.7584 79.2882 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U13 (at 0.09 2.37) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R63-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 /MA4))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R63-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 101 /M4))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 60 /MB4))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(R63-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 182.5331 79.6099 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U14 (at -0.106 2.438) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R64-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 /MA9))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R64-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 94 /M9))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 /MB9))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(R64-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 154.1538 105.0978 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U15 (at -0.012 2.372) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R65-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 76 /MA14))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R65-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 91 /M14))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 77 /MB14))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(R65-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 144.1017 62.191 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U16 (at 0.036 2.274) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(R72-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 /MA5))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(R72-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 98 /M5))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 /MB5))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(R72-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 113.7666 93.0529 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U17 (at 0 2.286) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(R73-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 68 /MA10))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(R73-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 95 /M10))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 69 /MB10))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(R73-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-motors:DFN-12-1EP_3x3mm_P0.5mm_EP1.70x2.50mm (layer F.Cu) (tedit 62BCBFA5)
    (at 154.3374 115.0218 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U18 (at -0.0057 2.3601) (layer F.SilkS))
    (fp_text value MAX14870 (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(R74-Pad1)"))
    (pad 2 smd rect (at -2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 78 /MA15))
    (pad 3 smd rect (at -2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 4 smd rect (at -2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(R74-Pad1)"))
    (pad 5 smd rect (at -2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /DIR))
    (pad 8 smd rect (at 2.05 0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 88 /M15))
    (pad 9 smd rect (at 2.05 0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.05 -0.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 11 smd rect (at 2.05 -0.75 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 79 /MB15))
    (pad 12 smd rect (at 2.05 -1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(R74-Pad1)"))
    (pad "" smd rect (at -0.4445 0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad 13 smd rect (at 0 0 180) (size 1.7 2.5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PWM))
    (pad 7 smd rect (at 2.05 1.25 180) (size 1.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /FAULT))
    (pad "" smd rect (at 0.4318 0.635 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at 0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (pad "" smd rect (at -0.4445 -0.6477 180) (size 0.8 1.2) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_3x3mm_P0.5mm_EP2.05x2.86mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Arduino_Mega:Arduino_1pin locked (layer F.Cu) (tedit 5524FDA7)
    (at 117.348 119.126)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P8 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P8-Pad1)"))
  )
  (module Socket_Arduino_Mega:Arduino_1pin locked (layer F.Cu) (tedit 5524FDBB)
    (at 199.898 119.126)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P10 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P10-Pad1)"))
  )
  (module Socket_Arduino_Mega:Arduino_1pin locked (layer F.Cu) (tedit 5524FDD2)
    (at 118.618 70.866)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P11 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P11-Pad1)"))
  )
  (module Socket_Arduino_Mega:Arduino_1pin locked (layer F.Cu) (tedit 5524FDCA)
    (at 169.418 86.106)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P12 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P12-Pad1)"))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 121.158 62.9412)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.1143 -1.3589) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 144.3355 79.756 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.7087 105.3592 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 164.1006 105.9307 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 120.5357 79.4893)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 2.71 0.04) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 154.1983 63.0418 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.4605 105.8037 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 163.4142 115.5728 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 135.7294 62.9748)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 2.6275 0.01) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 160.6898 80.0569 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0.0475 -1.4009) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.173 113.891 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0.0173 -1.2726) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 179.2456 105.8419 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.4324 80.1256 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 -1.41) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 177.0131 80.3899 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.7854 105.9669 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.7497 63.065 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 119.7102 93.4847)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at 0 -1.524) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.7862 115.9531 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 217.5637 64.2493 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D1 (at -4.24 0.14 180) (layer F.SilkS))
    (fp_text value US1A (at 0 2.6 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 24 +12V))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 171.7464 124.2476 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.032 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 /TEMP_D4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 173.2704 124.2476 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.0666 -0.0211) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 /TEMP_D4))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 155.3126 124.2349 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.286 0 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 /TEMP_D1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.8366 124.2349 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 2.286 0 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 /TEMP_D1))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 170.2224 124.2476 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.032 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 29 /TEMP_4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 153.7886 124.2349 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.286 0 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 /TEMP_1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 178.4393 124.1968 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.286 0 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 /TEMP_D5))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 179.9633 124.1968 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.286 0 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 /TEMP_D5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 160.6847 124.2349 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -2.032 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 105 /TEMP_D2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 162.2087 124.2349 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.27 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 105 /TEMP_D2))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 176.9153 124.1968 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -0.0346 -1.2743 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 /TEMP_5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 159.1607 124.2349 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0.067 -1.1346 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 /TEMP_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 184.4972 124.1841 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -2.1936 -0.1059 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 /TEMP_D6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.0212 124.1841 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -0.0543 -1.3546 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 /TEMP_D6))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 166.2219 124.2477 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at -2.0065 0.508 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 /TEMP_D3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.7459 124.2222 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.27 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 /TEMP_D3))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 182.9732 124.1841 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0.0162 -1.287 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 /TEMP_6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 164.6979 124.2222 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -2.032 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /TEMP_3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 174.0154 66.0654)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -2.794 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 113 /FAULT))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 108.7754 61.1224 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0.2 1.39) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 /M1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 144.3639 78.1391 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 /M6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 107.7087 103.6452 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 /M11))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 164.0078 104.3178 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 /M16))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.3954 66.2524 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at 0.05 1.42 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 115 "Net-(R29-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 151.0919 82.0293 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 116 "Net-(R30-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 113.7539 108.9152 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R31 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 117 "Net-(R31-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 169.4666 108.8393 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R32 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 118 "Net-(R32-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 108.4996 78.6732 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R33 (at 0.04 1.35) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 /M2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.1728 61.2638 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R34 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 /M7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 128.4605 104.0257 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R35 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 93 /M12))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 163.4142 113.7948 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R36 (at 0 1.524) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 /M17))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.3996 83.0132 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R41 (at -0.07 1.32 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 119 "Net-(R41-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 160.0384 65.7225 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R42 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 120 "Net-(R42-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133.9469 108.9787 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R43 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 121 "Net-(R43-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 168.8813 118.4247 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R44 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 122 "Net-(R44-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 124.6505 60.5028 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R45 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 /M3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 160.6898 78.4569 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R46 (at -0.0033 1.2917) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 97 /M8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 128.1684 112.3315 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R47 (at -0.06 1.23) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 /M13))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 179.2202 103.4289 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R51 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 87 /M18))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 129.6289 65.913 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R53 (at 0.07 1.4 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 123 "Net-(R53-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 167.894 82.2706 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R54 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 124 "Net-(R54-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 134.0262 117.4183 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R55 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 125 "Net-(R55-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 184.9882 108.3056 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R56 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 126 "Net-(R56-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 127.4124 78.4756 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R57 (at -0.02 1.54) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 /M4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 177.0131 78.6119 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R58 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 /M9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 148.8059 104.3559 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R59 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 /M14))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133.8199 82.3595 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R63 (at -2.5654 -0.127) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 127 "Net-(R63-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 183.7944 82.7405 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R64 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 128 "Net-(R64-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.1653 109.5502 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R65 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 129 "Net-(R65-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 138.7497 61.287 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R66 (at 0 1.524) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /M5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 107.9246 92.2909 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R67 (at 0 1.27) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 95 /M10))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 148.7862 114.1751 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R68 (at 0 1.524) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 /M15))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 144.0942 66.0273 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R72 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 130 "Net-(R72-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 113.7666 97.3709 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R73 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 131 "Net-(R73-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.3374 118.5778 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R74 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 500m (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 132 "Net-(R74-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 141.9352 91.821)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP2 (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value DIR (at 0 2.75) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 110 /DIR))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5005-5009_Compact (layer F.Cu) (tedit 5A0F774F)
    (at 219.9132 79.5782)
    (descr "Keystone Miniature THM Test Point 5005-5009, http://www.keyelco.com/product-pdf.cfm?p=1314")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP3 (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value GND (at 0 2.75) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5005-5009_Compact.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 108.7754 62.8924 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.17 -2.01) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 156.1719 80.1751)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.254 -1.27) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 120.3325 105.2449)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.286 0 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 175.5394 104.4194)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0.05 -1.22 -180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43 -180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 -180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 108.3496 80.3032 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -0.21 -1.44) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 166.4284 63.2505)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.27) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 140.1318 105.7275)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0.008 -1.288) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 175.9331 114.7826)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 -1.27) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.2314 62.2427 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 2.62 0.02 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 172.9486 80.2005)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 -1.27) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 140.7166 114.1046)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 -1.27) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 190.8683 105.0544)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 1.27) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 138.9102 80.1515)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 2.69 -0.04) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 188.7855 80.3148)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 0.16 1.25 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 160.8058 105.8358)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at -0.08 -1.25) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 150.4569 62.9031)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 0 -1.27) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.9246 93.8657 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 160.1851 114.935)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 0 -1.27) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.43) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +12V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 128.6002 89.1286 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J7 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value DSUB25-1-1 (at 1.27 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 /MB3))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /MA3))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /MB2))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 /MA2))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /MB1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 /MA1))
    (model ${KIPRJMOD}/facs-pcb-v2.3dshapes/61200621621.stp
      (offset (xyz 1 -2.5 4.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KIPRJMOD}/facs-pcb-v2.3dshapes/61200623021 (rev1).stp"
      (offset (xyz 1 -2.5 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 128.5621 99.4156 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J8 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value DSUB25-2-1 (at 1.27 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /MA10))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /MB10))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 /MA11))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 /MB11))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /MA12))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /MB12))
    (model ${KIPRJMOD}/facs-pcb-v2.3dshapes/61200621621.stp
      (offset (xyz 1 -2.5 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KIPRJMOD}/facs-pcb-v2.3dshapes/61200623021 (rev1).stp"
      (offset (xyz 1 -2.5 8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 177.5079 65.3415 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J9 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value DSUB25-1-4 (at 1.27 9.95 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 3.81) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(J9-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /ENC_6))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /ENC_5))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /ENC_4))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /ENC_3))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /ENC_2))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /ENC_1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 150.2029 99.5299 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J10 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value DSUB25-2-2 (at 1.27 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 /MB15))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 /MA15))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 /MB14))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 /MA14))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 /MB13))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /MA13))
    (model ${KIPRJMOD}/facs-pcb-v2.3dshapes/61200621621.stp
      (offset (xyz 1.5 -2.5 3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KIPRJMOD}/facs-pcb-v2.3dshapes/61200623021 (rev1).stp"
      (offset (xyz 1 -2.5 8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 149.9489 89.408 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J11 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value DSUB25-1-2 (at 1.27 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 /MA4))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 /MB4))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /MA5))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /MB5))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /MA6))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /MB6))
    (model ${KIPRJMOD}/facs-pcb-v2.3dshapes/61200621621.stp
      (offset (xyz 1.5 -2.5 3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KIPRJMOD}/facs-pcb-v2.3dshapes/61200623021 (rev1).stp"
      (offset (xyz 1 -2.5 8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 209.6643 112.2934)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J12 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value DSUB25-2-4 (at 1.27 9.95) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 3.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /TEMP_1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /TEMP_2))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /TEMP_3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /TEMP_4))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /TEMP_5))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /TEMP_6))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(J12-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 178.8287 99.822 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J13 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value DSUB25-2-3 (at 1.27 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 /MA16))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 /MB16))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 /MA17))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 /MB17))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 /MA18))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 /MB18))
    (model ${KIPRJMOD}/facs-pcb-v2.3dshapes/61200621621.stp
      (offset (xyz 1.5 -2.5 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KIPRJMOD}/facs-pcb-v2.3dshapes/61200623021 (rev1).stp"
      (offset (xyz 1 -2.5 8.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 178.9303 89.2048 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J14 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value DSUB25-1-3 (at 1.27 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /MB9))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /MA9))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /MB8))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /MA8))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /MB7))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /MA7))
    (model ${KIPRJMOD}/facs-pcb-v2.3dshapes/61200621621.stp
      (offset (xyz 1.5 -2.5 3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KIPRJMOD}/facs-pcb-v2.3dshapes/61200623021 (rev1).stp"
      (offset (xyz 1 -2.5 8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 209.8167 76.7715)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (fp_text reference J15 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value DSUB15-1 (at 1.27 20.11) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 8.89 -270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(J15-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /ENC_7))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /ENC_8))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /ENC_9))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /ENC_10))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /ENC_11))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /ENC_12))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /ENC_13))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /ENC_14))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /ENC_15))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /ENC_16))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /ENC_17))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /ENC_18))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(J15-Pad16)"))
    (model "${KIPRJMOD}/facs-pcb-v2.3dshapes/SBH11-_ _ _C-D08-ST-_ _.STEP"
      (offset (xyz 3 0 -3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x18_P2.54mm_Vertical_SMD (layer B.Cu) (tedit 59FED5CC)
    (at 198.628 92.456)
    (descr "surface-mounted straight pin header, 2x18, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x18 2.54mm double row")
    (attr smd)
    (fp_text reference P1 (at 0 23.92 180) (layer B.SilkS))
    (fp_text value Digital (at 0 -23.92 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -2.525 21.59) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.525 21.59) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.525 19.05) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 89 /M16))
    (pad 4 smd rect (at 2.525 19.05) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 87 /M18))
    (pad 5 smd rect (at -2.525 16.51) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 88 /M15))
    (pad 6 smd rect (at 2.525 16.51) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 86 /M17))
    (pad 7 smd rect (at -2.525 13.97) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 91 /M14))
    (pad 8 smd rect (at 2.525 13.97) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 136 "Net-(P1-Pad8)"))
    (pad 9 smd rect (at -2.525 11.43) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 90 /M13))
    (pad 10 smd rect (at 2.525 11.43) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 137 "Net-(P1-Pad10)"))
    (pad 11 smd rect (at -2.525 8.89) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 93 /M12))
    (pad 12 smd rect (at 2.525 8.89) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 49 /ENC_18))
    (pad 13 smd rect (at -2.525 6.35) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 92 /M11))
    (pad 14 smd rect (at 2.525 6.35) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 48 /ENC_17))
    (pad 15 smd rect (at -2.525 3.81) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 95 /M10))
    (pad 16 smd rect (at 2.525 3.81) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 47 /ENC_16))
    (pad 17 smd rect (at -2.525 1.27) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 94 /M9))
    (pad 18 smd rect (at 2.525 1.27) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 46 /ENC_15))
    (pad 19 smd rect (at -2.525 -1.27) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 97 /M8))
    (pad 20 smd rect (at 2.525 -1.27) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 45 /ENC_14))
    (pad 21 smd rect (at -2.525 -3.81) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 96 /M7))
    (pad 22 smd rect (at 2.525 -3.81) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 44 /ENC_13))
    (pad 23 smd rect (at -2.525 -6.35) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 99 /M6))
    (pad 24 smd rect (at 2.525 -6.35) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 43 /ENC_12))
    (pad 25 smd rect (at -2.525 -8.89) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 98 /M5))
    (pad 26 smd rect (at 2.525 -8.89) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 42 /ENC_11))
    (pad 27 smd rect (at -2.525 -11.43) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 101 /M4))
    (pad 28 smd rect (at 2.525 -11.43) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 41 /ENC_10))
    (pad 29 smd rect (at -2.525 -13.97) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 100 /M3))
    (pad 30 smd rect (at 2.525 -13.97) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 40 /ENC_9))
    (pad 31 smd rect (at -2.525 -16.51) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 103 /M2))
    (pad 32 smd rect (at 2.525 -16.51) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 39 /ENC_8))
    (pad 33 smd rect (at -2.525 -19.05) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 102 /M1))
    (pad 34 smd rect (at 2.525 -19.05) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 38 /ENC_7))
    (pad 35 smd rect (at -2.525 -21.59) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 36 smd rect (at 2.525 -21.59) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x18_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-pcb-v2:PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right locked (layer B.Cu) (tedit 630526B0)
    (at 140.208 119.126 270)
    (descr "surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x08 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference P2 (at 0 11.22 90) (layer B.SilkS))
    (fp_text value Power (at 0 -11.22 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 7 smd rect (at 1.655 -6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.655 -1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 139 +5VA))
    (pad 3 smd rect (at 1.655 3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 4 /Reset))
    (pad 1 smd rect (at 1.655 8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(P2-Pad1)"))
    (pad 8 smd rect (at -1.655 -8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 5 /Vin))
    (pad 6 smd rect (at -1.655 -3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.655 1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 21 +3V3))
    (pad 2 smd rect (at -1.655 6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /IOREF))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-pcb-v2:PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right locked (layer B.Cu) (tedit 630526B0)
    (at 163.068 119.126 270)
    (descr "surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x08 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference P3 (at 0 11.22 90) (layer B.SilkS))
    (fp_text value Analog (at 0 -11.22 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at -1.655 6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 104 /TEMP_D1))
    (pad 4 smd rect (at -1.655 1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 105 /TEMP_D2))
    (pad 6 smd rect (at -1.655 -3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 106 /TEMP_D3))
    (pad 8 smd rect (at -1.655 -8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 107 /TEMP_D4))
    (pad 1 smd rect (at 1.655 8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 26 /TEMP_1))
    (pad 3 smd rect (at 1.655 3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 27 /TEMP_2))
    (pad 5 smd rect (at 1.655 -1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 28 /TEMP_3))
    (pad 7 smd rect (at 1.655 -6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 29 /TEMP_4))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-pcb-v2:PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right locked (layer B.Cu) (tedit 630526B0)
    (at 185.928 119.126 270)
    (descr "surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x08 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference P4 (at 0 11.22 90) (layer B.SilkS))
    (fp_text value Analog (at 0 -11.22 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at -1.655 6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 108 /TEMP_D5))
    (pad 4 smd rect (at -1.655 1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 109 /TEMP_D6))
    (pad 6 smd rect (at -1.655 -3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 7 /A13))
    (pad 8 smd rect (at -1.655 -8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 9 /A15))
    (pad 1 smd rect (at 1.655 8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 30 /TEMP_5))
    (pad 3 smd rect (at 1.655 3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 31 /TEMP_6))
    (pad 5 smd rect (at 1.655 -1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 6 /A12))
    (pad 7 smd rect (at 1.655 -6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 8 /A14))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-pcb-v2:PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right locked (layer B.Cu) (tedit 630526B0)
    (at 157.988 70.866 270)
    (descr "surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x08 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference P6 (at 0 11.22 270) (layer B.SilkS))
    (fp_text value PWM (at 0 -11.22 270) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 7 smd rect (at 1.655 -6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 22 "/1(Tx0)"))
    (pad 5 smd rect (at 1.655 -1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 14 "/3(**)"))
    (pad 3 smd rect (at 1.655 3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 111 /PWM))
    (pad 1 smd rect (at 1.655 8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 12 "/7(**)"))
    (pad 8 smd rect (at -1.655 -8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 23 "/0(Rx0)"))
    (pad 6 smd rect (at -1.655 -3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 15 "/2(**)"))
    (pad 4 smd rect (at -1.655 1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 13 "/4(**)"))
    (pad 2 smd rect (at -1.655 6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 110 /DIR))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-pcb-v2:PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right locked (layer B.Cu) (tedit 630526B0)
    (at 180.848 70.866 270)
    (descr "surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x08 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference P7 (at 0 11.22 90) (layer B.SilkS))
    (fp_text value Communication (at 0 -11.22 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 7 smd rect (at 1.655 -6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 36 /ENC_5))
    (pad 5 smd rect (at 1.655 -1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 34 /ENC_3))
    (pad 3 smd rect (at 1.655 3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 32 /ENC_1))
    (pad 1 smd rect (at 1.655 8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 112 /SOL_V))
    (pad 8 smd rect (at -1.655 -8.89 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 37 /ENC_6))
    (pad 6 smd rect (at -1.655 -3.81 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 35 /ENC_4))
    (pad 4 smd rect (at -1.655 1.27 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 33 /ENC_2))
    (pad 2 smd rect (at -1.655 6.35 270) (size 2.51 1) (layers B.Cu B.Paste B.Mask)
      (net 113 /FAULT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-pcb-v2:TE_350422-1 (layer F.Cu) (tedit 63081211)
    (at 210.2612 62.738 270)
    (fp_text reference J5 (at -3.095 -6.08 90) (layer F.SilkS) hide)
    (fp_text value SOL_V (at 3.0226 5.3594 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 2.667 2.667) (drill 1.778) (layers *.Cu *.Mask)
      (net 24 +12V))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.667 2.667) (drill 1.778) (layers *.Cu *.Mask)
      (net 25 "Net-(D1-Pad2)"))
    (model ${KIPRJMOD}/facs-pcb-v2.3dshapes/350422-1.step
      (offset (xyz 0 0 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module facs-pcb-v2:TE_350422-1 (layer F.Cu) (tedit 63081211)
    (at 199.4789 62.3824 270)
    (fp_text reference J6 (at -3.095 -6.08 90) (layer F.SilkS) hide)
    (fp_text value 12V (at 4.5974 5.461 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.667 2.667) (drill 1.778) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 2.667 2.667) (drill 1.778) (layers *.Cu *.Mask)
      (net 24 +12V))
    (model ${KIPRJMOD}/facs-pcb-v2.3dshapes/350422-1.step
      (offset (xyz 0 0 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 221.4499 62.9666)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value IRLML2060 (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 221.2594 58.1279 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -0.4699 -1.4732 90) (layer F.SilkS))
    (fp_text value 330 (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 /SOL_V))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 114 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 219.6211 58.1279 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at -0.9779 2.2479 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 /SOL_V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 221.562401 124.359501) (end 221.5924 127.3595) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 224.5624 124.329502) (end 224.543398 58.2912) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 221.543399 58.321199) (end 224.543398 58.2912) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 106.369999 58.319999) (end 106.34 55.32) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text 1 (at 131.4577 114.8207 90) (layer F.SilkS))
  (gr_line (start 221.5924 127.3595) (end 103.3653 127.3683) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.34 55.32) (end 221.5134 55.3212) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.3653 127.3683) (end 103.37 58.349998) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 24) (net_name +12V) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 225.41865 128.143) (xy 101.88575 128.4224) (xy 101.07295 54.6735) (xy 224.60585 54.3941)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 225.69635 127.8322) (xy 101.8379 127.8262) (xy 101.4476 54.5719) (xy 225.2726 54.7751)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.743752 107.958019) (xy 184.276806 107.953112) (xy 184.277194 104.965274) (xy 185.731249 104.970181)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.678252 118.105319) (xy 168.211306 118.100412) (xy 168.211694 115.112574) (xy 169.665749 115.117481)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.060552 118.245019) (xy 153.593606 118.240112) (xy 153.593994 115.252274) (xy 155.048049 115.257181)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.765952 116.975019) (xy 133.299006 116.970112) (xy 133.299394 113.982274) (xy 134.753449 113.987181)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.198952 108.402519) (xy 168.732006 108.397612) (xy 168.732394 105.409774) (xy 170.186449 105.414681)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.943223 109.216104) (xy 153.311177 109.249297) (xy 153.352694 105.701874) (xy 154.971849 105.668681)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.727852 108.504119) (xy 133.260906 108.499212) (xy 133.261294 105.511374) (xy 134.715349 105.516281)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.496752 108.389819) (xy 113.029806 108.384912) (xy 113.030194 105.397074) (xy 114.484249 105.401981)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.509452 96.769319) (xy 113.042506 96.764412) (xy 113.042894 93.776574) (xy 114.496949 93.781481)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.119052 82.672319) (xy 113.652106 82.667412) (xy 113.652494 79.679574) (xy 115.106549 79.684481)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.648352 82.735819) (xy 132.181406 82.730912) (xy 132.181794 79.743074) (xy 133.635849 79.747981)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.729852 82.405619) (xy 149.047006 82.380219) (xy 149.047394 79.392381) (xy 150.717349 79.417781)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.531952 82.646919) (xy 165.823706 82.596119) (xy 165.824094 79.608281) (xy 167.519449 79.659081)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 183.356152 83.002519) (xy 181.762206 82.939019) (xy 181.762594 79.951181) (xy 183.343649 80.014681)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.661252 65.324119) (xy 158.927606 65.324119) (xy 158.927994 62.336281) (xy 160.648749 62.336281)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.002152 65.540019) (xy 143.344706 65.527319) (xy 143.345094 62.539481) (xy 144.989649 62.552181)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.384452 65.628919) (xy 128.752406 65.578119) (xy 128.752794 62.590281) (xy 130.371949 62.641081)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.246052 65.882919) (xy 113.779106 65.878012) (xy 113.779494 62.890174) (xy 115.233549 62.895081)
      )
    )
  )
)
