(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 23)
    (no_connects 0)
    (area 108.552857 92.634999 285.242 129.879)
    (thickness 1.6)
    (drawings 10)
    (tracks 42)
    (zones 0)
    (modules 11)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFB7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(SW1-Pad1)")
  (net 3 "Net-(SW1-Pad3)")
  (net 4 "Net-(SW1-Pad5)")
  (net 5 "Net-(P1/SCL1-Pad1)")
  (net 6 "Net-(P1/SCL1-Pad2)")
  (net 7 "Net-(P2/SDA1-Pad2)")
  (net 8 "Net-(P3/SCL0-Pad2)")
  (net 9 "Net-(P4/SDA0-Pad2)")
  (net 10 "Net-(SW2-Pad5)")
  (net 11 "Net-(SW2-Pad1)")
  (net 12 "Net-(SW2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(P1/SCL1-Pad1)")
    (add_net "Net-(P1/SCL1-Pad2)")
    (add_net "Net-(P2/SDA1-Pad2)")
    (add_net "Net-(P3/SCL0-Pad2)")
    (add_net "Net-(P4/SDA0-Pad2)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(SW1-Pad3)")
    (add_net "Net-(SW1-Pad5)")
    (add_net "Net-(SW2-Pad1)")
    (add_net "Net-(SW2-Pad3)")
    (add_net "Net-(SW2-Pad5)")
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A313A90)
    (at 118.11 107.95)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A313A9C)
    (at 140.97 107.95)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module teensy:Teensy30_31_32_LC (layer F.Cu) (tedit 5A2F46D8)
    (at 129.54 106.68)
    (fp_text reference U1 (at 0 -10.16) (layer F.SilkS) hide)
    (fp_text value Teensy-LC (at 0 10.16) (layer F.Fab) hide)
    (pad 20 thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 24 thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P4/SDA0-Pad2)"))
    (pad 26 thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P3/SCL0-Pad2)"))
    (pad 27 thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 28 thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 29 thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1/SCL1-Pad2)"))
    (pad 30 thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P2/SDA1-Pad2)"))
    (pad 31 thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 32 thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1/SCL1-Pad1)"))
    (pad 33 thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(SW2-Pad1)"))
    (pad 9 thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(SW2-Pad3)"))
    (pad 8 thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(SW2-Pad5)"))
    (pad 7 thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(SW1-Pad1)"))
    (pad 6 thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(SW1-Pad3)"))
    (pad 5 thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(SW1-Pad5)"))
    (pad 4 thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole rect (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module "Local Copy:PEC11R-4xxx-Sxxxx" (layer F.Cu) (tedit 5A30A318)
    (at 120.015 109.855 180)
    (descr http://www.bourns.com/docs/Product-Datasheets/pec11R.pdf)
    (fp_text reference SW1 (at 0 5.715 180) (layer B.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 0.1 -12.1 180) (layer F.Fab))
    (pad GND thru_hole rect (at -6.6 0 270) (size 3.2 2.4) (drill oval 2.7 1.9) (layers *.Cu *.Mask))
    (pad GND thru_hole rect (at 6.6 0 270) (size 3.2 2.4) (drill oval 2.7 1.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -2.5 -7 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 2.5 -7 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(SW1-Pad5)"))
    (pad 1 thru_hole circle (at -2.5 7.5 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(SW1-Pad1)"))
    (pad 3 thru_hole circle (at 2.5 7.5 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(SW1-Pad3)"))
    (pad 2 thru_hole circle (at 0 7.5 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connectors_JST:JST_EH_B02B-EH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A30A1E0)
    (at 114.935 95.25)
    (descr "JST EH series connector, B02B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference P1/SCL1 (at 1.27 1.905) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 1.25 3.5) (layer F.Fab))
    (fp_text user %R (at 1.25 -3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(P1/SCL1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(P1/SCL1-Pad2)"))
    (model Connectors_JST.3dshapes/JST_EH_B02B-EH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B02B-EH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A30A1DA)
    (at 123.825 95.25)
    (descr "JST EH series connector, B02B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference P2/SDA1 (at 1.27 1.905) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 1.25 3.5) (layer F.Fab))
    (fp_text user %R (at 1.25 -3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(P1/SCL1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(P2/SDA1-Pad2)"))
    (model Connectors_JST.3dshapes/JST_EH_B02B-EH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B02B-EH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A30A1D4)
    (at 132.715 95.25)
    (descr "JST EH series connector, B02B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference P3/SCL0 (at 1.27 1.905) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 1.25 3.5) (layer F.Fab))
    (fp_text user %R (at 1.25 -3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(P1/SCL1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(P3/SCL0-Pad2)"))
    (model Connectors_JST.3dshapes/JST_EH_B02B-EH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_EH_B02B-EH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A30A1CC)
    (at 141.605 95.25)
    (descr "JST EH series connector, B02B-EH-A, 2.50mm pitch, top entry")
    (tags "connector jst eh top vertical straight")
    (fp_text reference P4/SDA0 (at 1.27 1.905) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 1.25 3.5) (layer F.Fab))
    (fp_text user %R (at 1.25 -3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(P1/SCL1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.85 1.85) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(P4/SDA0-Pad2)"))
    (model Connectors_JST.3dshapes/JST_EH_B02B-EH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Local Copy:PEC11R-4xxx-Sxxxx" (layer F.Cu) (tedit 5A30A314)
    (at 129.54 109.855 180)
    (descr http://www.bourns.com/docs/Product-Datasheets/pec11R.pdf)
    (fp_text reference SW1POS2 (at 0 5.715 180) (layer B.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 0.1 -12.1 180) (layer F.Fab))
    (pad GND thru_hole rect (at -6.6 0 270) (size 3.2 2.4) (drill oval 2.7 1.9) (layers *.Cu *.Mask))
    (pad GND thru_hole rect (at 6.6 0 270) (size 3.2 2.4) (drill oval 2.7 1.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -2.5 -7 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 2.5 -7 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(SW1-Pad5)"))
    (pad 1 thru_hole circle (at -2.5 7.5 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(SW1-Pad1)"))
    (pad 3 thru_hole circle (at 2.5 7.5 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(SW1-Pad3)"))
    (pad 2 thru_hole circle (at 0 7.5 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "Local Copy:PEC11R-4xxx-Sxxxx" (layer F.Cu) (tedit 5A30A617)
    (at 139.065 109.855 180)
    (descr http://www.bourns.com/docs/Product-Datasheets/pec11R.pdf)
    (fp_text reference SW2 (at 0.127 5.715 180) (layer B.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 0.1 -12.1 180) (layer F.Fab))
    (pad GND thru_hole rect (at -6.6 0 270) (size 3.2 2.4) (drill oval 2.7 1.9) (layers *.Cu *.Mask))
    (pad GND thru_hole rect (at 6.6 0 270) (size 3.2 2.4) (drill oval 2.7 1.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -2.5 -7 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 2.5 -7 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(SW2-Pad5)"))
    (pad 1 thru_hole circle (at -2.5 7.5 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(SW2-Pad1)"))
    (pad 3 thru_hole circle (at 2.5 7.5 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(SW2-Pad3)"))
    (pad 2 thru_hole circle (at 0 7.5 180) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module moshozenfootprints:Moshozen (layer F.Cu) (tedit 0)
    (at 129.286 105.664)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text v1.0 (at 144.78 101.346) (layer F.SilkS))
  (gr_line (start 147.32 118.618) (end 147.32 119.126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.76 118.872) (end 111.76 119.126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 92.71) (end 147.32 97.155) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.76 97.155) (end 111.76 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "github.com/mtrudel/teensyhid\n" (at 112.268 112.268) (layer F.SilkS))
  (gr_line (start 111.76 118.745) (end 111.76 97.155) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 119.253) (end 111.76 119.253) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 97.155) (end 147.32 118.745) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.76 92.71) (end 147.32 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name "Net-(P1/SCL1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.32 100.33) (xy 111.76 100.33) (xy 111.76 92.71) (xy 147.32 92.71)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.574 119.126) (xy 111.76 119.126) (xy 111.76 100.838) (xy 147.32 100.838)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.574 119.126) (xy 111.76 119.126) (xy 111.76 92.71) (xy 147.32 92.71)
      )
    )
  )
)
