(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A5" portrait)
	(title_block
		(title "Mech Midi 1")
		(company "David Konsumer")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-A)")
	(net 2 "KR0")
	(net 3 "Net-(D2-A)")
	(net 4 "Net-(D3-A)")
	(net 5 "Net-(D4-A)")
	(net 6 "Net-(D5-A)")
	(net 7 "KR1")
	(net 8 "Net-(D6-A)")
	(net 9 "Net-(D7-A)")
	(net 10 "Net-(D8-A)")
	(net 11 "KR2")
	(net 12 "Net-(D9-A)")
	(net 13 "Net-(D10-A)")
	(net 14 "Net-(D11-A)")
	(net 15 "Net-(D12-A)")
	(net 16 "KR3")
	(net 17 "Net-(D13-A)")
	(net 18 "Net-(D14-A)")
	(net 19 "Net-(D15-A)")
	(net 20 "Net-(D16-A)")
	(net 21 "KR4")
	(net 22 "Net-(D17-A)")
	(net 23 "Net-(D18-A)")
	(net 24 "Net-(D19-A)")
	(net 25 "Net-(D20-A)")
	(net 26 "GND")
	(net 27 "5V")
	(net 28 "Net-(LED1-DOUT)")
	(net 29 "LED")
	(net 30 "Net-(LED2-DOUT)")
	(net 31 "Net-(LED3-DOUT)")
	(net 32 "Net-(LED4-DOUT)")
	(net 33 "Net-(LED5-DOUT)")
	(net 34 "Net-(LED6-DOUT)")
	(net 35 "Net-(LED7-DOUT)")
	(net 36 "Net-(LED8-DOUT)")
	(net 37 "Net-(LED10-DIN)")
	(net 38 "Net-(LED10-DOUT)")
	(net 39 "Net-(LED11-DOUT)")
	(net 40 "Net-(LED12-DOUT)")
	(net 41 "Net-(LED13-DOUT)")
	(net 42 "Net-(LED14-DOUT)")
	(net 43 "Net-(LED15-DOUT)")
	(net 44 "Net-(LED16-DOUT)")
	(net 45 "Net-(LED17-DOUT)")
	(net 46 "Net-(LED18-DOUT)")
	(net 47 "Net-(LED19-DOUT)")
	(net 48 "unconnected-(LED20-DOUT-Pad1)")
	(net 49 "KC0")
	(net 50 "KC1")
	(net 51 "KC2")
	(net 52 "KC3")
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 44.62 68.45)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S5"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "KC0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D5-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 82.72 125.6)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S19"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "KC2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(D19-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 111.27 87.5 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D12"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "KR2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D12-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 63.67 130.6 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED18"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "Net-(LED18-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(LED17-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 82.72 130.6 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED19"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "Net-(LED19-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "Net-(LED18-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 115 101.42)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MCU"
			(at 0 7.41 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin Header male with pin space 2.54mm. Pin Count -3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader_1x03_P2.54mm*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "5V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "LED")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 82.72 68.45)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S7"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "KC2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(D7-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 101.77 54.4 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED4"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(LED4-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(LED3-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 82.72 106.55)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S15"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "KC2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(D15-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 44.62 54.4 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED1"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(LED1-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "LED")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 101.77 49.4)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S4"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "KC3")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D4-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 44.415 73.3)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED8"
			(at 0 -2 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "Net-(LED8-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(LED7-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 63.67 68.45)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S6"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "KC1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D6-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 92.22 68.45 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D7"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "KR1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D7-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 111.27 125.6 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D20"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "KR4")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(D20-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 73.17 87.5 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D10"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "KR2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D10-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 63.67 49.4)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S2"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "KC1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D2-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 92.22 49.4 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D3"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "KR0")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 54.12 125.6 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D17"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "KR4")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(D17-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 101.77 92.5 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED12"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(LED12-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(LED11-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 44.62 125.6)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S17"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "KC0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(D17-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 73.17 106.55 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D14"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "KR3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(D14-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 101.835 111.55)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED13"
			(at 0 -2 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "Net-(LED13-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(LED12-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 73.17 68.45 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D6"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "KR1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 82.585 111.8)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED14"
			(at 0 -2 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "Net-(LED14-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "Net-(LED13-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 101.835 73.45)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED5"
			(at 0 -2 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "Net-(LED5-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(LED4-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 44.62 92.5 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED9"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "Net-(LED10-DIN)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "Net-(LED8-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 63.67 87.5)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S10"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "KC1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(D10-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 115 55.425)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ROW"
			(at 0 12.49 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin Header male with pin space 2.54mm. Pin Count -5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader_1x05_P2.54mm*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "KR0")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "KR1")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "KR2")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "KR3")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "KR4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 82.585 73.3)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED6"
			(at 0 -2 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(LED6-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "Net-(LED5-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 115 82.5)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 15.03 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin Header male with pin space 2.54mm. Pin Count -6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader_1x06_P2.54mm*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "GND")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "GND")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "GND")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "GND")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 92.22 106.55 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D15"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "KR3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(D15-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 82.72 54.4 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED3"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(LED3-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(LED2-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 101.77 68.45)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S8"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "KC3")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(D8-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 101.77 125.6)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S20"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "KC3")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(D20-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 114.75 72.17)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5V"
			(at 0 7.41 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin Header male with pin space 2.54mm. Pin Count -3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader_1x03_P2.54mm*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "5V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "5V")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 101.77 87.5)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S12"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "KC3")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D12-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 63.67 54.4 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED2"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(LED2-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(LED1-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 44.62 49.4)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S1"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "KC0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 115 41)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "COL"
			(at 0 10.5 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Pin Header male with pin space 2.54mm. Pin Count -4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader_1x04_P2.54mm*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "KC0")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "KC1")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "KC2")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "KC3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 54.12 87.5 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D9"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "KR2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D9-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 101.77 130.6 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED20"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "unconnected-(LED20-DOUT-Pad1)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "Net-(LED19-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 44.62 87.5)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S9"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "KC0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D9-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 73.17 125.6 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D18"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "KR4")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(D18-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 54.12 49.4 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D1"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "KR0")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 54.12 68.45 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D5"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "KR1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 63.665 73.45)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED7"
			(at 0 -2 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(LED7-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(LED6-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 54.12 106.55 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D13"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "KR3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D13-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 92.22 87.5 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D11"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "KR2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D11-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 111.27 106.55 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D16"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "KR3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(D16-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 73.17 49.4 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D2"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "KR0")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 44.62 130.6 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED17"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(LED17-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "Net-(LED16-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 92.22 125.6 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D19"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "KR4")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "Net-(D19-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 111.27 68.45 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D8"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "KR1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D8-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 44.62 106.55)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S13"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "KC0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(D13-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 82.72 87.5)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S11"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "KC2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D11-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 82.72 92.5 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED11"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(LED11-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(LED10-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 63.67 92.5 180)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED10"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(LED10-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "Net-(LED10-DIN)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55 180)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 82.72 49.4)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S3"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "KC2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(D3-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 63.75 111.5)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED15"
			(at 0 -2 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "Net-(LED15-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "Net-(LED14-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
		(layer "F.Cu")
		(at 44.25 111.5)
		(descr "2.0mm x 2.0mm Addressable RGB LED NeoPixel Nano, 12 mA, https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf")
		(tags "LED RGB NeoPixel Nano PLCC-4 2020")
		(property "Reference" "LED16"
			(at 0 -2 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WS2812B-2020"
			(at 0 2.2 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*-2020_PLCC4*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "Net-(LED16-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.915 0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "Net-(LED15-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.915 -0.55)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B-2020_PLCC4_2.0x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_Components:Diode_SOD-123"
		(layer "F.Cu")
		(at 111.27 49.4 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D4"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N148"
			(at 0 2.1 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_Components:Diode_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1N4148 (DO-35) or 1N4148W (SOD-123)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "KR0")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_Components.3dshapes/Diode_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 101.77 106.55)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S16"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "KC3")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(D16-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 63.67 125.6)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S18"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "KC1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(D18-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottoKeebs_MX:MX_PCB_1.00u"
		(layer "F.Cu")
		(at 63.67 106.55)
		(descr "MX keyswitch PCB Mount Keycap 1.00u")
		(tags "MX Keyboard Keyswitch Switch PCB Cutout Keycap 1.00u")
		(property "Reference" "S14"
			(at 0 -8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Keyswitch"
			(at 0 8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ScottoKeebs_MX:MX_PCB_1.00u"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "mechmidi1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.75 1.75)
			(drill 1.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "KC1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -5.08)
			(size 2.5 2.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(D14-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${SCOTTOKEEBS_KICAD}/3dmodels/ScottoKeebs_MX.3dshapes/MX_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 33.86 38.48)
		(end 117.36 135.98)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "konsumer/mechmidi1"
		(at 115.5 134.5 90)
		(layer "F.SilkS")
	)
	(zone
		(net 26)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 32.5 37.5) (xy 32.5 137.5) (xy 120 137.5) (xy 120 37.5)
			)
		)
	)
	(zone
		(net 26)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 32.5 37.5) (xy 32.5 137.5) (xy 120 137.5) (xy 120 37.5)
			)
		)
	)
)
