(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 49)
    (no_connects 8)
    (area 102.477499 51.677499 121.042501 88.022501)
    (thickness 1.6)
    (drawings 26)
    (tracks 235)
    (zones 0)
    (modules 7)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.3048)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.0254)
    (uvia_drill 0)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 102.5525 87.9475)
    (visible_elements FFFEFF5F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /a14)
  (net 3 /d3)
  (net 4 /a12)
  (net 5 /d4)
  (net 6 /a7)
  (net 7 /d5)
  (net 8 /a6)
  (net 9 /d6)
  (net 10 /a5)
  (net 11 /d7)
  (net 12 /a4)
  (net 13 /a3)
  (net 14 /a10)
  (net 15 /a2)
  (net 16 /a1)
  (net 17 /a11)
  (net 18 /a0)
  (net 19 /a9)
  (net 20 /d0)
  (net 21 /a8)
  (net 22 /d1)
  (net 23 /a13)
  (net 24 /d2)
  (net 25 /VCCO)
  (net 26 /~CE)
  (net 27 /VBAT1)
  (net 28 /~CEO)
  (net 29 /TOL)
  (net 30 /VBAT2)
  (net 31 /VCCI)
  (net 32 /~OE)
  (net 33 /~WE)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.635)
    (via_drill 0.3048)
    (uvia_dia 0.0254)
    (uvia_drill 0)
    (add_net /TOL)
    (add_net /a0)
    (add_net /a1)
    (add_net /a10)
    (add_net /a11)
    (add_net /a12)
    (add_net /a13)
    (add_net /a14)
    (add_net /a2)
    (add_net /a3)
    (add_net /a4)
    (add_net /a5)
    (add_net /a6)
    (add_net /a7)
    (add_net /a8)
    (add_net /a9)
    (add_net /d0)
    (add_net /d1)
    (add_net /d2)
    (add_net /d3)
    (add_net /d4)
    (add_net /d5)
    (add_net /d6)
    (add_net /d7)
    (add_net /~CE)
    (add_net /~CEO)
    (add_net /~OE)
    (add_net /~WE)
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.3048)
    (via_dia 0.635)
    (via_drill 0.3048)
    (uvia_dia 0.0254)
    (uvia_drill 0)
    (add_net /VBAT1)
    (add_net /VBAT2)
    (add_net /VCCI)
    (add_net /VCCO)
    (add_net GND)
  )
  (module Housings_DIP:DIP-28_W15.24mm_Socket (layer F.Cu) (tedit 593F0E9F)
    (at 104.14 53.34)
    (descr "28-lead dip package, row spacing 15.24 mm (600 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 15.24mm 600mil Socket")
    (fp_text reference J3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 62256 (at 7.62 35.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /a14))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /d3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /a12))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /d4))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /a7))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /d5))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /a6))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /d6))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /a5))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /d7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /a4))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /~CE))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /a3))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /a10))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /a2))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /~OE))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /a1))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /a11))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /a0))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /a9))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /d0))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /a8))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /d1))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /a13))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /d2))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /~WE))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /VCCI))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 593EEF2D)
    (at 111.76 60.325 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -3.175 0 450) (layer B.SilkS))
    (fp_text value 100n (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at -3.175 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 25 /VCCO))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module nelis_footprints:soljump_no_1 (layer B.Cu) (tedit 593EEE0D)
    (at 113.9825 57.785 180)
    (fp_text reference JP1 (at -2.54 0 450) (layer B.SilkS) hide)
    (fp_text value soljump_nc_1 (at 0 -1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 0.5 1.6) (layers B.Cu B.Paste B.Mask)
      (net 25 /VCCO))
    (pad 2 smd rect (at 1.1 0 180) (size 0.5 1.6) (layers B.Cu B.Paste B.Mask)
      (net 29 /TOL))
    (pad 1 smd rect (at -0.3 0.6 180) (size 1.6 0.4) (layers B.Cu B.Paste B.Mask)
      (net 25 /VCCO))
    (pad 2 smd rect (at 0.3 -0.6 180) (size 1.6 0.4) (layers B.Cu B.Paste B.Mask)
      (net 29 /TOL))
    (pad 2 smd rect (at -0.3 -0.3 180) (size 0.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 29 /TOL))
    (pad 1 smd rect (at 0.3 0.2 180) (size 0.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 25 /VCCO))
  )
  (module nelis_footprints:soljump_no_1 (layer B.Cu) (tedit 593EEE09)
    (at 109.5375 57.785 180)
    (fp_text reference JP2 (at 2.54 0 450) (layer B.SilkS) hide)
    (fp_text value soljump_no_1 (at 0 -1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 0.5 1.6) (layers B.Cu B.Paste B.Mask)
      (net 29 /TOL))
    (pad 2 smd rect (at 1.1 0 180) (size 0.5 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.3 0.6 180) (size 1.6 0.4) (layers B.Cu B.Paste B.Mask)
      (net 29 /TOL))
    (pad 2 smd rect (at 0.3 -0.6 180) (size 1.6 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.3 -0.3 180) (size 0.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.3 0.2 180) (size 0.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 29 /TOL))
  )
  (module Housings_SOIC:SOIC-16W_7.5x10.3mm_Pitch1.27mm (layer B.Cu) (tedit 593F0FEA)
    (at 111.76 68.58 180)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at 0 -0.635 180) (layer B.SilkS))
    (fp_text value DS1210S (at 0 -6.25 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -4.65 4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -4.65 3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 25 /VCCO))
    (pad 3 smd rect (at -4.65 1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -4.65 0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 27 /VBAT1))
    (pad 5 smd rect (at -4.65 -0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -4.65 -1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 29 /TOL))
    (pad 7 smd rect (at -4.65 -3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at -4.65 -4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.65 -4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 26 /~CE))
    (pad 10 smd rect (at 4.65 -3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 4.65 -1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 28 /~CEO))
    (pad 12 smd rect (at 4.65 -0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 4.65 0.635 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 /VBAT2))
    (pad 14 smd rect (at 4.65 1.905 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 4.65 3.175 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 /VCCI))
    (pad 16 smd rect (at 4.65 4.445 180) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16W_7.5x10.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-28W_7.5x17.9mm_Pitch1.27mm (layer F.Cu) (tedit 593F0FDD)
    (at 111.76 68.58)
    (descr "28-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC2 (at 0 0.635) (layer F.SilkS))
    (fp_text value 62256 (at 0 10.05) (layer F.Fab))
    (fp_text user %R (at 0 0.635) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /a14))
    (pad 2 smd rect (at -4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /a12))
    (pad 3 smd rect (at -4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /a7))
    (pad 4 smd rect (at -4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /a6))
    (pad 5 smd rect (at -4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /a5))
    (pad 6 smd rect (at -4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /a4))
    (pad 7 smd rect (at -4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /a3))
    (pad 8 smd rect (at -4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /a2))
    (pad 9 smd rect (at -4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /a1))
    (pad 10 smd rect (at -4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /a0))
    (pad 11 smd rect (at -4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /d0))
    (pad 12 smd rect (at -4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /d1))
    (pad 13 smd rect (at -4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /d2))
    (pad 14 smd rect (at -4.7 8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 4.7 8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /d3))
    (pad 16 smd rect (at 4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /d4))
    (pad 17 smd rect (at 4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /d5))
    (pad 18 smd rect (at 4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /d6))
    (pad 19 smd rect (at 4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /d7))
    (pad 20 smd rect (at 4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /~CEO))
    (pad 21 smd rect (at 4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /a10))
    (pad 22 smd rect (at 4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /~OE))
    (pad 23 smd rect (at 4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /a11))
    (pad 24 smd rect (at 4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /a9))
    (pad 25 smd rect (at 4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /a8))
    (pad 26 smd rect (at 4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /a13))
    (pad 27 smd rect (at 4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /~WE))
    (pad 28 smd rect (at 4.7 -8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /VCCO))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-28W_7.5x17.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 593F0DCA)
    (at 115.57 86.36 270)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J1 (at -2.54 -1.905 360) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at -2.54 -1.905 360) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /VBAT1))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /VBAT2))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_text "Duck&Cover\nElectronics\nIJmuiden\nHolland" (at 111.76 55.5625) (layer F.Cu))
  (gr_text 1 (at 116.84 62.865) (layer B.SilkS))
  (gr_text 1 (at 106.3625 59.055) (layer F.SilkS))
  (gr_text TOL (at 111.76 53.975) (layer B.SilkS))
  (gr_line (start 102.5525 87.9475) (end 102.5525 51.7525) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.9675 87.9475) (end 102.5525 87.9475) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.9675 51.7525) (end 120.9675 87.9475) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.5525 51.7525) (end 120.9675 51.7525) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "DS1230/35\nEliminator\n20170612-01" (at 111.76 80.645) (layer F.SilkS))
  (gr_text G (at 115.57 84.1375) (layer B.SilkS))
  (gr_text B2 (at 110.49 84.1375) (layer B.SilkS))
  (gr_text B1 (at 113.03 84.1375) (layer B.SilkS))
  (gr_text G (at 107.95 84.1375) (layer B.SilkS))
  (gr_text G (at 107.95 84.1375) (layer F.SilkS))
  (gr_text G (at 115.57 84.1375) (layer F.SilkS))
  (gr_text B2 (at 110.49 84.1375) (layer F.SilkS))
  (gr_text LO (at 113.9825 55.88) (layer B.SilkS))
  (gr_text HI (at 109.5375 55.88) (layer B.SilkS))
  (gr_text BOT (at 106.045 86.36) (layer B.Cu))
  (gr_text TOP (at 106.045 86.36) (layer F.Cu))
  (gr_text B1 (at 113.03 84.1375) (layer F.SilkS))
  (gr_text "Duck&Cover\nElectronics\nIJmuiden\nHolland" (at 111.76 55.5625) (layer F.Mask))
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.1575 82.8675) (xy 106.3625 82.8675) (xy 106.3625 80.3275) (xy 117.1575 80.3275)
      )
    )
  )
)
