(kicad_pcb (version 20171130) (host pcbnew 5.1.0-5.1.0)
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 423)
    (zones 0)
    (modules 40)
    (nets 39)
  )
  (page USLetter)
  (title_block
    (title "T-962 Temp Monitor and Fan Controller")
    (date 2019-03-27)
    (rev 1.2.3)
    (company "Copyright © 2018 by Aaron Williams")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.51)
    (via_min_drill 0.3)
    (user_via 0.51 0.3)
    (user_via 0.6 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0504)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 /FAN_PWM)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 +12V)
  (net 5 /DQ)
  (net 6 /D+)
  (net 7 /D-)
  (net 8 /P_D-)
  (net 9 +5V)
  (net 10 /P_D+)
  (net 11 "Net-(U5-Pad1)")
  (net 12 /FAN_PWM_OUT)
  (net 13 /N_ISP)
  (net 14 /N_RST)
  (net 15 /TXD0)
  (net 16 /RXD0)
  (net 17 /T1+)
  (net 18 /T1-)
  (net 19 /T0-)
  (net 20 /T0+)
  (net 21 /T2+)
  (net 22 /T2-)
  (net 23 /T3-)
  (net 24 /T3+)
  (net 25 "Net-(R3-Pad2)")
  (net 26 "Net-(J8-Pad4)")
  (net 27 "Net-(U5-Pad11)")
  (net 28 "Net-(U5-Pad12)")
  (net 29 "Net-(U5-Pad13)")
  (net 30 "Net-(U5-Pad14)")
  (net 31 "Net-(U5-Pad15)")
  (net 32 "Net-(U5-Pad17)")
  (net 33 "Net-(U5-Pad18)")
  (net 34 "Net-(U5-Pad19)")
  (net 35 "Net-(U5-Pad22)")
  (net 36 "Net-(U5-Pad23)")
  (net 37 "Net-(U5-Pad24)")
  (net 38 "Net-(R4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net /D+)
    (add_net /D-)
    (add_net /DQ)
    (add_net /FAN_PWM)
    (add_net /FAN_PWM_OUT)
    (add_net /N_ISP)
    (add_net /N_RST)
    (add_net /P_D+)
    (add_net /P_D-)
    (add_net /RXD0)
    (add_net /T0+)
    (add_net /T0-)
    (add_net /T1+)
    (add_net /T1-)
    (add_net /T2+)
    (add_net /T2-)
    (add_net /T3+)
    (add_net /T3-)
    (add_net /TXD0)
    (add_net GND)
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad13)")
    (add_net "Net-(U5-Pad14)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad17)")
    (add_net "Net-(U5-Pad18)")
    (add_net "Net-(U5-Pad19)")
    (add_net "Net-(U5-Pad22)")
    (add_net "Net-(U5-Pad23)")
    (add_net "Net-(U5-Pad24)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 165.862 61.468)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J9 (at 0.762 7.112) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /N_ISP))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /N_RST))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 155 51.025 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference D1 (at 0 -2.9 90) (layer F.SilkS))
    (fp_text value USBLC6-2SC6 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 /D+))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 /D-))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 /P_D-))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 /P_D+))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B02B-XH-AM_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 163.7 46 90)
    (descr "JST XH series connector, B02B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry boss")
    (fp_text reference J6 (at 5.9 2.6 180) (layer F.SilkS))
    (fp_text value "JST XH-B02B-XH-AM" (at 1.25 4.6 90) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 +12V))
    (pad "" np_thru_hole circle (at -1.6 2 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B02B-XH-AM_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 130.3 73.7 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 1.5 4.8 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223 (layer F.Cu) (tedit 5A02FF57)
    (at 141.9 43.4)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 -4.5) (layer F.SilkS))
    (fp_text value LD1117S33CTR (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-8_1x08_P2.54mm_Horizontal (layer F.Cu) (tedit 5B1EC514)
    (at 130.8 64.64 90)
    (descr "Terminal Block TE 282834-8, 8 pins, pitch 2.54mm, size 20.78x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-8 pitch 2.54mm size 20.78x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J2 (at -2.66 0 180) (layer F.SilkS))
    (fp_text value "TE 282834-8" (at 8.89 4.37 90) (layer F.Fab))
    (fp_text user %R (at 8.89 2 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 /T3+))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 /T3-))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 /T2+))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 /T2-))
    (pad 5 thru_hole circle (at 10.16 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 /T1+))
    (pad 6 thru_hole circle (at 12.7 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 /T1-))
    (pad 7 thru_hole circle (at 15.24 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 /T0+))
    (pad 8 thru_hole circle (at 17.78 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 /T0-))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-8_1x08_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 137.9 72.1)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H1 (at 3.8 -2.4) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHole:MountingHole_3mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 163.9 72.1)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H2 (at -4 2.5) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHole:MountingHole_3mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 137.9 35.1)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H3 (at 3.2 -2.9) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHole:MountingHole_3mm_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 163.9 35.1)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H4 (at 0 4.2) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Aaron:SW_SPST_KMR2 (layer F.Cu) (tedit 5BBAE414)
    (at 157.9 62.3 90)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW2 (at 1.7 3.4 180) (layer F.SilkS))
    (fp_text value SW_SPST_KMR2 (at 0 2.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.45 90) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /N_RST))
    (pad 2 smd rect (at -2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /N_RST))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_KMR2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/aaronw/kicad/library/aaron/packages3d/KMR231GLFS.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 152.905001 41.7)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 47.5K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 152.9 43.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.43 180) (layer F.SilkS))
    (fp_text value 22.1K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +5V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aaron:QFN-24-1EP_4x4mm_Pitch0.5mm_rounded_corners (layer F.Cu) (tedit 5BBEA763)
    (at 149.85 47.45 180)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U5 (at 0 -3.375 180) (layer F.SilkS))
    (fp_text value CP2102N-A01-QFN24 (at 0 3.375 180) (layer F.Fab))
    (pad 25 smd rect (at -0.65 -0.65 180) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 0.65 180) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65 180) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 0.65 180) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 24 smd roundrect (at -1.25 -1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(U5-Pad24)"))
    (pad 23 smd rect (at -0.75 -1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U5-Pad23)"))
    (pad 22 smd rect (at -0.25 -1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U5-Pad22)"))
    (pad 21 smd rect (at 0.25 -1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /RXD0))
    (pad 20 smd rect (at 0.75 -1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /TXD0))
    (pad 19 smd roundrect (at 1.25 -1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(U5-Pad19)"))
    (pad 18 smd roundrect (at 1.95 -1.25 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(U5-Pad18)"))
    (pad 17 smd rect (at 1.95 -0.75 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U5-Pad17)"))
    (pad 16 smd rect (at 1.95 -0.25 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 1.95 0.25 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U5-Pad15)"))
    (pad 14 smd rect (at 1.95 0.75 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U5-Pad14)"))
    (pad 13 smd roundrect (at 1.95 1.25 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(U5-Pad13)"))
    (pad 12 smd roundrect (at 1.25 1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(U5-Pad12)"))
    (pad 11 smd rect (at 0.75 1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U5-Pad11)"))
    (pad 10 smd rect (at 0.25 1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -0.25 1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R3-Pad2)"))
    (pad 8 smd rect (at -0.75 1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R4-Pad2)"))
    (pad 7 smd roundrect (at -1.25 1.95 270) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 6 smd roundrect (at -1.95 1.25 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 5 smd rect (at -1.95 0.75 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at -1.95 0.25 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /P_D-))
    (pad 3 smd rect (at -1.95 -0.25 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /P_D+))
    (pad 2 smd rect (at -1.95 -0.75 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.95 -1.25 180) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(U5-Pad1)"))
    (model ${KIGIT3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aaron:USB_Micro-B_Molex-105017-0001 (layer F.Cu) (tedit 5BBEAB0D)
    (at 165.2 54 90)
    (descr http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
    (tags "Micro-USB SMD Typ-B")
    (attr smd)
    (fp_text reference J8 (at 3.708 -3.148 180) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0.3 4.3375 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.6875 90) (layer Dwgs.User))
    (fp_text user %R (at 0 0.8875 90) (layer F.Fab))
    (pad 6 smd rect (at 1 1.2375 90) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.5 -1.4625 90) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.65 -1.4625 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 7 /D-))
    (pad 1 smd rect (at -1.3 -1.4625 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 5 smd rect (at 1.3 -1.4625 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 -1.4625 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J8-Pad4)"))
    (pad 3 smd rect (at 0 -1.4625 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 6 /D+))
    (pad 6 thru_hole circle (at 2.5 -1.4625 90) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1 1.2375 90) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -3.5 1.2375 270) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 3.5 1.2375 90) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.9 1.2375 90) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.9 1.2375 90) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex-105017-0001.step
      (offset (xyz 0 -1 1.15))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 147.1 41.2 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -0.7 1.7) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /DQ))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 149.9 43.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.3 0 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aaron:SW_SPST_KMR2 (layer F.Cu) (tedit 5BBAE414)
    (at 157.9 68.85 90)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW1 (at 2.35 3.3 180) (layer F.SilkS))
    (fp_text value SW_SPST_KMR2 (at 0 2.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.45 90) (layer F.Fab))
    (pad 1 smd rect (at -2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /N_ISP))
    (pad 2 smd rect (at -2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /N_ISP))
    (pad 2 smd rect (at 2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_KMR2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/aaronw/kicad/library/aaron/packages3d/KMR231GLFS.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Aaron:TDFN-10_3x4mm_P0.5mm (layer F.Cu) (tedit 5BEFB560)
    (at 142 65.6 270)
    (attr smd)
    (fp_text reference U6 (at 0 -3.8) (layer F.SilkS))
    (fp_text value MAX31850KATB+ (at 0 0 270) (layer F.Fab))
    (pad 10 smd rect (at -1 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -0.5 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 /T3-))
    (pad 8 smd rect (at 0 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 24 /T3+))
    (pad 7 smd rect (at 0.5 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at 0.5 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 6 smd rect (at 1 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at 1 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /DQ))
    (pad 11 smd rect (at 0 0 270) (size 2.3 2.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5BEFE3A7)
    (at 156.7 40.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 2.8 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.2 58.4 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /T2-))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /T2+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.6 66.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 1.4 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.3 64.2 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /T3-))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /T3+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B02B-XH-AM_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 152.3 62.3 180)
    (descr "JST XH series connector, B02B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry boss")
    (fp_text reference J5 (at 4.7 4.2) (layer F.SilkS))
    (fp_text value "JST XH-B02B-XH-AM" (at 1.25 4.6 180) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.6 2 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 +12V))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 12 /FAN_PWM_OUT))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B02B-XH-AM_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B02B-XH-AM_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B7754C5)
    (at 131.8 34.4 270)
    (descr "JST XH series connector, B02B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry boss")
    (fp_text reference J3 (at 5.1 -3.7) (layer F.SilkS))
    (fp_text value "JST XH-B02B-XH-AM" (at 1.25 4.6 270) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 +12V))
    (pad "" np_thru_hole circle (at -1.6 2 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B02B-XH-AM_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 153.2 33.7 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.7) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /DQ))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /FAN_PWM))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 153.26 55.3 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J10 (at 0 -3.06 180) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /D+))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D-))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 153.6 73.3 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "2.54mm pin header" (at 0 12.49 270) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /N_ISP))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /N_RST))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /TXD0))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /RXD0))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 148.6 38.2 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0.8 1.5) (layer F.SilkS))
    (fp_text value 100K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /FAN_PWM))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aaron:TDFN-10_3x4mm_P0.5mm (layer F.Cu) (tedit 5BEFB560)
    (at 141.9 48.8 270)
    (attr smd)
    (fp_text reference U1 (at 0 -3.8) (layer F.SilkS))
    (fp_text value MAX31850KATB+ (at 0 0 270) (layer F.Fab))
    (pad 11 smd rect (at 0 0 270) (size 2.3 2.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /DQ))
    (pad 6 smd rect (at 1 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.5 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 7 smd rect (at 0.5 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /T0+))
    (pad 8 smd rect (at 0 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /T0-))
    (pad 9 smd rect (at -0.5 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -1 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
  )
  (module Aaron:TDFN-10_3x4mm_P0.5mm (layer F.Cu) (tedit 5BEFB560)
    (at 141.9 53.7 270)
    (attr smd)
    (fp_text reference U3 (at 0 -3.8) (layer F.SilkS))
    (fp_text value MAX31850KATB+ (at 0 0 270) (layer F.Fab))
    (pad 10 smd rect (at -1 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -0.5 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /T1-))
    (pad 8 smd rect (at 0 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /T1+))
    (pad 7 smd rect (at 0.5 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.5 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 6 smd rect (at 1 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at 1 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /DQ))
    (pad 11 smd rect (at 0 0 270) (size 2.3 2.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Aaron:TDFN-10_3x4mm_P0.5mm (layer F.Cu) (tedit 5BEFB560)
    (at 141.9 59.7 270)
    (attr smd)
    (fp_text reference U4 (at 0 -3.9) (layer F.SilkS))
    (fp_text value MAX31850KATB+ (at 0 0 270) (layer F.Fab))
    (pad 11 smd rect (at 0 0 270) (size 2.3 2.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /DQ))
    (pad 6 smd rect (at 1 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.5 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 7 smd rect (at 0.5 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /T2+))
    (pad 8 smd rect (at 0 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 22 /T2-))
    (pad 9 smd rect (at -0.5 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -1 -1.92 270) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 136.7 47.4 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.2 0 180) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /T0+))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /T0-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 147.1 38.1875 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0.8875 -1.7 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.5 54.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.5) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.2 52.3 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -0.6 -1.3 90) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /T1-))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /T1+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.5 60.7)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 1.3) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.7 42.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 2.4 0) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.5 49.7)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -0.7 1.3) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer F.Cu) (tedit 5A02FF57)
    (at 149.565001 41)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q1 (at 1.334999 -1.9) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.65 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /FAN_PWM))
    (pad 2 smd rect (at -1 0.65 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /FAN_PWM_OUT))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text ISP (at 163.068 66.548) (layer B.SilkS))
  (gr_text GND (at 163.068 64.008) (layer B.SilkS))
  (gr_text RST (at 163.068 61.468) (layer B.SilkS))
  (gr_text GND (at 162.814 64.262) (layer F.SilkS))
  (gr_text "12V\nOUT" (at 156.9 46.4) (layer F.SilkS))
  (gr_text "+\n-" (at 160.1 44.9) (layer F.SilkS))
  (gr_text "J4:\n1 - GND\n2 - +3.3V" (at 160 45.2) (layer B.SilkS))
  (gr_text "+3\n\nGND" (at 131.7 72.4) (layer F.SilkS))
  (gr_text "J1:\n1 - DQ\n2 - FAN PWM (DAC0)\n3 - GND" (at 157.9 36.8) (layer B.SilkS))
  (gr_text "J3: 12V in\nJ5: Fan out\nJ6: 12V out" (at 160.45 68.475) (layer B.SilkS))
  (gr_text "J10: (USB)\n1 - GND\n2 - D+\n3 - D-\n4 - +5V" (at 146.3 45.1) (layer B.SilkS))
  (gr_text "J7:\n1 - N_ISP\n2 - N_RST\n3 - TXD0\n4 - RXD0\n5 - GND" (at 146.5 59.9) (layer B.SilkS))
  (gr_text "+ -" (at 151.2 65.5) (layer F.SilkS))
  (gr_text - (at 135.1 32.1) (layer F.SilkS))
  (gr_text + (at 135.1 37.7) (layer F.SilkS))
  (gr_text "12V In" (at 131.8 40.8) (layer F.SilkS))
  (gr_text "Rev 1.2.3" (at 156.7 37.6) (layer F.SilkS))
  (gr_text "Copyright © 2018\nAaron Williams" (at 155.448 57.912) (layer B.SilkS))
  (gr_text +T3- (at 135 63.3 90) (layer F.SilkS))
  (gr_text +T2- (at 135 58.3 90) (layer F.SilkS))
  (gr_text +T1- (at 135 53.2 90) (layer F.SilkS))
  (gr_text +T0- (at 135 48.2 90) (layer F.SilkS))
  (gr_text "GN FN DQ" (at 150.6 35.8) (layer F.SilkS))
  (gr_text "GN D+ D- +5" (at 157.2 57.5) (layer F.SilkS))
  (gr_text RST (at 161.7 62.3) (layer F.SilkS))
  (gr_text ISP (at 161.5 68.2) (layer F.SilkS))
  (gr_text "GN RX TX NR NI" (at 148.3 71.3) (layer F.SilkS))
  (gr_text "FAN OUT" (at 151.2 67.5) (layer F.SilkS))
  (gr_line (start 167.9 76.1) (end 163.8 76.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.9 31.1) (end 167.9 76.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.9 76.1) (end 163.8 76.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.9 31.1) (end 127.9 76.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.9 31.1) (end 127.9 31.1) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.8 31.2) (xy 167.8 31.2) (xy 167.846034 76.1) (xy 127.953966 76.1)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.9 31.1) (xy 167.9 31.1) (xy 167.9 76.1) (xy 127.9 76.1)
      )
    )
  )
)
