<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="21" y2="0" width="0" layer="20"/>
<wire x1="21" y1="0" x2="21" y2="34" width="0" layer="20"/>
<wire x1="21" y1="34" x2="0" y2="34" width="0" layer="20"/>
<wire x1="0" y1="34" x2="0" y2="0" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>ISP</text>
<text>Skylighting R3</text>
<text>Made At Noisebridge</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="DIODE-1N4148">
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="AVRISP">
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,54/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
<package name="1,6/0,9">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="phrobo">
<packages>
<package name="OSTOQ023251">
</package>
<package name="PHROBO-LOGO">
</package>
</packages>
</library>
<library name="attiny48">
<packages>
<package name="QFN50P500X500X100-33N">
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_8X200_NOTEXT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="7085" library="SparkFun" package="78XXL" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CLOCK" library="wirepad" package="2,54/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun" package="DIODE-1N4148" value=""/>
<element name="DATA" library="wirepad" package="2,54/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="2,54/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6"/>
<element name="LED_VCC" library="wirepad" package="2,54/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun" package="TACTILE_SWITCH_SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="E2,5-6" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VCC" library="phrobo" package="OSTOQ023251" value="OSTOQ023251">
<attribute name="NAME"/>
</element>
<element name="U1" library="attiny48" package="QFN50P500X500X100-33N" value="ATTINY48-MU">
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="OC_NEWARK" value="68T3773"/>
<attribute name="MPN" value="ATTINY48-MU"/>
<attribute name="SUPPLIER" value="ATMEL"/>
<attribute name="OC_FARNELL" value="1748547"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD0" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD1" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD2" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD3" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD4" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD5" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD6" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PD7" library="wirepad" package="1,6/0,9" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun" package="SJ_2S-NO" value="LED_VCC = VCC">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="phrobo" package="PHROBO-LOGO" value=""/>
<element name="U$2" library="ohw-logo" package="OSHW_8X200_NOTEXT" value=""/>
</elements>
<signals>
<signal name="N$6">
<contactref element="7085" pad="IN"/>
<contactref element="VCC" pad="P$1"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="ISP1" pad="6"/>
<contactref element="7085" pad="GND"/>
<contactref element="C1" pad="-"/>
<contactref element="GND" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="33"/>
<contactref element="VCC" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="ISP1" pad="2"/>
<contactref element="7085" pad="OUT"/>
<contactref element="C1" pad="+"/>
<contactref element="D1" pad="A"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="N$4">
<contactref element="ISP1" pad="5"/>
<contactref element="S1" pad="3"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="MOSI">
<contactref element="ISP1" pad="4"/>
<contactref element="U1" pad="15"/>
<contactref element="DATA" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="ISP1" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="SCK">
<contactref element="ISP1" pad="3"/>
<contactref element="U1" pad="17"/>
<contactref element="CLOCK" pad="1"/>
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$32">
<contactref element="U1" pad="30"/>
<contactref element="PD0" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="PD1" pad="1"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="N$34">
<contactref element="U1" pad="32"/>
<contactref element="PD2" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="PD3" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="U1" pad="2"/>
<contactref element="PD4" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="PD5" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$38">
<contactref element="U1" pad="10"/>
<contactref element="PD6" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="PD7" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="N$40">
<contactref element="LED_VCC" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$5">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$18">
</signal>
<signal name="N$20">
</signal>
<signal name="N$22">
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="N$31">
</signal>
<signal name="N$41">
</signal>
<signal name="N$42">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="N$46">
</signal>
<signal name="N$47">
</signal>
<signal name="N$48">
</signal>
<signal name="N$49">
</signal>
</signals>
</board>
</drawing>
</eagle>
