<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="8.89" y1="3.81" x2="83.82" y2="3.81" width="0" layer="20"/>
<wire x1="83.82" y1="3.81" x2="85.09" y2="5.08" width="0" layer="20" curve="90"/>
<wire x1="85.09" y1="5.08" x2="85.09" y2="58.42" width="0" layer="20"/>
<wire x1="85.09" y1="58.42" x2="83.82" y2="59.69" width="0" layer="20" curve="90"/>
<wire x1="83.82" y1="59.69" x2="69.596" y2="59.69" width="0" layer="20"/>
<wire x1="69.596" y1="59.69" x2="68.326" y2="58.42" width="0" layer="20" curve="90"/>
<wire x1="68.326" y1="58.42" x2="68.326" y2="50.546" width="0" layer="20"/>
<wire x1="68.326" y1="50.546" x2="67.31" y2="49.53" width="0" layer="20" curve="-90"/>
<wire x1="67.31" y1="49.53" x2="25.4" y2="49.53" width="0" layer="20"/>
<wire x1="25.4" y1="49.53" x2="24.13" y2="50.8" width="0" layer="20" curve="-90"/>
<wire x1="24.13" y1="50.8" x2="24.13" y2="58.42" width="0" layer="20"/>
<wire x1="24.13" y1="58.42" x2="22.86" y2="59.69" width="0" layer="20" curve="90"/>
<wire x1="22.86" y1="59.69" x2="8.89" y2="59.69" width="0" layer="20"/>
<wire x1="8.89" y1="59.69" x2="7.62" y2="58.42" width="0" layer="20" curve="90"/>
<wire x1="7.62" y1="58.42" x2="7.62" y2="5.08" width="0" layer="20"/>
<wire x1="7.62" y1="5.08" x2="8.89" y2="3.81" width="0" layer="20" curve="104.477512"/>
<text>NCIDdisplay
LED Matrix Shield
ncid.sourceforge.net
</text>
<text>+</text>
<text>-</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>SCL</text>
<text>IR</text>
<text>5V</text>
<text>GND</text>
<text>IR</text>
<text>5V</text>
<text>GND</text>
<text>This side faces LED panel
when assembled.
</text>
<text>Arduino plugs into this side
when assembled.
</text>
<text>*</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>Rev A</text>
</plain>
<libraries>
<library name="SparkFun-Boards2">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="UNO_R3_SHIELD">
<description>Uno R3 Compatible Board Layout</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="1X03">
</package>
<package name="2X5_NOSILK">
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="SOLDERJUMPER_REFLOW_NOPASTE">
</package>
</packages>
</library>
<library name="cclogo">
<packages>
<package name="CC-BY-SA">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Boards2" package="UNO_R3_SHIELD" value="ARDUINO_R3_SHIELD"/>
<element name="PWR" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH"/>
<element name="IR1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IR2" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X5_NOSILK" value="M05X2NO_SILK">
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="2X5_NOSILK" value="M05X2NO_SILK">
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="2X5_NOSILK" value="M05X2NO_SILK">
<attribute name="NAME"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="2X5_NOSILK" value="M05X2NO_SILK">
<attribute name="NAME"/>
</element>
<element name="YUN_5V" library="microbuilder" package="SOLDERJUMPER_REFLOW_NOPASTE" value=""/>
<element name="U$2" library="cclogo" package="CC-BY-SA" value=""/>
<element name="PWR1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="5V"/>
<contactref element="PWR" pad="PWR"/>
<contactref element="IR1" pad="3"/>
<contactref element="IR2" pad="3"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="YUN_5V" pad="1"/>
<contactref element="PWR1" pad="PWR"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="GND@2"/>
<contactref element="U$1" pad="GND@1"/>
<contactref element="U$1" pad="GND@0"/>
<contactref element="PWR" pad="GNDBREAK"/>
<contactref element="PWR" pad="GND"/>
<contactref element="IR1" pad="2"/>
<contactref element="IR2" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP4" pad="6"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP5" pad="10"/>
<contactref element="JP6" pad="10"/>
<contactref element="PWR1" pad="GNDBREAK"/>
<contactref element="PWR1" pad="GND"/>
</signal>
<signal name="WR">
<contactref element="JP1" pad="7"/>
<contactref element="JP4" pad="7"/>
<contactref element="U$1" pad="A2"/>
</signal>
<signal name="DTA">
<contactref element="JP1" pad="8"/>
<contactref element="JP4" pad="8"/>
<contactref element="U$1" pad="A1"/>
</signal>
<signal name="CS0">
<contactref element="U$1" pad="D4"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="CS1">
<contactref element="U$1" pad="D5"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="CS2">
<contactref element="U$1" pad="D6"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="CS3">
<contactref element="U$1" pad="D7"/>
<contactref element="JP5" pad="4"/>
<contactref element="JP6" pad="4"/>
</signal>
<signal name="CS4">
<contactref element="U$1" pad="D8"/>
<contactref element="JP5" pad="5"/>
<contactref element="JP6" pad="5"/>
</signal>
<signal name="TLS1">
<contactref element="U$1" pad="D9"/>
<contactref element="JP5" pad="6"/>
<contactref element="JP6" pad="6"/>
</signal>
<signal name="CS6">
<contactref element="JP5" pad="7"/>
<contactref element="JP6" pad="7"/>
<contactref element="U$1" pad="A3"/>
</signal>
<signal name="CS7_IR">
<contactref element="JP5" pad="8"/>
<contactref element="JP6" pad="8"/>
<contactref element="IR1" pad="1"/>
<contactref element="U$1" pad="A0"/>
<contactref element="IR2" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="SDA"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="SCL"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="VIN"/>
<contactref element="YUN_5V" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
