(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 140)
    (no_connects 0)
    (area 57.89712 36.4011 80.78782 91.540801)
    (thickness 1.6)
    (drawings 4)
    (tracks 980)
    (zones 0)
    (modules 39)
    (nets 51)
  )
  (page User 135.001 140.005)
  (title_block
    (title TinyK20)
    (date 2017-02-01)
    (rev 1)
    (company "University of Nairobi")
    (comment 1 @muriukidavid)
    (comment 2 karibe.co)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.16)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.50622 1.50622)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 154.8638 85.0646)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_00000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror true)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory mfg))
  )
  (net 0 "")
  (net 1 Vregin)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 3V3)
  (net 7 "Net-(C7-Pad2)")
  (net 8 "Net-(C10-Pad1)")
  (net 9 RESET)
  (net 10 /x-)
  (net 11 /x+)
  (net 12 Vreg)
  (net 13 D-)
  (net 14 D+)
  (net 15 "Net-(CON1-Pad6)")
  (net 16 "Net-(D2-Pad1)")
  (net 17 PTD4)
  (net 18 VBATT)
  (net 19 UART1_TX)
  (net 20 UART1_RX)
  (net 21 PTC1)
  (net 22 PTC0)
  (net 23 PTB16)
  (net 24 PTB17)
  (net 25 PTB0)
  (net 26 PTB1)
  (net 27 PTB2)
  (net 28 PTB3)
  (net 29 PTA4)
  (net 30 PTA3)
  (net 31 PTA2)
  (net 32 PTA1)
  (net 33 PTA0)
  (net 34 PTD7)
  (net 35 PTD6)
  (net 36 PTD5)
  (net 37 PTD3)
  (net 38 PTD2)
  (net 39 PTD1)
  (net 40 PTD0)
  (net 41 PTC7)
  (net 42 PTC6)
  (net 43 PTC5)
  (net 44 PTC2)
  (net 45 "Net-(R2-Pad2)")
  (net 46 "Net-(R3-Pad2)")
  (net 47 "Net-(P38-Pad2)")
  (net 48 5V)
  (net 49 "Net-(U1-Pad14)")
  (net 50 "Net-(U1-Pad15)")
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /x+)
    (add_net /x-)
    (add_net D+)
    (add_net D-)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(CON1-Pad6)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(P38-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net PTA0)
    (add_net PTA1)
    (add_net PTA2)
    (add_net PTA3)
    (add_net PTA4)
    (add_net PTB0)
    (add_net PTB1)
    (add_net PTB16)
    (add_net PTB17)
    (add_net PTB2)
    (add_net PTB3)
    (add_net PTC0)
    (add_net PTC1)
    (add_net PTC2)
    (add_net PTC5)
    (add_net PTC6)
    (add_net PTC7)
    (add_net PTD0)
    (add_net PTD1)
    (add_net PTD2)
    (add_net PTD3)
    (add_net PTD4)
    (add_net PTD5)
    (add_net PTD6)
    (add_net PTD7)
    (add_net RESET)
    (add_net UART1_RX)
    (add_net UART1_TX)
    (add_net VBATT)
    (add_net Vreg)
    (add_net Vregin)
  )
  (net_class POWER ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3V3)
    (add_net 5V)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 587E1741)
    (at 66.35242 45.72 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -1.4351 -1.1811 90) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_Round_Horizontal_2mm (layer F.Cu) (tedit 589F5CBF)
    (at 64.09182 54.9148)
    (descr "Crystal, Quarz, Rundgehaeuse, round, horizontal, liegend, Uhrenquarz, Diam. 2mm,")
    (tags "Crystal Quarz Rundgehaeuse round horizontal liegend Uhrenquarz Diam. 2mm")
    (fp_text reference Y2 (at -1.63352 -1.61036) (layer F.SilkS))
    (fp_text value 32.768kHz (at 0.000001 3.81) (layer F.Fab))
    (pad 1 thru_hole oval (at -0.521 0) (size 0.8 1.4) (drill 0.4 (offset 0 -0.3)) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U1-Pad15)"))
    (pad 2 thru_hole oval (at 0.6721 0) (size 0.8 1.4) (drill 0.4 (offset 0 -0.3)) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U1-Pad14)"))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 587E1ABE)
    (at 63.08852 41.3893 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -1.9304 0.0127 360) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 Vregin))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 587E1827)
    (at 69.36232 46.9011 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.35636 0.9271 180) (layer F.SilkS))
    (fp_text value 2.2u (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58A1D535)
    (at 69.35978 48.72228 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 1.50876 0.89408 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58A1E6C9)
    (at 66.40322 49.0982 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.9652 1.0922 90) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58A1E6F0)
    (at 64.01562 50.6603 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -1.2192 1.016 360) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 587C8E67)
    (at 75.14082 51.3207 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 2.2004 -0.0762 90) (layer F.SilkS))
    (fp_text value 2.2u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58A1E6DD)
    (at 66.75882 51.5874 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -0.18034 -1.34366 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 587E1A9E)
    (at 63.40602 57.6359 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 2.2225 0 360) (layer F.SilkS))
    (fp_text value 100nF (at 0.0094 -0.1016 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 587C8EA9)
    (at 65.47612 68.6435 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 2.2479 -0.1651 270) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 RESET))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 587A8705)
    (at 70.92442 83.1215 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at -2.6035 -0.5588 270) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 587E17B5)
    (at 75.21702 47.37608 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at -1.1328 -1.15824 180) (layer F.SilkS))
    (fp_text value BAS40-05 (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 48 5V))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 48 5V))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 Vregin))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 587C8EE5)
    (at 74.46552 80.7974)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference D2 (at 0.4953 1.6129) (layer F.SilkS))
    (fp_text value LED (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 PTD4))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 587C9245)
    (at 63.49238 45.57522 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D3 (at 1.08966 -1.33858 180) (layer F.SilkS))
    (fp_text value BAS40-05 (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 18 VBATT))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C10-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch1.27mm (layer F.Cu) (tedit 587C8F27)
    (at 64.76492 73.0123 90)
    (descr "Through hole pin header, pitch 1.27mm")
    (tags "pin header")
    (fp_text reference P35 (at 0.3302 -1.4224 90) (layer F.SilkS))
    (fp_text value CONN_5X2 (at 0 6.9 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.55 1.05) (drill 0.65 (offset -0.3 0)) (layers *.Cu *.Mask F.SilkS)
      (net 6 3V3))
    (pad 3 thru_hole oval (at 0 1.27 90) (size 1.55 1.05) (drill 0.65 (offset -0.3 0)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 2.54 90) (size 1.55 1.05) (drill 0.65 (offset -0.3 0)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 3.81 90) (size 1.55 1.05) (drill 0.65 (offset -0.3 0)) (layers *.Cu *.Mask F.SilkS)
      (net 20 UART1_RX))
    (pad 9 thru_hole oval (at 0 5.08 90) (size 1.55 1.05) (drill 0.65 (offset -0.3 0)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 1.27 1.27 90) (size 1.55 1.05) (drill 0.65 (offset 0.3 0)) (layers *.Cu *.Mask F.SilkS)
      (net 33 PTA0))
    (pad 6 thru_hole oval (at 1.27 2.54 90) (size 1.55 1.05) (drill 0.65 (offset 0.3 0)) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 1.27 3.81 90) (size 1.55 1.05) (drill 0.65 (offset 0.3 0)) (layers *.Cu *.Mask F.SilkS)
      (net 19 UART1_TX))
    (pad 10 thru_hole oval (at 1.27 5.08 90) (size 1.55 1.05) (drill 0.65 (offset 0.3 0)) (layers *.Cu *.Mask F.SilkS)
      (net 9 RESET))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.55 1.05) (drill 0.65 (offset 0.3 0)) (layers *.Cu *.Mask F.SilkS)
      (net 30 PTA3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz 0.025 -0.1 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_QFP:TQFP-48-1EP_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 587E1608)
    (at 70.51322 58.03 270)
    (descr "48-Lead Thin Quad Flatpack (PT) - 7x7x1.0 mm Body [TQFP] With Exposed Pad (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0.0418 -5.7218 270) (layer F.SilkS))
    (fp_text value MK20DX128VFT5 (at 0 5.95 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.2 -2.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at -4.2 -2.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -4.2 -1.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R2-Pad2)"))
    (pad 4 smd rect (at -4.2 -1.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R3-Pad2)"))
    (pad 5 smd rect (at -4.2 -0.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 6 smd rect (at -4.2 -0.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 Vregin))
    (pad 7 smd rect (at -4.2 0.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -4.2 0.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -4.2 1.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 10 smd rect (at -4.2 1.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 11 smd rect (at -4.2 2.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 12 smd rect (at -4.2 2.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 13 smd rect (at -2.75 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (pad 14 smd rect (at -2.25 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at -1.75 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at -1.25 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C10-Pad1)"))
    (pad 17 smd rect (at -0.75 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 PTA0))
    (pad 18 smd rect (at -0.25 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 PTA1))
    (pad 19 smd rect (at 0.25 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 PTA2))
    (pad 20 smd rect (at 0.75 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 PTA3))
    (pad 21 smd rect (at 1.25 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 PTA4))
    (pad 22 smd rect (at 1.75 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 23 smd rect (at 2.25 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 2.75 4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /x-))
    (pad 25 smd rect (at 4.2 2.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /x+))
    (pad 26 smd rect (at 4.2 2.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 RESET))
    (pad 27 smd rect (at 4.2 1.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 PTB0))
    (pad 28 smd rect (at 4.2 1.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 PTB1))
    (pad 29 smd rect (at 4.2 0.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 PTB2))
    (pad 30 smd rect (at 4.2 0.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 PTB3))
    (pad 31 smd rect (at 4.2 -0.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 PTB16))
    (pad 32 smd rect (at 4.2 -0.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 PTB17))
    (pad 33 smd rect (at 4.2 -1.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 PTC0))
    (pad 34 smd rect (at 4.2 -1.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 PTC1))
    (pad 35 smd rect (at 4.2 -2.25 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 PTC2))
    (pad 36 smd rect (at 4.2 -2.75 270) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 UART1_RX))
    (pad 37 smd rect (at 2.75 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 UART1_TX))
    (pad 38 smd rect (at 2.25 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 PTC5))
    (pad 39 smd rect (at 1.75 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 PTC6))
    (pad 40 smd rect (at 1.25 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 PTC7))
    (pad 41 smd rect (at 0.75 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 PTD0))
    (pad 42 smd rect (at 0.25 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 PTD1))
    (pad 43 smd rect (at -0.25 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 PTD2))
    (pad 44 smd rect (at -0.75 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 PTD3))
    (pad 45 smd rect (at -1.25 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 PTD4))
    (pad 46 smd rect (at -1.75 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 PTD5))
    (pad 47 smd rect (at -2.25 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 PTD6))
    (pad 48 smd rect (at -2.75 -4.2) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 PTD7))
    (pad 49 smd rect (at 0.875 0.875 270) (size 1.75 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.875 -0.875 270) (size 1.75 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.875 0.875 270) (size 1.75 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.875 -0.875 270) (size 1.75 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_QFP.3dshapes/TQFP-48-1EP_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58B04714)
    (at 60.43422 41.3004 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 1.143 -1.0795 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 Vregin))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 587C8ED3)
    (at 74.23912 78.7019 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 2.0701 1.3589 180) (layer F.SilkS))
    (fp_text value 1k (at -0.0254 0.254 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer B.Cu) (tedit 587C8AD0)
    (at 72.95642 63.6016)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 0.762) (layer B.SilkS))
    (fp_text value LT1129CST-3.3 (at 0 -0.762) (layer B.Fab) hide)
    (pad 4 smd rect (at 0 3.302) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 -3.302) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2.286 -3.302) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 6 3V3))
    (pad 1 smd rect (at -2.286 -3.302) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 Vregin))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 587C8E78)
    (at 73.51522 75.3618 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -1.524 -1.8034 360) (layer F.SilkS))
    (fp_text value 1k (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 41 PTC7))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(P38-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58A1E37A)
    (at 75.34402 44.8437)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference F1 (at -0.4064 -1.1176) (layer F.SilkS))
    (fp_text value FUSE_F (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 Vreg))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58B04705)
    (at 60.39612 39.7891)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 1.6002 -0.2032) (layer F.SilkS))
    (fp_text value INDUCTOR_F (at 2.5527 0.7112) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CON1-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58A6F1B8)
    (at 69.37502 45.3644 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L2 (at 1.3335 0.4064 270) (layer F.SilkS))
    (fp_text value INDUCTOR_F (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58A1E353)
    (at 72.39762 48.6283)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L3 (at -1.0541 0.7747) (layer F.SilkS))
    (fp_text value INDUCTOR_F (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:CONN-2x5-1.27-SMT (layer F.Cu) (tedit 58774A62)
    (at 66.83502 85.1408)
    (fp_text reference P38 (at 2.032 4.0132) (layer F.SilkS))
    (fp_text value CONN_5X2 (at -0.0762 4.191) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 2.54 -2) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at 2.54 2) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(P38-Pad2)"))
    (pad 3 smd rect (at 1.27 -2) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.27 2) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask)
      (net 43 PTC5))
    (pad 5 smd rect (at 0 -2) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0 2) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -1.27 -2) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask)
      (net 20 UART1_RX))
    (pad 8 smd rect (at -1.27 2) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask)
      (net 19 UART1_TX))
    (pad 9 smd rect (at -2.54 -2) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2.54 2) (size 0.76 2.4) (layers F.Cu F.Paste F.Mask)
      (net 26 PTB1))
    (model Pin_Headers.3dshapes/CONN-2.5-SMT.wrl
      (at (xyz 0 0 0.045))
      (scale (xyz 0.2 0.2 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-353 (layer F.Cu) (tedit 58A21382)
    (at 72.94372 87.3379)
    (descr SOT353)
    (attr smd)
    (fp_text reference U4 (at 1.0541 -0.0254 90) (layer F.SilkS))
    (fp_text value 74AHC1G125 (at 0.2794 0.7874 180) (layer F.Fab))
    (pad 1 smd rect (at -1.016 -0.635) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 25 PTB0))
    (pad 3 smd rect (at -1.016 0.635) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.016 -0.635) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at -1.016 0) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 42 PTC6))
    (pad 4 smd rect (at 1.016 0.635) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(P38-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-353.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.07000000000000001 0.09 0.08))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58A18371)
    (at 72.37222 46.482)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.9398 0.8001) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 D+))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58A1837D)
    (at 72.76592 44.7929)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.9398 0.9398) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 D-))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58A1D782)
    (at 70.49262 50.8635 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.0889 -1.3462 180) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58A1EBC8)
    (at 71.59752 73.5584 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.0955 -0.1143 90) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 RESET))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:CERALOCK-CSTCE8M00G15L99-R0 (layer F.Cu) (tedit 58A1AEAC)
    (at 65.03162 62.7891 270)
    (fp_text reference Y1 (at 0.3048 1.778 270) (layer F.SilkS))
    (fp_text value 8MHz (at 1.143 -1.6891 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 0.38 2) (layers F.Cu F.Paste F.Mask)
      (net 10 /x-))
    (pad 2 smd rect (at 1.2 0 270) (size 0.38 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2.4 0 270) (size 0.38 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /x+))
    (model /home/karibe/Documents/SPH336/newTinyK20/Documentation/CSTE_G15L.wrl
      (at (xyz 0.047 0 -0.002))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 0)
    (at 60.38342 82.3214 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 1.5113 11.2014 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 PTC1))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 PTC0))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 PTB17))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 PTB16))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 PTB3))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 PTB2))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 PTB1))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 PTB0))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 PTA4))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 PTA3))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 PTA2))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 PTA1))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 PTA0))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 VBATT))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 -0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 58A44FA9)
    (at 78.16342 44.2184)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -2.2098 -0.9622) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 1.5494 10.4551 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 PTD7))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 PTD6))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 PTD5))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 PTD4))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 PTD3))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 PTD2))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 PTD1))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 PTD0))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 PTC7))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 PTC6))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 PTC5))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 UART1_TX))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 UART1_RX))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 PTC2))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 -0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 58A451E6)
    (at 75.62342 40.8178 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at 1.8034 3.0988 180) (layer F.SilkS))
    (fp_text value JUMPER_F (at -1.7145 0.2413 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 Vreg))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 Vreg))
  )
  (module Connect:USB_Micro-B_karibe (layer F.Cu) (tedit 58A7136F)
    (at 69.02662 42.5958 180)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference CON1 (at 4.1529 -1.6256 360) (layer F.SilkS))
    (fp_text value USB-MICRO-B (at -0.0635 5.2197 180) (layer F.Fab) hide)
    (pad 3 smd rect (at -0.0009 0 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 D+))
    (pad 6 smd rect (at 3.35 0.125 180) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CON1-Pad6)"))
    (pad 6 smd rect (at 3.9 2.675 180) (size 1.9 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CON1-Pad6)"))
    (pad 4 smd rect (at 0.6491 0 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.2991 0 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.6509 0 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 D-))
    (pad 1 smd rect (at -1.3009 0 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 Vreg))
    (pad 6 smd rect (at -3.35 0.125 180) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CON1-Pad6)"))
    (pad 6 smd rect (at -3.9 2.675 180) (size 1.9 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CON1-Pad6)"))
    (model Connect.3dshapes/USB_MICRO_AB2_SMD.wrl
      (at (xyz 0 -0.22 0.055))
      (scale (xyz 0.41 0.41 0.41))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58A76F26)
    (at 76.32192 83.8294 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 2.1877 -0.0127 270) (layer B.SilkS))
    (fp_text value C (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:sdcard_1051620101 (layer B.Cu) (tedit 58B041B9)
    (at 75.63092 84.4746 180)
    (fp_text reference conn1 (at 6.02 -1.4 180) (layer B.SilkS))
    (fp_text value sdcard_1051620101 (at 5.79 8.61 180) (layer B.Fab))
    (pad P8 smd rect (at 1.5 0.295 180) (size 0.5 1) (layers B.Cu B.Paste B.Mask))
    (pad P7 smd rect (at 2.6 0.295 180) (size 0.5 1) (layers B.Cu B.Paste B.Mask)
      (net 41 PTC7))
    (pad P6 smd rect (at 3.7 0.295 180) (size 0.5 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad P5 smd rect (at 4.8 0.295 180) (size 0.5 1) (layers B.Cu B.Paste B.Mask)
      (net 43 PTC5))
    (pad P4 smd rect (at 5.9 0.295 180) (size 0.5 1) (layers B.Cu B.Paste B.Mask)
      (net 6 3V3))
    (pad P3 smd rect (at 7 0.295 180) (size 0.5 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PTC6))
    (pad P2 smd rect (at 8.1 0.295 180) (size 0.5 1) (layers B.Cu B.Paste B.Mask)
      (net 21 PTC1))
    (pad P1 smd rect (at 9.2 0.295 180) (size 0.5 1) (layers B.Cu B.Paste B.Mask))
    (pad G smd rect (at 0.325 3.305 180) (size 1.05 2.39) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad P9 smd rect (at 10.94 3.18 180) (size 0.72 0.78) (layers B.Cu B.Paste B.Mask)
      (net 22 PTC0))
    (pad G smd rect (at 10.94 4.45 180) (size 1.05 1.08) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad G smd rect (at 10.94 6.855 180) (size 1.05 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad G smd rect (at 0.325 6.285 180) (size 1.05 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad ~ smd rect (at 3.505 7.53 180) (size 2.91 0.55) (layers B.Cu B.Paste B.Mask))
    (pad ~ smd rect (at 7.695 7.53 180) (size 2.91 0.55) (layers B.Cu B.Paste B.Mask))
  )
  (module Buttons_Switches_SMD:SW_SPST_B3SL-1002P (layer F.Cu) (tedit 56ED9E57)
    (at 66.77942 77.8444 180)
    (descr "Middle Stroke Tactile Switch, B3SL")
    (tags "Middle Stroke Tactile Switch")
    (attr smd)
    (fp_text reference B1 (at 0 -4.5 180) (layer F.SilkS))
    (fp_text value Button (at 0 4.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2.875 -2 180) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 2.875 -2 180) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.875 2 180) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 9 RESET))
    (pad 2 smd rect (at -2.875 2 180) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 9 RESET))
  )
  (gr_line (start 80.55102 38.5826) (end 58.04662 38.5826) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 58.04662 91.4908) (end 58.04662 38.5826) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 58.04662 91.4908) (end 80.55102 91.4908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.55102 38.5826) (end 80.55102 91.4908) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.07202 38.608) (xy 58.07202 91.5035) (xy 80.55102 91.5035) (xy 80.55102 38.608)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65.98412 60.0456) (xy 62.08522 60.0329) (xy 62.08522 69.1642) (xy 65.97142 69.1515)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.99962 62.23) (xy 67.05092 62.23) (xy 67.03822 64.2747) (xy 65.34912 66.0273) (xy 62.98692 66.0273)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.17462 78.6638) (xy 74.17562 78.6511) (xy 74.12482 83.1596) (xy 66.18732 83.2231)
      )
    )
  )
)
