(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 11)
    (no_connects 0)
    (area 114.395238 98.3 210.135715 117.400001)
    (thickness 1.6)
    (drawings 35)
    (tracks 26)
    (zones 0)
    (modules 9)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 120 110)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net 3 "Net-(J2-Pad2)")
  (net 4 "Net-(R1-Pad1)")
  (net 5 "Net-(R1-Pad2)")
  (net 6 "Net-(J3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 591B7B37)
    (at 126 111.7)
    (fp_text reference J1 (at 2.5 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:TO-252-2 (layer F.Cu) (tedit 591B6AE9)
    (at 135.6 110)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U1 (at -3.9 0) (layer F.SilkS))
    (fp_text value LD1085Cxx (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at -4.2 2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 2.1 0) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 5 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 5 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 5 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 5 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 591B6AEF)
    (at 120 110)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference MK1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 591B6C6B)
    (at 196.2 110)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference MK2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804)
    (at 178.1 110 180)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R1 (at 0 -2.6 180) (layer F.SilkS))
    (fp_text value .30 (at -0.1 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.1 0 180) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 3.1 0 180) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512 (layer F.Cu) (tedit 58E0A804)
    (at 188.1 110 180)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R2 (at 0 -2.6 180) (layer F.SilkS))
    (fp_text value .33 (at -0.1 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.1 0 180) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 3.1 0 180) (size 1 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 591B7B34)
    (at 126 108.3)
    (fp_text reference J4 (at 2.5 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 6.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 591B7488)
    (at 145 110)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J2 (at 1.2 1.8) (layer F.SilkS) hide)
    (fp_text value "Nichrome Wire" (at 1.27 4.6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
  )
  (module Measurement_Points:Test_Point_2Pads (layer F.Cu) (tedit 591B748B)
    (at 168.7 110)
    (descr "Connecteurs 2 pins")
    (tags "CONN DEV")
    (attr virtual)
    (fp_text reference J3 (at 1.44 1.8) (layer F.SilkS) hide)
    (fp_text value "Nichrome Wire" (at 1.3 4.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.4 1.4) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
  )
  (gr_text - (at 128.4 108.3) (layer F.SilkS))
  (gr_text + (at 128.4 111.7) (layer F.SilkS))
  (dimension 7 (width 0.3) (layer F.Fab)
    (gr_text "7.000 mm" (at 204.35 110 270) (layer F.Fab))
    (feature1 (pts (xy 199.7 113.5) (xy 205.7 113.5)))
    (feature2 (pts (xy 199.7 106.5) (xy 205.7 106.5)))
    (crossbar (pts (xy 203 106.5) (xy 203 113.5)))
    (arrow1a (pts (xy 203 113.5) (xy 202.413579 112.373496)))
    (arrow1b (pts (xy 203 113.5) (xy 203.586421 112.373496)))
    (arrow2a (pts (xy 203 106.5) (xy 202.413579 107.626504)))
    (arrow2b (pts (xy 203 106.5) (xy 203.586421 107.626504)))
  )
  (gr_line (start 199.4 106.5) (end 199.4 113.5) (layer Edge.Cuts) (width 0.15))
  (dimension 82.6 (width 0.3) (layer F.Fab)
    (gr_text "82.600 mm" (at 158.1 99.65) (layer F.Fab))
    (feature1 (pts (xy 199.4 106) (xy 199.4 98.3)))
    (feature2 (pts (xy 116.8 106) (xy 116.8 98.3)))
    (crossbar (pts (xy 116.8 101) (xy 199.4 101)))
    (arrow1a (pts (xy 199.4 101) (xy 198.273496 101.586421)))
    (arrow1b (pts (xy 199.4 101) (xy 198.273496 100.413579)))
    (arrow2a (pts (xy 116.8 101) (xy 117.926504 101.586421)))
    (arrow2b (pts (xy 116.8 101) (xy 117.926504 100.413579)))
  )
  (gr_line (start 116.8 106.5) (end 116.8 113.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.8 106.5) (end 199.4 106.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.4 113.5) (end 116.8 113.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name "Net-(R1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.7 104.1) (xy 145.7 104.1) (xy 145.7 117.4) (xy 130.7 117.4)
      )
    )
  )
)
