(kicad_pcb (version 20171130) (host pcbnew 5.0-dev-unknown)
  (general
    (thickness 1)
    (drawings 5)
    (tracks 156)
    (zones 0)
    (modules 2)
    (nets 4)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.127)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.36)
    (user_trace_width 0.5)
    (user_trace_width 1.3)
    (trace_clearance 0.125)
    (zone_clearance 0.16)
    (zone_45_only yes)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.46)
    (via_drill 0.2)
    (via_min_size 0.46)
    (via_min_drill 0.2)
    (user_via 0.46 0.2)
    (user_via 0.6 0.3)
    (user_via 0.8 0.5)
    (user_via 1.3 1)
    (user_via 2 1)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.3 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.075)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x012fc_80000007)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 r)
  (net 3 b)
  (net_class Default "This is the default net class."
    (clearance 0.125)
    (trace_width 0.127)
    (via_dia 0.46)
    (via_drill 0.2)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
    (add_net b)
    (add_net r)
  )
  (module kicad_pcb:SMA_SW_TAB (layer F.Cu) (tedit 5A4CF845)
    (at 100 126 90)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference J1 (at -2.5 6.5 90) (layer F.SilkS))
    (fp_text value SMA_SW (at -1.05 1.6 90) (layer F.SilkS) hide)
    (fp_line (start -1.9 -0.5) (end 1.9 -0.5) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 1.9 0) (end 1.9 -0.5) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 1.9 0) (end 3.85 0) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -1.9 0) (end -1.9 -0.5) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -3.85 0) (end -3.85 5.75) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 3.85 0) (end 3.85 5.75) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -3.85 0) (end -1.9 0) (layer Edge.Cuts) (width 0.15))
    (pad 3 smd rect (at -3 0.5 90) (size 0.3 1) (layers B.Cu B.Mask)
      (net 3 b) (zone_connect 2))
    (pad 2 smd rect (at -2.5 2.75 90) (size 2 5.5) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.5 2.75 90) (size 2 5.5) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 2.25 5.25 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 1.95 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 2.45 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 3.95 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 1.45 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 4.45 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 4.95 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 3.45 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 2.95 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -2.25 5.25 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 4.95 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 4.45 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 3.95 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 3.45 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 2.95 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 2.45 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 1.95 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 1.45 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.5 1.05 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.45 1.05 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at -2.5 2.75 90) (size 2 5.5) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.65 0.2 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.65 0.2 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.35 0.6 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.35 0.6 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.2 0.2 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.2 0.2 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.05 1 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.05 1 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -0.9 0.6 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 0.9 0.6 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -0.75 0.2 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at 0 0.5 90) (size 0.36 1) (layers F.Cu F.Mask)
      (net 2 r) (zone_connect 2))
    (pad 2 thru_hole rect (at 0.75 0.2 90) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.5 2.75 90) (size 2 5.5) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module kicad_pcb:SMA_SW_TAB (layer F.Cu) (tedit 5A4CF853)
    (at 160 126 270)
    (descr DocString)
    (tags Keywords)
    (attr smd)
    (fp_text reference J2 (at 2.8 6.15 270) (layer F.SilkS))
    (fp_text value SMA_SW (at -1.05 1.6 270) (layer F.SilkS) hide)
    (fp_line (start -3.85 0) (end -1.9 0) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 3.85 0) (end 3.85 5.75) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -3.85 0) (end -3.85 5.75) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -1.9 0) (end -1.9 -0.5) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 1.9 0) (end 3.85 0) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 1.9 0) (end 1.9 -0.5) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -1.9 -0.5) (end 1.9 -0.5) (layer Edge.Cuts) (width 0.15))
    (pad 2 smd rect (at 2.5 2.75 270) (size 2 5.5) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 0.75 0.2 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at 0 0.5 270) (size 0.36 1) (layers F.Cu F.Mask)
      (net 2 r) (zone_connect 2))
    (pad 2 thru_hole rect (at -0.75 0.2 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 0.9 0.6 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -0.9 0.6 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.05 1 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.05 1 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.2 0.2 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.2 0.2 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.35 0.6 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.35 0.6 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.65 0.2 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.65 0.2 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at -2.5 2.75 270) (size 2 5.5) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.45 1.05 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.5 1.05 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 1.45 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 1.95 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 2.45 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 2.95 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 3.45 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 3.95 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 4.45 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -1.75 4.95 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at -2.25 5.25 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 2.95 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 3.45 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 4.95 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 4.45 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 1.45 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 3.95 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 2.45 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 1.75 1.95 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole rect (at 2.25 5.25 270) (size 0.45 0.45) (drill 0.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at 2.5 2.75 270) (size 2 5.5) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 smd rect (at -2.5 2.75 270) (size 2 5.5) (layers B.Cu B.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 3 smd rect (at 3 0.5 270) (size 0.3 1) (layers B.Cu B.Mask)
      (net 3 b) (zone_connect 2))
  )
  (gr_text "line7.kicad_pcb 60 mm OSHPark 2L" (at 121.8 123.25) (layer F.SilkS))
  (gr_text "0.16 mm gap" (at 147.5 128.5) (layer F.SilkS))
  (gr_text "0.8 mm CPWG" (at 147.25 123.25) (layer F.SilkS))
  (gr_line (start 105.75 122.15) (end 154.25 122.15) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.75 129.85) (end 154.25 129.85) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.5 124.5) (xy 160 124.5) (xy 160 127.5) (xy 99.5 127.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.7 124.5) (xy 160 124.5) (xy 160 127.5) (xy 99.7 127.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.75 122.5) (xy 159.75 129.5) (xy 100 129.5) (xy 100 122.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.5 122.5) (xy 160.5 129.5) (xy 99.7 129.5) (xy 99.7 122.5)
      )
    )
  )
)
