(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 0)
    (no_connects 0)
    (area 12.116999 129.718999 38.429001 179.399001)
    (thickness 1.6)
    (drawings 10)
    (tracks 8)
    (zones 0)
    (modules 3)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Desktop:58antenna1 (layer F.Cu) (tedit 0)
    (at 25.273 154.686)
    (fp_text reference Y* (at 0 0) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Desktop:58antenna1-back (layer B.Cu) (tedit 0)
    (at 25.273 167.259)
    (fp_text reference Y* (at 0 0) (layer B.SilkS) hide)
    (fp_text value AntennaBack (at 0.75 0) (layer B.SilkS) hide)
  )
  (module Connectors_Molex:Molex_SMA_Jack_Edge_Mount (layer F.Cu) (tedit 5B0F152D)
    (at 25.273 174.879 90)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference "" (at -1.72 7.11 90) (layer F.SilkS))
    (fp_text value "" (at -1.72 -7.11 90) (layer F.Fab))
    (pad 1 smd rect (at -1.72 0 90) (size 5.08 2.29) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.72 -4.38 90) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.72 4.38 90) (size 5.08 2.42) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.72 -4.38 90) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1.72 4.38 90) (size 5.08 2.42) (layers B.Cu B.Paste B.Mask))
    (pad 2 thru_hole circle (at 1.72 -4.38 90) (size 0.97 0.97) (drill 0.46) (layers *.Cu))
    (pad 2 thru_hole circle (at 1.72 4.38 90) (size 0.97 0.97) (drill 0.46) (layers *.Cu))
    (pad 2 smd rect (at 1.27 -4.38 90) (size 0.89 0.46) (layers F.Cu))
    (pad 2 smd rect (at 1.27 4.38 90) (size 0.89 0.46) (layers F.Cu))
    (pad 2 smd rect (at 1.27 -4.38 90) (size 0.89 0.46) (layers B.Cu))
    (pad 2 smd rect (at 1.27 4.38 90) (size 0.89 0.46) (layers B.Cu))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 12.192 129.794) (end 12.192 179.324) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 38.354 129.794) (end 12.192 129.794) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 38.354 179.324) (end 38.354 129.794) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 12.192 179.324) (end 38.354 179.324) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.225 139.827) (xy 22.225 133.731) (xy 28.448 133.604) (xy 28.448 133.731) (xy 28.448 139.827)
      )
    )
  )
)
