<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<hole x="25.4" y="50.8" drill="1.27"/>
<wire x1="27.94" y1="50.8" x2="22.86" y2="50.8" width="0.254" layer="20" curve="-348.578814"/>
<wire x1="22.86" y1="50.8" x2="27.94" y2="50.8" width="0.254" layer="20" curve="-180"/>
</plain>
<libraries>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="pogo-isp">
<packages>
<package name="AVR-POGO-6ISP">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CR2032-SMD">
</package>
<package name="EVQ-Q2">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="avr-7" package="SOIC14" value="TINY24/44/84-SSU"/>
<element name="BAT1" library="adafruit" package="CR2032-SMD" value="CR2032"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10k"/>
<element name="LED1" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED7" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED8" library="led" package="CHIP-LED0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="0"/>
<element name="R3" library="SparkFun-Resistors" package="0805" value="0"/>
<element name="R4" library="SparkFun-Resistors" package="0805" value="0"/>
<element name="R5" library="SparkFun-Resistors" package="0805" value="0"/>
<element name="R6" library="SparkFun-Resistors" package="0805" value="0"/>
<element name="R7" library="SparkFun-Resistors" package="0805" value="0"/>
<element name="R8" library="SparkFun-Resistors" package="0805" value="0"/>
<element name="R9" library="SparkFun-Resistors" package="0805" value="0"/>
<element name="JP1" library="pogo-isp" package="AVR-POGO-6ISP" value="POGO-6ISP"/>
<element name="SW1" library="adafruit" package="EVQ-Q2" value="SPST_TACT-EVQQ2"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1µF"/>
</elements>
<signals>
<signal name="SCK">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="8"/>
<contactref element="JP1" pad="1"/>
<contactref element="SW1" pad="A'"/>
<contactref element="SW1" pad="A"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="7"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="!RESET">
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="JP1" pad="6"/>
<contactref element="R2" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="BAT1" pad="-"/>
<contactref element="SW1" pad="B'"/>
<contactref element="SW1" pad="B"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="BAT1" pad="+$1"/>
<contactref element="IC1" pad="1"/>
<contactref element="BAT1" pad="+$2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="6"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="3"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="2"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="5"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="10"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="11"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="12"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="13"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="LED4" pad="C"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="LED3" pad="C"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="LED1" pad="C"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="LED2" pad="C"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="LED5" pad="C"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="LED6" pad="C"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="LED7" pad="C"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="LED8" pad="C"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
