(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "3v3")
  (net 7 "SCL_1")
  (net 8 "SDA_1")
  (net 9 "sig_1")
  (net 10 "HV_1")
  (net 11 "SCL_0")
  (net 12 "SDA_0")
  (net 13 "HV_0")
  (net 14 "sig_0")
  (net 15 "SCL_3")
  (net 16 "SDA_3")
  (net 17 "sig_3")
  (net 18 "HV_3")
  (net 19 "SCL_2")
  (net 20 "SDA_2")
  (net 21 "HV_2")
  (net 22 "sig_2")
  (net 23 "unconnected-(U1-Pad3)")
  (net 24 "unconnected-(U2-Pad3)")
  (net 25 "unconnected-(U3-Pad3)")
  (net 26 "unconnected-(U4-Pad3)")
  (net 27 "unconnected-(J1-Pad11)")
  (net 28 "unconnected-(J1-Pad9)")
  (footprint "libraries:detSocket" (layer "F.Cu")
    (tedit 628DCAEE)
    (at 5.08 -12.7)
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Detector_2" (at 2.794 10.668 unlocked) (layer "F.SilkS"))
    (fp_text value "detSocket" (at 0 -6.35 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 3.81 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)") (pinfunction "HV") (pintype "input"))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "sig_2") (pinfunction "Sig") (pintype "input"))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "unconnected-(U3-Pad3)") (pinfunction "Fast") (pintype "input+no_connect"))
    (pad "4" thru_hole circle (at 7.62 7.62) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "SCL_2") (pinfunction "SCL") (pintype "input"))
    (pad "5" thru_hole circle (at 7.62 5.08) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "SDA_2") (pinfunction "SDA") (pintype "input"))
    (pad "6" thru_hole circle (at 7.62 2.54) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "7" thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "3v3") (pinfunction "Vcc") (pintype "input"))
  )
  (footprint "libraries:detSocket" (layer "F.Cu")
    (tedit 628DCAEE)
    (at -12.7 -12.7)
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Detector_1" (at 4.572 10.668 unlocked) (layer "F.SilkS"))
    (fp_text value "detSocket" (at 0 -6.35 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 3.81 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pinfunction "HV") (pintype "input"))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "sig_1") (pinfunction "Sig") (pintype "input"))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 "unconnected-(U2-Pad3)") (pinfunction "Fast") (pintype "input+no_connect"))
    (pad "4" thru_hole circle (at 7.62 7.62) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "SCL_1") (pinfunction "SCL") (pintype "input"))
    (pad "5" thru_hole circle (at 7.62 5.08) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "SDA_1") (pinfunction "SDA") (pintype "input"))
    (pad "6" thru_hole circle (at 7.62 2.54) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "7" thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "3v3") (pinfunction "Vcc") (pintype "input"))
  )
  (footprint "libraries:detSocket" (layer "F.Cu")
    (tedit 628DCAEE)
    (at 5.08 5.08)
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Detector_3" (at 3.048 10.16 unlocked) (layer "F.SilkS"))
    (fp_text value "detSocket" (at 0 -6.35 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 3.81 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)") (pinfunction "HV") (pintype "input"))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "sig_3") (pinfunction "Sig") (pintype "input"))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "unconnected-(U4-Pad3)") (pinfunction "Fast") (pintype "input+no_connect"))
    (pad "4" thru_hole circle (at 7.62 7.62) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "SCL_3") (pinfunction "SCL") (pintype "input"))
    (pad "5" thru_hole circle (at 7.62 5.08) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "SDA_3") (pinfunction "SDA") (pintype "input"))
    (pad "6" thru_hole circle (at 7.62 2.54) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "7" thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "3v3") (pinfunction "Vcc") (pintype "input"))
  )
  (footprint "libraries:detSocket" (layer "F.Cu")
    (tedit 628DCAEE)
    (at -12.7 5.08)
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Detector_0" (at 4.318 10.16 unlocked) (layer "F.SilkS"))
    (fp_text value "detSocket" (at 0 -6.35 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.54 3.81 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)") (pinfunction "HV") (pintype "input"))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "sig_0") (pinfunction "Sig") (pintype "input"))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U1-Pad3)") (pinfunction "Fast") (pintype "input+no_connect"))
    (pad "4" thru_hole circle (at 7.62 7.62) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "SCL_0") (pinfunction "SCL") (pintype "input"))
    (pad "5" thru_hole circle (at 7.62 5.08) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "SDA_0") (pinfunction "SDA") (pintype "input"))
    (pad "6" thru_hole circle (at 7.62 2.54) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "7" thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "3v3") (pinfunction "Vcc") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at -10.16 -11.192 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0.746 1.778 90) (layer "B.SilkS"))
    (fp_text value "200" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 9 "sig_1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 8.128 -11.176 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "200" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 22 "sig_2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 13.716 2.032)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 1.27 1.778) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 15.494 -8.366 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at -2.81 0.254 180) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 20 "SDA_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at -11.684 2.032)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 1.016 1.778) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 15.24 9.144 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at -2.794 -0.254 180) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 16 "SDA_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 2.54 6.096 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "50" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 18 "HV_3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 5 "Net-(C4-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 13.6945 -14.986)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 1.7995 1.778) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at -4.064 -14.986)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 1.016 1.778) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at -7.874 9.144 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0.762 1.65 90) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 12 "SDA_0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at -11.684 -14.986)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 2.54 0.508 90) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at -7.874 13.208 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at -0.227064 -1.524 90) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 11 "SCL_0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at -14.986 6.096 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "50" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 13 "HV_0") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at -14.986 -13.716 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 2.794 0.254 90) (layer "B.SilkS"))
    (fp_text value "50" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 10 "HV_1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 15.494 -4.064 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at -2.794 0 180) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 19 "SCL_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 15.24 13.716 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at -0.762 -2.286 180) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 15 "SCL_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at -7.62 -8.636 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 1.016 1.778 90) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 8 "SDA_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 8.128 8.636 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 2.794 0 180) (layer "B.SilkS"))
    (fp_text value "200" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 17 "sig_3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 8.128 -14.732)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 2.54 0.254 270) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 4 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "molex 5034802000:MOLEX_5034802000" (layer "B.Cu")
    (tedit 628DC20F)
    (at 5.08 1.778)
    (property "MANUFACTURER" "Molex")
    (property "PARTREV" "H")
    (property "STANDARD" "Manufacturer Recommendation")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0.254 -1.8465) (layer "B.SilkS"))
    (fp_text value "5034802000" (at 7.874 -23.241) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.75 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "3v3") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at -4.25 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "SDA_0") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect locked (at -3.75 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "SCL_0") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect locked (at -3.25 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "sig_0") (pinfunction "4") (pintype "passive"))
    (pad "5" smd rect locked (at -2.75 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "HV_0") (pinfunction "5") (pintype "passive"))
    (pad "6" smd rect locked (at -2.25 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "SCL_1") (pinfunction "6") (pintype "passive"))
    (pad "7" smd rect locked (at -1.75 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "SDA_1") (pinfunction "7") (pintype "passive"))
    (pad "8" smd rect locked (at -1.25 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "sig_1") (pinfunction "8") (pintype "passive"))
    (pad "9" smd rect locked (at -0.75 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "unconnected-(J1-Pad9)") (pinfunction "9") (pintype "passive+no_connect"))
    (pad "10" smd rect locked (at -0.25 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "HV_1") (pinfunction "10") (pintype "passive"))
    (pad "11" smd rect locked (at 0.25 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "unconnected-(J1-Pad11)") (pinfunction "11") (pintype "passive+no_connect"))
    (pad "12" smd rect locked (at 0.75 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "HV_2") (pinfunction "12") (pintype "passive"))
    (pad "13" smd rect locked (at 1.25 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "sig_2") (pinfunction "13") (pintype "passive"))
    (pad "14" smd rect locked (at 1.75 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "SDA_2") (pinfunction "14") (pintype "passive"))
    (pad "15" smd rect locked (at 2.25 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "SCL_2") (pinfunction "15") (pintype "passive"))
    (pad "16" smd rect locked (at 2.75 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "HV_3") (pinfunction "16") (pintype "passive"))
    (pad "17" smd rect locked (at 3.25 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "sig_3") (pinfunction "17") (pintype "passive"))
    (pad "18" smd rect locked (at 3.75 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "SCL_3") (pinfunction "18") (pintype "passive"))
    (pad "19" smd rect locked (at 4.25 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "SDA_3") (pinfunction "19") (pintype "passive"))
    (pad "20" smd rect locked (at 4.75 0 270) (size 0.7 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "3v3") (pinfunction "20") (pintype "passive"))
    (pad "S1" smd rect locked (at -5.54 -2.65 270) (size 1 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" smd rect locked (at 5.54 -2.65 270) (size 1 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at -7.62 -4.064 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.778 90) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 7 "SCL_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at -10.16 6.604 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 1.27 1.778 90) (layer "B.SilkS"))
    (fp_text value "200" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 14 "sig_0") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 2.54 -14.732)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "50" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 21 "HV_2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 4 "Net-(C3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 2.54 10.414 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 5 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at -6.096 1.524 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "detBoard.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 6 "3v3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start -17.145 17.145) (end 17.145 -17.145) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "det_2" (at 3.048 -4.318) (layer "B.SilkS"))
  (gr_text "det_1" (at -13.97 -2.54) (layer "B.SilkS"))
  (gr_text "det_0" (at -13.462 13.208) (layer "B.SilkS"))
  (gr_text "DetArray V0.1" (at 5.842 15.494) (layer "B.SilkS"))
  (gr_text "det_3" (at 2.794 13.462) (layer "B.SilkS"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17.018 17.018)
        (xy -17.018 17.018)
        (xy -17.018 -17.018)
        (xy 17.018 -17.018)
      )
    )
  )
)
