(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 35)
    (zones 0)
    (modules 18)
    (nets 13)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 +5V)
  (net 10 GND)
  (net 11 "Net-(J5-Pad1)")
  (net 12 "Net-(J9-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J9-Pad1)")
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2A66A)
    (at 147.955 51.435)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J1 (at 0 -2.54) (layer F.Fab))
    (fp_text value 5V (at -3.81 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 9 +5V))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2A647)
    (at 147.955 46.99)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J2 (at 0 -2.54) (layer F.Fab))
    (fp_text value GND (at -3.81 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 10 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2A618)
    (at 147.955 66.675)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J5 (at 0 -2.54) (layer F.Fab))
    (fp_text value Y_IN (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 11 "Net-(J5-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2A5F1)
    (at 147.955 57.785)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J3 (at 0 -2.54) (layer F.Fab))
    (fp_text value Pr_IN (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2A5C5)
    (at 95.25 57.785)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J7 (at 0 -2.54) (layer F.Fab))
    (fp_text value Pr_OUT (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2A595)
    (at 147.955 62.23)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J4 (at 0 -2.54) (layer F.Fab))
    (fp_text value Pb_IN (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 2.54) (layers Top F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2A56F)
    (at 95.25 62.23)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J8 (at 0 -2.54) (layer F.Fab))
    (fp_text value Pb_OUT (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2A544)
    (at 95.25 66.675)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J9 (at 0 -2.54) (layer F.Fab))
    (fp_text value Y_OUT (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 12 "Net-(J9-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_5x10mm (layer Top) (tedit 63F2A50B)
    (at 95.25 46.99)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd virtual)
    (fp_text reference J6 (at 0 -2.54) (layer F.Fab))
    (fp_text value GND (at 3.81 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5.08 2.54) (layers Top F.Paste F.Mask)
      (net 10 GND))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer Top) (tedit 5AE5139B)
    (at 139.065 66.675 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 2.54) (layer F.SilkS))
    (fp_text value "10 ohm" (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J9-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer Top) (tedit 5AE5139B)
    (at 107.95 54.61 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 -2.37 90) (layer F.SilkS))
    (fp_text value "75 ohm" (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer Top) (tedit 5AE5139B)
    (at 114.935 46.99 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 2.54 90) (layer F.SilkS))
    (fp_text value "75 ohm" (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer Top) (tedit 5A1DD157)
    (at 123.825 61.595)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer Top) (tedit 5A1DD157)
    (at 123.825 53.975)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer Top) (tedit 5AE50CD5)
    (at 131.445 60.96)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 3.81 -2.12) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer Top) (tedit 5AE50CD5)
    (at 131.445 55.245)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 3.81 -2.12) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.81 2.12) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.SilkS))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user %R (at 4.11 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 107.95 63.5 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1.25 4.445) (layer F.SilkS))
    (fp_text value "220 uF" (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer Top) (tedit 5AE50EF0)
    (at 117.475 63.5 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 4.445) (layer F.SilkS))
    (fp_text value "220 uF" (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "S-ENC-YUV Mini-A v1.1\nKPackLabs 2023-03" (at 130.175 46.99) (layer F.SilkS))
  (gr_line (start 151.765 44.45) (end 151.765 69.215) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.44 44.45) (end 151.765 44.45) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.44 69.215) (end 91.44 44.45) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.765 69.215) (end 91.44 69.215) (layer Edge.Cuts) (width 0.1))
  (gr_text INPUT (at 142.24 62.23 90) (layer F.SilkS))
  (gr_text OUTPUT (at 100.965 62.23 90) (layer F.SilkS))
  (gr_text Y (at 144.145 66.675 90) (layer F.SilkS))
  (gr_text Pb (at 144.145 62.23 90) (layer F.SilkS))
  (gr_text Pr (at 144.145 57.785 90) (layer F.SilkS))
  (gr_text Y (at 99.06 66.675 90) (layer F.SilkS))
  (gr_text Pb (at 99.06 62.23 90) (layer F.SilkS))
  (gr_text Pr (at 99.06 57.785 90) (layer F.SilkS))
)
